<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-1.27" x2="50.165" y2="-1.27" width="0" layer="20"/>
<wire x1="50.165" y1="-1.27" x2="50.165" y2="19.685" width="0" layer="20"/>
<wire x1="50.165" y1="19.685" x2="50.145" y2="53.01" width="0" layer="20"/>
<wire x1="50.145" y1="53.01" x2="0" y2="53.01" width="0" layer="20"/>
<wire x1="0" y1="53.01" x2="0" y2="-1.27" width="0" layer="20"/>
<text>GROUND</text>
<text>5v</text>
<text>3.3v</text>
<text>RESET</text>
<text>CAN1</text>
<text>Rx</text>
<text>Tx</text>
<text>SPI0</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>C4</text>
<text>IO20</text>
<text>IO21</text>
<text>IO22</text>
<text>IO23</text>
<text>I2C0</text>
<text>SCL</text>
<text>SDA</text>
<text>UART0</text>
<text>RTS</text>
<text>CTS</text>
<text>Rx</text>
<text>Tx</text>
<text>ADC1</text>
<text>ADC2</text>
<text>DP</text>
<text>DP</text>
<text>DM</text>
<text>DM</text>
<text>I2C1</text>
<text>UART1</text>
<text>SPI0</text>
<text>SCL</text>
<text>SDA</text>
<text>Tx</text>
<text>Rx</text>
<text>CTS</text>
<text>RTS</text>
<text>C0</text>
<text>SCK</text>
<text>SO</text>
<text>SI</text>
<text>JTAG</text>
<text>10uF</text>
<text>.1uF</text>
<text>.33uF</text>
<text>5v</text>
<text>3.3v</text>
<text>MRDT Dev Brd V1.1</text>
<text>12.30.2013</text>
</plain>
<libraries>
<library name="freescale_lqfp_m4">
<packages>
<package name="QFP50P1600X1600X170-100N">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220-IGO">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="freescale_lqfp_m4" package="QFP50P1600X1600X170-100N" value="MK10DN512ZVLL10">
<attribute name="PACKAGE" value="LQFP-100"/>
<attribute name="OC_NEWARK" value="75T7577"/>
<attribute name="MPN" value="MK10DN512ZVLL10"/>
<attribute name="SUPPLIER" value="FREESCALE SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="2070276"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="TO220-IGO" value=""/>
<element name="IC2" library="SparkFun-PowerIC" package="TO220-IGO" value=""/>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-5MM" value=""/>
<element name="C2" library="SparkFun-Passives" package="CAP-PTH-5MM" value=""/>
<element name="C4" library="SparkFun-Passives" package="CAP-PTH-5MM" value="10u"/>
<element name="C5" library="SparkFun-Passives" package="CAP-PTH-5MM" value=".33u">
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="CAP-PTH-5MM" value=".1u"/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="JTAG_CON" library="SparkFun-Connectors" package="2X10" value="M10X2"/>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP2" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP3" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="JP4" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="Y6" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value="32MHz">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VBAT">
<contactref element="U1" pad="30"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="60"/>
<contactref element="U1" pad="88"/>
<contactref element="U1" pad="74"/>
<contactref element="IC2" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="41"/>
<contactref element="U1" pad="49"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="24"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JTAG_CON" pad="4"/>
<contactref element="JTAG_CON" pad="6"/>
<contactref element="JTAG_CON" pad="8"/>
<contactref element="JTAG_CON" pad="10"/>
<contactref element="JTAG_CON" pad="12"/>
<contactref element="JTAG_CON" pad="14"/>
<contactref element="JTAG_CON" pad="20"/>
<contactref element="JTAG_CON" pad="16"/>
<contactref element="JTAG_CON" pad="18"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP3" pad="9"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="+3V3">
<contactref element="IC2" pad="OUT"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="40"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U1" pad="75"/>
<contactref element="U1" pad="89"/>
<contactref element="U1" pad="61"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="23"/>
<contactref element="JTAG_CON" pad="1"/>
<contactref element="JTAG_CON" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP4" pad="8"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="52"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="R1" pad="P$1"/>
<contactref element="JTAG_CON" pad="15"/>
</signal>
<signal name="V+">
<contactref element="IC1" pad="IN"/>
<contactref element="C5" pad="1"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="OUT"/>
<contactref element="IC2" pad="IN"/>
<contactref element="C6" pad="1"/>
<contactref element="JP4" pad="9"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="JTAG_TCLK">
<contactref element="U1" pad="34"/>
<contactref element="JTAG_CON" pad="9"/>
</signal>
<signal name="JTAG_TDI">
<contactref element="U1" pad="35"/>
<contactref element="JTAG_CON" pad="5"/>
</signal>
<signal name="JTAG_TDO">
<contactref element="U1" pad="36"/>
<contactref element="JTAG_CON" pad="13"/>
</signal>
<signal name="JTAG_TMS">
<contactref element="U1" pad="37"/>
<contactref element="JTAG_CON" pad="7"/>
</signal>
<signal name="JTAG_TRST">
<contactref element="U1" pad="39"/>
</signal>
<signal name="JTAG-TRST">
<contactref element="JTAG_CON" pad="3"/>
</signal>
<signal name="UART1_TX">
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="UART1_RX">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="UART1_CTS">
<contactref element="U1" pad="3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="UART1_RTS">
<contactref element="U1" pad="4"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SPI0_C0">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="SPI0_SCK">
<contactref element="U1" pad="11"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="SPI0_SOUT">
<contactref element="U1" pad="12"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="SPI0_SIN">
<contactref element="U1" pad="13"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="SPI0_C4">
<contactref element="U1" pad="70"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="SPI0_C3">
<contactref element="U1" pad="71"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SPI0_C2">
<contactref element="U1" pad="72"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SPI0_C1">
<contactref element="U1" pad="73"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="ADC0_DP">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="ADC0_DM">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="ADC1_DP">
<contactref element="U1" pad="16"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="ADC1_DM">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="DAC0_OUT">
<contactref element="U1" pad="27"/>
</signal>
<signal name="I2C0_SCL">
<contactref element="U1" pad="53"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="12C0_SDA">
<contactref element="U1" pad="54"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="UART0_TX">
<contactref element="U1" pad="44"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="UART0_RX">
<contactref element="U1" pad="45"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="UART0_CTS">
<contactref element="U1" pad="46"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="UART0_RTS">
<contactref element="U1" pad="47"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GPIO20">
<contactref element="U1" pad="66"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="GPIO21">
<contactref element="U1" pad="67"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="GPIO22">
<contactref element="U1" pad="68"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="GPIO23">
<contactref element="U1" pad="69"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="U1" pad="82"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="U1" pad="83"/>
<contactref element="JP2" pad="2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="CAN1_RX">
<contactref element="U1" pad="90"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="CAN1_TX">
<contactref element="U1" pad="91"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$37">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$8">
<contactref element="U1" pad="50"/>
<contactref element="Y6" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C1" pad="1"/>
<contactref element="Y6" pad="1"/>
<contactref element="U1" pad="51"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
