(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 15)
    (zones 0)
    (modules 21)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 3.35)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
  )
  (module Diode_SMD:D_2512_6332Metric (layer F.Cu) (tedit 5E619E68)
    (at -6.19758 84.984 90)
    (descr "Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_2512_6332Metric (layer F.Cu) (tedit 5E619E6C)
    (at 3.80242 84.984 90)
    (descr "Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_2512_6332Metric (layer F.Cu) (tedit 5E619E63)
    (at -16.256 84.984 90)
    (descr "Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value LED (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -2.9 0 90) (size 1.35 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -3.16482 75.03414)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -1.32586 75.0189)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -3.11656 94.55658)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -1.2776 94.54134)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -2.25042 75.02906)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -2.20216 94.5515)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 3.77956 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -6.22044 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 3.80496 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -6.19504 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -13.11656 94.55658)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -11.2776 94.54134)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -12.20216 94.5515)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -11.32586 75.0189)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -13.16482 75.03414)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5D8333)
    (at -12.25042 75.02906)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -16.22044 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -16.19504 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_line (start -21.0947 75.69454) (end 9.144 75.692) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 9.144 96.3168) (end 9.144 75.69454) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -1.2649 77.75448) (end -1.2649 94.25178) (layer Edge.Cuts) (width 2))
  (gr_line (start -21.09724 96.3168) (end 9.144 96.3168) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -21.09724 96.01454) (end -21.09724 96.3168) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -11.2649 77.75448) (end -11.2649 94.25178) (layer Edge.Cuts) (width 2))
  (gr_line (start -21.09724 93.18498) (end -21.09724 96.01454) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -21.09724 79.16164) (end -21.0947 75.69454) (layer Edge.Cuts) (width 0.05))
  (dimension 1.64592 (width 0.12) (layer Dwgs.User)
    (gr_text "1.646 mm" (at -23.70836 81.30794 90) (layer Dwgs.User))
    (feature1 (pts (xy -16.00708 80.48498) (xy -23.024781 80.48498)))
    (feature2 (pts (xy -16.00708 82.1309) (xy -23.024781 82.1309)))
    (crossbar (pts (xy -22.43836 82.1309) (xy -22.43836 80.48498)))
    (arrow1a (pts (xy -22.43836 80.48498) (xy -21.851939 81.611484)))
    (arrow1b (pts (xy -22.43836 80.48498) (xy -23.024781 81.611484)))
    (arrow2a (pts (xy -22.43836 82.1309) (xy -21.851939 81.004396)))
    (arrow2b (pts (xy -22.43836 82.1309) (xy -23.024781 81.004396)))
  )
  (dimension 1.64592 (width 0.12) (layer Dwgs.User)
    (gr_text "1.646 mm" (at -23.8252 91.12758 90) (layer Dwgs.User))
    (feature1 (pts (xy -16.12392 90.30462) (xy -23.141621 90.30462)))
    (feature2 (pts (xy -16.12392 91.95054) (xy -23.141621 91.95054)))
    (crossbar (pts (xy -22.5552 91.95054) (xy -22.5552 90.30462)))
    (arrow1a (pts (xy -22.5552 90.30462) (xy -21.968779 91.431124)))
    (arrow1b (pts (xy -22.5552 90.30462) (xy -23.141621 91.431124)))
    (arrow2a (pts (xy -22.5552 91.95054) (xy -21.968779 90.824036)))
    (arrow2b (pts (xy -22.5552 91.95054) (xy -23.141621 90.824036)))
  )
  (gr_line (start -21.09724 93.18498) (end -21.09724 79.16164) (layer Edge.Cuts) (width 0.05))
)
