(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(BZ1-Pad1)")
  (net 2 "GND")
  (net 3 "BUZZ")
  (net 4 "Net-(Q1-Pad3)")
  (net 5 "+5V")
  (footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6" (layer "F.Cu")
    (tedit 5A030281)
    (at 121.5 85)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags "buzzer")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BZ1" (at 3.8 -7.2) (layer "F.SilkS") hide)
    (fp_text value "Buzzer" (at 3.8 7.4) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.01 -2.54) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.8 -4) (layer "F.Fab") hide)
    (fp_text user "+" (at -0.01 -2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BZ1-Pad1)") (pinfunction "-") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.6 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 124.6 88.375)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.4) (layer "B.SilkS") hide)
    (fp_text value "BC817" (at 0 -2.4) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "BUZZ") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(BZ1-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(Q1-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 125.25 81 180)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 2.54) (layer "B.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.54) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 127.25 81 180)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 2.54) (layer "B.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.54) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "B.Cu")
    (tedit 5DD6EB27)
    (at 123.25 81 180)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 2.54) (layer "B.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.54) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at 0 0 180) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "BUZZ") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 127.6 88.2 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Micro beeper.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 90) (layer "B.SilkS") hide)
    (fp_text value "R" (at 0 -1.43 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 125.25 85) (mid 125.25 85) (end 125.25 85) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 125.25 85) (end 131 86.75) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "-" (at 127.25 83) (layer "B.SilkS"))
  (gr_text "+" (at 125.25 83) (layer "B.SilkS"))
  (gr_text "B" (at 123.25 83.25) (layer "B.SilkS"))
)
