(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 43)
    (no_connects 0)
    (area 179.006499 60.896499 215.963501 83.883501)
    (thickness 1.6002)
    (drawings 11)
    (tracks 144)
    (zones 0)
    (modules 22)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 Vin)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 Vout)
  (net 5 Ven)
  (net 6 Vadj)
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(R2-Pad2)")
  (net 9 "Net-(T1-Pad3)")
  (net 10 "Net-(T1-Pad12)")
  (net 11 "Net-(T1-Pad11)")
  (net 12 "Net-(T1-Pad10)")
  (net 13 "Net-(D1-PadA)")
  (net 14 "Net-(Cc1-Pad2)")
  (net 15 "Net-(Cc1-Pad1)")
  (net 16 "Net-(Cs1-Pad2)")
  (net 17 "Net-(Rf1-Pad2)")
  (net 18 "Net-(Q1-Pad5)")
  (net 19 "Net-(Q1-Pad4)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(Cc1-Pad1)")
    (add_net "Net-(Cc1-Pad2)")
    (add_net "Net-(Cs1-Pad2)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(Rf1-Pad2)")
    (add_net "Net-(T1-Pad10)")
    (add_net "Net-(T1-Pad11)")
    (add_net "Net-(T1-Pad12)")
    (add_net "Net-(T1-Pad3)")
    (add_net Vadj)
    (add_net Ven)
    (add_net Vin)
    (add_net Vout)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 209.931 79.907 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 Vin))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 190.119 77.597 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 188.214 64.77 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 0 0 360) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 Vout))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D4214D)
    (at 187.579 78.105 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cc1 (at -1.651 0 180) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Cc1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Cc1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59D4211F)
    (at 197.739 70.739 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cs1 (at -2.032 -0.127 180) (layer F.SilkS))
    (fp_text value 560pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Cs1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 Vin))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-DO-219AB (layer F.Cu) (tedit 59CC5F67)
    (at 195.072 63.119)
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "ES1FL R3G" (at 0 0) (layer F.SilkS) hide)
    (pad A smd rect (at 1.5494 0 180) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-PadA)"))
    (pad C smd rect (at -1.5494 0) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 Vout))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 59CC5F9A)
    (at 180.34 66.04 90)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J2 (at 0.254 -1.7018 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0.5588 1.7272 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 Vout))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 184.404 64.262 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.905 360) (layer F.SilkS))
    (fp_text value 604k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 Vout))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 184.404 67.437 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.127 -1.778 360) (layer F.SilkS))
    (fp_text value 604k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 183.769 81.915 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.409 360) (layer F.SilkS))
    (fp_text value 10.2k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 183.896 70.866)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 30k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Vadj))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 59D42147)
    (at 185.674 77.978 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rc1 (at 0 2.286 360) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Cc1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 59D42130)
    (at 187.452 71.501)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference Rf1 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 Ven))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Rf1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010 (layer F.Cu) (tedit 59D42140)
    (at 188.468 74.295 180)
    (descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference Rsen1 (at -0.381 -2.032 360) (layer F.SilkS))
    (fp_text value 0.06 (at 0 2.4 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.45 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2.45 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59D42114)
    (at 197.739 67.056 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference Rs1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 249 (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Cs1-Pad2)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-WE-FLEX_ER11_5 (layer F.Cu) (tedit 59CD857C)
    (at 206.375 68.453 90)
    (attr smd)
    (fp_text reference T1 (at 0 0.508 180) (layer F.SilkS))
    (fp_text value WE-FLEX_ER11_5 (at -8.128 0.254 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 4.99872 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-PadA)"))
    (pad 2 smd rect (at 2.99974 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
    (pad 3 smd rect (at 0.99822 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(T1-Pad3)"))
    (pad 4 smd rect (at -0.99822 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(T1-Pad3)"))
    (pad 5 smd rect (at -2.99974 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 1 Vin))
    (pad 6 smd rect (at -4.99872 -5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(T1-Pad12)"))
    (pad 7 smd rect (at -4.99872 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(T1-Pad11)"))
    (pad 8 smd rect (at -2.99974 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.99822 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(T1-Pad10)"))
    (pad 10 smd rect (at 0.99822 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(T1-Pad10)"))
    (pad 11 smd rect (at 2.99974 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(T1-Pad11)"))
    (pad 12 smd rect (at 4.99872 5.97408 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(T1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 59CC5F94)
    (at 180.34 71.12 270)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J3 (at 0.254 2.286 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0.5588 1.7272 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 Vadj))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 Ven))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 59CC5FA3)
    (at 213.36 81.28 90)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J1 (at 0.254 -1.7018 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0.5588 1.7272 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 Vin))
  )
  (module nixiemisc:nixiemisc-SOIC8 (layer F.Cu) (tedit 59CC7C2E)
    (at 194.564 76.327)
    (descr "SMALL OUTLINE IC")
    (tags "SMALL OUTLINE IC")
    (attr smd)
    (fp_text reference U1 (at -3.302 -1.27 90) (layer F.SilkS) hide)
    (fp_text value LM3478SOIC8 (at 3.302 -1.905 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -0.635 2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Cc1-Pad1)"))
    (pad 3 smd rect (at 0.635 2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at 1.905 2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.905 -2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.635 -2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad4)"))
    (pad 7 smd rect (at -0.635 -2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Rf1-Pad2)"))
    (pad 8 smd rect (at -1.905 -2.59842) (size 0.59944 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 1 Vin))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 205.867 79.629 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module logos:Symbol_HighVoltage_Type2_SilkTop_VerySmall (layer F.Cu) (tedit 59CD8338)
    (at 201.422 79.502)
    (descr "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (tags "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (fp_text reference REF** (at -0.127 -5.715) (layer F.SilkS) hide)
    (fp_text value Symbol_HighVoltage_Type2_CopperTop_VerySmall (at -0.381 4.572) (layer F.Fab))
  )
  (module nixiemisc:nixiemisc-SO08 (layer F.Cu) (tedit 59D4358B)
    (at 193.294 68.44792)
    (descr "SOIC, 0.15 INCH WIDTH")
    (tags "SOIC, 0.15 INCH WIDTH")
    (attr smd)
    (fp_text reference Q1 (at -3.4798 0 180) (layer F.SilkS))
    (fp_text value AO4294 (at 3.5052 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.905 2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -0.635 2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0.635 2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 1.905 2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad4)"))
    (pad 5 smd rect (at 1.905 -2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
    (pad 6 smd rect (at 0.635 -2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
    (pad 7 smd rect (at -0.635 -2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
    (pad 8 smd rect (at -1.905 -2.79908) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad5)"))
  )
  (gr_text Ven (at 181.737 73.66 270) (layer F.SilkS))
  (gr_text Vadj (at 181.864 71.12 270) (layer F.SilkS))
  (gr_text GND (at 181.864 66.04 270) (layer F.SilkS))
  (gr_text HV (at 181.991 63.627 270) (layer F.SilkS))
  (gr_text GND (at 215.011 81.28 90) (layer F.SilkS))
  (gr_text 3V-12V (at 215.011 78.486 90) (layer F.SilkS))
  (gr_text "nixies.us\nhvps v0.1" (at 204.724 80.645) (layer B.Mask))
  (gr_line (start 215.9 60.96) (end 179.07 60.96) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 215.9 83.82) (end 215.9 60.96) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 179.07 83.82) (end 215.9 83.82) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 179.07 60.96) (end 179.07 83.82) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.324 61.214) (xy 179.324 83.566) (xy 215.646 83.566) (xy 215.646 61.214)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.438 62.484) (xy 202.438 74.041) (xy 210.693 74.041) (xy 210.693 61.214) (xy 202.438 61.214)
        (xy 202.438 62.865)
      )
    )
  )
  (zone (net 12) (net_name "Net-(T1-Pad10)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.487 66.675) (xy 213.487 70.231) (xy 211.201 70.231) (xy 211.201 66.675)
      )
    )
  )
  (zone (net 9) (net_name "Net-(T1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.263 66.675) (xy 199.263 70.231) (xy 201.549 70.231) (xy 201.549 66.675)
      )
    )
  )
  (zone (net 1) (net_name Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.549 72.263) (xy 201.549 70.612) (xy 197.104 70.612) (xy 197.104 75.057) (xy 193.294 75.057)
        (xy 193.294 72.263) (xy 191.77 72.263) (xy 191.77 77.343) (xy 197.231 77.343) (xy 197.231 81.28)
        (xy 207.264 81.28) (xy 207.264 80.137) (xy 214.884 80.137) (xy 214.884 77.216) (xy 201.803 77.216)
        (xy 198.755 74.168) (xy 198.755 72.263)
      )
    )
  )
  (zone (net 18) (net_name "Net-(Q1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.549 66.294) (xy 201.549 64.643) (xy 190.627 64.643) (xy 190.627 66.929) (xy 198.882 66.929)
        (xy 198.882 66.294)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.31 71.882) (xy 194.31 69.85) (xy 189.484 69.85) (xy 189.484 76.835) (xy 190.119 76.835)
        (xy 190.119 78.613) (xy 191.77 80.01) (xy 193.04 80.01) (xy 193.04 77.724) (xy 191.389 77.724)
        (xy 191.389 71.882)
      )
    )
  )
)
