(kicad_pcb (version 4) (host pcbnew 4.0.3-rc7-stable)
  (general
    (links 58)
    (no_connects 0)
    (area 126.224999 72.324999 168.508001 91.775001)
    (thickness 1.6)
    (drawings 17)
    (tracks 151)
    (zones 0)
    (modules 25)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.1)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 143.2 70.1236)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /Users/armil/projects/sensorboard/hardware/sensorboard/gerber/))
  )
  (net 0 "")
  (net 1 +6V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 TXD)
  (net 5 RXD)
  (net 6 GPIO0)
  (net 7 GPIO16)
  (net 8 CH_PD)
  (net 9 GPIO15)
  (net 10 "Net-(U1-Pad11)")
  (net 11 ADC_IN)
  (net 12 "Net-(C6-Pad1)")
  (net 13 "Net-(C6-Pad2)")
  (net 14 "Net-(R7-Pad2)")
  (net 15 "Net-(R9-Pad2)")
  (net 16 "Net-(U1-Pad5)")
  (net 17 "Net-(U1-Pad6)")
  (net 18 "Net-(U1-Pad7)")
  (net 19 SDL)
  (net 20 SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +6V)
    (add_net ADC_IN)
    (add_net CH_PD)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO15)
    (add_net GPIO16)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net RXD)
    (add_net SDA)
    (add_net SDL)
    (add_net TXD)
  )
  (net_class 3v3 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 563E9BC6)
    (at 163.8 74.5236)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 4.826 2.794 270) (layer F.SilkS) hide)
    (fp_text value PROG (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 TXD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 RXD))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO0))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 CH_PD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP8266:ESP-12 (layer F.Cu) (tedit 563E9CAC)
    (at 144.7 74.7236)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 7.0989 14.6764) (layer F.SilkS) hide)
    (fp_text value ESP-07v2 (at 6.992 1) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 GPIO16))
    (pad 2 smd oval (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 ADC_IN))
    (pad 3 smd oval (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 CH_PD))
    (pad 4 smd oval (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 GPIO16))
    (pad 5 smd oval (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad6)"))
    (pad 7 smd oval (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad7)"))
    (pad 8 smd oval (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd oval (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd oval (at 14 12) (size 2.5 1.1) (drill (offset 0.6 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 GPIO15))
    (pad 11 smd oval (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad11)"))
    (pad 12 smd oval (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 GPIO0))
    (pad 13 smd oval (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 20 SDA))
    (pad 14 smd oval (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 SDL))
    (pad 15 smd oval (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 RXD))
    (pad 16 smd oval (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 TXD))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 57814008)
    (at 132.75 84.4736)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -0.05 1.55 180) (layer F.SilkS))
    (fp_text value "60V 1A" (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57813136)
    (at 137.45 89.1736 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.5 2.5 270) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +6V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (zone_connect 2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 57813F9E)
    (at 129.95 86.9736)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U2 (at -0.6 -2.35) (layer F.SilkS))
    (fp_text value LMR16006Y (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R9-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:FGA8 (layer F.Cu) (tedit 5702A1FF)
    (at 166.2 88.3236)
    (solder_mask_margin 0.02)
    (fp_text reference U3 (at 0 -2.667 180) (layer F.SilkS))
    (fp_text value BME280 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.975 -1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -0.975 1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -0.325 -1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at -0.325 1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.325 -1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 SDA))
    (pad 6 smd rect (at 0.325 1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 0.975 -1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 SDL))
    (pad 5 smd rect (at 0.975 1.275) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813F1E)
    (at 166.5 82.2236)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 1.55 -0.05 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 SDL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813F3D)
    (at 166.5 83.8236)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.55 0.05 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 SDA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813FAA)
    (at 132.4 90.3236 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -1.7 0 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813FDF)
    (at 127.8 89.8236 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.1 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813FCA)
    (at 129.5 89.8236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.15 90) (layer F.SilkS))
    (fp_text value 33k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57814052)
    (at 129.7 74.5236 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.7 0 360) (layer F.SilkS))
    (fp_text value 47K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 ADC_IN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57814042)
    (at 128 74.5236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.75 0.05 180) (layer F.SilkS))
    (fp_text value 470K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 ADC_IN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813F5A)
    (at 141.4 85.6236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.7 0.05 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 GPIO16))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813EDC)
    (at 162.3 86.0236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.7 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 GPIO15))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57813ED9)
    (at 164 86.0236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.7 -0.05 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 GPIO0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5781404A)
    (at 131.4 74.5236 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.7 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 CH_PD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57814018)
    (at 127.3 85.1236 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.95 -0.5 270) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57813EF1)
    (at 162.3 88.8236 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.8 0 540) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57813F60)
    (at 141.4 88.5236 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -1.85 0 180) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57813F01)
    (at 163.8 88.8236 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.85 0 360) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_Reflow (layer F.Cu) (tedit 57813F6D)
    (at 137.5 79.7236 270)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow")
    (tags "Tantal Capacitor Size-D EIA-7343 Reflow")
    (attr smd)
    (fp_text reference C7 (at 1 0 360) (layer F.SilkS))
    (fp_text value 100uf (at -0.09906 3.59918 270) (layer F.Fab))
    (pad 2 smd rect (at 3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 smd rect (at -3.12 0 270) (size 2.37 2.43) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57813F82)
    (at 134.2 79.7236 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.15 0 360) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57813FF1)
    (at 133.55 88.1736)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.15 0.65 90) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +6V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:NR4018 (layer F.Cu) (tedit 57814058)
    (at 129.55 80.6736 90)
    (descr http://www.yuden.co.jp/productdata/catalog/en/wound04_e.pdf)
    (attr smd)
    (fp_text reference L1 (at 3.25 0.05 180) (layer F.SilkS))
    (fp_text value 10uh (at 0 -3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.6 3.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.6 3.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
  )
  (gr_line (start 168.425 91.5486) (end 168.425 91.4736) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.45 72.4236) (end 168.45 72.6236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 161.5 79.6236 90) (layer F.SilkS))
  (gr_text RX (at 161.5 77.1236 90) (layer F.SilkS))
  (gr_text TX (at 161.5 74.4236 90) (layer F.SilkS))
  (gr_line (start 126.3 91.6) (end 126.3 91.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.433 91.6) (end 126.3 91.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.3 72.4) (end 168.433 72.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.433 72.517) (end 168.433 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "ESP sensorboard v4.2" (at 148.1 74.0736) (layer B.SilkS))
  (gr_text z2amiller (at 151.85 89.7236) (layer B.SilkS))
  (gr_text PROG (at 163.1 82.1236) (layer F.SilkS))
  (gr_text "ESP-07\nESP-12" (at 151.9 77.9236) (layer F.SilkS))
  (gr_text "+ PWR" (at 139.95 87.5736 90) (layer F.SilkS))
  (gr_line (start 126.3 72.4) (end 126.3 91.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.3 72.7) (xy 126.3 91.6) (xy 168.3 91.4) (xy 168.3 72.5236) (xy 126.3 72.4)
        (xy 126.3 72.7)
      )
    )
  )
  (zone (net 1) (net_name +6V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.4 89.4236) (xy 135.6 89.4236) (xy 135.6 88.1236) (xy 138.8 88.1236) (xy 138.8 91.0236)
        (xy 131.8 91.0236) (xy 131.8 87.4236) (xy 130.3 87.4236) (xy 130.3 86.5236) (xy 133.4 86.5236)
        (xy 133.4 89.4236)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.1 86.5236) (xy 129.6 86.5236) (xy 129.6 87.4236) (xy 128.1 87.4236) (xy 127.1 88.4236)
        (xy 127.1 90.1236) (xy 128.5 90.1236) (xy 128.5 91.1236) (xy 127 91.1236) (xy 126.7 91.1236)
        (xy 126.7 86.5236) (xy 128.1 86.5236)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C6-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.2 86.4236) (xy 130.3 86.4236) (xy 130.3 85.2236) (xy 126.6 85.2236) (xy 126.6 81.3236)
        (xy 132.2 81.3236) (xy 132.2 86.4236)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.8 87.9236) (xy 135.4 87.9236) (xy 135.4 89.2236) (xy 133.6 89.2236) (xy 133.6 81.6236)
        (xy 133.4 81.6236) (xy 133.4 80.0236) (xy 138.9 80.0236) (xy 138.9 87.9236) (xy 138.8 87.9236)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.9 79.5236) (xy 132.6 79.5236) (xy 132 80.1236) (xy 127 80.1236) (xy 127 77.7236)
        (xy 133.6 77.7236) (xy 136.1 75.2236) (xy 138.9 75.2236) (xy 138.9 79.5236)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.3 91.4236) (xy 139.2 91.4236) (xy 139.2 72.5236) (xy 168.3 72.5236) (xy 168.3 91.4236)
      )
    )
  )
)
