(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 6)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BAT1-PadNeg)")
  (net 2 "Net-(BAT1-PadPos)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net "Net-(BAT1-PadNeg)")
    (add_net "Net-(BAT1-PadPos)")
  )
  (module Custom:SMD-Battery (layer F.Cu) (tedit 5F289AF6)
    (at 119.38 114.554 45)
    (fp_text reference BAT1 (at 0 -2.54 45) (layer F.SilkS))
    (fp_text value BS-7 (at 0 -5.08 45) (layer F.Fab))
    (pad Neg smd rect (at 0 -12.95 45) (size 3.75 4.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BAT1-PadNeg)"))
    (pad Pos smd rect (at 0 10.95 45) (size 4.75 4.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BAT1-PadPos)"))
  )
  (module Custom:SolderWirePad_1x01_SMD_2x3mm (layer F.Cu) (tedit 5F289D71)
    (at 102.616 121.158 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference - (at -0.508 2.54) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 3.302 90) (layer F.Fab))
    (fp_text user %R (at 0.381 0.254 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BAT1-PadNeg)"))
  )
  (module Custom:SolderWirePad_1x01_SMD_2x3mm (layer F.Cu) (tedit 5F289D71)
    (at 102.616 124.46 90)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference + (at -0.762 2.54 180) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 3.302 90) (layer F.Fab))
    (fp_text user %R (at 0.381 0.254 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BAT1-PadPos)"))
  )
  (gr_arc (start 102.7938 102.7938) (end 99.9998 102.7938) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 102.7938 124.206) (end 99.9998 124.206) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.2098 124.206) (end 132.0038 124.206) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.2098 102.7938) (end 132.0038 102.7938) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "2032 Breakout" (at 116.332 112.268) (layer B.SilkS))
  (gr_text "2032 Breakout" (at 102.362 107.188 270) (layer F.SilkS))
  (gr_line (start 99.9998 102.7938) (end 99.9998 124.206) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.7938 127) (end 129.2098 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.0038 102.7938) (end 132.0038 124.206) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.7938 99.9998) (end 129.2098 99.9998) (layer Edge.Cuts) (width 0.05))
)
