<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="2" y1="39" x2="2" y2="5" width="0" layer="20"/>
<wire x1="2" y1="5" x2="6" y2="1" width="0" layer="20"/>
<wire x1="6" y1="1" x2="48" y2="1" width="0" layer="20"/>
<wire x1="48" y1="1" x2="52" y2="5" width="0" layer="20"/>
<wire x1="52" y1="5" x2="52" y2="40" width="0" layer="20"/>
<wire x1="52" y1="40" x2="46" y2="46" width="0" layer="20"/>
<wire x1="46" y1="46" x2="9" y2="46" width="0" layer="20"/>
<wire x1="9" y1="46" x2="2" y2="39" width="0" layer="20"/>
<text>2018 made with &lt;3   suchahardman.com
guitar effects made in berlin, germany</text>
<text>piece o' cake
overdrive</text>
<text>+9V</text>
<text>GND</text>
<text>IN</text>
<text>OUT</text>
</plain>
<libraries>
<library name="supply pins">
<packages>
<package name="PAD4">
<description>&lt;b&gt;Square (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
<package name="PAD2">
<description>&lt;b&gt;Round Pad (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
<library name="caps-film">
<packages>
<package name="0.2&quot;.LRG">
<description>0.2" (5.08mm) spacing
&lt;p&gt;
&lt;b&gt;1uF caps&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="caps-elec">
<packages>
<package name="0501">
<description>0.08" (2mm) spacing</description>
</package>
</packages>
</library>
<library name="integrated circuits">
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="16MM_B.MOUNT">
<description>&lt;b&gt;16mm / Right-Angle /  PC Mount / Short Pin&lt;/b&gt;
&lt;p&gt;
For bottom-mount potentiometers
&lt;p&gt;
&lt;a href="http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/"&gt;http://smallbear-electronics.mybigcommerce.com/alpha-single-gang-16mm-right-angle-pc-mount/&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.3&quot;.B">
<description>0.3"  (7.62mm) lead spacing, 1/4W (flat)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="9V" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="C1" library="caps-film" package="0.2&quot;.LRG" value="12nF"/>
<element name="C2" library="caps-elec" package="0501" value="10uF"/>
<element name="C3" library="caps-elec" package="0501" value="10uF"/>
<element name="C4" library="caps-film" package="0.2&quot;.LRG" value="82nF"/>
<element name="C5" library="caps-film" package="0.2&quot;.LRG" value="470pF"/>
<element name="C6" library="caps-film" package="0.2&quot;.LRG" value="12nF"/>
<element name="C7" library="caps-film" package="0.2&quot;.LRG" value="56nF"/>
<element name="C8" library="caps-film" package="0.2&quot;.LRG" value="12nF"/>
<element name="GND" library="supply pins" package="PAD4" value="PADS.SQR_NL"/>
<element name="IC1" library="integrated circuits" package="DIP08" value="LM741"/>
<element name="IN" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="OUT" library="supply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="DRIVE" library="potentiometers" package="16MM_B.MOUNT" value="50kC"/>
<element name="PRESENCE" library="potentiometers" package="16MM_B.MOUNT" value="22kA"/>
<element name="LEVEL" library="potentiometers" package="16MM_B.MOUNT" value="50kA"/>
<element name="R10" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="R11" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="R12" library="resistors" package="0.3&quot;.B" value="220k"/>
<element name="R2" library="resistors" package="0.3&quot;.B" value="100k"/>
<element name="R3" library="resistors" package="0.3&quot;.B" value="120k"/>
<element name="R4" library="resistors" package="0.3&quot;.B" value="1M"/>
<element name="R5" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="R6" library="resistors" package="0.3&quot;.B" value="120R"/>
<element name="R7" library="resistors" package="0.3&quot;.B" value="100k"/>
<element name="R8" library="resistors" package="0.3&quot;.B" value="10k"/>
<element name="R9" library="resistors" package="0.3&quot;.B" value="1k"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R12" pad="1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="2"/>
<contactref element="PRESENCE" pad="3"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="PRESENCE" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="PRESENCE" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="2"/>
<contactref element="LEVEL" pad="3"/>
</signal>
<signal name="OUT">
<contactref element="LEVEL" pad="2"/>
<contactref element="OUT" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="C3" pad="P$2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R6" pad="1"/>
<contactref element="DRIVE" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="P$1"/>
<contactref element="R12" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="DRIVE" pad="3"/>
<contactref element="LEVEL" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="P$2"/>
<contactref element="GND" pad="P$1"/>
</signal>
<signal name="9V">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="9V" pad="P$1"/>
</signal>
<signal name="IN">
<contactref element="C1" pad="1"/>
<contactref element="IN" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="6"/>
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
