(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 117)
    (no_connects 1)
    (area 116.764999 93.904999 157.555001 111.835001)
    (thickness 1.6)
    (drawings 56)
    (tracks 437)
    (zones 0)
    (modules 46)
    (nets 50)
  )
  (page A4)
  (layers
    (0 Top signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 Bottom signal)
    (33 F.Adhes user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1225)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (trace_clearance 0.1225)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1225)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.441)
    (via_drill 0.245)
    (via_min_size 0.441)
    (via_min_drill 0.245)
    (user_via 0.6615 0.3185)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 0.5 0.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.3 0.3)
    (mod_text_width 0.05)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(BATT+1-Pad1)")
  (net 2 "Net-(BATT-1-Pad1)")
  (net 3 GND)
  (net 4 3.3v)
  (net 5 vtest)
  (net 6 "Net-(C33-Pad1)")
  (net 7 5v)
  (net 8 "Net-(IC3-Pad10)")
  (net 9 "Net-(LED1-Pad1)")
  (net 10 "Net-(LED2-Pad1)")
  (net 11 "Net-(LED3-Pad1)")
  (net 12 "Net-(Q1-Pad2)")
  (net 13 "Net-(Q2-Pad2)")
  (net 14 "Net-(Q3-Pad2)")
  (net 15 audio+)
  (net 16 audio-)
  (net 17 amp_en)
  (net 18 SDA)
  (net 19 SCL)
  (net 20 sd_en)
  (net 21 "Net-(SD1-Pad8)")
  (net 22 "Net-(SD1-Pad9)")
  (net 23 "Net-(SD1-Pad10)")
  (net 24 "Net-(SD1-PadB)")
  (net 25 "Net-(SD1-Pad11)")
  (net 26 miso)
  (net 27 sclk)
  (net 28 mosi)
  (net 29 "Net-(SD1-Pad1)")
  (net 30 "Net-(SD1-Pad12)")
  (net 31 "Net-(SD1-PadA)")
  (net 32 "Net-(SP+1-Pad1)")
  (net 33 "Net-(SP-1-Pad1)")
  (net 34 INT)
  (net 35 "Net-(U1-Pad6)")
  (net 36 "Net-(U2-Pad9)")
  (net 37 "Net-(U2-Pad10)")
  (net 38 "Net-(U2-Pad11)")
  (net 39 "Net-(C11-Pad1)")
  (net 40 "Net-(C12-Pad1)")
  (net 41 "Net-(C13-Pad1)")
  (net 42 "Net-(C14-Pad1)")
  (net 43 "Net-(IC3-Pad3)")
  (net 44 "Net-(Q4-Pad2)")
  (net 45 "Net-(Q5-Pad2)")
  (net 46 "Net-(Q6-Pad2)")
  (net 47 "Net-(LED4-Pad1)")
  (net 48 "Net-(LED5-Pad1)")
  (net 49 "Net-(LED6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1225)
    (trace_width 0.1225)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3v)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(IC3-Pad10)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(SD1-Pad1)")
    (add_net "Net-(SD1-Pad10)")
    (add_net "Net-(SD1-Pad11)")
    (add_net "Net-(SD1-Pad12)")
    (add_net "Net-(SD1-Pad8)")
    (add_net "Net-(SD1-Pad9)")
    (add_net "Net-(SD1-PadA)")
    (add_net "Net-(SD1-PadB)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad9)")
  )
  (net_class POWER ""
    (clearance 0.1225)
    (trace_width 1.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BATT-1-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LED3-Pad1)")
    (add_net "Net-(LED4-Pad1)")
    (add_net "Net-(LED5-Pad1)")
    (add_net "Net-(LED6-Pad1)")
  )
  (net_class medium ""
    (clearance 0.1225)
    (trace_width 0.5)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5v)
    (add_net GND)
    (add_net "Net-(BATT+1-Pad1)")
    (add_net "Net-(SP+1-Pad1)")
    (add_net "Net-(SP-1-Pad1)")
    (add_net audio+)
    (add_net audio-)
  )
  (net_class narrow ""
    (clearance 0.1225)
    (trace_width 0.1225)
    (via_dia 0.441)
    (via_drill 0.245)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net INT)
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net SCL)
    (add_net SDA)
    (add_net amp_en)
    (add_net miso)
    (add_net mosi)
    (add_net sclk)
    (add_net sd_en)
    (add_net vtest)
  )
  (module lightsaber_footprints:WSON-10 (layer Top) (tedit 588E4D52)
    (at 146.05 98.806 270)
    (fp_text reference U1 (at -1.8 0.9 360) (layer F.SilkS))
    (fp_text value LM48310 (at 0 0 270) (layer F.Fab))
    (pad 11 smd rect (at 0 0 270) (size 2 1.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 41 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at -0.5 1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 42 "Net-(C14-Pad1)"))
    (pad 3 smd rect (at 0 1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 4 smd rect (at 0.5 1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 17 amp_en))
    (pad 5 smd rect (at 1 1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 6 smd rect (at 1 -1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 35 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 0.5 -1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 33 "Net-(SP-1-Pad1)"))
    (pad 8 smd rect (at 0 -1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd rect (at -0.5 -1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 10 smd rect (at -1 -1.4 270) (size 0.25 0.6) (layers Top F.Paste F.Mask)
      (net 32 "Net-(SP+1-Pad1)"))
  )
  (module modules:DM3D-SF (layer Top) (tedit 57DDA3BF)
    (at 121.1326 102.743 270)
    (descr "Micro SD")
    (tags "Micro SD")
    (solder_mask_margin 0.1)
    (solder_paste_margin -0.05)
    (fp_text reference SD1 (at 0 -12.0904 270) (layer F.SilkS))
    (fp_text value microsd_socket (at 1.5 -7 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.25 270) (layer F.Fab) hide)
    (pad 8 smd rect (at -4.5 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 21 "Net-(SD1-Pad8)"))
    (pad 9 smd rect (at -5.7 0.75 270) (size 1.3 1.5) (layers Top F.Paste F.Mask)
      (net 22 "Net-(SD1-Pad9)"))
    (pad 10 smd rect (at -5.95 -6.85 270) (size 0.8 1.5) (layers Top F.Paste F.Mask)
      (net 23 "Net-(SD1-Pad10)"))
    (pad B smd rect (at -5.625 -8.35 270) (size 1.45 1) (layers Top F.Paste F.Mask)
      (net 24 "Net-(SD1-PadB)"))
    (pad 11 smd rect (at 6 -7.5 270) (size 0.8 1.4) (layers Top F.Paste F.Mask)
      (net 25 "Net-(SD1-Pad11)"))
    (pad 7 smd rect (at -3.4 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 28 mosi))
    (pad 6 smd rect (at -2.3 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at -1.2 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 27 sclk))
    (pad 4 smd rect (at -0.1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 3 smd rect (at 1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 26 miso))
    (pad 2 smd rect (at 2.1 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 20 sd_en))
    (pad 1 smd rect (at 3.2 0.875 270) (size 0.55 1.75) (layers Top F.Paste F.Mask)
      (net 29 "Net-(SD1-Pad1)"))
    (pad 12 smd rect (at 5.65 0.75 270) (size 1.5 1.5) (layers Top F.Paste F.Mask)
      (net 30 "Net-(SD1-Pad12)"))
    (pad A smd rect (at 5.6 -9.8 270) (size 1 1.55) (layers Top F.Paste F.Mask)
      (net 31 "Net-(SD1-PadA)"))
  )
  (module lightsaber_footprints:teensy32++ (layer Top) (tedit 57F3461B)
    (at 135.89 102.87)
    (fp_text reference U0 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Teensy_3.1 (at -1.8415 -10.3505) (layer F.Fab) hide)
    (pad 5 thru_hole circle (at -2.54 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(Q6-Pad2)"))
    (pad 4 thru_hole circle (at -5.08 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(Q5-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(Q4-Pad2)"))
    (pad 28 thru_hole circle (at 17.78 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 audio+))
    (pad 0 thru_hole circle (at -15.24 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 sd_en))
    (pad 2 thru_hole circle (at -10.16 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 INT))
    (pad 1 thru_hole circle (at -12.7 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 amp_en))
    (pad 11 thru_hole circle (at 12.7 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 miso))
    (pad 12 thru_hole circle (at 15.24 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 mosi))
    (pad 13 thru_hole circle (at 15.24 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 sclk))
    (pad 14 thru_hole circle (at 12.7 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 vtest))
    (pad 18 thru_hole circle (at 2.54 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 SDA))
    (pad 19 thru_hole circle (at 0 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 SCL))
    (pad 21 thru_hole circle (at -5.08 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(Q3-Pad2)"))
    (pad 22 thru_hole circle (at -7.62 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(Q2-Pad2)"))
    (pad 23 thru_hole circle (at -10.16 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 24 thru_hole circle (at -12.7 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 3.3v))
    (pad 25 thru_hole circle (at -15.24 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 audio-))
    (pad 26 thru_hole circle (at -17.78 -7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 5v))
    (pad 27 thru_hole circle (at -17.78 7.62) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 28 thru_hole circle (at 15.24 -5.08) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 audio+))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 57DDA2B7)
    (at 153.162 100.33 270)
    (fp_text reference Q3 (at 0 0.75 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 14 "Net-(Q3-Pad2)"))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 11 "Net-(LED3-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA295)
    (at 156.21 95.25)
    (fp_text reference BATT+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.048 0.127) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(BATT+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA298)
    (at 156.21 97.79)
    (fp_text reference BATT-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.048 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(BATT-1-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DD92C6)
    (at 134.62 105.918 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C32 (at -0.762 -0.889 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.635 -0.889 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DD92FF)
    (at 141.224 104.14 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at 1.651 -0.381 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.778 0.127 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C33-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2AB)
    (at 156.21 107.95)
    (fp_text reference KILL-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.302 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module lightsaber_footprints:2520 (layer Top) (tedit 57DD929D)
    (at 138.684 107.696 270)
    (fp_text reference L1 (at 0 0.889 270) (layer F.SilkS))
    (fp_text value "4.7 uH 1.2A" (at 0 -0.762 360) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 0.8 2) (layers Top F.Paste F.Mask)
      (net 43 "Net-(IC3-Pad3)"))
    (pad 2 smd rect (at 1 0 270) (size 0.8 2) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2A8)
    (at 156.21 105.41)
    (fp_text reference LED1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(LED1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2A3)
    (at 156.21 102.87)
    (fp_text reference LED2 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(LED2-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA29B)
    (at 156.21 100.33)
    (fp_text reference LED3 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 3.175 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(LED3-Pad1)"))
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA0CC)
    (at 148.844 97.282)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference r11 (at -0.508 -0.889) (layer F.SilkS))
    (fp_text value 2.2k (at 0.635 -0.889) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 40 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 15 audio+))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA01E)
    (at 141.351 98.425 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference r12 (at 0.635 -0.889 180) (layer F.SilkS))
    (fp_text value 2.2k (at -0.381 -0.889 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 16 audio-))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD9291)
    (at 136.398 108.204 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R31 (at -0.381 -0.889 90) (layer F.SilkS))
    (fp_text value 2M (at 0.508 -0.889 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD931C)
    (at 143.002 103.886)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R32 (at -0.381 -0.889) (layer F.SilkS))
    (fp_text value 2M (at 0.635 -0.889) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DD92B3)
    (at 136.144 105.918 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R33 (at 1.397 0 90) (layer F.SilkS))
    (fp_text value 220k (at 1.524 0.508 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57FACC0E)
    (at 145.415 103.886)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R34 (at 1.397 -0.254) (layer F.SilkS))
    (fp_text value 220k (at 1.524 0.254) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA363)
    (at 153.67 110.49)
    (fp_text reference SP+1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SP+1-Pad1)"))
  )
  (module lightsaber_footprints:1pin (layer Top) (tedit 57DDA2D3)
    (at 156.21 110.49)
    (fp_text reference SP-1 (at 0 1) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(SP-1-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57DDA08C)
    (at 133.858 99.568 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0.762 -0.762 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.381 -0.762 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA075)
    (at 134.366 97.282)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at -0.508 -0.889) (layer F.SilkS))
    (fp_text value 2.2k (at 0.635 -0.889) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 18 SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57DDA03D)
    (at 138.176 97.028 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 1.143 -0.254 270) (layer F.SilkS))
    (fp_text value 2.2k (at 1.143 0.889 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 19 SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:LGA-14L (layer Top) (tedit 57DDA060)
    (at 136.652 99.568)
    (fp_text reference U2 (at 0 0.127) (layer F.SilkS))
    (fp_text value LSM6DS3H (at 1.905 0.254 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -1.25 -0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.25 0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -1.25 0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 34 INT))
    (pad 5 smd rect (at -0.5 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 6 smd rect (at 0 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 0.5 1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1.25 0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 9 smd rect (at 1.25 0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 36 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 1.25 -0.25) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 37 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 1.25 -0.75) (size 0.55 0.25) (layers Top F.Paste F.Mask)
      (net 38 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 0.5 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 13 smd rect (at 0 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 19 SCL))
    (pad 14 smd rect (at -0.5 -1) (size 0.25 0.55) (layers Top F.Paste F.Mask)
      (net 18 SDA))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 57DDA2C9)
    (at 153.162 107.442 270)
    (fp_text reference Q1 (at 0 0.75 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad1)"))
  )
  (module lightsaber_footprints:DMG7430LFG (layer Top) (tedit 57DDA2C1)
    (at 153.162 103.886 270)
    (fp_text reference Q2 (at 0 0.75 270) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -0.75 270) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at -0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 3 smd rect (at 0.325 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 2 smd rect (at 0.975 1.625 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 13 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at 0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.325 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at -0.975 -1.3 270) (size 0.42 0.7) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
    (pad 1 smd rect (at 0 -0.325 270) (size 2.37 1.9) (layers Top F.Paste F.Mask)
      (net 10 "Net-(LED2-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57FACD50)
    (at 141.351 96.901 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0.9525 0.8255 180) (layer F.SilkS))
    (fp_text value 3.3nF (at -0.5715 0.762 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57FACC3D)
    (at 148.844 99.06 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -0.889 270) (layer F.SilkS))
    (fp_text value 3.3nF (at 0.762 0.889 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 40 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 588E5663)
    (at 146.05 96.52)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 1.27 -0.381) (layer F.SilkS))
    (fp_text value 1uF (at 1.3335 0.127) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 41 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 40 "Net-(C12-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57F345AC)
    (at 143.256 97.536 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0.5715 0.889 90) (layer F.SilkS))
    (fp_text value 1uF (at -0.5715 0.889 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 42 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 39 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 57FACC07)
    (at 146.558 106.426 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0.0635 -1.016 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 57F344AC)
    (at 138.684 105.156 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C34 (at -0.1905 1.2065 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 124.46 103.9495 180)
    (fp_text reference LED4 (at 0.635 -0.508 450) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5 180) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0 180) (size 1.5 3) (layers Bottom B.Mask)
      (net 47 "Net-(LED4-Pad1)"))
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 128.397 104.013)
    (fp_text reference LED5 (at 0.635 -0.508 270) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0) (size 1.5 3) (layers Bottom B.Mask)
      (net 48 "Net-(LED5-Pad1)"))
  )
  (module lightsaber_footprints:PAD (layer Bottom) (tedit 57F330B7)
    (at 132.3975 103.886)
    (fp_text reference LED6 (at 0.635 -0.508 270) (layer B.SilkS))
    (fp_text value Pad (at 0 0.5) (layer B.Fab) hide)
    (pad 1 connect rect (at 0 0) (size 1.5 3) (layers Bottom B.Mask)
      (net 49 "Net-(LED6-Pad1)"))
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57FACC5A)
    (at 143.637 101.092 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 -0.9525 270) (layer F.SilkS))
    (fp_text value 100k (at 0.0635 0.9525 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 17 amp_en))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 57FACD38)
    (at 135.128 101.854 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R41 (at -0.381 -1.016 180) (layer F.SilkS))
    (fp_text value 10k (at 1.143 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 20 sd_en))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 124.46 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 44 "Net-(Q4-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 47 "Net-(LED4-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 128.397 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 45 "Net-(Q5-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 48 "Net-(LED5-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:SOT-23F (layer Bottom) (tedit 57F339F1)
    (at 132.3975 107.569 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 1.778 180) (layer B.SilkS))
    (fp_text value Q_NMOS_DGS (at 0 -1.778 180) (layer B.Fab))
    (pad 2 smd rect (at -0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 46 "Net-(Q6-Pad2)"))
    (pad 3 smd rect (at 0.95 -1.00076 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 2 "Net-(BATT-1-Pad1)"))
    (pad 1 smd rect (at 0 0.99822 180) (size 0.8001 0.8001) (layers Bottom B.Mask)
      (net 49 "Net-(LED6-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:QFN-10-PAD (layer Top) (tedit 57F329D6)
    (at 143.002 106.934 270)
    (descr 9)
    (fp_text reference IC3 (at 1.5 1 360) (layer F.SilkS))
    (fp_text value TPS61200 (at 0 -0.5 270) (layer F.Fab))
    (pad 15 smd rect (at 1.524 0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd rect (at 1.524 -0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at -1.524 0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 0 0 270) (size 2.4 1.65) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd oval (at -0.5 -1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd oval (at 1 1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 6 smd oval (at 1 -1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 4 smd oval (at 0.5 1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd oval (at 0 1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 43 "Net-(IC3-Pad3)"))
    (pad 1 smd oval (at -1 1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 6 "Net-(C33-Pad1)"))
    (pad 2 smd oval (at -0.5 1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 7 smd oval (at 0.5 -1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 5 vtest))
    (pad 8 smd oval (at 0 -1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 1 "Net-(BATT+1-Pad1)"))
    (pad 10 smd oval (at -1 -1.5 270) (size 0.23 0.8) (layers Top F.Paste F.Mask)
      (net 8 "Net-(IC3-Pad10)"))
    (pad 12 smd rect (at -1.524 -0.254 270) (size 1.5 0.28) (layers Top F.Paste F.Mask)
      (net 3 GND))
  )
  (module Capacitors_SMD:C_0402 (layer Top) (tedit 57FACCD8)
    (at 137.414 102.108 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0.508 -0.762 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.762 -0.762 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 4 3.3v))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 57FACC26)
    (at 146.05 101.473)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -0.254 -1.016) (layer F.SilkS))
    (fp_text value 10uF (at 0.762 -1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 5v))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_footprints:fiduciary (layer Top) (tedit 57F463E7)
    (at 153.67 97.536)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (module lightsaber_footprints:fiduciary (layer Top) (tedit 57F463E7)
    (at 118.11 98.044)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (solder_mask_margin 0.6) (clearance 0.5))
  )
  (gr_text ID (at 133.35 96.52) (layer B.SilkS))
  (gr_text "LED6-\n" (at 133.731 104.9655 90) (layer B.SilkS))
  (gr_text "LED5-\n" (at 129.667 104.9655 90) (layer B.SilkS))
  (gr_text "LED4-\n" (at 125.7935 104.902 90) (layer B.SilkS))
  (gr_line (start 133.604 111.76) (end 125.984 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 110.49) (end 134.62 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.128 109.982) (end 146.05 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135.128 110.49) (end 134.62 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 133.604 110.744) (end 134.62 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 93.98) (end 118.11 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.112 95.758) (end 132.588 95.758) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 95.758) (end 140.208 95.758) (layer Edge.Cuts) (width 0.15))
  (gr_text buttons (at 143.7005 97.2185) (layer B.SilkS))
  (gr_text 3 (at 141.732 96.52) (layer B.SilkS))
  (gr_text 2 (at 143.764 96.52) (layer B.SilkS))
  (gr_text 1 (at 145.796 96.52) (layer B.SilkS))
  (gr_text SPKR+ (at 151.892 108.712 315) (layer B.SilkS))
  (gr_text "SPKR-\n" (at 154.432 108.966 315) (layer B.SilkS))
  (gr_text "BATT+\n" (at 154.432 96.774 45) (layer B.SilkS))
  (gr_text "BATT-\n" (at 154.178 98.552) (layer B.SilkS))
  (gr_text "audio in\n" (at 148.59 97.79) (layer B.SilkS))
  (gr_text "LED3-\n" (at 153.924 100.838) (layer B.SilkS))
  (gr_text "LED2-\n" (at 153.924 102.87) (layer B.SilkS))
  (gr_text LED1- (at 153.924 104.902) (layer B.SilkS))
  (gr_text "GND\n" (at 154.432 107.442) (layer B.SilkS))
  (gr_text GND (at 118.11 108.331 90) (layer B.SilkS))
  (gr_text "TeensySaber V2.2, by Fredrik Hubinette\nhttp://fredrik.hubbe.net/lightsaber/\n" (at 145.7325 100.1395) (layer B.SilkS))
  (gr_line (start 116.84 110.49) (end 116.84 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.11 110.49) (end 118.11 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.11 95.25) (end 116.84 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 110.49) (end 147.32 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 109.982) (end 146.05 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 95.25) (end 147.32 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 94.996) (end 139.7 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.812 110.49) (end 146.812 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.812 95.25) (end 147.32 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.208 95.25) (end 140.208 95.758) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 93.98) (end 138.684 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 93.98) (end 148.336 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 93.98) (end 155.448 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 95.25) (end 157.48 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 111.76) (end 156.21 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.336 110.744) (end 148.336 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 156.21 110.49) (end 157.48 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 156.21 95.25) (end 156.21 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.336 94.996) (end 147.32 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.684 94.996) (end 138.684 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 95.25) (end 132.08 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 94.996) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135.636 94.996) (end 134.62 94.996) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.112 95.25) (end 134.62 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.588 95.25) (end 132.588 95.758) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.064 94.996) (end 131.064 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.636 93.98) (end 138.43 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.984 111.76) (end 118.11 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 93.98) (end 155.448 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Bottom) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.226 96.647) (xy 152.4 96.647) (xy 149.606 98.425) (xy 149.606 108.077) (xy 154.94 108.077)
        (xy 154.94 100.965) (xy 157.226 99.187)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.511 98.933) (xy 151.511 100.965) (xy 149.606 100.965) (xy 149.606 98.933)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.511 104.521) (xy 149.606 104.521) (xy 149.606 102.235) (xy 151.511 102.235)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.511 108.077) (xy 149.606 108.077) (xy 149.606 105.791) (xy 151.511 105.791)
      )
    )
  )
  (zone (net 11) (net_name "Net-(LED3-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.416 99.314) (xy 156.591 99.314) (xy 156.718 99.314) (xy 157.226 99.822) (xy 157.226 100.838)
        (xy 156.591 101.346) (xy 153.416 101.346)
      )
    )
  )
  (zone (net 11) (net_name "Net-(LED3-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.718 99.314) (xy 157.226 99.822) (xy 157.226 100.838) (xy 156.591 101.346) (xy 153.416 101.346)
        (xy 153.416 99.314)
      )
    )
  )
  (zone (net 10) (net_name "Net-(LED2-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.083 101.854) (xy 156.718 101.854) (xy 157.226 102.489) (xy 157.226 103.378) (xy 156.718 103.886)
        (xy 155.067 104.775) (xy 153.543 105.029) (xy 153.289 104.902) (xy 153.035 104.648) (xy 153.035 102.87)
        (xy 153.289 102.616)
      )
    )
  )
  (zone (net 10) (net_name "Net-(LED2-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.289 101.981) (xy 156.083 101.854) (xy 156.718 101.854) (xy 157.226 102.489) (xy 157.226 103.378)
        (xy 156.718 103.886) (xy 155.067 104.775) (xy 153.543 105.029) (xy 153.289 104.902) (xy 153.035 104.648)
        (xy 153.035 102.87)
      )
    )
  )
  (zone (net 9) (net_name "Net-(LED1-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 108.585) (xy 153.289 108.204) (xy 153.289 106.172) (xy 155.448 104.775) (xy 156.337 104.267)
        (xy 157.226 104.902) (xy 157.226 106.299) (xy 154.432 108.585)
      )
    )
  )
  (zone (net 9) (net_name "Net-(LED1-Pad1)") (layer Top) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.289 106.172) (xy 156.337 104.267) (xy 157.226 104.902) (xy 157.226 106.299) (xy 154.432 108.585)
        (xy 153.67 108.585) (xy 153.289 108.204)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 91.948) (xy 159.258 91.948) (xy 159.258 113.284) (xy 114.3 113.284) (xy 114.3 110.109)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BATT-1-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1225))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.415 98.171) (xy 148.336 92.837) (xy 159.258 94.107) (xy 157.226 99.06) (xy 152.781 99.06)
        (xy 152.654 108.077) (xy 151.765 108.077) (xy 151.765 115.8875) (xy 118.618 114.554) (xy 118.364 101.473)
        (xy 141.605 101.092) (xy 142.113 98.171) (xy 143.891 96.774)
      )
    )
  )
)
