(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x0001000_7ffffffe)
      (plot_on_all_layers_selection 0x0020020_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../../../../Desktop/PCB_printfiles/")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-+IN)")
  (net 2 "Net-(U1-M1)")
  (net 3 "Net-(U1-M2)")
  (net 4 "Net-(U1-M4)")
  (net 5 "Net-(U1-M3)")
  (net 6 "unconnected-(U1-PC-Pad2)")
  (net 7 "unconnected-(U1-PR-Pad3)")
  (net 8 "unconnected-(U1-SC-Pad7)")
  (net 9 "Net-(U1--IN)")
  (net 10 "Net-(U1--OUT)")
  (net 11 "Net-(U1-+OUT)")
  (net 12 "Net-(F1-Pad1)")
  (footprint "WAGO 2 Port:CONN_2604-1102_WAG" (layer "F.Cu")
    (at 119.199999 80 -90)
    (tags "2604-1102 ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "2604-1102")
    (attr through_hole)
    (fp_text reference "J4" (at 2.725001 4.099999 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "2604-1102" (at 2.725001 4.099999 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.725001 4.099999 -90 unlocked) (layer "F.Fab"))
    (pad "1_1" thru_hole circle (at 0 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "1_1") (pintype "unspecified"))
    (pad "1_2" thru_hole circle (at 0 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "1_2") (pintype "unspecified"))
    (pad "2_1" thru_hole circle (at 5 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "2_1") (pintype "unspecified"))
    (pad "2_2" thru_hole circle (at 5 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "2_2") (pintype "unspecified"))
  )
  (footprint "476_Capacitor:CAP_PAN_8X11.5_PAN" (layer "F.Cu")
    (at 151 117 90)
    (tags "ECA2AM470B ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "ECA2AM470B")
    (attr through_hole)
    (fp_text reference "C5" (at 1.7526 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "47 uF" (at 1.7526 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.4224 1.4224) (drill 0.9144) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 3.5052 0 90) (size 1.4224 1.4224) (drill 0.9144) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pintype "unspecified"))
  )
  (footprint "WAGO 4 Port:CONN_2604-1104_WAG" (layer "F.Cu")
    (at 139.966187 33.446487 -90)
    (tags "2604-1104 ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "2604-1104")
    (attr through_hole)
    (fp_text reference "J1" (at 7.75 4.099999 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "2604-1104" (at 7.75 4.099999 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.75 4.099999 -90 unlocked) (layer "F.Fab"))
    (pad "1_1" thru_hole circle (at 0 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "1_1") (pintype "unspecified"))
    (pad "1_2" thru_hole circle (at 0 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "1_2") (pintype "unspecified"))
    (pad "2_1" thru_hole circle (at 5 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "2_1") (pintype "unspecified"))
    (pad "2_2" thru_hole circle (at 5 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "2_2") (pintype "unspecified"))
    (pad "3_1" thru_hole circle (at 10 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "3_1") (pintype "unspecified"))
    (pad "3_2" thru_hole circle (at 10 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "3_2") (pintype "unspecified"))
    (pad "4_1" thru_hole circle (at 15.000001 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "4_1") (pintype "unspecified"))
    (pad "4_2" thru_hole circle (at 15.000001 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(F1-Pad1)") (pinfunction "4_2") (pintype "unspecified"))
  )
  (footprint "472_Capacitor:CAP_C317C_MR_X7R_KEM" (layer "F.Cu")
    (at 121 56 -90)
    (tags "C317C472K1R5TA ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "C317C472K1R5TA")
    (attr through_hole)
    (fp_text reference "C3" (at 2.54 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7 nF" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1-M3)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pintype "unspecified"))
  )
  (footprint "472_Capacitor:CAP_C317C_MR_X7R_KEM" (layer "F.Cu")
    (at 183.907887 56.026372 -90)
    (tags "C317C472K1R5TA ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "C317C472K1R5TA")
    (attr through_hole)
    (fp_text reference "C2" (at 2.54 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7 nF" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1-M2)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pintype "unspecified"))
  )
  (footprint "476_Capacitor:CAP_PAN_8X11.5_PAN" (layer "F.Cu")
    (at 139 117 90)
    (tags "ECA2AM470B ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "ECA2AM470B")
    (attr through_hole)
    (fp_text reference "C6" (at 1.7526 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "47 uF" (at 1.7526 0 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.7526 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.4224 1.4224) (drill 0.9144) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 3.5052 0 90) (size 1.4224 1.4224) (drill 0.9144) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pintype "unspecified"))
  )
  (footprint "WAGO 2 Port:CONN_2604-1102_WAG" (layer "F.Cu")
    (at 119.27782 66.393579 -90)
    (tags "2604-1102 ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "2604-1102")
    (attr through_hole)
    (fp_text reference "J3" (at 2.725001 4.099999 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "2604-1102" (at 2.725001 4.099999 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.725001 4.099999 -90 unlocked) (layer "F.Fab"))
    (pad "1_1" thru_hole circle (at 0 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "1_1") (pintype "unspecified"))
    (pad "1_2" thru_hole circle (at 0 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "1_2") (pintype "unspecified"))
    (pad "2_1" thru_hole circle (at 5 0 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "2_1") (pintype "unspecified"))
    (pad "2_2" thru_hole circle (at 5 8.199999 270) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "2_2") (pintype "unspecified"))
  )
  (footprint "472_Capacitor:CAP_C317C_MR_X7R_KEM" (layer "F.Cu")
    (at 120.84959 101.667131 -90)
    (tags "C317C472K1R5TA ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "C317C472K1R5TA")
    (attr through_hole)
    (fp_text reference "C4" (at 2.54 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7 nF" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-M4)") (pintype "unspecified"))
  )
  (footprint "Fuse:Fuseholder_Clip-6.3x32mm_Littelfuse_102_Inline_P34.21x7.62mm_D2.54mm_Horizontal" (layer "F.Cu")
    (at 125.895 125)
    (descr "Fuseholder Clips, 6.3x32mm Cylinder Fuse, Pins Inline, Horizontal, Littelfuse 102 Bowed Leads, https://www.littelfuse.com/~/media/electronics/datasheets/fuse_clips/littelfuse_fuse_clip_102_122_datasheet.pdf.pdf")
    (tags "fuse clip open")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fuse")
    (property "ki_keywords" "fuse")
    (attr through_hole)
    (fp_text reference "F1" (at 17.1 0.36) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 17.1 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 17.1 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 2.54) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "1" thru_hole roundrect (at 7.62 0) (size 3.5 3.5) (drill 2.54) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 26.59 0) (size 3.5 3.5) (drill 2.54) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pintype "passive"))
    (pad "2" thru_hole circle (at 34.21 0) (size 3.5 3.5) (drill 2.54) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-6.3x32mm_Littelfuse_102_Inline_P34.21x7.62mm_D2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "472_Capacitor:CAP_C317C_MR_X7R_KEM" (layer "F.Cu")
    (at 183.934748 101.687758 -90)
    (tags "C317C472K1R5TA ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "C317C472K1R5TA")
    (attr through_hole)
    (fp_text reference "C1" (at 2.54 0 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7 nF" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(U1-M1)") (pintype "unspecified"))
  )
  (footprint "WAGO 4 Port:CONN_2604-1104_WAG" (layer "F.Cu")
    (at 148.800001 49 90)
    (tags "2604-1104 ")
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "2604-1104")
    (attr through_hole)
    (fp_text reference "J2" (at 7.75 4.099999 90 unlocked) (layer "F.SilkS"))
    (fp_text value "2604-1104" (at 7.75 4.099999 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.75 4.099999 90 unlocked) (layer "F.Fab"))
    (pad "1_1" thru_hole circle (at 0 0 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "1_1") (pintype "unspecified"))
    (pad "1_2" thru_hole circle (at 0 8.199999 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "1_2") (pintype "unspecified"))
    (pad "2_1" thru_hole circle (at 5 0 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "2_1") (pintype "unspecified"))
    (pad "2_2" thru_hole circle (at 5 8.199999 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "2_2") (pintype "unspecified"))
    (pad "3_1" thru_hole circle (at 10 0 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "3_1") (pintype "unspecified"))
    (pad "3_2" thru_hole circle (at 10 8.199999 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "3_2") (pintype "unspecified"))
    (pad "4_1" thru_hole circle (at 15.000001 0 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "4_1") (pintype "unspecified"))
    (pad "4_2" thru_hole circle (at 15.000001 8.199999 90) (size 1.905 1.905) (drill 1.397) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "4_2") (pintype "unspecified"))
  )
  (footprint "Vicor Power Library:DC_DC_Converter_V48B24C250BL" (layer "F.Cu")
    (at 176.6 99.18 180)
    (property "Sheetfile" "ARCSnake PCB.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 22.61 -0.5 180 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(U1-+IN)") (pinfunction "+IN") (pintype "input"))
    (pad "2" thru_hole circle (at 0 10.16 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(U1-PC-Pad2)") (pinfunction "PC") (pintype "input+no_connect"))
    (pad "3" thru_hole circle (at 0 25.4 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(U1-PR-Pad3)") (pinfunction "PR") (pintype "input+no_connect"))
    (pad "4" thru_hole circle (at 0 35.56 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1--IN)") (pinfunction "-IN") (pintype "input"))
    (pad "5" thru_hole circle (at 48.26 35.56 180) (size 8.2 8.2) (drill 7.19) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "-OUT") (pintype "output"))
    (pad "6" thru_hole circle (at 48.26 25.4 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1--OUT)") (pinfunction "-S") (pintype "output"))
    (pad "7" thru_hole circle (at 48.26 17.78 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-SC-Pad7)") (pinfunction "SC") (pintype "output+no_connect"))
    (pad "8" thru_hole circle (at 48.26 10.16 180) (size 6.1 6.1) (drill 5.08) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "+S") (pintype "output"))
    (pad "9" thru_hole circle (at 48.26 0 180) (size 8.2 8.2) (drill 7.19) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-+OUT)") (pinfunction "+OUT") (pintype "output"))
    (pad "10" thru_hole circle (at 7.6 -7.6 180) (size 4.2 4.2) (drill 3.3) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(U1-M1)") (pinfunction "M1") (pintype "passive"))
    (pad "11" thru_hole circle (at 7.6 43.18 180) (size 4.2 4.2) (drill 3.3) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1-M2)") (pinfunction "M2") (pintype "passive"))
    (pad "12" thru_hole circle (at 40.64 43.18 180) (size 4.2 4.2) (drill 3.3) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1-M3)") (pinfunction "M3") (pintype "passive"))
    (pad "13" thru_hole circle (at 40.64 -7.6 180) (size 4.2 4.2) (drill 3.3) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-M4)") (pinfunction "M4") (pintype "passive"))
  )
  (gr_line (start 186 44) (end 186 111)
    (layer "Edge.Cuts"))
  (gr_line (start 102 111) (end 102 44)
    (layer "Edge.Cuts"))
  (gr_line (start 166 44) (end 186 44)
    (layer "Edge.Cuts"))
  (gr_line (start 166 29.5) (end 166 44)
    (layer "Edge.Cuts"))
  (gr_line (start 122 111) (end 102 111)
    (layer "Edge.Cuts"))
  (gr_line (start 122 44) (end 122 29.5)
    (layer "Edge.Cuts"))
  (gr_line (start 122 130) (end 122 111)
    (layer "Edge.Cuts"))
  (gr_line (start 164 111) (end 164 130)
    (layer "Edge.Cuts"))
  (gr_line (start 102 44) (end 122 44)
    (layer "Edge.Cuts"))
  (gr_line (start 186 111) (end 164 111)
    (layer "Edge.Cuts"))
  (gr_line (start 122 29.5) (end 166 29.5)
    (layer "Edge.Cuts"))
  (gr_line (start 164 130) (end 122 130)
    (layer "Edge.Cuts"))
  (gr_text "F2: Fuse-,\n	C1+, \n	C5+, C6+,\n	IN+" (at 187 50) (layer "Cmts.User"))
  (gr_text "B1: WAGO2-,\n	C3-, OUT-" (at 87 49) (layer "Cmts.User"))
  (gr_text "B2: WAGO2+,\n	C4+, OUT+" (at 87 80) (layer "Cmts.User"))
  (gr_text "B3: WAGO4-,\n	C2-\n	C5-, C6-,\n	IN-" (at 165 119) (layer "Cmts.User"))
  (gr_text "F1: WAGO4+,\n	Fuse+" (at 123 27) (layer "Cmts.User"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 111) (xy 122 130))
    (height 47)
    (gr_text "19.0000 mm" (at 73.85 120.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 42) (xy 102 42))
    (height 25)
    (gr_text "20.0000 mm" (at 112 15.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 111) (xy 164 111))
    (height 29)
    (gr_text "42.0000 mm" (at 143 138.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 166 29.5) (xy 166 44))
    (height -44)
    (gr_text "14.5000 mm" (at 208.85 36.75 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 102 44) (xy 102 111))
    (height 26.999999)
    (gr_text "67.0000 mm" (at 73.850001 77.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 42) (xy 166 42))
    (height -25)
    (gr_text "44.0000 mm" (at 144 15.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 166 42) (xy 186 42))
    (height -25)
    (gr_text "20.0000 mm" (at 176 15.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 111) (xy 102 111))
    (height -29)
    (gr_text "20.0000 mm" (at 112 138.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 186 44) (xy 186 111))
    (height -24)
    (gr_text "67.0000 mm" (at 208.85 77.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 122 29.5) (xy 122 44))
    (height 47)
    (gr_text "14.5000 mm" (at 73.85 36.75 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 164 111) (xy 164 130))
    (height -46)
    (gr_text "19.0000 mm" (at 208.85 120.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 164 111) (xy 186 111))
    (height 29)
    (gr_text "22.0000 mm" (at 175 138.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 12) (net_name "Net-(F1-Pad1)") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 123 30.5)
        (xy 144 30.5)
        (xy 144 111)
        (xy 136 111)
        (xy 136 129)
        (xy 123 129)
      )
    )
  )
  (zone (net 1) (net_name "Net-(U1-+IN)") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 112)
        (xy 137 112)
        (xy 137 129)
        (xy 163 129)
        (xy 163 110)
        (xy 185 110)
        (xy 185 45)
        (xy 165 45)
        (xy 165 30.5)
        (xy 145 30.5)
      )
    )
  )
  (zone (net 9) (net_name "Net-(U1--IN)") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 30.5)
        (xy 165 30.5)
        (xy 165 59)
        (xy 185 59)
        (xy 185 104)
        (xy 163 104)
        (xy 163 129)
        (xy 123 129)
        (xy 123 110)
        (xy 145 110)
      )
    )
  )
  (zone (net 10) (net_name "Net-(U1--OUT)") (layer "B.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 103 45)
        (xy 119 45)
        (xy 119 59)
        (xy 144 59)
        (xy 144 82)
        (xy 123 82)
        (xy 123 75)
        (xy 103 75)
      )
    )
  )
  (zone (net 11) (net_name "Net-(U1-+OUT)") (layer "B.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 103 75)
        (xy 122 75)
        (xy 122 82)
        (xy 144 82)
        (xy 144 104)
        (xy 103 104)
      )
    )
  )
)
