(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Spectrum Analyzer: Timebase")
    (date "2022-05-29")
    (rev "0.2")
    (company "Andy McCann KA3KAF and Doug McCann KA3KAG")
    (comment 1 "Terry White K7TAU")
    (comment 2 "Wes Hayward W7ZOI")
    (comment 3 "Original Design by:")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (grid_origin 50.8 101.854)
    (pcbplotparams
      (layerselection 0x0000030_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C401-Pad1)")
  (net 2 "Net-(C401-Pad2)")
  (net 3 "GND")
  (net 4 "Net-(C402-Pad2)")
  (net 5 "Net-(C403-Pad1)")
  (net 6 "Net-(C404-Pad2)")
  (net 7 "Net-(C405-Pad2)")
  (net 8 "Net-(C406-Pad1)")
  (net 9 "Net-(D401-Pad1)")
  (net 10 "Net-(D401-Pad2)")
  (net 11 "Net-(D402-Pad1)")
  (net 12 "Net-(D403-Pad1)")
  (net 13 "Net-(D404-Pad2)")
  (net 14 "Net-(D405-Pad2)")
  (net 15 "VCO_Out")
  (net 16 "Out")
  (net 17 "V+15")
  (net 18 "V-15")
  (net 19 "Net-(R4-Pad2)")
  (net 20 "Net-(R418-Pad1)")
  (net 21 "Net-(R417-Pad1)")
  (net 22 "Net-(R401-Pad2)")
  (net 23 "Net-(R406-Pad2)")
  (net 24 "Net-(R411-Pad2)")
  (net 25 "Net-(R412-Pad2)")
  (net 26 "Net-(R413-Pad2)")
  (net 27 "Net-(R415-Pad2)")
  (net 28 "Net-(R418-Pad2)")
  (net 29 "Net-(R419-Pad2)")
  (net 30 "Net-(R420-Pad1)")
  (net 31 "Net-(R421-Pad2)")
  (net 32 "Net-(R424-Pad2)")
  (net 33 "Net-(R426-Pad2)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 64.262 33.528)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R411" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "12k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C401-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R411-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 61.976 54.61 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R401" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "56k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R401-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 54.102 78.342 -90)
    (descr "Soldered wire connection, for 3 times 0.127 mm² wires, basic insulation, conductor diameter 0.48mm, outer diameter 1mm, size source Multi-Contact FLEXI-E/HK 0.127 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.127sqmm")
    (property "Field8" "Span")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot3.lib")
    (property "Spice_Model" "pot_lin3")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr exclude_from_pos_files)
    (fp_text reference "R5" (at 3.7 -2.54 90) (layer "F.SilkS"))
    (fp_text value "5k" (at 3.7 2.05 90) (layer "F.Fab"))
    (fp_text user "Span" (at 3.7 -3.81 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.7 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "Net-(C401-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.7 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(R418-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.4 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(R417-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 64.262 28.956)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R405" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D401-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 99.568 73.406 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R423" (at 4.064 -0.254) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C404-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 103.124 77.216)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R425" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R424-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 93.218 57.404)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4148.mod")
    (property "Spice_Model" "D1N4148")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D405" (at 4.064 2.286) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.286) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D404-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D405-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 54.102 74.058 90)
    (descr "Soldered wire connection, for 3 times 0.127 mm² wires, basic insulation, conductor diameter 0.48mm, outer diameter 1mm, size source Multi-Contact FLEXI-E/HK 0.127 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.127sqmm")
    (property "Field8" "Fine Tune")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot2.lib")
    (property "Spice_Model" "pot_lin2")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr exclude_from_pos_files)
    (fp_text reference "R4" (at 3.7 2.54 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.7 2.05 90) (layer "F.Fab"))
    (fp_text user "Fine Tune" (at 3.954 3.81 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.7 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.7 0 90) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(R4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.4 0 90) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "V-15") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 99.568 77.216 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R426" (at 4.064 -0.254) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R426-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 110.998 64.008 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C402" (at 9.652 0) (layer "F.SilkS"))
    (fp_text value "22u" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C402-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 88.646 64.008 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C403" (at 9.144 0.254) (layer "F.SilkS"))
    (fp_text value "22u" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C403-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.612 49.022)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R406" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C401-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R406-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:TE_5-1634503-1" (layer "F.Cu")
    (tedit 6292C70A)
    (at 124.968 37.846)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J9" (at -0.254 -2.286) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 3.76275 6.61328) (layer "F.Fab"))
    (fp_text user "Scope X Input" (at 0 7.112 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Out") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.13 -3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.13 -3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle locked (at 3.13 3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle locked (at -3.13 3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/FreeCad/5-1634503-1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/FreeCad/5-1634503-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 103.124 80.772)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R427" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "22" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C405-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "V-15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:TE_5-1634503-1" (layer "F.Cu")
    (tedit 6292C70A)
    (at 124.714 53.086)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.794) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 3.76275 6.61328) (layer "F.Fab"))
    (fp_text user "VCO Control" (at 0 7.366 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "VCO_Out") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.13 -3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.13 -3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle locked (at 3.13 3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle locked (at -3.13 3.13) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/FreeCad/5-1634503-1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/FreeCad/5-1634503-1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 114.554 48.514 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R410" (at 4.064 0 -270) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D405-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "V-15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 110.236 33.782)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4148.mod")
    (property "Spice_Model" "D1N4148")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D408" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.032) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "VCO_Out") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 54.102 54.72 -90)
    (descr "Soldered wire connection, for 3 times 0.127 mm² wires, basic insulation, conductor diameter 0.48mm, outer diameter 1mm, size source Multi-Contact FLEXI-E/HK 0.127 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.127sqmm")
    (property "Field8" "Sweep Rate")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot.lib")
    (property "Spice_Model" "pot_lin")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr exclude_from_pos_files)
    (fp_text reference "R6" (at 3.7 -2.54 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.7 2.05 90) (layer "F.Fab"))
    (fp_text user "Sweep Rate" (at 3.7 -3.81 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.7 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 18 "V-15") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.7 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(R401-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.4 0 270) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 114.554 66.548 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R428" (at 4.064 -0.254 90) (layer "F.SilkS"))
    (fp_text value "22" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C403-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C406-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 120.142 28.956)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R416" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "390" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R415-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 54.8 29.854)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle locked (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SnapEDA Library:DIP794W45P254L959H508Q8" (layer "F.Cu")
    (tedit 6292BB96)
    (at 87.63 41.402)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "TL072-dual.lib")
    (property "Spice_Model" "TL072c")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U402" (at 0.094 -0.508) (layer "F.SilkS"))
    (fp_text value "LM358" (at 10.865 5.607) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 25 "Net-(R412-Pad2)") (pintype "output"))
    (pad "2" thru_hole circle locked (at -3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 24 "Net-(R411-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole circle locked (at -3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 4 "Net-(C402-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole circle locked (at 3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 26 "Net-(R413-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole circle locked (at 3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 27 "Net-(R415-Pad2)") (pintype "output"))
    (pad "8" thru_hole circle locked (at 3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 5 "Net-(C403-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (model "${KIPRJMOD}/FreeCad/OPA347PA010.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 75.692 33.528)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R412" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R411-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R412-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 132.08 97.854)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle locked (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 92.964 87.884)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C405" (at 8.238 -0.3965) (layer "F.SilkS"))
    (fp_text value "100u" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(C405-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 100.584 52.578 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4148.mod")
    (property "Spice_Model" "D1N4148")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D404" (at 3.81 -2.286) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D403-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D404-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 54.8 97.854)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle locked (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 98.044 33.782)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R429" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "470" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R426-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "VCO_Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 61.722 89.916 180)
    (descr "Soldered wire connection, for 3 times 0.127 mm² wires, basic insulation, conductor diameter 0.48mm, outer diameter 1mm, size source Multi-Contact FLEXI-E/HK 0.127 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.127sqmm")
    (property "Field8" "Tune")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot4.lib")
    (property "Spice_Model" "pot_lin4")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr exclude_from_pos_files)
    (fp_text reference "R3" (at 2.032 -2.54) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.7 2.05) (layer "F.Fab"))
    (fp_text user "Tune" (at 6.604 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.7 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.7 0 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(C404-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.4 0 180) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "V-15") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 94.234 28.702 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4148.mod")
    (property "Spice_Model" "D1N4148")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D402" (at 3.81 -2.032) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.032) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D402-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D401-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 86.614 33.528)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R413" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R412-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R413-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 132.334 29.854)
    (descr "Mounting Hole 2.7mm, M2.5, DIN965")
    (tags "mounting hole 2.7mm m2.5 din965")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle locked (at 0 0) (size 4.7 4.7) (layers "F.Cu" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.358 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R419" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R418-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R419-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:CUI_PJ-007" locked (layer "F.Cu")
    (tedit 62935144)
    (at 53.3785 40.074)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Model" "Jack-DC")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J404" (at 8.5975 0) (layer "F.SilkS"))
    (fp_text value "Jack-DC" (at 8.3435 3.81) (layer "F.Fab"))
    (fp_text user "+15" (at 13.1695 0 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.4 2.8) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 18 "V-15") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5 0) (size 1.4 2.8) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 2.5 -2.7) (size 2.8 1.4) (drill oval 1.5 0.8) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/FreeCad/CUI_DEVICES_PJ-009.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 81.534 49.022)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R407" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R406-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D404-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 63.5 68.58)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C401" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value "1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "Net-(C401-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 109.22 28.956)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R415" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R413-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R415-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 70.502 88.0265)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C404" (at 9 -0.1425) (layer "F.SilkS"))
    (fp_text value "100u" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C404-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.612 52.832)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R402" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "680k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C401-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "V-15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:DIP794W45P254L959H508Q8" (layer "F.Cu")
    (tedit 6292BB96)
    (at 85.09 73.406)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "TL072-dual.lib")
    (property "Spice_Model" "TL072c")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U403" (at -0.254 -0.254) (layer "F.SilkS"))
    (fp_text value "LM358" (at 10.865 5.607) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 29 "Net-(R419-Pad2)") (pintype "output"))
    (pad "2" thru_hole circle locked (at -3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 28 "Net-(R418-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole circle locked (at -3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 7 "Net-(C405-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole circle locked (at 3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole circle locked (at 3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 33 "Net-(R426-Pad2)") (pintype "output"))
    (pad "8" thru_hole circle locked (at 3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 8 "Net-(C406-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (model "${KIPRJMOD}/FreeCad/OPA347PA010.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.612 57.404)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R404" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "V+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C403-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 109.484 72.136)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Field8" "Centering")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot5.lib")
    (property "Spice_Model" "pot_lin5")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "R424" (at -2.54 -3.66) (layer "F.SilkS"))
    (fp_text value "5k" (at -2.54 3.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R424-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "V-15") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:DIP794W45P254L959H508Q8" (layer "F.Cu")
    (tedit 6292BB96)
    (at 74.77 41.402)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "TL072-dual.lib")
    (property "Spice_Model" "TL072c")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U401" (at 0 -0.254) (layer "F.SilkS"))
    (fp_text value "LM358" (at 10.865 5.607) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 2 "Net-(C401-Pad2)") (pintype "output"))
    (pad "2" thru_hole circle locked (at -3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 1 "Net-(C401-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole circle locked (at -3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 4 "Net-(C402-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 23 "Net-(R406-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole circle locked (at 3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole circle locked (at 3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 10 "Net-(D401-Pad2)") (pintype "output"))
    (pad "8" thru_hole circle locked (at 3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers *.Cu *.Mask)
      (net 5 "Net-(C403-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (model "${KIPRJMOD}/FreeCad/OPA347PA010.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 103.124 49.022)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R409" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "V+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D403-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 75.438 28.702)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4148.mod")
    (property "Spice_Model" "D1N4148")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D401" (at 3.81 2.032) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 2.032) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D401-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D401-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.358 81.026)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R417" (at 3.81 0.254) (layer "F.SilkS"))
    (fp_text value "51" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R417-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 111.506 57.404 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4735A.lib")
    (property "Spice_Model" "DI_1N4735A")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "D406" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4735" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.032) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D405-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 98.298 28.956)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R414" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D402-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R413-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.358 77.216)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R422" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "240k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R4-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 87.894 81.788)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Field8" "Cal Max Span")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "Pot6.lib")
    (property "Spice_Model" "pot_lin6")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "R420" (at 5.07 0) (layer "F.SilkS"))
    (fp_text value "5k" (at -2.54 3.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R420-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R420-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R419-Pad2)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 103.632 52.578)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Lib_File" "1N4735A.lib")
    (property "Spice_Model" "DI_1N4735A")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "2 1")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "D403" (at 4.318 2.286) (layer "F.SilkS"))
    (fp_text value "1N4735" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0.508 2.286) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D403-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 89.154 52.832 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R403" (at 4.064 0) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C402-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "V-15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SnapEDA Library:CUI_PJ-007" locked (layer "F.Cu")
    (tedit 62935144)
    (at 53.6325 48.514)
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (property "Spice_Model" "Jack-DC")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J402" (at 8.5975 0.058) (layer "F.SilkS"))
    (fp_text value "Jack-DC" (at 8.0895 3.614) (layer "F.Fab"))
    (fp_text user "-15" (at 13.1695 0 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole oval locked (at 0 0) (size 1.4 2.8) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 17 "V+15") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 5 0) (size 1.4 2.8) (drill oval 0.8 1.5) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 2.5 -2.7) (size 2.8 1.4) (drill oval 1.5 0.8) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/FreeCad/CUI_DEVICES_PJ-009.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF2)
    (at 114.156 42.0215 180)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "C406" (at 8.492 -0.3965) (layer "F.SilkS"))
    (fp_text value "100u" (at 9 4.12) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C406-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 18 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 70.358 73.66)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R418" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R418-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R418-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 99.568 69.596 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R421" (at 3.81 -0.254) (layer "F.SilkS"))
    (fp_text value "6.8k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R420-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R421-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 99.822 49.022 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Timebase.kicad_sch")
    (property "Sheetname" "TimeBase")
    (attr through_hole)
    (fp_text reference "R408" (at 4.064 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D401-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D404-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 50.8 25.4) (end 136.144 101.854) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Doug McCann\nKA3KAG" (at 99.568 95.504) (layer "F.SilkS"))
  (gr_text "Andy McCann\nKA3KAF" (at 78.232 95.504) (layer "F.SilkS"))
  (zone (net 3) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.144 101.854)
        (xy 50.8 101.854)
        (xy 50.8 25.4)
        (xy 136.144 25.4)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.144 101.854)
        (xy 50.8 101.854)
        (xy 50.8 25.4)
        (xy 136.144 25.4)
      )
    )
  )
)
