(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 84)
    (zones 0)
    (modules 12)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 /SDAin)
  (net 7 /SCKin)
  (net 8 /SCKout)
  (net 9 /SDAout)
  (net 10 /Vpp)
  (net 11 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +5V)
    (add_net /SCKin)
    (add_net /SCKout)
    (add_net /SDAin)
    (add_net /SDAout)
    (add_net /Vpp)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(Q1-Pad1)")
  )
  (module neonpixel:SMD_pad (layer B.Cu) (tedit 5EB0150F)
    (at 138.4 55)
    (fp_text reference J4 (at 0 -0.5) (layer B.Fab) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 -1.2) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 /Vpp))
  )
  (module neonpixel:NeonPins (layer F.Cu) (tedit 5EB006B1)
    (at 148.8 56.1 90)
    (fp_text reference J1 (at 0 0.5 90) (layer F.Fab) hide)
    (fp_text value Conn_01x02_Female (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 2 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 2 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module neonpixel:SMD_inductor (layer F.Cu) (tedit 5EAFED1A)
    (at 147.2 55.4 270)
    (fp_text reference L1 (at 0 0.5 90) (layer F.Fab) hide)
    (fp_text value 10uH (at 0 -2.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.6 2 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.6 2 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module neonpixel:SMD_Diode (layer F.Cu) (tedit 5EAFEAE2)
    (at 149.5 55.8 270)
    (fp_text reference D1 (at 0 0.5 90) (layer F.Fab) hide)
    (fp_text value D_Schottky (at 0 -2.4 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.5 1.5 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.5 1.5 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module neonpixel:SMD_3_pin_254 (layer B.Cu) (tedit 5EAED37C)
    (at 134.5 53.5 180)
    (fp_text reference J3 (at 0 2.56) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -2.56) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 3 smd rect (at 0 -5.08 180) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /SCKout))
    (pad 1 smd rect (at 0 0 180) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -2.54 180) (size 3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /SDAout))
  )
  (module neonpixel:SMD_3_pin_254 (layer F.Cu) (tedit 5EAED37C)
    (at 134.5 58.58 180)
    (fp_text reference J2 (at 0 -2.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 2.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08 180) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDAin))
    (pad 1 smd rect (at 0 0 180) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0 2.54 180) (size 3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCKin))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 138.9 56.1 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference PIC (at -1.4 -0.1 90) (layer F.SilkS))
    (fp_text value PIC16F15313 (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCKout))
    (pad 6 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDAout))
    (pad 5 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 /Vpp))
    (pad 3 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDAin))
    (pad 2 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCKin))
    (pad 1 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 142.4 58.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0.1 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0.2 0.41 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 148.25 53.8 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.15 0) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 143.9 57.05)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.6 -1.35) (layer B.SilkS))
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 147.9 58.5 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.1 1.6) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 142.4 54.3 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -0.1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 152.5 56.1) (end 152.000002 54.700002) (angle -140.6923752) (layer Edge.Cuts) (width 0.05))
  (gr_text "pierre muth" (at 144.7 54.4) (layer B.Mask))
  (gr_text NeonPixel (at 143.3 53.5) (layer B.Mask))
  (gr_text Vpp (at 139 55) (layer B.SilkS))
  (gr_text Din (at 137.2 54.4) (layer F.SilkS))
  (gr_text Cin (at 137.2 56) (layer F.SilkS))
  (gr_text "Cout\n" (at 137.1 59.1) (layer B.SilkS))
  (gr_text Dout (at 137.1 56.5) (layer B.SilkS))
  (gr_text GND (at 136.9 54.4) (layer B.SilkS))
  (gr_text 5v (at 137.2 57.7) (layer F.SilkS))
  (gr_line (start 152 59.6) (end 152 57.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 52.6) (end 152 54.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133 52.6) (end 133 59.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 52.6) (end 133 52.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133 59.6) (end 152 59.6) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 133.5 52.6) (xy 149.6 52.6) (xy 149.6 59.6) (xy 133.5 59.6)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 133.5 59.6) (xy 133.5 52.6) (xy 149.7 52.6) (xy 149.7 59.6)
      )
    )
  )
)
