<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="0" x2="109.2" y2="0" width="0" layer="20"/>
<wire x1="109.2" y1="0" x2="109.2" y2="55.55" width="0" layer="20"/>
<wire x1="109.2" y1="55.55" x2="21.59" y2="55.55" width="0" layer="20"/>
<wire x1="21.59" y1="55.55" x2="21.59" y2="0" width="0" layer="20"/>
<text>Z Encoder Shield v 2.0
Allen Institute for Brain Science
May 2018</text>
<circle x="67.31" y="36.83" radius="2.83980625" width="0.0762" layer="20"/>
</plain>
<libraries>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B35N61">
<description>&lt;b&gt;BNC CONNECTOR&lt;/b&gt;&lt;p&gt;
M/A COM&lt;p&gt;
www.macom.com&lt;p&gt;
distributor Farnell 149-452</description>
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F15H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="ARDUINO-NOHOLE">
</package>
<package name="6MM">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CAMERA" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="IN" library="con-subd" package="F15H" value="IN">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="LED" library="con-coax" package="B35N61" value="BN35N61">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="OUT" library="con-subd" package="F15H" value="OUT">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="adafruit" package="0207/5V" value="24 kΩ"/>
<element name="U1" library="adafruit" package="ARDUINO-NOHOLE" value="ARDUINO-NOHOLE"/>
<element name="TM1" library="adafruit" package="6MM" value="50 kΩ"/>
<element name="U$1" library="holes" package="3,6" value=""/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="3V"/>
</signal>
<signal name="N$4">
<contactref element="IN" pad="4"/>
<contactref element="OUT" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IN" pad="5"/>
<contactref element="OUT" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IN" pad="6"/>
<contactref element="OUT" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="IN" pad="7"/>
<contactref element="OUT" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IN" pad="8"/>
<contactref element="OUT" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="IN" pad="10"/>
<contactref element="OUT" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="IN" pad="12"/>
<contactref element="OUT" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="IN" pad="13"/>
<contactref element="OUT" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="IN" pad="14"/>
<contactref element="OUT" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="IN" pad="15"/>
<contactref element="OUT" pad="15"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="D3"/>
<contactref element="CAMERA" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="LED" pad="1"/>
<contactref element="U1" pad="D4"/>
</signal>
<signal name="N$16">
<contactref element="IN" pad="1"/>
<contactref element="OUT" pad="1"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="GND2"/>
<contactref element="U1" pad="GND1"/>
<contactref element="OUT" pad="2"/>
<contactref element="IN" pad="2"/>
<contactref element="LED" pad="2"/>
<contactref element="LED" pad="3"/>
<contactref element="LED" pad="4"/>
<contactref element="LED" pad="5"/>
<contactref element="CAMERA" pad="2"/>
<contactref element="CAMERA" pad="3"/>
<contactref element="CAMERA" pad="4"/>
<contactref element="CAMERA" pad="5"/>
<contactref element="U1" pad="GND"/>
<contactref element="TM1" pad="E"/>
</signal>
<signal name="N$30">
<contactref element="IN" pad="3"/>
<contactref element="OUT" pad="3"/>
<contactref element="U1" pad="A2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="A1"/>
<contactref element="IN" pad="9"/>
<contactref element="OUT" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="A0"/>
<contactref element="OUT" pad="11"/>
<contactref element="IN" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="AREF"/>
<contactref element="R1" pad="1"/>
<contactref element="TM1" pad="S"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="5V"/>
<contactref element="R1" pad="2"/>
<contactref element="TM1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
