<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<text>3V3</text>
<text>GND</text>
<text>RXD</text>
<text>TXD</text>
<wire x1="0.254" y1="3.81" x2="0.254" y2="33.02" width="0.4064" layer="20"/>
<wire x1="0.254" y1="33.02" x2="4.318" y2="37.084" width="0.4064" layer="20" curve="-90"/>
<wire x1="4.318" y1="37.084" x2="56.134" y2="37.084" width="0.4064" layer="20"/>
<wire x1="56.134" y1="37.084" x2="60.198" y2="33.02" width="0.4064" layer="20" curve="-90"/>
<wire x1="60.198" y1="33.02" x2="60.198" y2="3.81" width="0.4064" layer="20"/>
<wire x1="60.198" y1="3.81" x2="56.388" y2="0" width="0.4064" layer="20" curve="-90"/>
<wire x1="56.388" y1="0" x2="4.064" y2="0" width="0.4064" layer="20"/>
<wire x1="4.064" y1="0" x2="0.254" y2="3.81" width="0.4064" layer="20" curve="-90"/>
<hole x="4.2418" y="4.0132" drill="3"/>
<hole x="56.261" y="4.0132" drill="3"/>
<hole x="56.261" y="32.9946" drill="3"/>
<hole x="4.2672" y="32.9946" drill="3"/>
<text>ANT</text>
<text>Tinkerman 2016
RFM69 GATEWAY
0.4.20160829</text>
<text>IO5</text>
</plain>
<libraries>
<library name="xose">
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="TACTILE-BUTTON-SMD">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="ESP-12-SMD">
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="RFM69CW-XXXS2">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMA_EDGELAUNCH">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="xose" package="SOT223" value="AMS1117-3.3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="OC_NEWARK" value="14P6981"/>
</element>
<element name="R1" library="xose" package="AXIAL-0.4" value="10K"/>
<element name="R2" library="xose" package="AXIAL-0.4" value="10K"/>
<element name="FLASH" library="xose" package="TACTILE-BUTTON-SMD" value=""/>
<element name="RESET" library="xose" package="TACTILE-BUTTON-SMD" value=""/>
<element name="C1" library="xose" package="C050-025X075" value="100nF"/>
<element name="C2" library="xose" package="CPOL-RADIAL-10UF-25V" value="47uF"/>
<element name="J1" library="xose" package="POWER_JACK_PTH" value="">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="R3" library="xose" package="AXIAL-0.4" value="10K"/>
<element name="R4" library="xose" package="AXIAL-0.4" value="10K"/>
<element name="C3" library="xose" package="C050-025X075" value="100nF"/>
<element name="R5" library="xose" package="AXIAL-0.4" value="10K"/>
<element name="C4" library="xose" package="C050-025X075" value="100nF"/>
<element name="IC1" library="xose" package="ESP-12-SMD" value="ESP-12-SMD"/>
<element name="U1" library="xose" package="RFM69CW-XXXS2" value="RFM69CW"/>
<element name="X1" library="adafruit" package="SMA_EDGELAUNCH" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X01NS" value=""/>
<element name="JP3" library="xose" package="1X05" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="FLASH" pad="2"/>
<contactref element="RESET" pad="2"/>
<contactref element="FLASH" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="GND"/>
<contactref element="U1" pad="14"/>
<contactref element="R5" pad="P$1"/>
<contactref element="X1" pad="GND@4"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X1" pad="GND@3"/>
<contactref element="U1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="X1" pad="GND@1"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="P$1"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="RESET"/>
</signal>
<signal name="3V3">
<contactref element="R4" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="VCC"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GPIO0">
<contactref element="R1" pad="P$1"/>
<contactref element="FLASH" pad="3"/>
<contactref element="FLASH" pad="4"/>
<contactref element="IC1" pad="GPIO0"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="TX"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="RX"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="GPIO2"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="8"/>
<contactref element="IC1" pad="GPIO12"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="IC1" pad="GPIO13"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="6"/>
<contactref element="IC1" pad="GPIO14"/>
</signal>
<signal name="NSS">
<contactref element="U1" pad="7"/>
<contactref element="R5" pad="P$2"/>
<contactref element="IC1" pad="GPIO15"/>
</signal>
<signal name="ANT">
<contactref element="U1" pad="1"/>
<contactref element="X1" pad="P"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GPIO4">
<contactref element="U1" pad="9"/>
<contactref element="IC1" pad="GPIO4"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="CH_PD"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$2">
</signal>
<signal name="GPIO5">
<contactref element="JP3" pad="3"/>
<contactref element="IC1" pad="GPIO5"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="13"/>
<contactref element="IC1" pad="GPIO16"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
