(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 39)
    (zones 0)
    (modules 6)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad3)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad5)")
  (net 4 "Net-(P2-Pad3)")
  (net 5 "Net-(P2-Pad2)")
  (net 6 GND)
  (net 7 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(P1-Pad5)")
  )
  (net_class Signal ""
    (clearance 0.2)
    (trace_width 0.2032)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
  )
  (module Connect:USB_A (layer F.Cu) (tedit 5A617DDA)
    (at 123.19 108.585)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P2 (at -12.065 -11.43) (layer F.SilkS))
    (fp_text value Female (at 3.83794 7.43458) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11286 -0.00212 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole circle (at 4.57286 -0.00212 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54086 -0.00212 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at 0.00086 -0.00212 270) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 +5V))
    (pad 5 thru_hole circle (at 10.16086 2.66488 270) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad5)"))
    (pad 5 thru_hole circle (at -3.55514 2.66488 270) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad5)"))
    (model Connect.3dshapes/USB_A.wrl
      (offset (xyz 3.555999946594238 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:USB_A_Male (layer F.Cu) (tedit 5A617DD5)
    (at 123.19 87.63 180)
    (fp_text reference P1 (at 12.065 -2.54 180) (layer F.SilkS))
    (fp_text value Male (at -1.905 3.175 180) (layer F.Fab))
    (pad 4 thru_hole circle (at -7.2 -4.4 180) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole circle (at -4.6 -4.4 180) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at -2.6 -4.4 180) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -4.4 180) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 +5V))
    (pad 5 thru_hole circle (at -9.6 -2.9 180) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad5)"))
    (pad 5 thru_hole circle (at 2.4 -2.9 180) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad5)"))
    (pad "" np_thru_hole circle (at -5.9 -2.8 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.3 -2.8 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5A617E83)
    (at 121.92 102.235)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at -10.16 -5.715) (layer F.SilkS))
    (fp_text value 75k (at -10.16 1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(P2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5A617E89)
    (at 121.92 105.41)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 20.955 -3.175) (layer F.SilkS))
    (fp_text value 50k (at 20.955 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(P2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5A617E84)
    (at 121.92 95.25)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at -10.16 -3.81) (layer F.SilkS))
    (fp_text value 75k (at -10.16 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(P2-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5A617E87)
    (at 121.92 98.425)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 20.955 -1.27) (layer F.SilkS))
    (fp_text value 50k (at 19.05 -3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "California\nCybersecurity\nInstitute" (at 126.59 111.53) (layer B.Mask))
  (gr_text "Charge Safely" (at 134.58 99.79 90) (layer F.SilkS))
  (dimension 18.415 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7250 in" (at 126.6925 83.725) (layer Dwgs.User))
    (feature1 (pts (xy 135.9 88.25) (xy 135.9 82.375)))
    (feature2 (pts (xy 117.485 88.25) (xy 117.485 82.375)))
    (crossbar (pts (xy 117.485 85.075) (xy 135.9 85.075)))
    (arrow1a (pts (xy 135.9 85.075) (xy 134.773496 85.661421)))
    (arrow1b (pts (xy 135.9 85.075) (xy 134.773496 84.488579)))
    (arrow2a (pts (xy 117.485 85.075) (xy 118.611504 85.661421)))
    (arrow2b (pts (xy 117.485 85.075) (xy 118.611504 84.488579)))
  )
  (dimension 25.42526 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0010 in" (at 112.302521 100.928845 89.74084682) (layer Dwgs.User))
    (feature1 (pts (xy 117.475 113.665) (xy 113.758585 113.64819)))
    (feature2 (pts (xy 117.59 88.24) (xy 113.873585 88.22319)))
    (crossbar (pts (xy 114.46 88.225843) (xy 114.345 113.650843)))
    (arrow1a (pts (xy 114.345 113.650843) (xy 113.763681 112.521698)))
    (arrow1b (pts (xy 114.345 113.650843) (xy 114.93651 112.527003)))
    (arrow2a (pts (xy 114.46 88.225843) (xy 113.86849 89.349683)))
    (arrow2b (pts (xy 114.46 88.225843) (xy 115.041319 89.354988)))
  )
  (gr_text "X=43k, 1A" (at 127.635 93.98 90) (layer B.SilkS))
  (gr_text "X=75k, .5A" (at 125.73 93.98 90) (layer B.SilkS))
  (gr_text Male (at 126.43 89.26 180) (layer F.SilkS))
  (gr_text Female (at 126.365 111.125) (layer F.SilkS))
  (gr_text 51k (at 127 105.41) (layer F.SilkS))
  (gr_text 51k (at 127 98.425) (layer F.SilkS))
  (gr_text X (at 127 102.235) (layer F.SilkS))
  (gr_text 75k (at 127 95.25) (layer F.SilkS))
  (gr_line (start 135.89 113.665) (end 117.475 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.9 88.26) (end 135.89 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.49 88.26) (end 135.9 88.26) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.475 113.665) (end 117.49 88.26) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text CCIC (at 119.12 99.79 90) (layer F.SilkS))
  (zone (net 7) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.475 87.63) (xy 126.365 87.63) (xy 126.365 113.665) (xy 117.475 113.665)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 87.63) (xy 135.89 87.63) (xy 135.89 113.665) (xy 127 113.665)
      )
    )
  )
  (zone (net 3) (net_name "Net-(P1-Pad5)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.475 87.63) (xy 135.89 87.63) (xy 135.89 113.665) (xy 117.475 113.665)
      )
    )
  )
)
