<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="20.32" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="60.96" y2="0" width="0" layer="20"/>
<wire x1="60.96" y1="0" x2="63.5" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="63.5" y1="2.54" x2="63.5" y2="20.32" width="0" layer="20"/>
<wire x1="63.5" y1="20.32" x2="60.96" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="60.96" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="2.54" y1="22.86" x2="0" y2="20.32" width="0" layer="20" curve="90"/>
<hole x="48.26" y="2.54" drill="2.54"/>
<hole x="48.26" y="20.32" drill="2.54"/>
<text>Capable Robot 
SenseTemp Adapter
[CRY8EI]</text>
</plain>
<libraries>
<library name="CapableRobot">
<packages>
<package name="CONN-2X8-050-SMT-ZT">
</package>
<package name="CRC-LOGO-7-SILK">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="B"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SENSETEMP" library="CapableRobot" package="CONN-2X8-050-SMT-ZT" value="CONN-16ZT">
<attribute name="MPN" value="3221-16-0300-00"/>
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="CapableRobot" package="CRC-LOGO-7-SILK" value="CRC-LOGO7SILK"/>
<element name="RTD1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="RTD2" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="RTD3" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="RTD4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
</signal>
<signal name="RTDIN1+">
<contactref element="SENSETEMP" pad="3"/>
<contactref element="SENSETEMP" pad="4"/>
<contactref element="RTD1" pad="2"/>
</signal>
<signal name="RTDIN1-">
<contactref element="SENSETEMP" pad="1"/>
<contactref element="SENSETEMP" pad="2"/>
<contactref element="RTD1" pad="1"/>
</signal>
<signal name="RTDIN2+">
<contactref element="SENSETEMP" pad="7"/>
<contactref element="SENSETEMP" pad="8"/>
<contactref element="RTD2" pad="2"/>
</signal>
<signal name="RTDIN2-">
<contactref element="SENSETEMP" pad="5"/>
<contactref element="SENSETEMP" pad="6"/>
<contactref element="RTD2" pad="1"/>
</signal>
<signal name="RTDIN3+">
<contactref element="SENSETEMP" pad="11"/>
<contactref element="SENSETEMP" pad="12"/>
<contactref element="RTD3" pad="2"/>
</signal>
<signal name="RTDIN3-">
<contactref element="SENSETEMP" pad="9"/>
<contactref element="SENSETEMP" pad="10"/>
<contactref element="RTD3" pad="1"/>
</signal>
<signal name="RTDIN4+">
<contactref element="SENSETEMP" pad="15"/>
<contactref element="SENSETEMP" pad="16"/>
<contactref element="RTD4" pad="2"/>
</signal>
<signal name="RTDIN4-">
<contactref element="SENSETEMP" pad="13"/>
<contactref element="SENSETEMP" pad="14"/>
<contactref element="RTD4" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$1">
</signal>
<signal name="OUT">
</signal>
</signals>
</board>
</drawing>
</eagle>
