<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="49" y1="39" x2="65" y2="39" width="0.2" layer="20"/>
<wire x1="49" y1="39" x2="49" y2="52" width="0.2" layer="20"/>
<wire x1="65" y1="39" x2="65" y2="52" width="0.2" layer="20"/>
<wire x1="65" y1="52" x2="68" y2="52" width="0.2" layer="20"/>
<wire x1="49" y1="52" x2="46" y2="52" width="0.2" layer="20"/>
<wire x1="46" y1="52" x2="46" y2="70" width="0.2" layer="20"/>
<wire x1="46" y1="70" x2="49.4" y2="70" width="0.2" layer="20"/>
<wire x1="64.5" y1="70" x2="68" y2="70" width="0.2" layer="20"/>
<wire x1="68" y1="70" x2="68" y2="52" width="0.2" layer="20"/>
<wire x1="49.4" y1="70" x2="49.4" y2="53.6" width="0.2" layer="20"/>
<wire x1="49.4" y1="53.6" x2="64.5" y2="53.6" width="0.2" layer="20"/>
<wire x1="64.5" y1="53.6" x2="64.5" y2="70" width="0.2" layer="20"/>
</plain>
<libraries>
<library name="sd-mmc">
<packages>
<package name="TF-PULL-REVERSE">
<description>TF / Micro SD socket is PUSH-PUSH type, the card can be pushed into and auto locked and pushed out by simply press the card.
&lt;p&gt;
Surface Mounting type.</description>
</package>
</packages>
</library>
<library name="untitled">
<packages>
<package name="CONNECTOR">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SD1" library="sd-mmc" package="TF-PULL-REVERSE" value="TF-HOLDERREVERSE"/>
<element name="U$1" library="untitled" package="CONNECTOR" value="CONNECTOR"/>
<element name="TP1" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP7" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP8" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="VCC"/>
<contactref element="TP8" pad="TP"/>
<contactref element="SD1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="CMD"/>
<contactref element="SD1" pad="3"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="DAT0"/>
<contactref element="SD1" pad="7"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="DAT1"/>
<contactref element="SD1" pad="8"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="DAT2"/>
<contactref element="SD1" pad="1"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="DAT3"/>
<contactref element="SD1" pad="2"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="CLK"/>
<contactref element="SD1" pad="5"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="INS"/>
<contactref element="TP7" pad="TP"/>
<contactref element="SD1" pad="6"/>
<contactref element="SD1" pad="S3"/>
<contactref element="SD1" pad="S2"/>
<contactref element="SD1" pad="S1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
