(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0)")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 70)
    (zones 0)
    (modules 12)
    (nets 11)
  )
  (page A4)
  (title_block
    (title Lever)
    (date 2020-01-21)
    (rev 1.1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad1)")
  (net 2 "Net-(U1-Pad7)")
  (net 3 "Net-(U1-Pad4)")
  (net 4 /Vcc)
  (net 5 /GND)
  (net 6 /DIO_A)
  (net 7 /DIO_B)
  (net 8 /DIO_C)
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DIO_A)
    (add_net /DIO_B)
    (add_net /DIO_C)
    (add_net /GND)
    (add_net /Vcc)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad7)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5E2898D4)
    (at 132.715 74.676)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 -270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DIO_B))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5E2898C2)
    (at 113.03 94.615 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Vcc))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)"))
  )
  (module Capacitor_SMD:CP_Elec_6.3x4.9 (layer F.Cu) (tedit 5BCA39CF)
    (at 101.0285 86.106 90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 4.1275 -2.54 180) (layer F.SilkS))
    (fp_text value "470 µF" (at 0 4.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.8 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 5 /GND))
    (pad 1 smd roundrect (at -2.8 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 /Vcc))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x4.9.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 121.6025 94.8055 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0.0635 1.3335 270) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Vcc))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 133.604 90.424 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 133.604 94.996 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 127 92.71 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -4.5085 -3.4925 180) (layer F.SilkS))
    (fp_text value ATtiny84-20SSU (at 0 5.28 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user e (at 0 0 90) (layer F.Fab) hide)
    (pad 14 smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (pad 13 smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)"))
    (pad 9 smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /DIO_A))
    (pad 8 smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(J3-Pad1)"))
    (pad 7 smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DIO_C))
    (pad 4 smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(U1-Pad4)"))
    (pad 3 smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /Vcc))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 133.35 84.1375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 100.965 73.66)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 100.965 94.615)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module asl_footprints:AVR_ISP (layer F.Cu) (tedit 5E2766C0)
    (at 125.095 81.28 180)
    (fp_text reference X1 (at 0.127 8.128) (layer F.SilkS))
    (fp_text value AVR_ISP (at -1.27 -8.255) (layer F.Fab))
    (pad 6 thru_hole circle (at 1.27 2.54 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 5 thru_hole circle (at -1.27 2.54 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad4)"))
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad7)"))
    (pad 3 thru_hole circle (at -1.27 0 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 /DIO_A))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 /Vcc))
    (pad 1 thru_hole circle (at -1.27 -2.54 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (model ${KIPRJMOD}/libs/3d/ICSP.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:RJ45_SMD_Vertical (layer F.Cu) (tedit 5E2768F3)
    (at 112.395 80.518 180)
    (fp_text reference J1 (at 5.969 7.62) (layer F.SilkS))
    (fp_text value RJ45_pyControl (at 0.635 -2.54) (layer F.Fab) hide)
    (fp_text user J2 (at 0 7.62) (layer F.SilkS) hide)
    (pad 7 smd rect (at 3.175 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 4.445 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 1.905 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vcc) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 0.635 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 8 /DIO_C) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -4.445 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 /DIO_A) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -3.175 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 5 /GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -1.905 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad MNT smd rect (at 0 7.62 270) (size 4.5 8.8) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -0.635 -8.31 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIO_B) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/libs/3d/RJ45_smd_vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Lever\nv1.1\n" (at 100.965 78.74) (layer F.SilkS))
  (gr_text Gnd (at 135.382 74.676) (layer F.SilkS))
  (gr_text 5V (at 110.49 96.774) (layer B.SilkS))
  (gr_text Gnd (at 107.95 96.774) (layer B.SilkS))
  (gr_text Gnd (at 107.95 96.774) (layer F.SilkS))
  (gr_text 5V (at 110.49 96.774) (layer F.SilkS))
  (dimension 32.385 (width 0.15) (layer Dwgs.User)
    (gr_text "1.2750 in" (at 117.1575 65.375) (layer Dwgs.User))
    (feature1 (pts (xy 133.35 69.85) (xy 133.35 66.088579)))
    (feature2 (pts (xy 100.965 69.85) (xy 100.965 66.088579)))
    (crossbar (pts (xy 100.965 66.675) (xy 133.35 66.675)))
    (arrow1a (pts (xy 133.35 66.675) (xy 132.223496 67.261421)))
    (arrow1b (pts (xy 133.35 66.675) (xy 132.223496 66.088579)))
    (arrow2a (pts (xy 100.965 66.675) (xy 102.091504 67.261421)))
    (arrow2b (pts (xy 100.965 66.675) (xy 102.091504 66.088579)))
  )
  (dimension 20.955 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8250 in" (at 90.14 84.1375 270) (layer Dwgs.User))
    (feature1 (pts (xy 100.965 94.615) (xy 90.853579 94.615)))
    (feature2 (pts (xy 100.965 73.66) (xy 90.853579 73.66)))
    (crossbar (pts (xy 91.44 73.66) (xy 91.44 94.615)))
    (arrow1a (pts (xy 91.44 94.615) (xy 90.853579 93.488496)))
    (arrow1b (pts (xy 91.44 94.615) (xy 92.026421 93.488496)))
    (arrow2a (pts (xy 91.44 73.66) (xy 90.853579 74.786504)))
    (arrow2b (pts (xy 91.44 73.66) (xy 92.026421 74.786504)))
  )
  (gr_arc (start 133.35 94.615) (end 133.35 98.425) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100.965 94.615) (end 97.155 94.615) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100.965 73.66) (end 100.965 69.85) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 133.35 73.66) (end 137.16 73.66) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.155 94.615) (end 97.155 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.35 98.425) (end 100.965 98.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 73.66) (end 137.16 94.615) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.965 69.85) (end 133.35 69.85) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 104.14) (xy 92.075 104.14) (xy 92.075 66.675) (xy 140.97 66.675)
      )
    )
  )
  (zone (net 5) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 105.41) (xy 91.44 105.41) (xy 91.44 66.04) (xy 141.605 66.04)
      )
    )
  )
)
