(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 53)
    (zones 0)
    (modules 13)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.76)
    (user_trace_width 0.76)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad14)")
  (net 2 "Net-(J1-Pad17)")
  (net 3 "Net-(J1-Pad20)")
  (net 4 "Net-(J1-Pad23)")
  (net 5 "Net-(J1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad23)")
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 110.8 122)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J7 (at 0 2.25) (layer Dwgs.User))
    (fp_text value Y- (at 0.25 2.35) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad20)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 106 122)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J9 (at 0 2.25) (layer Dwgs.User))
    (fp_text value Y+ (at 0.3 2.3) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad23)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey_MDM_182-25FE-ND:digikey_MDM_182-25FE-ND (layer F.Cu) (tedit 0)
    (at 120.8 107.5)
    (fp_text reference J1 (at -7.3025 0.549999) (layer F.SilkS))
    (fp_text value DB25_Female_MountingHoles (at -7.3025 0.549999) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 28 thru_hole circle (at 4.972502 0.549999 90) (size 3.048 3.048) (drill 2.54) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -19.577502 0.549999 90) (size 3.048 3.048) (drill 2.54) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -0.635 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at -1.905 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -3.175 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -4.445 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad17)"))
    (pad 18 thru_hole circle (at -5.715 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -6.985 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -8.255 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad20)"))
    (pad 21 thru_hole circle (at -9.525 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -10.795 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -12.065 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad23)"))
    (pad 24 thru_hole circle (at -13.335 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -14.605 1.099998) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.27 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 3 thru_hole circle (at -2.54 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.81 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -5.08 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 6 thru_hole circle (at -6.35 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -7.62 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -8.89 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 9 thru_hole circle (at -10.16 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -11.43 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -12.7 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -13.97 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -15.24 0) (size 0.8636 0.8636) (drill 0.6096) (layers *.Cu *.Mask))
  )
  (module digikey_10pin_1175-1627-ND:digikey_10pin_1175-1627-ND (layer F.Cu) (tedit 0)
    (at 110.9 114.2)
    (fp_text reference J5 (at 2.54 -0.635) (layer Cmts.User))
    (fp_text value 3220-10-0100-00 (at 2.54 -0.635) (layer Cmts.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 10 thru_hole circle (at 5.08 -1.27) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 9 thru_hole circle (at 5.08 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad14)"))
    (pad 8 thru_hole circle (at 3.81 -1.27) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad17)"))
    (pad 6 thru_hole circle (at 2.54 -1.27) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 5 thru_hole circle (at 2.54 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad20)"))
    (pad 4 thru_hole circle (at 1.27 -1.27) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad23)"))
    (pad 2 thru_hole circle (at 0 -1.27) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.1684 1.1684) (drill 0.7112) (layers *.Cu *.Mask))
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 97.5 112.5)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J11 (at 0 2.25) (layer Dwgs.User))
    (fp_text value GND (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 116 122)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J6 (at 0 2.25) (layer Dwgs.User))
    (fp_text value X- (at 0.25 2.4) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad17)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 119.5 102.9)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J4 (at 0 2.25) (layer Dwgs.User))
    (fp_text value GND (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 108.15 102.9)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J3 (at 0 2.25) (layer Dwgs.User))
    (fp_text value GND (at 0 -2.05) (layer F.SilkS))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.0mm_L10.0mm (layer F.Cu) (tedit 5A1DC084)
    (at 121 122)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference J2 (at 0 2.25) (layer Dwgs.User))
    (fp_text value X+ (at 0.35 2.45) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad14)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 127.186 121.195)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.7) (layer Cmts.User))
    (fp_text value MountingHole (at 0 3.7) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 127.186 100.875)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.7) (layer Cmts.User))
    (fp_text value MountingHole (at 0.06 4) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 99.5 121.195)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.7) (layer Cmts.User))
    (fp_text value MountingHole (at 0 3.7) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 99.5 100.875)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.7) (layer Cmts.User))
    (fp_text value MountingHole (at 0 3.7) (layer Dwgs.User))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (dimension 12.800391 (width 0.15) (layer Dwgs.User)
    (gr_text "12.800 mm" (at 126.612854 112.10475 359.5523858) (layer Dwgs.User))
    (feature1 (pts (xy 133 113.8) (xy 133.007279 112.868307)))
    (feature2 (pts (xy 120.2 113.7) (xy 120.207279 112.768307)))
    (crossbar (pts (xy 120.202698 113.35471) (xy 133.002698 113.45471)))
    (arrow1a (pts (xy 133.002698 113.45471) (xy 131.871647 114.032312)))
    (arrow1b (pts (xy 133.002698 113.45471) (xy 131.88081 112.859507)))
    (arrow2a (pts (xy 120.202698 113.35471) (xy 121.324586 113.949913)))
    (arrow2b (pts (xy 120.202698 113.35471) (xy 121.333749 112.777108)))
  )
  (gr_text "V1\nHM" (at 130.95 124.8) (layer F.SilkS))
  (gr_text "Version 1, June 2023" (at 113.25 98.25) (layer B.SilkS))
  (gr_text "MEMS Breakout: MDM to 10pin — INVERTED\n" (at 113.35 96.4) (layer B.SilkS))
  (gr_text "MEMS Breakout: MDM to 10pin — INVERTED" (at 113.45 96.4) (layer F.SilkS))
  (gr_line (start 94 95) (end 133 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 95) (end 94 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133 127) (end 94 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133 95) (end 133 127) (layer Edge.Cuts) (width 0.15))
)
