(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 20)
    (no_connects 0)
    (area 129.464999 88.824999 167.413715 121.572001)
    (thickness 1.6002)
    (drawings 39)
    (tracks 61)
    (zones 0)
    (modules 5)
    (nets 17)
  )
  (page USLetter)
  (title_block
    (title RS422-breakout)
    (date 2017-05-15)
    (rev 1)
    (company "Space Sciences Laboratory")
    (comment 1 "Drawn by David Sundkvist")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/davids/KiCAD/TRICE2/RS422_breakout/gerbers))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 1A)
  (net 4 1Y)
  (net 5 1Z)
  (net 6 G)
  (net 7 2Z)
  (net 8 2Y)
  (net 9 2A)
  (net 10 4A)
  (net 11 4Y)
  (net 12 4Z)
  (net 13 ~G~)
  (net 14 3Z)
  (net 15 3Y)
  (net 16 3A)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net 1A)
    (add_net 1Y)
    (add_net 1Z)
    (add_net 2A)
    (add_net 2Y)
    (add_net 2Z)
    (add_net 3A)
    (add_net 3Y)
    (add_net 3Z)
    (add_net 4A)
    (add_net 4Y)
    (add_net 4Z)
    (add_net G)
    (add_net VCC)
    (add_net ~G~)
  )
  (net_class Ground ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 591A3A21)
    (at 142.24 93.98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 591A3A24)
    (at 142.24 97.79 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 591A3A16)
    (at 142.24 105.41)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 6.35) (layer F.SilkS))
    (fp_text value AM26LV31 (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 1A))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 1Y))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 1Z))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 G))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 2Z))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 2Y))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 2A))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 3A))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 3Y))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 3Z))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 ~G~))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 4Z))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 4Y))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 4A))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 134.62 93.98)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 1A))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 1Y))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 1Z))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 G))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 2Z))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 2Y))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 2A))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 149.86 93.98)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 4A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 4Y))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 4Z))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 ~G~))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 3Z))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 3Y))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 3A))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text 3B (at 152.908 112.268) (layer F.SilkS))
  (gr_text 3A (at 152.908 109.728) (layer F.SilkS))
  (gr_text 3Y (at 152.908 107.188) (layer F.SilkS))
  (gr_text 4Y (at 152.908 102.108) (layer F.SilkS))
  (gr_text 4A (at 152.908 99.568) (layer F.SilkS))
  (gr_text 4B (at 152.908 97.028) (layer F.SilkS))
  (gr_text 2B (at 132.588 109.22) (layer F.SilkS))
  (gr_text 2A (at 132.588 106.68) (layer F.SilkS))
  (gr_text 2Y (at 132.588 104.14) (layer F.SilkS))
  (gr_text 1Y (at 132.588 99.06) (layer F.SilkS))
  (gr_text 1A (at 132.588 96.52) (layer F.SilkS))
  (gr_text 1B (at 132.588 93.98) (layer F.SilkS))
  (dimension 27.94 (width 0.3) (layer Eco1.User)
    (gr_text "1.1000 in" (at 161.878 102.87 90) (layer Eco1.User))
    (feature1 (pts (xy 153.162 88.9) (xy 163.228 88.9)))
    (feature2 (pts (xy 153.162 116.84) (xy 163.228 116.84)))
    (crossbar (pts (xy 160.528 116.84) (xy 160.528 88.9)))
    (arrow1a (pts (xy 160.528 88.9) (xy 161.114421 90.026504)))
    (arrow1b (pts (xy 160.528 88.9) (xy 159.941579 90.026504)))
    (arrow2a (pts (xy 160.528 116.84) (xy 161.114421 115.713496)))
    (arrow2b (pts (xy 160.528 116.84) (xy 159.941579 115.713496)))
  )
  (dimension 25.4 (width 0.3) (layer Eco1.User)
    (gr_text "1.0000 in" (at 142.24 120.222) (layer Eco1.User))
    (feature1 (pts (xy 154.94 115.316) (xy 154.94 121.572)))
    (feature2 (pts (xy 129.54 115.316) (xy 129.54 121.572)))
    (crossbar (pts (xy 129.54 118.872) (xy 154.94 118.872)))
    (arrow1a (pts (xy 154.94 118.872) (xy 153.813496 119.458421)))
    (arrow1b (pts (xy 154.94 118.872) (xy 153.813496 118.285579)))
    (arrow2a (pts (xy 129.54 118.872) (xy 130.666504 119.458421)))
    (arrow2b (pts (xy 129.54 118.872) (xy 130.666504 118.285579)))
  )
  (gr_text 2A/ (at 131.572 108.712) (layer F.SilkS))
  (gr_text 2Y/ (at 131.572 106.172) (layer F.SilkS))
  (gr_text 2Z/ (at 131.572 103.632) (layer F.SilkS))
  (gr_text G (at 132.08 101.6) (layer F.SilkS))
  (gr_text 1Z/ (at 131.572 98.552) (layer F.SilkS))
  (gr_text 1Y/ (at 131.572 96.012) (layer F.SilkS))
  (gr_text 1A/ (at 131.572 93.472) (layer F.SilkS))
  (gr_text 3A/ (at 152.4 111.252) (layer F.SilkS))
  (gr_text 3Y/ (at 152.4 108.712) (layer F.SilkS))
  (gr_text 4Z/ (at 152.4 101.092) (layer F.SilkS))
  (gr_text 4A/ (at 152.4 96.012) (layer F.SilkS))
  (gr_text ~G~ (at 152.654 104.14) (layer F.SilkS))
  (gr_text 4Y/ (at 152.4 98.552) (layer F.SilkS))
  (gr_text 3Z/ (at 152.4 106.172) (layer F.SilkS))
  (gr_text VCC (at 152.4 93.98) (layer F.SilkS))
  (gr_text GND (at 132.08 111.76) (layer F.SilkS))
  (gr_text "RS422 AM26LV31X/AM26LV32X\nRev. 1, D. S., 2017" (at 142.24 114.3) (layer F.SilkS))
  (gr_arc (start 130.81 115.57) (end 130.81 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.81 90.17) (end 129.54 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 90.17) (end 153.67 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 115.57) (end 154.94 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 115.57) (end 129.54 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 116.84) (end 130.81 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 90.17) (end 154.94 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 88.9) (end 153.67 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 115.57) (xy 130.81 114.3) (xy 130.81 91.44) (xy 132.08 90.17) (xy 152.4 90.17)
        (xy 153.67 91.44) (xy 153.67 114.3) (xy 152.4 115.57)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 115.57) (xy 130.81 114.3) (xy 130.81 91.44) (xy 132.08 90.17) (xy 152.4 90.17)
        (xy 153.67 91.44) (xy 153.67 114.3) (xy 152.4 115.57)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.15) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 144.272 99.0854) (xy 144.7546 99.0854) (xy 144.7546 99.9236) (xy 144.272 99.9236) (xy 144.272 100.0252)
        (xy 143.6116 100.6856) (xy 143.7386 100.6856) (xy 143.7386 110.5662) (xy 142.6972 110.5662) (xy 142.6972 100.6856)
        (xy 142.7226 100.6856) (xy 142.5194 100.4824) (xy 141.478 98.8314) (xy 144.272 98.8314)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.478 94.742) (xy 143.002 94.742) (xy 143.002 97.028) (xy 141.478 97.028)
      )
    )
  )
)
