(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "+15V")
  (net 4 "GND")
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "-15V")
  (net 8 "unconnected-(U1-Pad9)")
  (net 9 "Net-(U1-Pad12)")
  (net 10 "unconnected-(U1-Pad13)")
  (net 11 "unconnected-(U2-Pad2)")
  (net 12 "unconnected-(U2-Pad9)")
  (net 13 "unconnected-(U2-Pad13)")
  (net 14 "Net-(R1-Pad2)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R5-Pad2)")
  (footprint "Package_DIP:DIP-14_W7.62mm_Socket_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 111.76 58.415)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS") hide)
    (fp_text value "SSM2056" (at 3.81 7.625 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)") (pinfunction "Release") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Trim") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)") (pinfunction "Decay") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R5-Pad2)") (pinfunction "Attack") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)") (pinfunction "Trig") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad6)") (pinfunction "Gate") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "-15V") (pinfunction "-V") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "unconnected-(U1-Pad9)") (pinfunction "Substrate") (pintype "output+no_connect"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Out") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pinfunction "Cap") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad12)") (pinfunction "Sustain") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "unconnected-(U1-Pad13)") (pinfunction "N.C.") (pintype "no_connect"))
    (pad "14" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+15V") (pinfunction "+V") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 91.44 73.66)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at -0.127 1.27) (layer "F.SilkS"))
    (fp_text value "2K7" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 91.44 71.12)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at -0.127 -1.27) (layer "F.SilkS"))
    (fp_text value "4K7" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 91.44 67.31)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at -0.127 1.27) (layer "F.SilkS"))
    (fp_text value "220K" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+15V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 91.44 64.77)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at -0.127 -1.29) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+15V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 122.682 71.04 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -1.945 0.635 90) (layer "F.SilkS"))
    (fp_text value "68nF" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 91.44 58.42)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at -0.127 -1.27) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+15V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 101.346 58.415)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS") hide)
    (fp_text value "to SSM2050 socket" (at 3.81 7.625 -90) (layer "B.SilkS"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)") (pinfunction "Release") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "unconnected-(U2-Pad2)") (pinfunction "N.C.") (pintype "no_connect"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)") (pinfunction "Decay") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R5-Pad2)") (pinfunction "Attack") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)") (pinfunction "Trig") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad6)") (pinfunction "Gate") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Gnd") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "-15V") (pinfunction "-V") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "unconnected-(U2-Pad9)") (pinfunction "N.C.") (pintype "no_connect"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "Out") (pintype "output"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)") (pinfunction "Cap") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad12)") (pinfunction "Sustain") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "unconnected-(U2-Pad13)") (pinfunction "N.C.") (pintype "no_connect"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+15V") (pinfunction "+V") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint ".Projet:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 99.06 60.96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "SSM2050 to SSM2056 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 7.747 -1.27 180) (layer "F.SilkS"))
    (fp_text value "4K7" (at 3.81 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_poly
    (pts
      (xy 124.213231 56.644047)
      (xy 124.330953 56.761769)
      (xy 124.414194 56.905948)
      (xy 124.457284 57.066758)
      (xy 124.46 57.15)
      (xy 124.46 74.93)
      (xy 124.457284 75.013242)
      (xy 124.414194 75.174052)
      (xy 124.330953 75.318231)
      (xy 124.213231 75.435953)
      (xy 124.069052 75.519194)
      (xy 123.908242 75.562284)
      (xy 123.825 75.565)
      (xy 90.805 75.565)
      (xy 90.721758 75.562284)
      (xy 90.560948 75.519194)
      (xy 90.416769 75.435953)
      (xy 90.299047 75.318231)
      (xy 90.215806 75.174052)
      (xy 90.172716 75.013242)
      (xy 90.17 74.93)
      (xy 90.17 57.15)
      (xy 90.172716 57.066758)
      (xy 90.215806 56.905948)
      (xy 90.299047 56.761769)
      (xy 90.416769 56.644047)
      (xy 90.560948 56.560806)
      (xy 90.721758 56.517716)
      (xy 90.805 56.515)
      (xy 123.825 56.515)
      (xy 123.908242 56.517716)
      (xy 124.069052 56.560806)
    ) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Add\n22K||R47(22K)\n10K||R74(10K)\n10K||R79(10K)\n\nRemove\nT6(2N3819)\nC10(10nF)\nC11(10nF)\n\nUnused\nT1(2N3906)\nR66(47K)\nR67(100K)\nR68(10K)\n\nChange/verify\nR53=100K\nR54=100K\nR62=100K\nR63=100K" (at 98.171 66.04) (layer "B.SilkS"))
  (gr_text "by" (at 123.19 64.77 90) (layer "F.SilkS"))
  (gr_text "for Kobol Xpdr I" (at 121.92 64.77 90) (layer "F.SilkS"))
  (gr_text "Rev1" (at 122.555 74.295) (layer "B.Mask"))
  (gr_text "G.Müller" (at 123.19 63.5 90) (layer "F.Mask"))
  (zone (net 4) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.05) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 124.46 75.565)
        (xy 90.17 75.565)
        (xy 90.17 56.515)
        (xy 124.46 56.515)
      )
    )
  )
)
