(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 44)
    (zones 0)
    (modules 4)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad7)")
  (net 2 /PIN6)
  (net 3 /PIN8)
  (net 4 /VCC)
  (net 5 /GND)
  (net 6 /RESET)
  (net 7 /SET)
  (net 8 /RX)
  (net 9 /TX)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /PIN6)
    (add_net /PIN8)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SET)
    (add_net /TX)
    (add_net "Net-(J2-Pad7)")
  )
  (net_class pwr ""
    (clearance 0.1524)
    (trace_width 0.4572)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /GND)
    (add_net /VCC)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 5C0E0038)
    (at 78.105 69.215)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference J1 (at 0.635 -1.695) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 16.764 10.16) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /VCC))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /VCC))
    (pad 3 thru_hole oval (at 0 1.27) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 4 thru_hole oval (at 1.27 1.27) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 5 thru_hole oval (at 0 2.54) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /RESET))
    (pad 6 thru_hole oval (at 1.27 2.54) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /PIN6))
    (pad 7 thru_hole oval (at 0 3.81) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /RX))
    (pad 8 thru_hole oval (at 1.27 3.81) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /PIN8))
    (pad 9 thru_hole oval (at 0 5.08) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /TX))
    (pad 10 thru_hole oval (at 1.27 5.08) (size 1.1 1.1) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 /SET))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5BFCE79E)
    (at 68.58 84.455)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 2.54 0) (layer F.SilkS))
    (fp_text value TestPoint (at 11.176 8.128) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 /PIN8))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5BFCE7A3)
    (at 68.58 86.36)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 2.54 0) (layer F.SilkS))
    (fp_text value TestPoint (at 8.128 5.08) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 2 /PIN6))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 65.405 70.104 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x07 (at 0 -17.57 180) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RESET))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RX))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /TX))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SET))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text TX (at 76.708 74.168) (layer F.SilkS))
  (gr_text GND (at 76.2 70.612) (layer F.SilkS))
  (gr_text +5V (at 75.565 69.088) (layer F.SilkS))
  (gr_text RX (at 76.708 72.644) (layer F.SilkS))
  (gr_text SET (at 81.28 74.168) (layer F.SilkS))
  (gr_text "RESET\n" (at 76.708 71.628) (layer F.SilkS))
  (gr_text GND (at 80.772 70.612) (layer F.SilkS))
  (gr_text +5V (at 80.772 69.088) (layer F.SilkS))
  (gr_text 1 (at 74.93 69.088) (layer F.SilkS))
  (gr_text "+5\n\nGND\n\nRESET\n\nRX\n\nTX\n\nSET\n" (at 71.374 78.232) (layer B.SilkS))
  (gr_text "PMS7003 Breakout\nRev 2 (C) Infnorm" (at 77.978 83.566 90) (layer F.SilkS))
  (gr_text "Signals @ 3.3V" (at 79.756 83.82 90) (layer F.SilkS))
  (gr_text RESET (at 69.85 75.565) (layer F.SilkS))
  (gr_text RX (at 68.58 78.105) (layer F.SilkS))
  (gr_text TX (at 68.58 80.645) (layer F.SilkS))
  (gr_text SET (at 69.215 83.185) (layer F.SilkS))
  (gr_text GND (at 69.215 73.025) (layer F.SilkS))
  (gr_text +5 (at 68.58 69.85) (layer F.SilkS))
  (gr_line (start 62.23 88.265) (end 62.23 67.31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.915 88.265) (end 62.23 88.265) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.915 67.31) (end 81.915 88.265) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.23 67.31) (end 81.915 67.31) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.58 67.31) (xy 81.915 67.31) (xy 81.915 88.265) (xy 62.23 88.265) (xy 62.23 67.31)
      )
    )
  )
)
