(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 117)
    (tracks 2189)
    (zones 0)
    (modules 78)
    (nets 147)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 /VBAT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 /VRAM)
  (net 5 /XTAL1)
  (net 6 /XTAL2)
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 /TX_LED)
  (net 10 /RX_LED)
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 /~RTSB)
  (net 14 /RXDB)
  (net 15 /TXDB)
  (net 16 /~CTSB)
  (net 17 /PA0)
  (net 18 /PA1)
  (net 19 /~BSTB~)
  (net 20 /PA2)
  (net 21 /BRDY)
  (net 22 /PA3)
  (net 23 /PB7)
  (net 24 /PA4)
  (net 25 /PB6)
  (net 26 /PA5)
  (net 27 /PB5)
  (net 28 /PA6)
  (net 29 /PB4)
  (net 30 /PA7)
  (net 31 /PB3)
  (net 32 /ARDY)
  (net 33 /PB2)
  (net 34 /~ASTB~)
  (net 35 /PB1)
  (net 36 /PB0)
  (net 37 /A15)
  (net 38 /A14)
  (net 39 /A13)
  (net 40 /A12)
  (net 41 /A11)
  (net 42 /A10)
  (net 43 /A9)
  (net 44 /A8)
  (net 45 /A7)
  (net 46 /A6)
  (net 47 /A5)
  (net 48 /A4)
  (net 49 /A3)
  (net 50 /A2)
  (net 51 /A1)
  (net 52 /A0)
  (net 53 /~M1)
  (net 54 /~RESET)
  (net 55 /CPU_CLK)
  (net 56 /~INT)
  (net 57 /~MREQ)
  (net 58 /~WR)
  (net 59 /~RD)
  (net 60 /~IORQ)
  (net 61 /D0)
  (net 62 /D1)
  (net 63 /D2)
  (net 64 /D3)
  (net 65 /D4)
  (net 66 /D5)
  (net 67 /D6)
  (net 68 /D7)
  (net 69 /~RFSH)
  (net 70 /CH_A_CLK)
  (net 71 /~BUSACK)
  (net 72 /~HALT)
  (net 73 /~BUSREQ)
  (net 74 /~WAIT)
  (net 75 /~NMI)
  (net 76 /TXDA)
  (net 77 /RXDA)
  (net 78 /USR5)
  (net 79 /USR1)
  (net 80 /USR6)
  (net 81 /IEI)
  (net 82 /USR7)
  (net 83 /IEO)
  (net 84 /CH_A_CLKI)
  (net 85 /CH_B_CLKI)
  (net 86 "Net-(R1-Pad1)")
  (net 87 /MA17)
  (net 88 /MA14)
  (net 89 /MA16)
  (net 90 /MA15)
  (net 91 /MA18)
  (net 92 "Net-(RV1-Pad2)")
  (net 93 "Net-(U1-Pad30)")
  (net 94 "Net-(U1-Pad31)")
  (net 95 "Net-(U1-Pad36)")
  (net 96 /~RTSA)
  (net 97 /~CTSA)
  (net 98 "Net-(U1-Pad40)")
  (net 99 "Net-(U1-Pad42)")
  (net 100 "Net-(U1-Pad43)")
  (net 101 "Net-(U1-Pad51)")
  (net 102 "Net-(U1-Pad52)")
  (net 103 "Net-(U1-Pad70)")
  (net 104 "Net-(U1-Pad73)")
  (net 105 "Net-(U1-Pad76)")
  (net 106 "Net-(U1-Pad77)")
  (net 107 /CTC_CLK)
  (net 108 /~ROM_CS)
  (net 109 /~RAM_CS)
  (net 110 "Net-(U6-Pad5)")
  (net 111 /~RAM_CSI)
  (net 112 "Net-(X1-Pad1)")
  (net 113 +3V3)
  (net 114 /UART_CLK)
  (net 115 /TCK)
  (net 116 /TDO)
  (net 117 /TMS)
  (net 118 /TDI)
  (net 119 /CH_B_CLK)
  (net 120 "Net-(U5-Pad5)")
  (net 121 "Net-(U5-Pad6)")
  (net 122 "Net-(U5-Pad7)")
  (net 123 "Net-(U5-Pad8)")
  (net 124 "Net-(U5-Pad14)")
  (net 125 "Net-(U5-Pad16)")
  (net 126 "Net-(U6-Pad1)")
  (net 127 "Net-(U6-Pad7)")
  (net 128 "Net-(U6-Pad8)")
  (net 129 "Net-(U6-Pad18)")
  (net 130 "Net-(U6-Pad19)")
  (net 131 "Net-(R2-Pad1)")
  (net 132 /VBUS)
  (net 133 /VFTDI)
  (net 134 /WDOG)
  (net 135 /VSER)
  (net 136 /LED_OUT)
  (net 137 "Net-(C16-Pad1)")
  (net 138 "Net-(C17-Pad1)")
  (net 139 "Net-(C18-Pad1)")
  (net 140 "Net-(D4-Pad2)")
  (net 141 "Net-(J5-Pad4)")
  (net 142 "Net-(R25-Pad1)")
  (net 143 "Net-(R26-Pad2)")
  (net 144 "Net-(J7-Pad8)")
  (net 145 "Net-(J7-Pad7)")
  (net 146 "Net-(J7-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /ARDY)
    (add_net /BRDY)
    (add_net /CH_A_CLK)
    (add_net /CH_A_CLKI)
    (add_net /CH_B_CLK)
    (add_net /CH_B_CLKI)
    (add_net /CPU_CLK)
    (add_net /CTC_CLK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IEI)
    (add_net /IEO)
    (add_net /LED_OUT)
    (add_net /MA14)
    (add_net /MA15)
    (add_net /MA16)
    (add_net /MA17)
    (add_net /MA18)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA2)
    (add_net /PA3)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /RXDA)
    (add_net /RXDB)
    (add_net /RX_LED)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /TXDA)
    (add_net /TXDB)
    (add_net /TX_LED)
    (add_net /UART_CLK)
    (add_net /USR1)
    (add_net /USR5)
    (add_net /USR6)
    (add_net /USR7)
    (add_net /WDOG)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net /~ASTB~)
    (add_net /~BSTB~)
    (add_net /~BUSACK)
    (add_net /~BUSREQ)
    (add_net /~CTSA)
    (add_net /~CTSB)
    (add_net /~HALT)
    (add_net /~INT)
    (add_net /~IORQ)
    (add_net /~M1)
    (add_net /~MREQ)
    (add_net /~NMI)
    (add_net /~RAM_CS)
    (add_net /~RAM_CSI)
    (add_net /~RD)
    (add_net /~RESET)
    (add_net /~RFSH)
    (add_net /~ROM_CS)
    (add_net /~RTSA)
    (add_net /~RTSB)
    (add_net /~WAIT)
    (add_net /~WR)
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad18)")
    (add_net "Net-(U6-Pad19)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad7)")
    (add_net "Net-(U6-Pad8)")
    (add_net "Net-(X1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /VBAT)
    (add_net /VBUS)
    (add_net /VFTDI)
    (add_net /VRAM)
    (add_net /VSER)
    (add_net GND)
    (add_net VCC)
  )
  (module Package_SO:SSOP-32_11.305x20.495mm_P1.27mm (layer F.Cu) (tedit 5B9E9FB6)
    (at 134.62 111.76)
    (descr "SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (attr smd)
    (fp_text reference U3 (at -7.3025 -11.1125) (layer F.SilkS))
    (fp_text value AS6C4008 (at -1.5875 -11.1125) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -6.55 -9.525) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /MA18))
    (pad 2 smd roundrect (at -6.55 -8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /MA16))
    (pad 3 smd roundrect (at -6.55 -6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /MA14))
    (pad 4 smd roundrect (at -6.55 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /A12))
    (pad 5 smd roundrect (at -6.55 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A7))
    (pad 6 smd roundrect (at -6.55 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /A6))
    (pad 7 smd roundrect (at -6.55 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /A5))
    (pad 8 smd roundrect (at -6.55 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /A4))
    (pad 9 smd roundrect (at -6.55 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /A3))
    (pad 10 smd roundrect (at -6.55 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /A2))
    (pad 11 smd roundrect (at -6.55 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /A1))
    (pad 12 smd roundrect (at -6.55 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /A0))
    (pad 13 smd roundrect (at -6.55 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /D0))
    (pad 14 smd roundrect (at -6.55 6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /D1))
    (pad 15 smd roundrect (at -6.55 8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /D2))
    (pad 16 smd roundrect (at -6.55 9.525) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 17 smd roundrect (at 6.55 9.525) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /D3))
    (pad 18 smd roundrect (at 6.55 8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /D4))
    (pad 19 smd roundrect (at 6.55 6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /D5))
    (pad 20 smd roundrect (at 6.55 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /D6))
    (pad 21 smd roundrect (at 6.55 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /D7))
    (pad 22 smd roundrect (at 6.55 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 /~RAM_CS))
    (pad 23 smd roundrect (at 6.55 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /A10))
    (pad 24 smd roundrect (at 6.55 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /~RD))
    (pad 25 smd roundrect (at 6.55 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /A11))
    (pad 26 smd roundrect (at 6.55 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /A9))
    (pad 27 smd roundrect (at 6.55 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A8))
    (pad 28 smd roundrect (at 6.55 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /A13))
    (pad 29 smd roundrect (at 6.55 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /~WR))
    (pad 30 smd roundrect (at 6.55 -6.985) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 /MA17))
    (pad 31 smd roundrect (at 6.55 -8.255) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /MA15))
    (pad 32 smd roundrect (at 6.55 -9.525) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /VRAM))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-32_11.305x20.495mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:PLCC-32_SMD-Socket (layer F.Cu) (tedit 5D13F9FD)
    (at 154.94 111.76)
    (descr "PLCC, 32 pins, surface mount")
    (tags "plcc smt")
    (attr smd)
    (fp_text reference U2 (at -8.5725 -11.36) (layer F.SilkS))
    (fp_text value SST39SF040 (at -2.8575 -11.43) (layer F.SilkS))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 21 smd rect (at 5.3225 5.08) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 68 /D7))
    (pad 22 smd rect (at 5.3225 3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 108 /~ROM_CS))
    (pad 13 smd rect (at -5.3225 5.08) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 61 /D0))
    (pad 12 smd rect (at -5.3225 3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 52 /A0))
    (pad 29 smd rect (at 5.3225 -5.08) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 88 /MA14))
    (pad 28 smd rect (at 5.3225 -3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 39 /A13))
    (pad 27 smd rect (at 5.3225 -2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 44 /A8))
    (pad 26 smd rect (at 5.3225 -1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 43 /A9))
    (pad 25 smd rect (at 5.3225 0) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 41 /A11))
    (pad 24 smd rect (at 5.3225 1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 /~RD))
    (pad 23 smd rect (at 5.3225 2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 20 smd rect (at 3.81 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 67 /D6))
    (pad 19 smd rect (at 2.54 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 66 /D5))
    (pad 18 smd rect (at 1.27 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 65 /D4))
    (pad 17 smd rect (at 0 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 64 /D3))
    (pad 16 smd rect (at -1.27 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -2.54 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 63 /D2))
    (pad 14 smd rect (at -3.81 6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 62 /D1))
    (pad 11 smd rect (at -5.3225 2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 51 /A1))
    (pad 10 smd rect (at -5.3225 1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 50 /A2))
    (pad 9 smd rect (at -5.3225 0) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 49 /A3))
    (pad 8 smd rect (at -5.3225 -1.27) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 48 /A4))
    (pad 7 smd rect (at -5.3225 -2.54) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 47 /A5))
    (pad 6 smd rect (at -5.3225 -3.81) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 46 /A6))
    (pad 5 smd rect (at -5.3225 -5.08) (size 1.925 0.7) (layers F.Cu F.Paste F.Mask)
      (net 45 /A7))
    (pad 30 smd rect (at 3.81 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 87 /MA17))
    (pad 31 smd rect (at 2.54 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 58 /~WR))
    (pad 32 smd rect (at 1.27 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 4 smd rect (at -3.81 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 40 /A12))
    (pad 3 smd rect (at -2.54 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 90 /MA15))
    (pad 2 smd rect (at -1.27 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 89 /MA16))
    (pad 1 smd rect (at 0 -6.5925) (size 0.7 1.925) (layers F.Cu F.Paste F.Mask)
      (net 91 /MA18))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_SMD-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:PQFP-100_14x20mm_P0.65mm (layer F.Cu) (tedit 5B56F226)
    (at 179.705 105.7275 90)
    (descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_qfp_generator.py")
    (tags "PQFP QFP")
    (attr smd)
    (fp_text reference U1 (at 0 -12.95 90) (layer F.SilkS))
    (fp_text value Z84C15-QFP (at 0 12.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -8.125 -9.425 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /A5))
    (pad 2 smd roundrect (at -8.125 -8.775 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /A4))
    (pad 3 smd roundrect (at -8.125 -8.125 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /A3))
    (pad 4 smd roundrect (at -8.125 -7.475 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /A2))
    (pad 5 smd roundrect (at -8.125 -6.825 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /A1))
    (pad 6 smd roundrect (at -8.125 -6.175 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /A0))
    (pad 7 smd roundrect (at -8.125 -5.525 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /~RFSH))
    (pad 8 smd roundrect (at -8.125 -4.875 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /~M1))
    (pad 9 smd roundrect (at -8.125 -4.225 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /~RESET))
    (pad 10 smd roundrect (at -8.125 -3.575 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /~BUSREQ))
    (pad 11 smd roundrect (at -8.125 -2.925 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /~WAIT))
    (pad 12 smd roundrect (at -8.125 -2.275 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /~BUSACK))
    (pad 13 smd roundrect (at -8.125 -1.625 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /~WR))
    (pad 14 smd roundrect (at -8.125 -0.975 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /~RD))
    (pad 15 smd roundrect (at -8.125 -0.325 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /~IORQ))
    (pad 16 smd roundrect (at -8.125 0.325 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 17 smd roundrect (at -8.125 0.975 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /~MREQ))
    (pad 18 smd roundrect (at -8.125 1.625 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /~HALT))
    (pad 19 smd roundrect (at -8.125 2.275 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~INT))
    (pad 20 smd roundrect (at -8.125 2.925 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /ARDY))
    (pad 21 smd roundrect (at -8.125 3.575 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /~ASTB~))
    (pad 22 smd roundrect (at -8.125 4.225 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /PA7))
    (pad 23 smd roundrect (at -8.125 4.875 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /PA6))
    (pad 24 smd roundrect (at -8.125 5.525 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /PA5))
    (pad 25 smd roundrect (at -8.125 6.175 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /PA4))
    (pad 26 smd roundrect (at -8.125 6.825 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /PA3))
    (pad 27 smd roundrect (at -8.125 7.475 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /PA2))
    (pad 28 smd roundrect (at -8.125 8.125 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /PA1))
    (pad 29 smd roundrect (at -8.125 8.775 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /PA0))
    (pad 30 smd roundrect (at -8.125 9.425 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(U1-Pad30)"))
    (pad 31 smd roundrect (at -6.175 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 "Net-(U1-Pad31)"))
    (pad 32 smd roundrect (at -5.525 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /RXDA))
    (pad 33 smd roundrect (at -4.875 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /CH_A_CLK))
    (pad 34 smd roundrect (at -4.225 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /CH_A_CLK))
    (pad 35 smd roundrect (at -3.575 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /TXDA))
    (pad 36 smd roundrect (at -2.925 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(U1-Pad36)"))
    (pad 37 smd roundrect (at -2.275 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /~RTSA))
    (pad 38 smd roundrect (at -1.625 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /~CTSA))
    (pad 39 smd roundrect (at -0.975 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 "Net-(U1-Pad36)"))
    (pad 40 smd roundrect (at -0.325 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(U1-Pad40)"))
    (pad 41 smd roundrect (at 0.325 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 42 smd roundrect (at 0.975 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 "Net-(U1-Pad42)"))
    (pad 43 smd roundrect (at 1.625 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 "Net-(U1-Pad43)"))
    (pad 44 smd roundrect (at 2.275 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /~CTSB))
    (pad 45 smd roundrect (at 2.925 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /~RTSB))
    (pad 46 smd roundrect (at 3.575 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 "Net-(U1-Pad43)"))
    (pad 47 smd roundrect (at 4.225 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /TXDB))
    (pad 48 smd roundrect (at 4.875 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 /CH_B_CLK))
    (pad 49 smd roundrect (at 5.525 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 /CH_B_CLK))
    (pad 50 smd roundrect (at 6.175 11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RXDB))
    (pad 51 smd roundrect (at 8.125 9.425 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(U1-Pad51)"))
    (pad 52 smd roundrect (at 8.125 8.775 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(U1-Pad52)"))
    (pad 53 smd roundrect (at 8.125 8.125 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /PB0))
    (pad 54 smd roundrect (at 8.125 7.475 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /PB1))
    (pad 55 smd roundrect (at 8.125 6.825 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /PB2))
    (pad 56 smd roundrect (at 8.125 6.175 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /PB3))
    (pad 57 smd roundrect (at 8.125 5.525 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /PB4))
    (pad 58 smd roundrect (at 8.125 4.875 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /PB5))
    (pad 59 smd roundrect (at 8.125 4.225 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /PB6))
    (pad 60 smd roundrect (at 8.125 3.575 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PB7))
    (pad 61 smd roundrect (at 8.125 2.925 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /~BSTB~))
    (pad 62 smd roundrect (at 8.125 2.275 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /BRDY))
    (pad 63 smd roundrect (at 8.125 1.625 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /~NMI))
    (pad 64 smd roundrect (at 8.125 0.975 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 65 smd roundrect (at 8.125 0.325 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /XTAL1))
    (pad 66 smd roundrect (at 8.125 -0.325 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /XTAL2))
    (pad 67 smd roundrect (at 8.125 -0.975 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 68 smd roundrect (at 8.125 -1.625 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /CPU_CLK))
    (pad 69 smd roundrect (at 8.125 -2.275 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /CPU_CLK))
    (pad 70 smd roundrect (at 8.125 -2.925 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(U1-Pad70)"))
    (pad 71 smd roundrect (at 8.125 -3.575 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 /IEO))
    (pad 72 smd roundrect (at 8.125 -4.225 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /IEI))
    (pad 73 smd roundrect (at 8.125 -4.875 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(U1-Pad73)"))
    (pad 74 smd roundrect (at 8.125 -5.525 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /CH_A_CLKI))
    (pad 75 smd roundrect (at 8.125 -6.175 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /CH_B_CLKI))
    (pad 76 smd roundrect (at 8.125 -6.825 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(U1-Pad76)"))
    (pad 77 smd roundrect (at 8.125 -7.475 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 "Net-(U1-Pad77)"))
    (pad 78 smd roundrect (at 8.125 -8.125 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(U1-Pad76)"))
    (pad 79 smd roundrect (at 8.125 -8.775 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 /CTC_CLK))
    (pad 80 smd roundrect (at 8.125 -9.425 90) (size 1.75 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 /UART_CLK))
    (pad 81 smd roundrect (at 6.175 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 /UART_CLK))
    (pad 82 smd roundrect (at 5.525 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /D7))
    (pad 83 smd roundrect (at 4.875 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /D6))
    (pad 84 smd roundrect (at 4.225 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /D5))
    (pad 85 smd roundrect (at 3.575 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /D4))
    (pad 86 smd roundrect (at 2.925 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /D3))
    (pad 87 smd roundrect (at 2.275 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /D2))
    (pad 88 smd roundrect (at 1.625 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /D1))
    (pad 89 smd roundrect (at 0.975 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /D0))
    (pad 90 smd roundrect (at 0.325 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 91 smd roundrect (at -0.325 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /A15))
    (pad 92 smd roundrect (at -0.975 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /A14))
    (pad 93 smd roundrect (at -1.625 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /A13))
    (pad 94 smd roundrect (at -2.275 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /A12))
    (pad 95 smd roundrect (at -2.925 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /A11))
    (pad 96 smd roundrect (at -3.575 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /A10))
    (pad 97 smd roundrect (at -4.225 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /A9))
    (pad 98 smd roundrect (at -4.875 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A8))
    (pad 99 smd roundrect (at -5.525 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A7))
    (pad 100 smd roundrect (at -6.175 -11.125 90) (size 0.5 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /A6))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery:BatteryHolder_Keystone_1058_1x2032 (layer B.Cu) (tedit 589EE147)
    (at 160.02 106.68 90)
    (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
    (tags "Keystone type 1058 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at -15.24 -6.35 90) (layer B.SilkS))
    (fp_text value CR2032 (at -15.24 -5.08 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -14.68 0 90) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBAT))
    (pad 2 smd rect (at 14.68 0 90) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1058_1x2032.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 144.78 88.9)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U4 (at 0 -7.45) (layer F.SilkS))
    (fp_text value EPM7064AETC44 (at -2.2225 7.3025) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 /TDI))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 /A3))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 /A4))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 /A5))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /A6))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 /TMS))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /A7))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 +3V3))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 61 /D0))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 /D1))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 /D2))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 88 /MA14))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 /MA15))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 89 /MA16))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 +3V3))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 64 /D3))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 65 /D4))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 /D5))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 87 /MA17))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 91 /MA18))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 52 /A0))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 /A1))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 115 /TCK))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 134 /WDOG))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /A15))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 +3V3))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 136 /LED_OUT))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /A14))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 /TDO))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 /~IORQ))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 /~WR))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 107 /CTC_CLK))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 /UART_CLK))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 /~M1))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 /~RESET))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 57 /~MREQ))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 +3V3))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 /~RAM_CSI))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 108 /~ROM_CS))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 /A2))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 200.66 113.03)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C21 (at 1.905 -2.54) (layer B.SilkS))
    (fp_text value 47uF (at -1.5875 -2.54) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.55 0) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 3 VCC))
    (pad 2 smd roundrect (at 2.55 0) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Micro_USB_B (layer F.Cu) (tedit 5EADA3B1)
    (at 213.36 102.5525 90)
    (descr "Connector, Micro USB, Type B, Receptacle")
    (tags "MICRO USB RECEPTACLE")
    (fp_text reference J1 (at -2.54 -6.6675 90) (layer F.SilkS))
    (fp_text value Serial_A (at 1.27 -6.6675 90) (layer F.SilkS))
    (pad 5 smd rect (at 1.3 -4.4 90) (size 0.395 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -4.4 90) (size 0.395 1.85) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 1 smd rect (at -1.3 -4.4 90) (size 0.395 1.85) (layers F.Cu F.Paste F.Mask)
      (net 132 /VBUS))
    (pad 2 smd rect (at -0.65 -4.4 90) (size 0.395 1.85) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(C17-Pad1)"))
    (pad 3 smd rect (at 0 -4.4 90) (size 0.395 1.85) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(C16-Pad1)"))
    (pad 6 thru_hole circle (at 2.5 -4.15 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 -4.15 90) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 3.5 -1.45 90) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at -3.5 -1.45 90) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module My_Components:Conn_Pin_Header_5x2_2.54mm (layer F.Cu) (tedit 5EAC6F9B)
    (at 209.55 116.84 90)
    (descr "Pin Header, 13x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 13x2")
    (fp_text reference J6 (at -5.08 -3.4925 90) (layer F.SilkS))
    (fp_text value RC2014_SERIAL (at 1.5875 -3.4925 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 /TXDA))
    (pad 2 thru_hole circle (at -5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /TXDB))
    (pad 3 thru_hole circle (at -2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 /RXDA))
    (pad 4 thru_hole circle (at -2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXDB))
    (pad 5 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 /USR1))
    (pad 6 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 /USR5))
    (pad 7 thru_hole circle (at 2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 /IEI))
    (pad 8 thru_hole circle (at 2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 /USR6))
    (pad 9 thru_hole circle (at 5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 /IEO))
    (pad 10 thru_hole circle (at 5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 /USR7))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 172.72 109.22 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.43 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 154.94 99.06 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 2.2225 1.27 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.9525 1.27 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 135.495 99.06)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.57 -0.635) (layer F.SilkS))
    (fp_text value 100nF (at 3.57 0.635) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /VRAM))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 200.66 92.71 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -1.27 -1.27 90) (layer F.SilkS))
    (fp_text value 100nF (at 1.905 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 193.04 104.14 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 2.2225 1.27 90) (layer B.SilkS))
    (fp_text value 100nF (at -0.9525 1.27 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 178.435 90.4875 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -2.54 -1.27 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.9525 -1.27 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 198.12 107.95 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 100nF (at -0.3175 -1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 133 /VFTDI))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 182.88 91.44 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -1.397 -1.27 90) (layer F.SilkS))
    (fp_text value 33pF (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /XTAL1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.72 91.44 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at -1.5875 -1.27 90) (layer F.SilkS))
    (fp_text value 33pF (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /XTAL2))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 205.74 92.71 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 47pF (at 0 -1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 205.74 107.95 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 47pF (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 "Net-(C17-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 193.04 92.71 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value POWER (at 0 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 195.58 92.71 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value TX (at 2.54 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /TX_LED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 198.12 92.71 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value RX (at 2.54 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /RX_LED))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 200.66 113.03)
    (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F1 (at -1.651 -2.54) (layer F.SilkS))
    (fp_text value 0.5A (at 0.889 -2.54) (layer F.SilkS))
    (fp_text user %R (at 0.3175 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 132 /VBUS))
    (pad 1 smd roundrect (at -2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 203.2 87.63)
    (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F2 (at -1.5875 2.54) (layer F.SilkS))
    (fp_text value 0.5A (at 1.27 2.54) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 3 VCC))
    (pad 2 smd roundrect (at 2.225 0) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 135 /VSER))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 128.27 121.92 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 3.175 -0.635 90) (layer B.SilkS))
    (fp_text value 10k (at 3.175 0.635 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 142 "Net-(R25-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 135.89 121.92 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 29.4k (at 0 -3.175 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 143 "Net-(R26-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_TC33X_Vertical (layer B.Cu) (tedit 5C165D15)
    (at 132.08 121.92 90)
    (descr "Potentiometer, Bourns, TC33X, Vertical, https://www.bourns.com/pdfs/TC33.pdf")
    (tags "Potentiometer Bourns TC33X Vertical")
    (attr smd)
    (fp_text reference RV1 (at 3.81 -1.27 90) (layer B.SilkS))
    (fp_text value 2k (at 3.81 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (fp_text user "Wiper may be\nanywhere within\ncircle shown" (at -0.15 0.8 90) (layer Cmts.User))
    (pad 1 smd rect (at -1.8 1 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 143 "Net-(R26-Pad2)"))
    (pad 3 smd rect (at -1.8 -1 90) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 142 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 1.45 0 90) (size 1.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(RV1-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_TC33X_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 138.43 111.76 180)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -4.445 6.35 180) (layer B.SilkS))
    (fp_text value MAX691xWE (at 0 -6.35 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /VBAT))
    (pad 2 smd rect (at -4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /VRAM))
    (pad 3 smd rect (at -4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 4 smd rect (at -4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(U5-Pad5)"))
    (pad 6 smd rect (at -4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(U5-Pad6)"))
    (pad 7 smd rect (at -4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at -4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at 4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(RV1-Pad2)"))
    (pad 10 smd rect (at 4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 75 /~NMI))
    (pad 11 smd rect (at 4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 134 /WDOG))
    (pad 12 smd rect (at 4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 109 /~RAM_CS))
    (pad 13 smd rect (at 4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 111 /~RAM_CSI))
    (pad 14 smd rect (at 4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(U5-Pad14)"))
    (pad 15 smd rect (at 4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 54 /~RESET))
    (pad 16 smd rect (at 4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(U5-Pad16)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-20_3.9x8.7mm_P0.635mm (layer F.Cu) (tedit 5A4A2523)
    (at 200.66 100.33 90)
    (descr "SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U6 (at 0 -5.4 90) (layer F.SilkS))
    (fp_text value FT231XS (at 0 5.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.6 -2.8575 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U6-Pad1)"))
    (pad 2 smd rect (at -2.6 -2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 97 /~CTSA))
    (pad 3 smd rect (at -2.6 -1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 133 /VFTDI))
    (pad 4 smd rect (at -2.6 -0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 76 /TXDA))
    (pad 5 smd rect (at -2.6 -0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U6-Pad5)"))
    (pad 6 smd rect (at -2.6 0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.6 0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U6-Pad7)"))
    (pad 8 smd rect (at -2.6 1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U6-Pad8)"))
    (pad 9 smd rect (at -2.6 2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 96 /~RTSA))
    (pad 10 smd rect (at -2.6 2.8575 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /TX_LED))
    (pad 11 smd rect (at 2.6 2.8575 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R1-Pad1)"))
    (pad 12 smd rect (at 2.6 2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R2-Pad1)"))
    (pad 13 smd rect (at 2.6 1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 133 /VFTDI))
    (pad 14 smd rect (at 2.6 0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 133 /VFTDI))
    (pad 15 smd rect (at 2.6 0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 16 smd rect (at 2.6 -0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.6 -0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /RX_LED))
    (pad 18 smd rect (at 2.6 -1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U6-Pad18)"))
    (pad 19 smd rect (at 2.6 -2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U6-Pad19)"))
    (pad 20 smd rect (at 2.6 -2.8575 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 77 /RXDA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_3.9x8.7mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 56D1B4CB)
    (at 130.2258 95.631)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.8) (layer F.Fab))
    (fp_text value 3.2mm (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 157.48 91.44 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 100nF (at -3.81 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 147.0025 113.03 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.43 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 142.24 91.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 100nF (at 0 1.27) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 147.32 91.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 100nF (at 0 1.27) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 142.24 86.36 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 147.32 86.36 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 174.625 90.17 270)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C19 (at -2.54 -2.54 270) (layer B.SilkS))
    (fp_text value 10uF (at 2.2225 -2.54 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 170.4975 95.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C18 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.43 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 139 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 166.37 90.17 270)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C20 (at -3.81 2.54 270) (layer B.SilkS))
    (fp_text value 10uF (at -0.9525 2.54 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels (layer B.Cu) (tedit 5C745336)
    (at 175.26 101.6 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 3.175 2.8575 90) (layer B.SilkS))
    (fp_text value CH_A_CLK (at -1.5875 2.8575 90) (layer B.SilkS))
    (fp_text user 1 (at -2.6 0 90) (layer B.SilkS))
    (fp_text user 3 (at 2.6 0 90) (layer B.SilkS))
    (pad 1 smd custom (at -1.3 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 114 /UART_CLK) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
      ))
    (pad 2 smd rect (at 0 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 70 /CH_A_CLK))
    (pad 3 smd custom (at 1.3 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 84 /CH_A_CLKI) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels (layer B.Cu) (tedit 5C745336)
    (at 172.72 101.6 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 3.175 -1.905 90) (layer B.SilkS))
    (fp_text value CH_B_CLK (at -1.5875 -1.905 90) (layer B.SilkS))
    (fp_text user 3 (at 2.6 0 90) (layer B.SilkS))
    (fp_text user 1 (at -2.6 0 90) (layer B.SilkS))
    (pad 3 smd custom (at 1.3 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 85 /CH_B_CLKI) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 90) (size 1 1.5) (layers B.Cu B.Mask)
      (net 119 /CH_B_CLK))
    (pad 1 smd custom (at -1.3 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 114 /UART_CLK) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 170.4975 86.36 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 2.8575 180) (layer B.SilkS))
    (fp_text value LDO_BYP (at 1.5875 1.5875) (layer B.SilkS))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 113 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 170.4975 90.17 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at 2.8575 1.27 270) (layer B.SilkS))
    (fp_text value TPS79333-EP (at 4.7625 -6.985) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 4 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 139 "Net-(C18-Pad1)"))
    (pad 5 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 113 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5A0FD1B2)
    (at 177.8 91.44)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -2.2225 -2.8575) (layer F.SilkS))
    (fp_text value 16MHz (at 0.9525 -2.8575) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /XTAL2))
    (pad 2 smd rect (at 1.45 1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.45 -1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /XTAL1))
    (pad 4 smd rect (at -1.45 -1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 130.175 111.76 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 0 3.175 270) (layer B.SilkS))
    (fp_text value RAM_CS (at 0 1.905 270) (layer B.SilkS))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 109 /~RAM_CS) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 111 /~RAM_CSI) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 147.0025 109.22 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value VRAM (at 0 1.905 90) (layer B.SilkS))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 /VRAM) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module My_Components:Conn_Pin_Header_6x1_2.54mm (layer F.Cu) (tedit 5C6700F5)
    (at 210.82 87.63 90)
    (descr "Pin Header, 6x1, 2.54mm pitch")
    (tags "CONN 6x1")
    (fp_text reference J2 (at -6.35 -2.2225 90) (layer F.SilkS))
    (fp_text value Serial_B (at 0 -2.2225 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /~RTSB))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 /VSER))
    (pad 4 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /RXDB))
    (pad 5 thru_hole circle (at 3.81 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /TXDB))
    (pad 6 thru_hole circle (at 6.35 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /~CTSB))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_13x2_2.54mm (layer F.Cu) (tedit 5C670022)
    (at 187.96 82.55)
    (descr "Pin Header, 13x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 13x2")
    (fp_text reference J3 (at -13.97 3.556) (layer F.SilkS))
    (fp_text value Parallel (at -8.89 3.556) (layer F.SilkS))
    (pad 1 thru_hole rect (at -15.24 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 2 thru_hole circle (at -15.24 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at -12.7 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PA0))
    (pad 4 thru_hole circle (at -12.7 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at -10.16 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /PA1))
    (pad 6 thru_hole circle (at -10.16 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /~BSTB~))
    (pad 7 thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PA2))
    (pad 8 thru_hole circle (at -7.62 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /BRDY))
    (pad 9 thru_hole circle (at -5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /PA3))
    (pad 10 thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /PB7))
    (pad 11 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PA4))
    (pad 12 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PB6))
    (pad 13 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PA5))
    (pad 14 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PB5))
    (pad 15 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /PA6))
    (pad 16 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PB4))
    (pad 17 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /PA7))
    (pad 18 thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /PB3))
    (pad 19 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /ARDY))
    (pad 20 thru_hole circle (at 7.62 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /PB2))
    (pad 21 thru_hole circle (at 10.16 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~ASTB~))
    (pad 22 thru_hole circle (at 10.16 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /PB1))
    (pad 23 thru_hole circle (at 12.7 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole circle (at 12.7 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /PB0))
    (pad 25 thru_hole circle (at 15.24 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 26 thru_hole circle (at 15.24 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_34x1_2.54mm (layer F.Cu) (tedit 5EAC6F3C)
    (at 168.91 127)
    (descr "Pin Header, 39x1, 2.54mm pitch")
    (tags "CONN 39x1")
    (fp_text reference J4 (at -41.91 -2.2225) (layer F.SilkS))
    (fp_text value RC2014_BUS (at -35.56 -2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -41.91 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /A15))
    (pad 2 thru_hole circle (at -39.37 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A14))
    (pad 3 thru_hole circle (at -36.83 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /A13))
    (pad 4 thru_hole circle (at -34.29 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /A12))
    (pad 5 thru_hole circle (at -31.75 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /A11))
    (pad 6 thru_hole circle (at -29.21 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /A10))
    (pad 7 thru_hole circle (at -26.67 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /A9))
    (pad 8 thru_hole circle (at -24.13 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A8))
    (pad 9 thru_hole circle (at -21.59 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /A7))
    (pad 10 thru_hole circle (at -19.05 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /A6))
    (pad 11 thru_hole circle (at -16.51 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /A5))
    (pad 12 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /A4))
    (pad 13 thru_hole circle (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A3))
    (pad 14 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /A2))
    (pad 15 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /A1))
    (pad 16 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /A0))
    (pad 17 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 18 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 19 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~M1))
    (pad 20 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~RESET))
    (pad 21 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /CPU_CLK))
    (pad 22 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /~INT))
    (pad 23 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /~MREQ))
    (pad 24 thru_hole circle (at 16.51 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /~WR))
    (pad 25 thru_hole circle (at 19.05 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /~RD))
    (pad 26 thru_hole circle (at 21.59 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /~IORQ))
    (pad 27 thru_hole circle (at 24.13 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /D0))
    (pad 28 thru_hole circle (at 26.67 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /D1))
    (pad 29 thru_hole circle (at 29.21 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /D2))
    (pad 30 thru_hole circle (at 31.75 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /D3))
    (pad 31 thru_hole circle (at 34.29 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /D4))
    (pad 32 thru_hole circle (at 36.83 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /D5))
    (pad 33 thru_hole circle (at 39.37 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /D6))
    (pad 34 thru_hole circle (at 41.91 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /D7))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_10x1_2.54mm (layer F.Cu) (tedit 5C67000A)
    (at 179.07 124.46)
    (descr "Pin Header, 10x1, 2.54mm pitch")
    (tags "CONN 10x1")
    (fp_text reference J5 (at -23.1775 0) (layer F.SilkS))
    (fp_text value RC2014_EXT (at -17.145 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /~RFSH))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(J5-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 114 /UART_CLK))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /~BUSACK))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 /~HALT))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 /~BUSREQ))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 /~WAIT))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 /~NMI))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Pin_Header_5x2_2.54mm (layer F.Cu) (tedit 5EAC6F9B)
    (at 160.02 82.55)
    (descr "Pin Header, 13x2, 2.54mm pitch")
    (tags "CONN PIN HEADER 13x2")
    (fp_text reference J7 (at -2.54 3.81) (layer F.SilkS))
    (fp_text value JTAG (at 3.81 3.81) (layer F.SilkS))
    (pad 10 thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 /TDI))
    (pad 8 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(J7-Pad8)"))
    (pad 7 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 145 "Net-(J7-Pad7)"))
    (pad 6 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 146 "Net-(J7-Pad6)"))
    (pad 5 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 117 /TMS))
    (pad 4 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 113 +3V3))
    (pad 3 thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 116 /TDO))
    (pad 2 thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 115 /TCK))
    (model pin_array/pins_array_13x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 203.2 92.71 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 27 (at 0.9525 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 137 "Net-(C16-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 203.2 107.95 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0.9525 1.27 90) (layer F.SilkS))
    (fp_text value 27 (at -1.27 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(R2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 138 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 193.04 87.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0.9525 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at -1.27 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 195.58 87.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0.9525 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at -1.27 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 198.12 87.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0.9525 1.27 270) (layer F.SilkS))
    (fp_text value 1k (at -1.27 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 193.04 123.19 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (autoplace_cost180 2)
    (attr smd)
    (fp_text reference R7 (at 0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 3.4925 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /D0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 195.58 123.19 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /D1))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 198.12 123.19 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /D2))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 200.66 123.19 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /D3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 203.2 123.19 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 1.905 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /D4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 195.58 118.11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at -0.635 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /D5))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 198.12 118.11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -0.635 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /D6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 200.66 118.11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -0.635 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 1.905 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /D7))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 182.88 120.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /~INT))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 190.5 120.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /~NMI))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 185.42 120.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /~BUSREQ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 187.96 120.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -0.9525 -1.27 90) (layer F.SilkS))
    (fp_text value 4.7k (at 2.2225 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 /~WAIT))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 203.2 118.11 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 0.635 1.27 270) (layer F.SilkS))
    (fp_text value 10k (at -1.905 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 /IEI))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 175.26 120.65 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at -0.9525 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 1.905 1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /~RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 154.94 87.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -1.27 1.27 270) (layer B.SilkS))
    (fp_text value 10k (at 1.27 1.27 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 115 /TCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 157.48 87.63 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 1.27 -1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -1.27 -1.27 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 116 /TDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 160.02 87.63 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 1.27 -1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -1.27 -1.27 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 117 /TMS))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 162.56 87.63 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 1.27 -1.27 90) (layer B.SilkS))
    (fp_text value 10k (at -1.27 -1.27 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 118 /TDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 5A02FC95)
    (at 170.18 119.38 180)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 2.2225 -2.2225 180) (layer F.SilkS))
    (fp_text value RESET (at -1.5875 -2.2225 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 54 /~RESET))
    (pad 2 smd rect (at 1.7 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_SMD_EuroQuartz_XO91-4Pin_7.0x5.0mm_HandSoldering (layer F.Cu) (tedit 58CD3345)
    (at 164.465 91.44)
    (descr "Miniature Crystal Clock Oscillator EuroQuartz XO91 series, http://cdn-reichelt.de/documents/datenblatt/B400/XO91.pdf, hand-soldering, 7.0x5.0mm^2 package")
    (tags "SMD SMT crystal oscillator hand-soldering")
    (attr smd)
    (fp_text reference X1 (at -4.1275 4.1275) (layer F.SilkS))
    (fp_text value 1.8432MHz (at 1.5875 4.1275) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.25 2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(X1-Pad1)"))
    (pad 2 smd rect (at 3.25 2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 3.25 -2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 114 /UART_CLK))
    (pad 4 smd rect (at -3.25 -2.1) (size 3.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_EuroQuartz_XO91-4Pin_7.0x5.0mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 154.94 92.71 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at -1.27 -1.27 90) (layer F.SilkS))
    (fp_text value CPU (at 1.5875 -1.27 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 136 /LED_OUT))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 154.94 87.63 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.27 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 140 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Tiny Z80 - Version 1.0\nCopyright (C) 2020 Sergey Kiselev" (at 195.8975 92.71) (layer B.SilkS))
  (gr_text GPL3 (at 187.325 92.075) (layer F.SilkS))
  (gr_text "Design files and documentation:\ngithub.com/skiselev/tiny_z80" (at 195.8975 96.8375) (layer B.SilkS))
  (gr_text IEO (at 212.4075 111.76 90) (layer B.SilkS))
  (gr_text IEI (at 212.4075 114.3 90) (layer B.SilkS))
  (gr_text TXDA (at 212.4075 121.92 90) (layer B.SilkS))
  (gr_text TXDB (at 206.6925 121.92 90) (layer B.SilkS))
  (gr_text RXDB (at 206.6925 119.38 90) (layer B.SilkS))
  (gr_text RXDA (at 212.4075 119.38 90) (layer B.SilkS))
  (gr_text ~CTSB (at 212.725 81.28 90) (layer B.SilkS))
  (gr_text TXDB (at 212.725 83.82 90) (layer B.SilkS))
  (gr_text RXDB (at 212.725 86.36 90) (layer B.SilkS))
  (gr_text 5V (at 212.725 88.9 90) (layer B.SilkS))
  (gr_text ~RTSB (at 212.725 91.44 90) (layer B.SilkS))
  (gr_text GND (at 212.725 93.98 270) (layer B.SilkS))
  (gr_text GND (at 154.94 79.6925) (layer B.SilkS))
  (gr_text GND (at 165.1 79.6925) (layer B.SilkS))
  (gr_text 3.3V (at 157.48 79.6925) (layer B.SilkS))
  (gr_text TDI (at 165.1 85.4075) (layer B.SilkS))
  (gr_text TMS (at 160.02 85.4075) (layer B.SilkS))
  (gr_text TDO (at 157.48 85.4075) (layer B.SilkS))
  (gr_text TCK (at 154.94 85.4075) (layer B.SilkS))
  (gr_text PB7 (at 182.88 79.6925) (layer B.SilkS))
  (gr_text PB6 (at 185.42 79.6925) (layer B.SilkS))
  (gr_text PB5 (at 187.96 79.6925) (layer B.SilkS))
  (gr_text PB4 (at 190.5 79.6925) (layer B.SilkS))
  (gr_text PB3 (at 193.04 79.6925) (layer B.SilkS))
  (gr_text PB2 (at 195.58 79.6925) (layer B.SilkS))
  (gr_text PB1 (at 198.12 79.6925) (layer B.SilkS))
  (gr_text PB0 (at 200.66 79.6925) (layer B.SilkS))
  (gr_text PA7 (at 193.04 85.725) (layer B.SilkS))
  (gr_text PA6 (at 190.5 85.725) (layer B.SilkS))
  (gr_text PA5 (at 187.96 85.725) (layer B.SilkS))
  (gr_text PA4 (at 185.42 85.725) (layer B.SilkS))
  (gr_text PA3 (at 182.88 85.725) (layer B.SilkS))
  (gr_text PA2 (at 180.34 85.725) (layer B.SilkS))
  (gr_text PA1 (at 177.8 85.725) (layer B.SilkS))
  (gr_text PA0 (at 175.26 85.725) (layer B.SilkS))
  (gr_text VCC (at 173.0375 85.725) (layer B.SilkS))
  (gr_text VCC (at 203.2 79.6925) (layer B.SilkS))
  (gr_text GND (at 200.66 85.725) (layer B.SilkS))
  (gr_text GND (at 203.2 85.725) (layer B.SilkS))
  (gr_text GND (at 175.26 79.6925) (layer B.SilkS))
  (gr_text GND (at 172.72 79.6925) (layer B.SilkS))
  (gr_text ARDY (at 195.58 85.725) (layer B.SilkS))
  (gr_text ~ASTB (at 198.12 85.725) (layer B.SilkS))
  (gr_text ~BSTB (at 177.8 79.883) (layer B.SilkS))
  (gr_text BRDY (at 180.34 79.6925) (layer B.SilkS))
  (gr_text ~IORQ (at 190.5 122.8725) (layer B.SilkS))
  (gr_text ~NMI (at 190.5 121.285) (layer B.SilkS))
  (gr_text ~WAIT (at 187.96 121.285) (layer B.SilkS))
  (gr_text ~RD (at 187.96 122.8725) (layer B.SilkS))
  (gr_text ~WR (at 185.42 122.8725) (layer B.SilkS))
  (gr_text ~BREQ (at 185.42 121.285) (layer B.SilkS))
  (gr_text ~MREQ (at 182.88 122.8725) (layer B.SilkS))
  (gr_text ~HALT (at 182.88 121.285) (layer B.SilkS))
  (gr_text ~BACK (at 180.34 121.285) (layer B.SilkS))
  (gr_text ~INT (at 180.34 122.8725) (layer B.SilkS))
  (gr_text UCLK (at 177.8 121.285) (layer B.SilkS))
  (gr_text CCLK (at 177.8 122.8725) (layer B.SilkS))
  (gr_text ~RESET (at 175.26 122.8725) (layer B.SilkS))
  (gr_text ~RFSH (at 172.72 121.285) (layer B.SilkS))
  (gr_text ~M1 (at 172.72 122.8725) (layer B.SilkS))
  (gr_text VCC (at 170.18 121.285) (layer B.SilkS))
  (gr_text VCC (at 170.18 122.8725) (layer B.SilkS))
  (gr_text GND (at 167.64 121.285) (layer B.SilkS))
  (gr_text GND (at 167.64 122.8725) (layer B.SilkS))
  (gr_text D0 (at 193.04 125.4125) (layer B.SilkS))
  (gr_text D1 (at 195.58 125.4125) (layer B.SilkS))
  (gr_text D2 (at 198.12 125.4125) (layer B.SilkS))
  (gr_text D3 (at 200.66 125.4125) (layer B.SilkS))
  (gr_text D4 (at 203.2 125.4125) (layer B.SilkS))
  (gr_text D5 (at 205.74 125.4125) (layer B.SilkS))
  (gr_text D6 (at 208.28 125.4125) (layer B.SilkS))
  (gr_text D7 (at 210.82 125.4125) (layer B.SilkS))
  (gr_text A0 (at 165.1 125.4125) (layer B.SilkS))
  (gr_text A1 (at 162.56 125.4125) (layer B.SilkS))
  (gr_text A2 (at 160.02 125.4125) (layer B.SilkS))
  (gr_text A3 (at 157.48 125.4125) (layer B.SilkS))
  (gr_text A4 (at 154.94 125.4125) (layer B.SilkS))
  (gr_text A5 (at 152.4 125.4125) (layer B.SilkS))
  (gr_text A6 (at 149.86 125.4125) (layer B.SilkS))
  (gr_text A7 (at 147.32 125.4125) (layer B.SilkS))
  (gr_text A8 (at 144.78 125.4125) (layer B.SilkS))
  (gr_text A9 (at 142.24 125.4125) (layer B.SilkS))
  (gr_text A10 (at 139.7 125.4125) (layer B.SilkS))
  (gr_text A11 (at 137.16 125.4125) (layer B.SilkS))
  (gr_text A12 (at 134.62 125.4125) (layer B.SilkS))
  (gr_text A13 (at 132.08 125.4125) (layer B.SilkS))
  (gr_text A14 (at 129.54 125.4125) (layer B.SilkS))
  (gr_text A15 (at 127 125.4125) (layer B.SilkS))
  (gr_text "Tiny Z80 - Version 1.0\nCopyright (C) 2020 Sergey Kiselev" (at 180.34 95.1865) (layer F.SilkS))
  (gr_line (start 125.49418 93.60448) (end 139.90868 79.18998) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.1966 127.7366) (end 125.1966 94.3229) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.0806 128.7526) (end 126.2126 128.7526) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.0966 79.9084) (end 214.0966 127.7366) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.6271 78.8924) (end 213.0806 78.8924) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.6271 79.9084) (end 140.6271 78.8924) (angle -45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.2126 94.3229) (end 125.1966 94.3229) (angle 45) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 126.2126 127.7366) (end 125.1966 127.7366) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 213.0806 79.9084) (end 214.0966 79.9084) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 213.0806 127.7366) (end 213.0806 128.7526) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.095 128.905) (xy 125.095 93.98) (xy 140.335 78.74) (xy 214.3125 78.74) (xy 214.3125 128.905)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.095 93.98) (xy 140.335 78.74) (xy 214.3125 78.74) (xy 214.3125 128.905) (xy 125.095 128.905)
      )
    )
  )
)
