(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 80)
    (no_connects 0)
    (area 128.067999 98.857999 174.446001 122.122001)
    (thickness 1.6)
    (drawings 108)
    (tracks 563)
    (zones 0)
    (modules 24)
    (nets 45)
  )
  (page A4)
  (title_block
    (title Mightyduino)
    (date 2017-01-07)
    (rev 1.3)
    (company dev76.org)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.18)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.5)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.0762)
    (uvia_drill 0.0254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 /RESET)
  (net 5 /DTR)
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 /RAW)
  (net 10 /D5)
  (net 11 /D6)
  (net 12 /D7)
  (net 13 "Net-(IC1-Pad7)")
  (net 14 "Net-(IC1-Pad8)")
  (net 15 /D8)
  (net 16 /D9)
  (net 17 /D10)
  (net 18 /D11)
  (net 19 /D12)
  (net 20 /D13)
  (net 21 /D14)
  (net 22 /D15)
  (net 23 /D16)
  (net 24 /D17)
  (net 25 /D18)
  (net 26 /D19)
  (net 27 /D20)
  (net 28 /D21)
  (net 29 /D22)
  (net 30 /D23)
  (net 31 /A7)
  (net 32 /A6)
  (net 33 /A5)
  (net 34 /A4)
  (net 35 /A3)
  (net 36 /A2)
  (net 37 /A1)
  (net 38 /A0)
  (net 39 /D0)
  (net 40 /D1)
  (net 41 /D2)
  (net 42 /D3)
  (net 43 /D4)
  (net 44 "Net-(C7-Pad1)")
  (net_class Default "Esta é a classe de net default."
    (clearance 0.18)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.0762)
    (uvia_drill 0.0254)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net /D2)
    (add_net /D20)
    (add_net /D21)
    (add_net /D22)
    (add_net /D23)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /DTR)
    (add_net /RAW)
    (add_net /RESET)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5848302E)
    (at 170.18 107.315 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -1.016 1.397 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58482FD1)
    (at 152.4 116.84 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.436841 45) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5848307C)
    (at 168.275 116.205)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.889 -1.397) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 58482F7E)
    (at 133.35 112.80902 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 2.25298 0.762 270) (layer F.SilkS))
    (fp_text value blue (at 0 1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 90) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58482FBA)
    (at 133.35 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference F1 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 500mA (at -1.27 2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /RAW))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-44_10x10mm_Pitch0.8mm locked (layer F.Cu) (tedit 58436163)
    (at 145.415 110.49 315)
    (descr "LQFP44 (see Appnote_PCB_Guidelines_TRINAMIC_packages.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -7.65 315) (layer F.SilkS) hide)
    (fp_text value ATMEGA644P-A (at 0 7.65 315) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.85 -4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 10 /D5))
    (pad 2 smd rect (at -5.85 -3.2 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 11 /D6))
    (pad 3 smd rect (at -5.85 -2.4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 12 /D7))
    (pad 4 smd rect (at -5.85 -1.6 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 5 smd rect (at -5.85 -0.8 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 6 smd rect (at -5.85 0 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -5.85 0.8 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -5.85 1.6 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -5.85 2.4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 15 /D8))
    (pad 10 smd rect (at -5.85 3.2 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 16 /D9))
    (pad 11 smd rect (at -5.85 4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 17 /D10))
    (pad 12 smd rect (at -4 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 18 /D11))
    (pad 13 smd rect (at -3.2 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 19 /D12))
    (pad 14 smd rect (at -2.4 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 20 /D13))
    (pad 15 smd rect (at -1.6 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 21 /D14))
    (pad 16 smd rect (at -0.8 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 22 /D15))
    (pad 17 smd rect (at 0 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 18 smd rect (at 0.8 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.6 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 23 /D16))
    (pad 20 smd rect (at 2.4 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 24 /D17))
    (pad 21 smd rect (at 3.2 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 25 /D18))
    (pad 22 smd rect (at 4 5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 26 /D19))
    (pad 23 smd rect (at 5.85 4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 27 /D20))
    (pad 24 smd rect (at 5.85 3.2 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 28 /D21))
    (pad 25 smd rect (at 5.85 2.4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 29 /D22))
    (pad 26 smd rect (at 5.85 1.6 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 30 /D23))
    (pad 27 smd rect (at 5.85 0.8 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 28 smd rect (at 5.85 0 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 5.85 -0.8 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 30 smd rect (at 5.85 -1.6 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 31 /A7))
    (pad 31 smd rect (at 5.85 -2.4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 32 /A6))
    (pad 32 smd rect (at 5.85 -3.2 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 33 /A5))
    (pad 33 smd rect (at 5.85 -4 315) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 34 /A4))
    (pad 34 smd rect (at 4 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 35 /A3))
    (pad 35 smd rect (at 3.2 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 36 /A2))
    (pad 36 smd rect (at 2.4 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 37 /A1))
    (pad 37 smd rect (at 1.6 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 38 /A0))
    (pad 38 smd rect (at 0.8 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 39 smd rect (at 0 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 40 smd rect (at -0.8 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 39 /D0))
    (pad 41 smd rect (at -1.6 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 40 /D1))
    (pad 42 smd rect (at -2.4 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 41 /D2))
    (pad 43 smd rect (at -3.2 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 42 /D3))
    (pad 44 smd rect (at -4 -5.85 45) (size 1.6 0.56) (layers F.Cu F.Paste F.Mask)
      (net 43 /D4))
    (model Housings_QFP.3dshapes/LQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 (layer B.Cu) (tedit 58441C24)
    (at 172.72 100.33 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 /D0))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 /D1))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 41 /D2))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 42 /D3))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 43 /D4))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 /D5))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 /D6))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 /D7))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 /D8))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 /D9))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 /D10))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 /D11))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 /D12))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 /D13))
    (pad 15 thru_hole oval (at 0 -35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 /D14))
    (pad 16 thru_hole oval (at 0 -38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 /D15))
    (pad 17 thru_hole oval (at 0 -40.64 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 -43.18 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 58436159)
    (at 129.54 116.84 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /DTR))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D9))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D8))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /RAW))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x18 (layer B.Cu) (tedit 58441C28)
    (at 129.54 120.65 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 5.1 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 /RAW))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /RESET))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 /D16))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 /D17))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 /D18))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 /D19))
    (pad 7 thru_hole oval (at 0 -15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 /D20))
    (pad 8 thru_hole oval (at 0 -17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 /D21))
    (pad 9 thru_hole oval (at 0 -20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 /D22))
    (pad 10 thru_hole oval (at 0 -22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 /D23))
    (pad 11 thru_hole oval (at 0 -25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /A7))
    (pad 12 thru_hole oval (at 0 -27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /A6))
    (pad 13 thru_hole oval (at 0 -30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /A5))
    (pad 14 thru_hole oval (at 0 -33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /A4))
    (pad 15 thru_hole oval (at 0 -35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 /A3))
    (pad 16 thru_hole oval (at 0 -38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 /A2))
    (pad 17 thru_hole oval (at 0 -40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 /A1))
    (pad 18 thru_hole oval (at 0 -43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 /A0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58482F9C)
    (at 136.525 114.935 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.127 1.397 270) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /D0))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5848306C)
    (at 172.085 116.84)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.143 -1.27) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5848300C)
    (at 165.735 106.045 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -0.127 1.397 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_TL3342 (layer F.Cu) (tedit 58436140)
    (at 159.385 110.49 270)
    (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
    (tags "SPST Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -3.75 270) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 3.75 270) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.15 -1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.15 1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 3.15 1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (model /Users/paulo/MEOCloud/kicad/mightyduino/3d/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:CSTCEv2 (layer F.Cu) (tedit 58482FC7)
    (at 137.795 105.41 225)
    (fp_text reference X1 (at 0 1.524 225) (layer F.SilkS))
    (fp_text value "CSTCE 16MHZ" (at 0 -1.778 225) (layer F.Fab) hide)
    (pad 3 smd rect (at 0 -0.0365 225) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.2 -0.0365 225) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad8)"))
    (pad 1 smd rect (at -1.2 -0.0365 225) (size 0.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad7)"))
    (model /Users/paulo/MEOCloud/kicad/mightyduino/cstce4.wrl
      (at (xyz 0.06 0.025 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58483050)
    (at 173.228 107.68 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -2.556 0.254 90) (layer F.SilkS))
    (fp_text value 470p (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58483046)
    (at 170.01 110.81)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -2.9034 0.061 90) (layer F.SilkS))
    (fp_text value MIC5219-3.3YM5 (at -0.05 2.35) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C7-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58482F8D)
    (at 133.731 116.84 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /DTR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5848305B)
    (at 170.08602 114.173)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -0.16002 -1.143) (layer F.SilkS))
    (fp_text value red (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:logo_small_solder_mask (layer B.Cu) (tedit 0)
    (at 168.91 110.49 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module parts:dev76logo (layer B.Cu) (tedit 0)
    (at 161.29 115.57 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module parts:logo_oshw (layer B.Cu) (tedit 0)
    (at 163.576 113.792 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module parts:specs (layer B.Cu) (tedit 0)
    (at 157.226 110.49)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Reflow (layer F.Cu) (tedit 58713733)
    (at 164.211 113.665 270)
    (descr "Tantal Cap. , Size A, EIA-3216, Reflow")
    (tags "Tantal Capacitor Size-A EIA-3216 reflow")
    (attr smd)
    (fp_text reference C1 (at -1.27 -1.8415 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1.31 0 270) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.31 0 270) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Reflow (layer F.Cu) (tedit 5871371D)
    (at 170.2435 104.394 180)
    (descr "Tantal Cap. , Size A, EIA-3216, Reflow")
    (tags "Tantal Capacitor Size-A EIA-3216 reflow")
    (attr smd)
    (fp_text reference C3 (at 3.1115 0.508 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.31 0 180) (size 1.8 1.23) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text v1.3 (at 173.355 116.205 90) (layer B.SilkS))
  (gr_text "2017\nDev76.org" (at 138.303 110.4138 90) (layer B.SilkS))
  (gr_line (start 128.143 98.933) (end 128.143 98.933) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.143 122.047) (end 128.143 98.933) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.371 122.047) (end 128.143 122.047) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.371 98.933) (end 174.371 122.047) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.143 98.933) (end 174.371 98.933) (layer Edge.Cuts) (width 0.15))
  (gr_text ~SS (at 162.56 103.505 90) (layer B.SilkS))
  (gr_text INT0 (at 147.32 103.505 90) (layer B.SilkS))
  (gr_text TX0 (at 149.86 103.505 90) (layer B.SilkS))
  (gr_text RX0 (at 152.4 103.505 90) (layer B.SilkS))
  (gr_text SDA (at 137.16 117.475 90) (layer B.SilkS))
  (gr_text SCL (at 134.62 117.475 90) (layer B.SilkS))
  (gr_text SCK (at 154.94 103.505 90) (layer B.SilkS))
  (gr_text MISO (at 157.48 103.505 90) (layer B.SilkS))
  (gr_text MOSI (at 160.02 103.505 90) (layer B.SilkS))
  (gr_text LED (at 172.7708 103.886 90) (layer F.SilkS))
  (gr_text LED (at 172.72 104.775 90) (layer B.SilkS))
  (gr_text 21 (at 147.32 118.745) (layer B.SilkS))
  (gr_text 23 (at 152.4 118.745) (layer B.SilkS))
  (gr_text 10 (at 147.32 102.235 180) (layer B.SilkS))
  (gr_text 11 (at 144.78 102.235 180) (layer B.SilkS))
  (gr_text GND (at 132.08 102.235 180) (layer B.SilkS))
  (gr_text VCC (at 129.5146 102.235 180) (layer B.SilkS))
  (gr_text 15 (at 134.62 102.235 180) (layer B.SilkS))
  (gr_text 2 (at 167.64 102.235 180) (layer B.SilkS))
  (gr_text 3 (at 165.1 102.235 180) (layer B.SilkS))
  (gr_text 1 (at 170.18 102.235 180) (layer B.SilkS))
  (gr_text 0 (at 172.72 102.235 180) (layer B.SilkS))
  (gr_text 13 (at 139.7 102.235 180) (layer B.SilkS))
  (gr_text 14 (at 137.16 102.235 180) (layer B.SilkS))
  (gr_text 12 (at 142.24 102.235 180) (layer B.SilkS))
  (gr_text 9 (at 149.86 102.235 180) (layer B.SilkS))
  (gr_text 4 (at 162.56 102.235 180) (layer B.SilkS))
  (gr_text 5 (at 160.02 102.235 180) (layer B.SilkS))
  (gr_text 8 (at 152.4 102.235 180) (layer B.SilkS))
  (gr_text 6 (at 157.48 102.235 180) (layer B.SilkS))
  (gr_text 7 (at 154.94 102.235 180) (layer B.SilkS))
  (gr_text RAW (at 129.667 118.618) (layer B.SilkS))
  (gr_text RST (at 132.207 118.745) (layer B.SilkS))
  (gr_text A1 (at 170.18 118.745) (layer B.SilkS))
  (gr_text A0 (at 172.72 118.745) (layer B.SilkS))
  (gr_text A3 (at 165.1 118.745) (layer B.SilkS))
  (gr_text A2 (at 167.64 118.745) (layer B.SilkS))
  (gr_text 17 (at 137.033 118.745) (layer B.SilkS))
  (gr_text 18 (at 139.573 118.745) (layer B.SilkS))
  (gr_text 16 (at 134.493 118.745) (layer B.SilkS))
  (gr_text 19 (at 142.113 118.745) (layer B.SilkS))
  (gr_text 22 (at 149.86 118.745) (layer B.SilkS))
  (gr_text 20 (at 145.034 118.745) (layer B.SilkS))
  (gr_text A5 (at 160.02 118.745) (layer B.SilkS))
  (gr_text A4 (at 162.56 118.745) (layer B.SilkS))
  (gr_text A7 (at 154.94 118.745) (layer B.SilkS))
  (gr_text A6 (at 157.48 118.745) (layer B.SilkS))
  (gr_text RESET (at 156.0068 110.49 90) (layer F.SilkS))
  (gr_text RAW (at 131.561123 109.223181 90) (layer F.SilkS))
  (gr_text GND (at 131.561123 106.683181 90) (layer F.SilkS))
  (gr_text TX (at 131.561123 114.303181 90) (layer F.SilkS))
  (gr_text RX (at 131.561123 111.763181 90) (layer F.SilkS))
  (gr_text DTR (at 131.318 116.84 90) (layer F.SilkS))
  (gr_text VCC (at 131.561123 104.143181 90) (layer F.SilkS))
  (gr_text DTR (at 131.572 116.84 90) (layer B.SilkS))
  (gr_text TX (at 131.572 114.3 90) (layer B.SilkS))
  (gr_text RX (at 131.572 111.76 90) (layer B.SilkS))
  (gr_text RAW (at 131.572 109.22 90) (layer B.SilkS))
  (gr_text GND (at 131.572 106.68 90) (layer B.SilkS))
  (gr_text VCC (at 131.572 104.14 90) (layer B.SilkS))
  (gr_text VCC (at 129.5146 102.1588 180) (layer F.SilkS))
  (gr_text GND (at 132.08 102.362 180) (layer F.SilkS))
  (gr_text 0 (at 172.72 102.362 180) (layer F.SilkS))
  (gr_text 1 (at 170.18 102.362 180) (layer F.SilkS))
  (gr_text 5 (at 160.02 102.362 180) (layer F.SilkS))
  (gr_text 4 (at 162.56 102.362 180) (layer F.SilkS))
  (gr_text 3 (at 165.1 102.362 180) (layer F.SilkS))
  (gr_text 2 (at 167.64 102.362 180) (layer F.SilkS))
  (gr_text 6 (at 157.48 102.362 180) (layer F.SilkS))
  (gr_text 7 (at 154.94 102.362 180) (layer F.SilkS))
  (gr_text 11 (at 145.0594 102.2985 180) (layer F.SilkS))
  (gr_text 9 (at 149.86 102.362 180) (layer F.SilkS))
  (gr_text 10 (at 147.574 102.108 180) (layer F.SilkS))
  (gr_text 8 (at 152.4 102.362 180) (layer F.SilkS))
  (gr_text 13 (at 139.7 102.362 180) (layer F.SilkS))
  (gr_text 12 (at 142.24 102.362 180) (layer F.SilkS))
  (gr_text 14 (at 137.16 102.362 180) (layer F.SilkS))
  (gr_text 15 (at 134.62 102.362 180) (layer F.SilkS))
  (gr_text RAW (at 129.667 118.872) (layer F.SilkS))
  (gr_text RST (at 132.207 118.745) (layer F.SilkS))
  (gr_text 17 (at 137.033 118.745) (layer F.SilkS))
  (gr_text 19 (at 142.113 118.745) (layer F.SilkS))
  (gr_text 16 (at 134.493 118.745) (layer F.SilkS))
  (gr_text 18 (at 139.573 118.745) (layer F.SilkS))
  (gr_text 21 (at 147.828 118.872) (layer F.SilkS))
  (gr_text 23 (at 152.908 118.745) (layer F.SilkS))
  (gr_text 20 (at 145.034 118.745) (layer F.SilkS))
  (gr_text 22 (at 149.86 118.745) (layer F.SilkS))
  (gr_text A6 (at 157.48 118.745) (layer F.SilkS))
  (gr_text A4 (at 162.56 118.745) (layer F.SilkS))
  (gr_text A7 (at 154.94 118.745) (layer F.SilkS))
  (gr_text A5 (at 160.02 118.745) (layer F.SilkS))
  (gr_text A3 (at 165.1 118.745) (layer F.SilkS))
  (gr_text A2 (at 167.64 118.745) (layer F.SilkS))
  (gr_text A1 (at 170.18 118.745) (layer F.SilkS))
  (gr_text A0 (at 172.72 118.745) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.445 102.235) (xy 173.99 102.235) (xy 173.99 118.745) (xy 131.445 118.745)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.445 102.235) (xy 173.99 102.235) (xy 173.99 118.745) (xy 132.08 118.745) (xy 131.445 118.745)
      )
    )
  )
)
