(kicad_pcb (version 20171130) (host pcbnew 5.1.12-84ad8e8a86~92~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 71)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.254)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 /active)
  (net 4 /radial)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net /active)
    (add_net /radial)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
  )
  (module Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount (layer F.Cu) (tedit 5DAA3454)
    (at 162.995 100.965 90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (attr smd)
    (fp_text reference J1 (at 0 -0.435 90) (layer B.SilkS))
    (fp_text value "SMA EDGE" (at 0 13 90) (layer F.Fab))
    (fp_text user "Board Thickness: 1.57mm" (at 0 5.915 90) (layer Cmts.User))
    (fp_text user "PCB Edge" (at 0 14.17 90) (layer Dwgs.User))
    (fp_text user %R (at 0 4.79 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0.2 90) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2.825 0 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.825 0 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.825 0 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.825 0 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module minicircuits_footprints:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5A365E23)
    (at 150.495 100.965 180)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference TR1 (at -4.445 -3.175 90) (layer F.SilkS))
    (fp_text value ADT1.5-122 (at 0 5.08) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /active))
    (pad 5 smd rect (at 2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /radial))
    (pad 3 smd rect (at -2.54 2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.54 0 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/RF_Mini-Circuits.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 142.875 97.155)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H2 (at -5.08 0) (layer F.SilkS))
    (fp_text value radial (at -6.35 0) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 /radial))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 4 /radial))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 56DDBAEA)
    (at 142.875 104.775)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference H1 (at -5.08 0) (layer F.SilkS))
    (fp_text value active (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /active))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 3 /active))
  )
  (gr_text "Dipole \nBalun" (at 151.765 100.965 90) (layer B.SilkS))
  (gr_line (start 146.05 105.664) (end 165.1 105.664) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.05 105.664) (end 146.05 112.0775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.05 89.8525) (end 146.05 96.266) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 96.266) (end 146.05 96.266) (layer Edge.Cuts) (width 0.05))
  (gr_text "#2 Screw\n1/4\" Element" (at 147.955 100.965 90) (layer B.SilkS))
  (gr_text - (at 146.685 96.012 90) (layer F.SilkS))
  (gr_text + (at 146.685 105.918 90) (layer F.SilkS))
  (gr_text "v2, rev-\nZ. LEFFKE\nVT-NSI\n20220209" (at 156.845 97.155 90) (layer B.SilkS))
  (gr_line (start 146.05 112.0775) (end 139.7 112.0775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 96.266) (end 165.1 105.664) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 89.8525) (end 146.05 89.8525) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 112.0775) (end 139.7 89.8525) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 105.41) (xy 149.86 105.41) (xy 149.86 96.52) (xy 165.1 96.52)
      )
    )
  )
  (zone (net 4) (net_name /radial) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 99.06) (xy 144.78 100.33) (xy 140.97 100.33) (xy 139.7 99.06) (xy 139.7 89.8525)
        (xy 146.05 89.8525)
      )
    )
  )
  (zone (net 3) (net_name /active) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 102.87) (xy 146.05 112.0775) (xy 139.7 112.0775) (xy 139.7 102.87) (xy 140.97 101.6)
        (xy 144.78 101.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 112.0775) (xy 139.7 112.0775) (xy 139.7 89.8525) (xy 146.05 89.8525)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 112.0775) (xy 139.7 112.0775) (xy 139.7 89.8525) (xy 146.05 89.8525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 99.06) (xy 164.465 99.695) (xy 164.465 102.235) (xy 165.1 102.87) (xy 165.1 105.41)
        (xy 149.86 105.41) (xy 149.86 96.52) (xy 165.1 96.52)
      )
    )
  )
)
