(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 38)
    (zones 0)
    (modules 9)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(Q1-Pad3)")
  (net 3 "Net-(Q1-Pad2)")
  (net 4 +1V5)
  (net 5 VCC)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(SW1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V5)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(SW1-Pad2)")
    (add_net VCC)
  )
  (module HVPS:MSS22D18D (layer B.Cu) (tedit 5FB07A98)
    (at 140.4874 104.902 180)
    (fp_text reference switch (at 0.7366 -4.318 180) (layer B.SilkS))
    (fp_text value MSS22D18D (at 0 0.5 180) (layer B.Fab))
    (pad 2 smd rect (at -0.6496 -7.9384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -3.1496 -7.9384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad3)"))
    (pad 3 smd rect (at 1.8504 -7.9384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 1.8504 -2.4384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -0.6496 -2.4384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -3.1496 -2.4384 180) (size 1.1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad3)"))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 144.9721 116.13642)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -0.09144 90) (layer F.SilkS))
    (fp_text value "2.2uF 250v" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 151.1173 113.0681 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D1 (at 2.68796 0) (layer F.SilkS))
    (fp_text value F16V27 (at 2.54 2.42) (layer F.Fab))
    (fp_text user K (at 0 -2) (layer F.Fab))
    (fp_text user %R (at 2.78 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB06055)
    (at 148.55444 115.90528)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference anode (at 1.8669 -0.14986 215) (layer F.SilkS))
    (fp_text value "HV out" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FB02375)
    (at 141.3637 115.81384)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference cathode (at -1.40716 -1.01854 90) (layer F.SilkS))
    (fp_text value "GND out" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8001) (layers *.Cu *.Mask)
      (net 5 VCC))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5FAF3929)
    (at 146.36496 101.90226)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference GND (at 1.97104 0.02794 270) (layer F.SilkS))
    (fp_text value "GND in" (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill0.8mm (layer F.Cu) (tedit 5A2676A0)
    (at 143.82496 101.90226)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference 1v5 (at -1.94056 -0.02286 270) (layer F.SilkS))
    (fp_text value 1v5 (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 +1V5))
  )
  (module "USB Micro numitronWatch:XFT-5383" (layer F.Cu) (tedit 5FAF23EA)
    (at 145.51152 100.44556)
    (fp_text reference T1 (at -0.20066 4.29134) (layer F.SilkS))
    (fp_text value "Flash XFMR" (at 0.03048 1.91644) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.82956 4.03352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 2.17044 4.03352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 +1V5))
    (pad 3 thru_hole circle (at -2.82956 10.03352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(SW1-Pad2)"))
    (pad 5 thru_hole circle (at -0.32956 10.03352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.17044 10.03352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
  )
  (module Package_TO_SOT_THT:TO-92L_Inline (layer F.Cu) (tedit 5A279A44)
    (at 151.13 106.934 270)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (fp_text reference Q1 (at 1.19 -1.778 90) (layer F.SilkS))
    (fp_text value 2SD2470 (at 1.19 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.19 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole roundrect (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole roundrect (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "this side" (at 139.1666 110.49) (layer B.SilkS))
  (gr_text "this\nside\nup" (at 149.8727 103.40086) (layer B.SilkS))
  (gr_text "components\nthis side" (at 139.59586 103.86822 50) (layer F.SilkS))
  (gr_text "this side down" (at 138.5316 109.601 90) (layer F.SilkS))
  (gr_circle (center 145.034 109.2454) (end 154.034 109.2454) (layer Edge.Cuts) (width 0.12))
  (gr_text "Layout by\nAnalogTek" (at 145.34896 107.29468) (layer F.SilkS))
)
