<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="3.81" x2="41.58" y2="3.81" width="0" layer="20"/>
<wire x1="41.58" y1="3.81" x2="41.58" y2="55.87" width="0" layer="20"/>
<wire x1="41.58" y1="55.87" x2="2.54" y2="55.87" width="0" layer="20"/>
<wire x1="2.54" y1="55.87" x2="2.54" y2="3.81" width="0" layer="20"/>
<text>©Jed Hodson
2013 </text>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
</package>
<package name="1X08">
</package>
<package name="1X01NS">
</package>
<package name="FTDI_BASIC">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL28-3" value="MEGA8-P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="OLED_TERMINAL" library="SparkFun-Connectors" package="AVR_ICSP" value=""/>
<element name="Q1" library="crystal" package="HC49/S" value="16MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pF"/>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="22pF"/>
<element name="RESET" library="jumper" package="JP1" value=""/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="10K"/>
<element name="I2C" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="PINS_0-7" library="SparkFun-Connectors" package="1X08" value=""/>
<element name="PWR" library="SparkFun-Connectors" package="1X01NS" value=""/>
<element name="GND" library="SparkFun-Connectors" package="1X01NS" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="FTDI_BASIC" value="FTDI_BASICPTH"/>
<element name="ANALOG" library="SparkFun-Connectors" package="1X03" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="GND" pad="1"/>
<contactref element="OLED_TERMINAL" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="I2C" pad="4"/>
<contactref element="JP1" pad="GND"/>
<contactref element="RESET" pad="1"/>
<contactref element="IC1" pad="22"/>
<contactref element="ANALOG" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="VCC"/>
<contactref element="PWR" pad="1"/>
<contactref element="OLED_TERMINAL" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="21"/>
<contactref element="I2C" pad="3"/>
<contactref element="R1" pad="P$2"/>
<contactref element="ANALOG" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="27"/>
<contactref element="I2C" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="I2C" pad="1"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="TXO"/>
<contactref element="IC1" pad="3"/>
<contactref element="PINS_0-7" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="RXI"/>
<contactref element="IC1" pad="2"/>
<contactref element="PINS_0-7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="PINS_0-7" pad="3"/>
<contactref element="IC1" pad="4"/>
<contactref element="OLED_TERMINAL" pad="9"/>
</signal>
<signal name="N$14">
<contactref element="PINS_0-7" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="OLED_TERMINAL" pad="10"/>
</signal>
<signal name="N$15">
<contactref element="PINS_0-7" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="OLED_TERMINAL" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="PINS_0-7" pad="7"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="PINS_0-7" pad="8"/>
<contactref element="IC1" pad="13"/>
<contactref element="OLED_TERMINAL" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="OLED_TERMINAL" pad="5"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$19">
<contactref element="OLED_TERMINAL" pad="6"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="19"/>
<contactref element="OLED_TERMINAL" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="PINS_0-7" pad="6"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="ANALOG" pad="2"/>
<contactref element="IC1" pad="23"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
