(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 53)
    (zones 0)
    (modules 25)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 162 57)
    (grid_origin 162 57)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "export/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-PadS)")
  (net 2 "Net-(J1-PadT)")
  (net 3 "Net-(J1-PadTN)")
  (net 4 "Net-(J2-PadTN)")
  (net 5 "Net-(J2-PadT)")
  (net 6 "Net-(J2-PadS)")
  (net 7 "Net-(J3-PadS)")
  (net 8 "Net-(J3-PadT)")
  (net 9 "Net-(J3-PadTN)")
  (net 10 "Net-(J4-PadTN)")
  (net 11 "Net-(J4-PadT)")
  (net 12 "Net-(J4-PadS)")
  (net 13 "Net-(J11-Pad1)")
  (net 14 "Net-(J11-Pad2)")
  (net 15 "Net-(J11-Pad3)")
  (net 16 "Net-(J10-PadTN)")
  (net 17 "Net-(J10-PadT)")
  (net 18 "Net-(J10-PadS)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-PadS)")
    (add_net "Net-(J1-PadT)")
    (add_net "Net-(J1-PadTN)")
    (add_net "Net-(J10-PadS)")
    (add_net "Net-(J10-PadT)")
    (add_net "Net-(J10-PadTN)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J2-PadS)")
    (add_net "Net-(J2-PadT)")
    (add_net "Net-(J2-PadTN)")
    (add_net "Net-(J3-PadS)")
    (add_net "Net-(J3-PadT)")
    (add_net "Net-(J3-PadTN)")
    (add_net "Net-(J4-PadS)")
    (add_net "Net-(J4-PadT)")
    (add_net "Net-(J4-PadTN)")
  )
  (module "chillpizza:graphic jackets bg 2" (layer B.Cu) (tedit 0)
    (at 170 122 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module "chillpizza:graphic jackets bg 1" (layer B.Cu) (tedit 0)
    (at 164 122 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 174)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 156)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 138)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 102)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 84)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic schematic thonk" (layer F.Cu) (tedit 0)
    (at 167 120)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:graphic jack gang stack" (layer F.Cu) (tedit 0)
    (at 169.75 181.75 270)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module "chillpizza:beat farm vertical only a" (layer F.Cu) (tedit 0)
    (at 167 65)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "chillpizza:beat farm vertical no a" (layer F.Cu) (tedit 0)
    (at 167 65)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 164.5 182.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 164.5 60)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 81.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-PadT)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-PadS)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 99.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-PadT)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-PadS)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 117.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-PadT)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-PadS)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 135.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-PadT)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-PadS)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 153.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J11-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 164.5 171.5 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J10-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J10-PadT)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J10-PadS)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 74 180)
    (fp_text reference J1 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-PadT)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-PadS)"))
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-PadTN)"))
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 92 180)
    (fp_text reference J2 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-PadTN)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-PadS)"))
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-PadT)"))
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 110 180)
    (fp_text reference J3 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J3-PadT)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J3-PadS)"))
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J3-PadTN)"))
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 128 180)
    (fp_text reference J4 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J4-PadTN)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J4-PadS)"))
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J4-PadT)"))
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 146 180)
    (fp_text reference J9 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J11-Pad2)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J11-Pad1)"))
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J11-Pad3)"))
  )
  (module chillpizza:THONKICONN_mill_kicad (layer F.Cu) (tedit 604EA002)
    (at 167 164 180)
    (fp_text reference J10 (at 3.81 6.35) (layer F.SilkS) hide)
    (fp_text value AudioJack2_SwitchT (at 0 -7.62) (layer F.Fab) hide)
    (fp_text user PUR** (at 5.08 -1.27) (layer F.SilkS) hide)
    (pad TN thru_hole oval (at 0 3.38 180) (size 2 1.5) (drill 1.1 (offset 0 -0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J10-PadTN)"))
    (pad S thru_hole oval (at 0 5.08 180) (size 2 1.5) (drill 1.1 (offset 0 0.15)) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J10-PadS)"))
    (pad T thru_hole circle (at 0 -4.92 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J10-PadT)"))
  )
  (gr_line (start 172 57) (end 162 57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172 185.5) (end 172 57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162 185.5) (end 172 185.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162 57) (end 162 185.5) (layer Edge.Cuts) (width 0.05))
)
