(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 109)
    (zones 0)
    (modules 8)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../Downloads/gerber/"))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 "Net-(IC1-Pad28)")
  (net 3 "Net-(IC1-Pad27)")
  (net 4 +3V0)
  (net 5 +VDC)
  (net 6 SCK)
  (net 7 !SS)
  (net 8 MOSI)
  (net 9 MISO)
  (net 10 /SDA)
  (net 11 /SCL)
  (net 12 /DIO0)
  (net 13 /A2)
  (net 14 /A3)
  (net 15 /~reset)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net !SS)
    (add_net +3V0)
    (add_net +VDC)
    (add_net /A2)
    (add_net /A3)
    (add_net /DIO0)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /~reset)
    (add_net Earth)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net SCK)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 115.64112 89.92616 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x10_Female (at 0 -15.03 270) (layer B.Fab))
    (fp_text user %R (at 0 -6.35) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A3))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A2))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 138.50112 89.92616 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x04_Female (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 -3.81) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V0))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCL))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:Ai-Thinker-Ra-01-LoRa (layer F.Cu) (tedit 5A57D4D7)
    (at 154.94 86.36 90)
    (descr "Ai Thinker Ra-01 LoRa")
    (tags "LoRa Ra-01")
    (attr smd)
    (fp_text reference U1 (at 0 -1 90) (layer F.SilkS))
    (fp_text value Ai-Thinker-Ra-01 (at 0 9.75 90) (layer F.Fab))
    (fp_text user %R (at 0 1 90) (layer F.Fab))
    (pad 16 smd rect (at 8 -7 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 15 smd rect (at 8 -5 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 !SS))
    (pad 14 smd rect (at 8 -3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 MOSI))
    (pad 13 smd rect (at 8 -1 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 MISO))
    (pad 12 smd rect (at 8 1 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 SCK))
    (pad 11 smd rect (at 8 3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 8 5 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 8 7 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 8 smd rect (at -8 7 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -8 5 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -8 3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -8 1 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /DIO0))
    (pad 4 smd rect (at -8 -1 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /~reset))
    (pad 3 smd rect (at -8 -3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V0))
    (pad 2 smd rect (at -8 -5 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 1 smd rect (at -8 -7 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/Ai-Thinker-Ra-01-LoRa.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer B.Cu) (tedit 5A1DD157)
    (at 121.21388 86.40572 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U3 (at 1.27 3.56 90) (layer B.SilkS))
    (fp_text value MCP1700-2502E_TO92 (at 1.27 -2.79 90) (layer B.Fab))
    (fp_text user %R (at 1.27 0 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 +3V0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 Earth))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm (layer B.Cu) (tedit 5BC5C9B9)
    (at 116.89588 83.566 90)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (fp_text reference C1 (at 0.75 3.25 270) (layer B.SilkS))
    (fp_text value "1 uF" (at 0.75 -3.25 270) (layer B.Fab))
    (fp_text user %R (at 0.75 0 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 1.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 +VDC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 5FB9AC23)
    (at 129.615001 86.538999)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference IC1 (at -13.97 10.16) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(IC1-Pad28)"))
    (pad 27 thru_hole oval (at 7.62 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad27)"))
    (pad 1 thru_hole oval (at -13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at -8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at -6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 Earth))
    (pad 5 thru_hole oval (at -3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 /DIO0))
    (pad 6 thru_hole oval (at -1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 /~reset))
    (pad 13 thru_hole oval (at 13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 !SS))
    (pad 14 thru_hole oval (at 11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole oval (at 1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole oval (at -1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A2))
    (pad 20 thru_hole oval (at -3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A3))
    (pad 21 thru_hole oval (at -6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V0))
    (pad 22 thru_hole oval (at -8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at -11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 Earth))
    (pad 24 thru_hole oval (at -13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at -2.54 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SDA))
    (pad 26 thru_hole oval (at -5.08 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCL))
    (pad 27 thru_hole oval (at 13.97 -5.08) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 13.97 -2.54) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(IC1-Pad28)"))
    (pad 29 thru_hole oval (at 13.97 0) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 Earth) (zone_connect 2))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz -3.809999942779541 5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 13.96999979019165 2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (offset (xyz 0 7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl
      (offset (xyz 0 -7.619999885559082 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 6.349999904632568 5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl
      (offset (xyz -1.269999980926514 0 12.19199981689453))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (offset (xyz 1.269999980926514 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (offset (xyz 13.96999979019165 -7.619999885559082 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (offset (xyz 13.96999979019165 7.619999885559082 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 13.96999979019165 5.079999923706055 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 7.619999885559082 5.079999923706055 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz -2.539999961853027 5.079999923706055 11.30299983024597))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (offset (xyz -7.619999885559082 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (offset (xyz 13.96999979019165 -4.444999933242798 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (offset (xyz -16.50999975204468 -6.349999904632568 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (offset (xyz -7.619999885559082 -1.269999980926514 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (offset (xyz 13.96999979019165 -3.174999952316284 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (offset (xyz -7.619999885559082 1.269999980926514 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl
      (offset (xyz -8.889999866485596 3.809999942779541 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl
      (offset (xyz -8.889999866485596 -3.809999942779541 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (offset (xyz -10.15999984741211 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (offset (xyz -12.69999980926514 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/switch/smd_push.wrl
      (offset (xyz 10.15999984741211 0 13.01749980449676))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 154.1526 90.81008)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 4 +3V0))
  )
  (module TestPoint:TestPoint_Pad_1.5x1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 149.25548 90.86596)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 1.648) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 Earth))
  )
  (gr_text "Lora v1.0 TJH" (at 155.19908 83.73364 90) (layer B.SilkS))
  (gr_line (start 156.95168 77.3684) (end 156.9466 77.37856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.55908 77.3684) (end 156.95168 77.3684) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.55908 95.39224) (end 114.55908 77.3684) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.9466 95.39224) (end 114.55908 95.39224) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.9466 77.37856) (end 156.9466 95.39224) (layer Edge.Cuts) (width 0.1))
  (gr_text VCC (at 121.43232 80.43164) (layer F.SilkS))
  (gr_text A3 (at 122.46864 81.32572) (layer F.SilkS))
  (gr_text "GND\nNSS\nMOSI\nMISO\nSCK\nDIO5\nDIO4\nGND" (at 155.11272 79.8322 90) (layer F.SilkS))
  (gr_text "ANT\nGND\n3.3\nReset\nDI00\nDI01\nDI02\nDI03" (at 155.03144 93.10624 90) (layer F.SilkS))
  (gr_text 11 (at 141.92504 80.391) (layer F.SilkS))
  (gr_text 12 (at 139.46632 80.391) (layer F.SilkS))
  (gr_text 13 (at 139.64412 81.8896) (layer F.SilkS))
  (gr_text A4 (at 127.17272 83.68284) (layer F.SilkS))
  (gr_text A5 (at 124.32284 83.61172) (layer F.SilkS))
  (gr_text A2 (at 128.46812 80.60436) (layer F.SilkS))
  (gr_text "Tx\nRx\nRst\nGnd\n2\n3\n4\n5\n6\n7\n8\n9" (at 129.62636 93.04528 90) (layer F.SilkS))
  (gr_text "Pro mini 8Mhz" (at 129.58572 86.38032) (layer F.SilkS))
  (gr_text "AI Ra-01" (at 155.83916 84.7852) (layer F.SilkS))
  (gr_text "Vin\nGND\nGND\nA3\nA4\nnc\nVCC\nGND\nSCL\nSDA" (at 127.127 88.7476 90) (layer B.SilkS))
  (zone (net 1) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.95676 95.008906) (xy 114.56416 95.37192) (xy 114.56416 77.35824) (xy 156.95676 77.030375)
      )
    )
  )
  (zone (net 1) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.95676 95.239846) (xy 114.67084 95.33128) (xy 114.63528 95.33128) (xy 114.62004 77.32776) (xy 156.95676 77.246475)
      )
    )
  )
)
