<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="-0.4" y1="-0.3" x2="27.8999625" y2="-0.3" width="0" layer="20"/>
<wire x1="27.8999625" y1="-0.3" x2="27.7999625" y2="22.74996875" width="0" layer="20"/>
<wire x1="27.7999625" y1="22.74996875" x2="-0.4" y2="22.79996875" width="0" layer="20"/>
<wire x1="-0.4" y1="22.79996875" x2="-0.4" y2="-0.3" width="0" layer="20"/>
<text>!RST</text>
<text>!RDNY</text>
<text>N/C</text>
<text>MISO</text>
<text>MOSI</text>
<text>!REQN</text>
<text>SCK</text>
<text>RXD</text>
<text>TXD</text>
<text>ACTIVE</text>
<text>GND</text>
<text>3.3V</text>
<text>AVDD</text>
<text>VDD</text>
<text>GND</text>
<text>3.3V</text>
<text>www.nabiltewolde.com</text>
<text>CC-BY-SA</text>
</plain>
<libraries>
<library name="FitnessDevice">
<packages>
<package name="QFN-32">
<description>&lt;h3&gt;QFN 32-Pin package w/ Thermal Pad&lt;/h3&gt;
&lt;B&gt;Applicable Parts:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;nRF8001&lt;/ul&gt;</description>
</package>
<package name="CRYSTAL-2.5X3.5">
</package>
<package name="CRYSTAL-ABS10">
<description>Crystals 32.768KHz 9pF - ABS10-32.768KHZ-9-T</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0603">
</package>
<package name="0603-RES">
</package>
<package name="1X03_LOCK">
</package>
<package name="LED-0603">
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="1X10_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="FitnessDevice" package="QFN-32" value="NRF8001"/>
<element name="C9" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C10" library="SparkFun" package="0603-CAP" value="100nF"/>
<element name="C11" library="SparkFun" package="0603-CAP" value="33nF"/>
<element name="C13" library="SparkFun" package="0603-CAP" value="12.5pF"/>
<element name="C14" library="SparkFun" package="0603-CAP" value="12.5pF"/>
<element name="C12" library="SparkFun" package="0603-CAP" value="100nF"/>
<element name="C3" library="SparkFun" package="0603-CAP" value="2.2nF"/>
<element name="C4" library="SparkFun" package="0603-CAP" value="0"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1.8pF"/>
<element name="C6" library="SparkFun" package="0603-CAP" value="1.2pF"/>
<element name="C8" library="SparkFun" package="0603-CAP" value="1.0nF"/>
<element name="C7" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C1" library="SparkFun" package="0603-CAP" value="18pF"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="18pF"/>
<element name="L1" library="SparkFun" package="0603" value="8.2nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="SparkFun" package="0603" value="3.9nH"/>
<element name="L2" library="SparkFun" package="0603" value="5.6nH"/>
<element name="L5" library="SparkFun" package="0603" value="15nH"/>
<element name="L4" library="SparkFun" package="0603" value="10uF"/>
<element name="R1" library="SparkFun" package="0603-RES" value="22k"/>
<element name="X1" library="FitnessDevice" package="CRYSTAL-2.5X3.5" value="16MHz"/>
<element name="X2" library="FitnessDevice" package="CRYSTAL-ABS10" value="32.768kHz"/>
<element name="JP2" library="SparkFun" package="1X03_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED-0603" value=""/>
<element name="R2" library="SparkFun" package="0603-RES" value=""/>
<element name="J$1" library="SparkFun" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="JP3" library="SparkFun" package="1X10_LOCK" value="M10LOCK"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="EP"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="30"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="C12" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="18"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="23"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J$1" pad="GND@0"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@1"/>
</signal>
<signal name="N$1">
<contactref element="L5" pad="2"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="L4" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="N$4">
<contactref element="C7" pad="1"/>
<contactref element="L5" pad="1"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="3"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="L3" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$9">
<contactref element="L2" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$13">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="L2" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="L3" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="J$1" pad="SIG"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="25"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="28"/>
<contactref element="X1" pad="P$3"/>
</signal>
<signal name="!RESET">
<contactref element="U1" pad="19"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C13" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="X2" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="C14" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="X2" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="14"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="13"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="12"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="11"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="10"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="7"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="ACTIVE">
<contactref element="U1" pad="6"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="VDD">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="U1" pad="9"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="AVDD">
<contactref element="JP2" pad="3"/>
<contactref element="U1" pad="26"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
