<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="31.115" x2="59.69" y2="31.115" width="0" layer="20"/>
<wire x1="59.69" y1="31.115" x2="59.69" y2="69.85" width="0" layer="20"/>
<wire x1="59.69" y1="69.85" x2="0" y2="69.85" width="0" layer="20"/>
<wire x1="0" y1="69.85" x2="0" y2="31.115" width="0" layer="20"/>
<text>DATA TRAVEL
-AND-
EXPERIMENTS</text>
<text>20130907
KPS</text>
</plain>
<libraries>
<library name="conn">
<packages>
<package name="J-8-MINIDIN-KMD11">
<description>Mini-DIN Socket.
&lt;p&gt;
Pads are numbered corresponding to Mini-DIN 8 connector pins.</description>
</package>
<package name="J-8-RJ12-TE5555163">
<description>RJ12 (RJ11) 6p6c connector, low profile.
&lt;p&gt;
e.g. &lt;a href="http://www.digikey.ca/product-detail/en/5555163-1/A31420-ND/769564"&gt;TE 5555163-1&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="ic">
<packages>
<package name="IC-ATMEGA32U2-NOOGROOVE">
</package>
</packages>
</library>
<library name="misc">
<packages>
<package name="2H-300-P-SMALLSS">
</package>
<package name="2H-100-P-EXTSS">
</package>
<package name="2H-300-N-NOSS">
</package>
</packages>
</library>
<library name="switch">
<packages>
<package name="SW-TACTILE-RA">
</package>
</packages>
</library>
<library name="glyphs">
<packages>
<package name="GLYPH-DT&amp;E-100">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="ic" package="IC-ATMEGA32U2-NOOGROOVE" value="Micropendous 32U2"/>
<element name="JK2" library="conn" package="J-8-MINIDIN-KMD11" value="KM2"/>
<element name="JK1" library="conn" package="J-8-MINIDIN-KMD11" value="KM1"/>
<element name="D2" library="misc" package="2H-100-P-EXTSS" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="misc" package="2H-100-P-EXTSS" value="LED"/>
<element name="R2" library="misc" package="2H-300-N-NOSS" value="150Ω"/>
<element name="R1" library="misc" package="2H-300-N-NOSS" value="150Ω"/>
<element name="JF1" library="conn" package="J-8-RJ12-TE5555163" value="FS1"/>
<element name="JF2" library="conn" package="J-8-RJ12-TE5555163" value="FS2"/>
<element name="SW1" library="switch" package="SW-TACTILE-RA" value="SW-TACTILE-RA"/>
<element name="D3" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="D4" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="D5" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="D6" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="D7" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="D8" library="misc" package="2H-300-P-SMALLSS" value="1N4148"/>
<element name="U$2" library="glyphs" package="GLYPH-DT&amp;E-100" value=""/>
</elements>
<signals>
<signal name="1MISO">
<contactref element="U1" pad="PB3"/>
<contactref element="JK1" pad="1"/>
</signal>
<signal name="1MOSI">
<contactref element="U1" pad="PB2"/>
<contactref element="JK1" pad="7"/>
</signal>
<signal name="1SCK">
<contactref element="U1" pad="PB1"/>
<contactref element="JK1" pad="6"/>
</signal>
<signal name="1!SS">
<contactref element="U1" pad="PB0"/>
<contactref element="JK1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="GND"/>
<contactref element="JF1" pad="1"/>
<contactref element="JF2" pad="1"/>
<contactref element="JK2" pad="3"/>
<contactref element="JK1" pad="3"/>
<contactref element="JK1" pad="GND"/>
<contactref element="JK2" pad="GND"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="+5V"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JF2" pad="6"/>
<contactref element="JF1" pad="6"/>
<contactref element="JK2" pad="5"/>
<contactref element="JK1" pad="5"/>
</signal>
<signal name="2MOSI">
<contactref element="U1" pad="PD3"/>
<contactref element="JK2" pad="7"/>
</signal>
<signal name="2MISO">
<contactref element="U1" pad="PD2"/>
<contactref element="JK2" pad="1"/>
</signal>
<signal name="2SCK">
<contactref element="U1" pad="PD5"/>
<contactref element="JK2" pad="6"/>
</signal>
<signal name="2!SS">
<contactref element="JK2" pad="4"/>
<contactref element="U1" pad="PD4"/>
</signal>
<signal name="1INT">
<contactref element="U1" pad="PD1"/>
<contactref element="JK1" pad="8"/>
</signal>
<signal name="2INT">
<contactref element="U1" pad="PD0"/>
<contactref element="JK2" pad="8"/>
</signal>
<signal name="2!RST">
<contactref element="U1" pad="PB4"/>
<contactref element="JK2" pad="2"/>
</signal>
<signal name="1!RST">
<contactref element="U1" pad="PB5"/>
<contactref element="JK1" pad="2"/>
</signal>
<signal name="F1">
<contactref element="U1" pad="PC5"/>
<contactref element="D3" pad="A"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="F3">
<contactref element="U1" pad="PC7"/>
<contactref element="D5" pad="A"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LED2">
<contactref element="D2" pad="C"/>
<contactref element="U1" pad="PB7"/>
</signal>
<signal name="LED1">
<contactref element="D1" pad="C"/>
<contactref element="U1" pad="PB6"/>
</signal>
<signal name="2!FS">
<contactref element="JF2" pad="4"/>
<contactref element="U1" pad="PC4"/>
</signal>
<signal name="1!FS">
<contactref element="JF1" pad="4"/>
<contactref element="U1" pad="PC2"/>
</signal>
<signal name="F2">
<contactref element="U1" pad="PC6"/>
<contactref element="D4" pad="A"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="PD7"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D3" pad="C"/>
<contactref element="JF1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D4" pad="C"/>
<contactref element="JF1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="D5" pad="C"/>
<contactref element="JF1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="D8" pad="C"/>
<contactref element="JF2" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="D7" pad="C"/>
<contactref element="JF2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="D6" pad="C"/>
<contactref element="JF2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
