(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 61)
    (no_connects 0)
    (area 49.949999 49.949999 97.050001 122.050001)
    (thickness 1.6)
    (drawings 49)
    (tracks 162)
    (zones 0)
    (modules 29)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(R2-Pad1)")
  (net 5 +12V)
  (net 6 "Net-(JP3-Pad1)")
  (net 7 "Net-(JP2-Pad1)")
  (net 8 "Net-(P1-Pad2)")
  (net 9 "Net-(P2-Pad5)")
  (net 10 "Net-(JP5-Pad1)")
  (net 11 "Net-(JP5-Pad2)")
  (net 12 "Net-(D3-Pad2)")
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(D4-Pad1)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 "Net-(D5-Pad1)")
  (net 17 "Net-(D5-Pad2)")
  (net 18 "Net-(D6-Pad1)")
  (net 19 "Net-(D6-Pad2)")
  (net 20 "Net-(D7-Pad1)")
  (net 21 "Net-(JP4-Pad1)")
  (net 22 "Net-(P2-Pad2)")
  (net 23 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(R2-Pad1)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5862ABD0)
    (at 92 116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5862ABD0)
    (at 92 56)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5862ABD0)
    (at 55 116)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5834BF35)
    (at 55.88 62.23 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 3.175 2.54 270) (layer F.SilkS))
    (fp_text value 1K (at 6.35 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 58599F9D)
    (at 80.01 107.95 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 -0.635 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5867F131)
    (at 67.31 105.41 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 4.59 0.31 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 GND))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 585FF4B5)
    (at 92.71 100.33 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 6.985 2.54 270) (layer F.SilkS))
    (fp_text value D (at 5.08 -2.54 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 5835A316)
    (at 55.88 76.2 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D2 (at 6.985 2.54 270) (layer F.SilkS))
    (fp_text value 10V (at 3.81 2.54 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 585FF1F2)
    (at 90.17 85.09 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0 5.08 180) (layer F.SilkS))
    (fp_text value ACCUM (at -2.54 1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +12V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58599D90)
    (at 57.15 93.98 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value "LO EN" (at 2.54 1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(JP3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5834C1D3)
    (at 55.88 100.33 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 3.175 -2.54 270) (layer F.SilkS))
    (fp_text value 390* (at 7.62 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 585FF159)
    (at 62.23 107.95 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 6.35 2.54 270) (layer F.SilkS))
    (fp_text value R (at 5.12 0.495 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm_LongPads (layer F.Cu) (tedit 585FF831)
    (at 63.5 96.52 90)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 0 -3.175 90) (layer F.SilkS))
    (fp_text value LM3914_LED_BAR_DRIVER (at 5.08 10.16 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(JP3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(JP4-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad1)"))
    (pad 16 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad1)"))
    (pad 17 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 18 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-18_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 5859AA0E)
    (at 84.328 114.3 270)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -2.54 2.54 270) (layer F.SilkS))
    (fp_text value 47uF (at 4.445 -3.81 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 5867F136)
    (at 73.66 102.87 270)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at -1.37 3.66 270) (layer F.SilkS))
    (fp_text value 10uF (at -1.905 -3.81 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5834C6E0)
    (at 86.36 105.41 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U1 (at 3.81 2.54 90) (layer F.SilkS))
    (fp_text value LM7812 (at -1.27 2.54 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 +12V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5834C5D7)
    (at 90.17 91.44)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "HI EN" (at 2.54 1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(JP4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 585FF840)
    (at 64.77 78.74 90)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U4 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value LTV-845 (at 6.35 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(D5-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +12V))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(D6-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad5)"))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(JP5-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(JP5-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad2)"))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 67.31 85.09 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 72.39 85.09 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 77.47 85.09 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 82.55 85.09 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 62.23 104.14 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.91 3.06 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 +12V))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 585FFD4B)
    (at 72.39 66.04 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 3SPD (at -2.54 1.27 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(JP5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(JP5-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-3-3,5-h (layer F.Cu) (tedit 585EF7D0)
    (at 73.5 114.5)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at 0 5.3) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 -5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 3.5 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at -3.5 -0.7) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (model ${KIWALTER3DMOD}/walter/conn_pt-1_5/pt_1,5-3-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_pt-1,5:pt_1,5-6-3,5-h (layer F.Cu) (tedit 585EF740)
    (at 73.5 57.5 180)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P2 (at 0 5.3 180) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at 0 -5 180) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 5.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at 8.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 GND))
    (pad 3 thru_hole circle (at 1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(JP5-Pad1)"))
    (pad 4 thru_hole circle (at -1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(JP5-Pad2)"))
    (pad 5 thru_hole circle (at -5.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P2-Pad5)"))
    (pad 6 thru_hole circle (at -8.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 5 +12V))
    (model ${KIWALTER3DMOD}/walter/conn_pt-1_5/pt_1,5-6-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_5x2mm (layer F.Cu) (tedit 0)
    (at 89.5 72.5)
    (descr "CC BY-NC-SA logo, 5x2mm")
    (fp_text reference G*** (at 0.2 -0.7) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 0.2) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5862ABD0)
    (at 55 56)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connect:GS2 (layer F.Cu) (tedit 5867EFE6)
    (at 92.71 105.41 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 1.78 0 270) (layer F.SilkS) hide)
    (fp_text value NoReg (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
  )
  (gr_arc (start 51 51) (end 50 51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 96 51) (end 96 50) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 51 121) (end 51 122) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 96 121) (end 97 121) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 37 (width 0.3) (layer Cmts.User)
    (gr_text "37.000 mm" (at 73.5 44.65) (layer Cmts.User))
    (feature1 (pts (xy 92 48) (xy 92 43.3)))
    (feature2 (pts (xy 55 48) (xy 55 43.3)))
    (crossbar (pts (xy 55 46) (xy 92 46)))
    (arrow1a (pts (xy 92 46) (xy 90.873496 46.586421)))
    (arrow1b (pts (xy 92 46) (xy 90.873496 45.413579)))
    (arrow2a (pts (xy 55 46) (xy 56.126504 46.586421)))
    (arrow2b (pts (xy 55 46) (xy 56.126504 45.413579)))
  )
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 44.65 86 270) (layer Cmts.User))
    (feature1 (pts (xy 48 116) (xy 43.3 116)))
    (feature2 (pts (xy 48 56) (xy 43.3 56)))
    (crossbar (pts (xy 46 56) (xy 46 116)))
    (arrow1a (pts (xy 46 116) (xy 45.413579 114.873496)))
    (arrow1b (pts (xy 46 116) (xy 46.586421 114.873496)))
    (arrow2a (pts (xy 46 56) (xy 45.413579 57.126504)))
    (arrow2b (pts (xy 46 56) (xy 46.586421 57.126504)))
  )
  (gr_text 3.2mm (at 59.5 53.5) (layer B.SilkS))
  (gr_text 60mm (at 51 86 90) (layer B.SilkS))
  (gr_text 37mm (at 73.5 51) (layer B.SilkS))
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 102.85 86 270) (layer Cmts.User))
    (feature1 (pts (xy 99 122) (xy 104.2 122)))
    (feature2 (pts (xy 99 50) (xy 104.2 50)))
    (crossbar (pts (xy 101.5 50) (xy 101.5 122)))
    (arrow1a (pts (xy 101.5 122) (xy 100.913579 120.873496)))
    (arrow1b (pts (xy 101.5 122) (xy 102.086421 120.873496)))
    (arrow2a (pts (xy 101.5 50) (xy 100.913579 51.126504)))
    (arrow2b (pts (xy 101.5 50) (xy 102.086421 51.126504)))
  )
  (dimension 47 (width 0.3) (layer Cmts.User)
    (gr_text "47.000 mm" (at 73.5 127.85) (layer Cmts.User))
    (feature1 (pts (xy 97 124) (xy 97 129.2)))
    (feature2 (pts (xy 50 124) (xy 50 129.2)))
    (crossbar (pts (xy 50 126.5) (xy 97 126.5)))
    (arrow1a (pts (xy 97 126.5) (xy 95.873496 127.086421)))
    (arrow1b (pts (xy 97 126.5) (xy 95.873496 125.913579)))
    (arrow2a (pts (xy 50 126.5) (xy 51.126504 127.086421)))
    (arrow2b (pts (xy 50 126.5) (xy 51.126504 125.913579)))
  )
  (gr_text G (at 64.5 63) (layer F.SilkS))
  (gr_text jeditekunum (at 89.535 69.85) (layer F.SilkS))
  (gr_text "Fan Speed\nAdapter" (at 89.535 63.5) (layer F.SilkS))
  (gr_text 47mm (at 73.5 121) (layer F.SilkS))
  (gr_text v2 (at 89.535 67.31) (layer F.SilkS))
  (gr_text 4 (at 78.75 63) (layer F.SilkS))
  (gr_text 3 (at 75.25 63) (layer F.SilkS))
  (gr_text 2 (at 71.75 63) (layer F.SilkS))
  (gr_text 1 (at 68.25 63) (layer F.SilkS))
  (gr_text + (at 82.25 62.75) (layer F.SilkS))
  (gr_text 0-10V (at 73.5 109.5) (layer F.SilkS))
  (gr_text + (at 80.264 117.348) (layer F.SilkS))
  (gr_text G (at 66.548 117.348) (layer F.SilkS))
  (gr_text "72mm DIN" (at 95.885 86.36 90) (layer F.SilkS))
  (gr_line (start 51 50) (end 96 50) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97 121) (end 97 51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51 122) (end 96 122) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 51) (end 50 121) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97 122) (xy 50 122) (xy 50 50) (xy 97 50) (xy 97 122)
      )
    )
    (polygon
      (pts        (xy 52 52) (xy 52 120) (xy 95 120) (xy 95 52) (xy 52 52)
      )
    )
  )
)
