(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 126)
    (zones 0)
    (modules 36)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J3-Pad3)")
  (net 12 "Net-(J5-Pad1)")
  (net 13 "Net-(J5-Pad2)")
  (net 14 "Net-(J5-Pad3)")
  (net 15 "Net-(J4-Pad3)")
  (net 16 "Net-(J4-Pad2)")
  (net 17 "Net-(J4-Pad1)")
  (net 18 "Net-(J5-Pad4)")
  (net 19 "Net-(POT1-Pad4)")
  (net 20 "Net-(POT1-Pad3)")
  (net 21 "Net-(POT1-Pad1)")
  (net 22 "Net-(POT2-Pad1)")
  (net 23 "Net-(POT2-Pad3)")
  (net 24 "Net-(POT2-Pad4)")
  (net 25 "Net-(POT3-Pad4)")
  (net 26 "Net-(POT3-Pad3)")
  (net 27 "Net-(POT3-Pad1)")
  (net 28 "Net-(POT4-Pad1)")
  (net 29 "Net-(POT4-Pad3)")
  (net 30 "Net-(POT4-Pad4)")
  (net 31 "Net-(R5-Pad2)")
  (net 32 "Net-(R6-Pad2)")
  (net 33 "Net-(R3-Pad1)")
  (net 34 "Net-(R7-Pad1)")
  (net 35 "Net-(R9-Pad2)")
  (net 36 "Net-(R10-Pad2)")
  (net 37 "Net-(R11-Pad1)")
  (net 38 "Net-(R13-Pad2)")
  (net 39 "Net-(R14-Pad2)")
  (net 40 "Net-(R15-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(POT1-Pad1)")
    (add_net "Net-(POT1-Pad3)")
    (add_net "Net-(POT1-Pad4)")
    (add_net "Net-(POT2-Pad1)")
    (add_net "Net-(POT2-Pad3)")
    (add_net "Net-(POT2-Pad4)")
    (add_net "Net-(POT3-Pad1)")
    (add_net "Net-(POT3-Pad3)")
    (add_net "Net-(POT3-Pad4)")
    (add_net "Net-(POT4-Pad1)")
    (add_net "Net-(POT4-Pad3)")
    (add_net "Net-(POT4-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R9-Pad2)")
  )
  (module LogoLibrary:HighResSilkScreen (layer B.Cu) (tedit 0)
    (at 141.478 104.013 90)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 128.8415 60.198 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S1 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value EG1218 (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.925 60.198 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.1155 79.121 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.173 98.8695 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(J3-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9E)
    (at 117.6655 115.824 90)
    (descr "terminal block Metz Connect Type101_RT01603HBWC, 3 pins, pitch 5.08mm, size 15.2x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01603HBWC pitch 5.08mm size 15.2x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J4 (at 13.8557 -0.127 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 5.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9E)
    (at 117.6655 76.581 90)
    (descr "terminal block Metz Connect Type101_RT01603HBWC, 3 pins, pitch 5.08mm, size 15.2x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01603HBWC pitch 5.08mm size 15.2x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J2 (at 13.843 -0.0508 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 5.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 101.8286 44.6532)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0.103274 -3.175) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 159.8295 45.0215)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 101.981 139.6238)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0.306474 3.8354) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 160.259626 139.507826)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference "  " (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0.1016 4.0132) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.173 118.3005 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5A02FC95)
    (at 131.5085 130.3655)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW5 (at 0 -4.05) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 4.15) (layer F.Fab))
    (fp_text user %R (at 0 -4.05) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (pad 1 smd rect (at -3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad 1 smd rect (at 3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9E)
    (at 117.602 57.658 90)
    (descr "terminal block Metz Connect Type101_RT01603HBWC, 3 pins, pitch 5.08mm, size 15.2x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01603HBWC pitch 5.08mm size 15.2x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J1 (at 13.8303 0.1651 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 5.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01604HBWC_1x04_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9F)
    (at 117.729 138.3665 90)
    (descr "terminal block Metz Connect Type101_RT01604HBWC, 4 pins, pitch 5.08mm, size 20.3x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01604HBWC pitch 5.08mm size 20.3x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J5 (at -3.429 0.0254 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 8.128 -3.1496 90) (layer F.Fab))
    (fp_text user %R (at 7.62 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad 4 thru_hole circle (at 15.24 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad4)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01604HBWC_1x04_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9E)
    (at 117.5385 96.4565 90)
    (descr "terminal block Metz Connect Type101_RT01603HBWC, 3 pins, pitch 5.08mm, size 15.2x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01603HBWC pitch 5.08mm size 15.2x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J3 (at 13.9319 -0.0635 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 5.08 5.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01603HBWC_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type101_RT01602HBWC_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294E9E)
    (at 143.383 132.715 90)
    (descr "terminal block Metz Connect Type101_RT01602HBWC, 2 pins, pitch 5.08mm, size 10.2x8mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_311011_RT016xxHBWC_OFF-022771S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type101_RT01602HBWC pitch 5.08mm size 10.2x8mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J6 (at 2.54 -5.06 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 2.54 5.06 90) (layer F.Fab))
    (fp_text user %R (at 2.54 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad4)"))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type101_RT01602HBWC_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 128.9685 79.121 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S2 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value EG1218 (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(R6-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(R5-Pad2)"))
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 129.413 98.933 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S3 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value EG1218 (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(R9-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(R10-Pad2)"))
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 130.556 118.3005 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference S4 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value EG1218 (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(R13-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad1)"))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(R14-Pad2)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.493 55.1815 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(POT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.617 74.1045 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(POT2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.623 93.9165 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(POT3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 135.639 113.284 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0.13 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 39 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(POT4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.284 50.4825 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(POT1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.6015 88.011 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(POT3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.367 49.146 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.414 68.8975 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(POT2-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.427 108.1405 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 40 "Net-(R15-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(POT4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.4305 86.614 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(J3-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.4305 67.5005 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 "Net-(J2-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.494 106.7465 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_Small_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 40 "Net-(R15-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Rotary_Encoder (layer F.Cu) (tedit 5E3C50FC)
    (at 154.305 49.9745 270)
    (fp_text reference POT1 (at 6.701 9.8425 90) (layer F.SilkS))
    (fp_text value PTV09A-4025F-B503 (at 5.125 9.725 90) (layer F.Fab))
    (fp_text user %R (at 5.65 0.125 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 8.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(POT1-Pad3)"))
    (pad 2 thru_hole circle (at 5.7 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at 3.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(POT1-Pad1)"))
    (pad 4 thru_hole rect (at 11.4 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 19 "Net-(POT1-Pad4)"))
    (pad 4 thru_hole rect (at 0 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 19 "Net-(POT1-Pad4)"))
  )
  (module digikey-footprints:Rotary_Encoder (layer F.Cu) (tedit 5E3C50FC)
    (at 154.432 68.229 270)
    (fp_text reference POT2 (at 6.5405 9.525 90) (layer F.SilkS))
    (fp_text value PTV09A-4025F-B503 (at 5.125 9.725 90) (layer F.Fab))
    (fp_text user %R (at 5.65 0.125 90) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 24 "Net-(POT2-Pad4)"))
    (pad 4 thru_hole rect (at 11.4 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 24 "Net-(POT2-Pad4)"))
    (pad 1 thru_hole circle (at 3.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(POT2-Pad1)"))
    (pad 2 thru_hole circle (at 5.7 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 3 thru_hole circle (at 8.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(POT2-Pad3)"))
  )
  (module digikey-footprints:Rotary_Encoder (layer F.Cu) (tedit 5E3C50FC)
    (at 154.4955 87.406 270)
    (fp_text reference POT3 (at 6.1295 9.652 90) (layer F.SilkS))
    (fp_text value PTV09A-4025F-B503 (at 5.125 9.725 90) (layer F.Fab))
    (fp_text user %R (at 5.65 0.125 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 8.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(POT3-Pad3)"))
    (pad 2 thru_hole circle (at 5.7 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad3)"))
    (pad 1 thru_hole circle (at 3.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(POT3-Pad1)"))
    (pad 4 thru_hole rect (at 11.4 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 25 "Net-(POT3-Pad4)"))
    (pad 4 thru_hole rect (at 0 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 25 "Net-(POT3-Pad4)"))
  )
  (module digikey-footprints:Rotary_Encoder (layer F.Cu) (tedit 5E3C50FC)
    (at 154.4955 107.2815 270)
    (fp_text reference POT4 (at 7.239 9.5885 90) (layer F.SilkS))
    (fp_text value PTV09A-4025F-B503 (at 5.125 9.725 90) (layer F.Fab))
    (fp_text user %R (at 5.65 0.125 90) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 30 "Net-(POT4-Pad4)"))
    (pad 4 thru_hole rect (at 11.4 0 270) (size 2.8 3.6) (drill oval 1.8 2.6) (layers *.Cu *.Mask)
      (net 30 "Net-(POT4-Pad4)"))
    (pad 1 thru_hole circle (at 3.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(POT4-Pad1)"))
    (pad 2 thru_hole circle (at 5.7 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad3)"))
    (pad 3 thru_hole circle (at 8.2 7.5 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(POT4-Pad3)"))
  )
  (gr_text TT (at 153.924 130.3655) (layer F.SilkS))
  (gr_text TP/RG (at 106.8705 122.428) (layer F.SilkS))
  (gr_text WM1 (at 108.0135 103.124) (layer F.SilkS))
  (gr_text WM2 (at 107.696 84.074) (layer F.SilkS))
  (gr_text WM3 (at 107.5055 64.3255) (layer F.SilkS))
  (gr_text WM4 (at 108.077 44.8945) (layer F.SilkS))
  (gr_line (start 99.2378 42.5958) (end 99.2378 141.6685) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.8982 42.5958) (end 99.8982 41.9354) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.8982 141.6685) (end 99.2378 141.6685) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 162.2806 42.5704) (end 162.941 42.5704) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 162.306 141.6685) (end 162.306 142.3289) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text FW.WM4TPRG.0.3 (at 150.4569 140.8049) (layer F.SilkS))
  (gr_line (start 162.306 142.3289) (end 99.8982 142.3289) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162.941 42.5704) (end 162.9664 141.6685) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.8982 41.9354) (end 162.2806 41.91) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.2552 142.0368) (xy 110.6297 142.0368) (xy 110.6043 42.545) (xy 162.2298 42.545)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.2552 142.0368) (xy 110.6297 142.0114) (xy 110.6043 42.5196) (xy 162.2298 42.545)
      )
    )
  )
)
