(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/VC0")
  (net 2 "GND")
  (net 3 "/VC1")
  (net 4 "/VC2")
  (net 5 "/VC3")
  (net 6 "/VC4")
  (net 7 "/VC5")
  (net 8 "/AVDD")
  (net 9 "/VDD")
  (net 10 "/LD")
  (net 11 "Net-(D1-Pad2)")
  (net 12 "/B5+")
  (net 13 "Net-(J1-Pad2)")
  (net 14 "Net-(J3-Pad1)")
  (net 15 "Net-(J5-Pad2)")
  (net 16 "/PACK-")
  (net 17 "/CBI_in")
  (net 18 "/LPWR_in")
  (net 19 "/CSG_in")
  (net 20 "/DSG_in")
  (net 21 "unconnected-(J13-Pad6)")
  (net 22 "/CBI_out")
  (net 23 "/CSG")
  (net 24 "/DSG")
  (net 25 "/SRP_out")
  (net 26 "/SRN_out")
  (net 27 "Net-(J1-Pad3)")
  (net 28 "/OCDP")
  (net 29 "Net-(J1-Pad4)")
  (net 30 "Net-(J1-Pad5)")
  (net 31 "/CTRD")
  (net 32 "/SRN")
  (net 33 "/CTRC")
  (net 34 "Net-(JP1-Pad1)")
  (net 35 "/SRP")
  (net 36 "/CBI")
  (net 37 "/LPWR")
  (net 38 "Net-(R12-Pad1)")
  (net 39 "/PRES")
  (net 40 "Net-(JP1-Pad3)")
  (net 41 "Net-(JP2-Pad2)")
  (net 42 "Net-(JP3-Pad3)")
  (net 43 "Net-(JP5-Pad3)")
  (net 44 "unconnected-(J13-Pad7)")
  (net 45 "Net-(JP9-Pad2)")
  (net 46 "Net-(JP7-Pad2)")
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 68.072 84.582 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP5" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "CTRC" (at -0.058 -1.912 90) (layer "F.SilkS"))
    (pad "1" smd rect (at -1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 33 "/CTRC") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 43 "Net-(JP5-Pad3)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 63.5 99.568 -90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8 -270) (layer "F.SilkS") hide)
    (fp_text value "OCDP" (at -0.008 1.89 -270) (layer "F.SilkS"))
    (fp_text user "1" (at -2.6 0 -270) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 34 "Net-(JP1-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 28 "/OCDP") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 40 "Net-(JP1-Pad3)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A42A)
    (at 74.295 78.74 -90)
    (descr "Through hole angled socket strip, 1x07, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x07 2.54mm single row")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at -4.38 -2.77 90) (layer "F.SilkS") hide)
    (fp_text value "To Upper unit" (at 2.07 7.425 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -5.775 7.62) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/PACK-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/CSG_in") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/DSG_in") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/CBI_in") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/LPWR_in") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J13-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J13-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 59.182 84.582 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "PRES" (at 0.012 -1.932 90) (layer "F.SilkS"))
    (fp_text user "3" (at 2.6 0 90) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(J5-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 41 "Net-(JP2-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 18 "/LPWR_in") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A42D)
    (at 52.295 85.725)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -4.38 -2.77) (layer "F.SilkS"))
    (fp_text value "Cells" (at 2.005 6.235 270 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -5.775 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (zone_connect 1))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/B5+") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 74.295 105.41 -90)
    (descr "Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J15" (at 4.385 -2.27 90) (layer "F.SilkS") hide)
    (fp_text value "To lower unit" (at -2.09 7.175 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.77 7.62) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/PACK-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/CSG") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/DSG") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/CBI_out") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/LPWR") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/SRP_out") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/SRN_out") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 59.182 99.568 -90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP7" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "CBI" (at 0.002 1.852 90) (layer "F.SilkS"))
    (fp_text user "1" (at -2.6 0 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 22 "/CBI_out") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 46 "Net-(JP7-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "B") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 53.34 105.41)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.7mm_M2.5_ISO7380" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A41B)
    (at 80.137 97.155 180)
    (descr "Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -4.38 -2.77) (layer "F.SilkS"))
    (fp_text value "Temp" (at 2.737 1.405 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -5.775 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 63.5 92.075 -90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP6" (at 0 -1.8 -270) (layer "F.SilkS") hide)
    (fp_text value "SRP" (at -0.045 1.88 -270) (layer "F.SilkS"))
    (fp_text user "1" (at -2.6 0 -270) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 35 "/SRP") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 25 "/SRP_out") (pinfunction "B") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 53.34 78.74)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.7mm_M2.5_ISO7380" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A41B)
    (at 80.137 89.535 180)
    (descr "Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -4.38 -2.77) (layer "F.SilkS"))
    (fp_text value "PRES sw" (at 2.607 1.305 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -5.775 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 63.5 84.582 90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "CTRD" (at -0.028 -1.88 90) (layer "F.SilkS"))
    (fp_text user "3" (at 2.6 0 90) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 31 "/CTRD") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 42 "Net-(JP3-Pad3)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 80.01 78.74)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.7mm_M2.5_ISO7380" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 80.01 105.41)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.7mm_M2.5_ISO7380" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 59.182 92.075 -90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at 0 -1.8 -270) (layer "F.SilkS") hide)
    (fp_text value "SRN" (at -0.145 1.902 -270) (layer "F.SilkS"))
    (fp_text user "1" (at -2.6 0 -270) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 32 "/SRN") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 26 "/SRN_out") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 74.48 99.59 -90)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP9" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "NB cells" (at -0.67 1.97 90) (layer "F.SilkS"))
    (fp_text user "3" (at 2.6 0 90) (layer "F.SilkS") hide)
    (fp_text user "1" (at -2.6 0 90) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 45 "Net-(JP9-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 270) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 8 "/AVDD") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.75 97.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -1.05 -1.2) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 12 "/B5+") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 7 "/VC5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.766 99.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -1.066 -1.241) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 12 "/B5+") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 9 "/VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.753 86.9735)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.953 -1.2735) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 3 "/VC1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.753 94.5935)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -1.053 -1.1935) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 30 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "/VC4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 59.817 95.758 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.258 -0.017 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 7 "/VC5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "/VC4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 68.183 85.725)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0.017 1.375) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 41 "Net-(JP2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 39 "/PRES") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.753 84.4335)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -1.053 -1.2335) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "/VC0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 75.447 88.4)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -2.447 -0.2) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.025 0) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 10 "/LD") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0) (size 1.15 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 11 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 74.025 101.6 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -1.075 1.2) (layer "B.SilkS"))
    (fp_text value "487k" (at -0.111 -2.794) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 40 "Net-(JP1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 56.8375 102.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -1.0375 -1.3) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 9 "/VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 75.422 90.932 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 2.422 0.132) (layer "B.SilkS"))
    (fp_text value "450k" (at 0 -0.068) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 11 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 16 "/PACK-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 61.976 93.345 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 2.145 0.024 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "/VC4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 5 "/VC3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.785 92.0535)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -1.085 -1.2535 180) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 29 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 5 "/VC3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 76.82 94.3 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -1.03 -1.38 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 36 "/CBI") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 46 "Net-(JP7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 74.6 94.3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 1.01 -1.34 270) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 38 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 14 "Net-(J3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 59.817 85.725 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.225 0.083 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 3 "/VC1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (layer "B.Cu")
    (tedit 5E476F32)
    (at 68.199 92.329)
    (descr "TSSOP, 24 Pin (JEDEC MO-153 Var AD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "MANUFACTURER" "Texas Instruments")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm")
    (property "PARTREV" "H")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 4.85 180) (layer "B.SilkS"))
    (fp_text value "BQ7791501PWR" (at 0 -4.85 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.8625 3.575) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/AVDD") (pinfunction "AVDD") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/VC5") (pinfunction "VC5") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/VC4") (pinfunction "VC4") (pintype "input"))
    (pad "5" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/VC3") (pinfunction "VC3") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/VC2") (pinfunction "VC2") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/VC1") (pinfunction "VC1") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "/VC0") (pinfunction "VC0") (pintype "input"))
    (pad "9" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "10" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/SRP") (pinfunction "SRP") (pintype "input"))
    (pad "11" smd roundrect (at -2.8625 -2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "/SRN") (pinfunction "SRN") (pintype "input"))
    (pad "12" smd roundrect (at -2.8625 -3.575) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/DSG") (pinfunction "DSG") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -3.575) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/CSG") (pinfunction "CHG") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/LD") (pinfunction "LD") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "/LPWR") (pinfunction "LPWR") (pintype "output"))
    (pad "16" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/CBI") (pinfunction "CBI") (pintype "input"))
    (pad "17" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/OCDP") (pinfunction "OCDP") (pintype "input"))
    (pad "18" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J3-Pad1)") (pinfunction "TS") (pintype "input"))
    (pad "19" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R12-Pad1)") (pinfunction "VTB") (pintype "output"))
    (pad "20" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(JP9-Pad2)") (pinfunction "CCFG") (pintype "input"))
    (pad "21" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/CBI_in") (pinfunction "CBO") (pintype "output"))
    (pad "22" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/PRES") (pinfunction "PRES") (pintype "input"))
    (pad "23" smd roundrect (at 2.8625 2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "/CTRC") (pinfunction "CTRC") (pintype "input"))
    (pad "24" smd roundrect (at 2.8625 3.575) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/CTRD") (pinfunction "CTRD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 56.753 89.5135)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -0.953 -1.2135) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 27 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 4 "/VC2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 59.817 90.805 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.205 -0.017 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 5 "/VC3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 4 "/VC2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 61.214 100.457 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 2.257 0.086) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 8 "/AVDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 56.7475 81.8935 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.0475 1.2935 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 1 "/VC0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 74.025 99.06 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -1.075 1.26 180) (layer "B.SilkS"))
    (fp_text value "10M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 34 "Net-(JP1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 69.723 82.534 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -0.004 -1.447 90) (layer "B.SilkS"))
    (fp_text value "10M" (at 0.066 -0.077 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 19 "/CSG_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 43 "Net-(JP5-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 75.422 85.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.322 0) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 10 "/LD") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 67.31 82.534 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -0.024 1.33 90) (layer "B.SilkS"))
    (fp_text value "10M" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 20 "/DSG_in") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 42 "Net-(JP3-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 61.976 88.476 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "simpleBMS.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.276 0.024 180) (layer "B.SilkS"))
    (fp_text value "0.1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 4 "/VC2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 3 "/VC1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 49.8 76.47) (end 49.8 108.95) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49.8 108.95) (end 83.55 108.95) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49.8 76.47) (end 51.07 75.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.55 108.95) (end 83.55 75.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 51.07 75.2) (end 83.55 75.2) (layer "Edge.Cuts") (width 0.1))
  (gr_text "C1-" (at 53.4924 80.7212 270) (layer "F.SilkS"))
  (gr_text "3" (at 75.7 99.1) (layer "F.SilkS"))
  (gr_text "Other\nTop" (at 69.91 84.71) (layer "F.SilkS"))
  (gr_text "C5+" (at 53.34 100.5 270) (layer "F.SilkS"))
  (gr_text "5-NC" (at 75.7 102.14) (layer "F.SilkS"))
  (gr_text "4" (at 75.67 100.63) (layer "F.SilkS"))
  (gr_text "Other\nBottom" (at 65.37 99.54) (layer "F.SilkS"))
  (gr_text "Other\nBottom" (at 65.53 92.18) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.5 108.9)
        (xy 49.9 108.9)
        (xy 49.8 75.3)
        (xy 83.5 75.2)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.5 108.9)
        (xy 49.9 108.9)
        (xy 49.8 75.3)
        (xy 83.5 75.2)
      )
    )
  )
)
