(kicad_pcb (version 4) (host pcbnew no-vcs-found-product)
  (general
    (links 130)
    (no_connects 0)
    (area 135.909267 68.27 193.725715 104.9319)
    (thickness 1.6)
    (drawings 13)
    (tracks 249)
    (zones 0)
    (modules 83)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.1016)
    (pad_size 2 3.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C101-Pad1)")
  (net 2 "Net-(C101-Pad2)")
  (net 3 "Net-(C102-Pad1)")
  (net 4 GND)
  (net 5 +3V3)
  (net 6 "Net-(C105-Pad2)")
  (net 7 "Net-(C106-Pad2)")
  (net 8 "Net-(C107-Pad2)")
  (net 9 "Net-(C108-Pad2)")
  (net 10 "Net-(C109-Pad2)")
  (net 11 "Net-(C110-Pad2)")
  (net 12 "Net-(C111-Pad2)")
  (net 13 +5V)
  (net 14 "Net-(C116-Pad1)")
  (net 15 "Net-(C116-Pad2)")
  (net 16 "Net-(C117-Pad1)")
  (net 17 "Net-(C117-Pad2)")
  (net 18 "Net-(C118-Pad2)")
  (net 19 "Net-(C119-Pad2)")
  (net 20 "Net-(C120-Pad2)")
  (net 21 "Net-(C121-Pad2)")
  (net 22 "Net-(J102-Pad1)")
  (net 23 "Net-(L101-Pad2)")
  (net 24 "Net-(L102-Pad1)")
  (net 25 "Net-(L102-Pad2)")
  (net 26 "Net-(L103-Pad1)")
  (net 27 "Net-(L103-Pad2)")
  (net 28 /SCL)
  (net 29 /SDA)
  (net 30 "Net-(P102-Pad1)")
  (net 31 "Net-(P103-Pad1)")
  (net 32 "Net-(P106-Pad1)")
  (net 33 "Net-(P108-Pad1)")
  (net 34 "Net-(R105-Pad2)")
  (net 35 "Net-(R107-Pad2)")
  (net 36 "Net-(R108-Pad2)")
  (net 37 "Net-(T101-Pad2)")
  (net 38 "Net-(U101-Pad1)")
  (net 39 "Net-(U102-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C101-Pad2)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C107-Pad2)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C110-Pad2)")
    (add_net "Net-(C111-Pad2)")
    (add_net "Net-(C116-Pad1)")
    (add_net "Net-(C116-Pad2)")
    (add_net "Net-(C117-Pad1)")
    (add_net "Net-(C117-Pad2)")
    (add_net "Net-(C118-Pad2)")
    (add_net "Net-(C119-Pad2)")
    (add_net "Net-(C120-Pad2)")
    (add_net "Net-(C121-Pad2)")
    (add_net "Net-(L101-Pad2)")
    (add_net "Net-(L102-Pad1)")
    (add_net "Net-(L102-Pad2)")
    (add_net "Net-(L103-Pad1)")
    (add_net "Net-(L103-Pad2)")
    (add_net "Net-(P102-Pad1)")
    (add_net "Net-(P103-Pad1)")
    (add_net "Net-(P108-Pad1)")
    (add_net "Net-(R105-Pad2)")
    (add_net "Net-(R107-Pad2)")
    (add_net "Net-(R108-Pad2)")
    (add_net "Net-(T101-Pad2)")
    (add_net "Net-(U101-Pad1)")
    (add_net "Net-(U102-Pad1)")
  )
  (net_class 50ohm ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C109-Pad2)")
    (add_net "Net-(J102-Pad1)")
    (add_net "Net-(P106-Pad1)")
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 178.054 102.108)
    (fp_text reference REF**15135 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 176.784 102.108)
    (fp_text reference REF**15125 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 175.514 102.108)
    (fp_text reference REF**15115 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 178.054 100.838)
    (fp_text reference REF**15134 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 176.784 100.838)
    (fp_text reference REF**15124 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 175.514 100.838)
    (fp_text reference REF**15114 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 178.054 99.568)
    (fp_text reference REF**15133 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 176.784 99.568)
    (fp_text reference REF**15123 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 175.514 99.568)
    (fp_text reference REF**15113 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 178.054 98.298)
    (fp_text reference REF**15132 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 176.784 98.298)
    (fp_text reference REF**15122 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 175.514 98.298)
    (fp_text reference REF**15112 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 178.054 97.028)
    (fp_text reference REF**15131 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 176.784 97.028)
    (fp_text reference REF**15121 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FAA66)
    (at 175.514 97.028)
    (fp_text reference REF**15111 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 5 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 181.102 93.726)
    (fp_text reference REF**154 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 167.894 79.502)
    (fp_text reference REF**153 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 165.354 79.502)
    (fp_text reference REF**143 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 162.814 79.502)
    (fp_text reference REF**133 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 160.274 79.502)
    (fp_text reference REF**123 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 180.848 79.502)
    (fp_text reference REF**152 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 178.308 79.502)
    (fp_text reference REF**142 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 175.768 79.502)
    (fp_text reference REF**132 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 173.228 79.502)
    (fp_text reference REF**122 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 170.688 79.502)
    (fp_text reference REF**112 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 151.13 102.108)
    (fp_text reference REF**151 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 148.59 102.108)
    (fp_text reference REF**141 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 146.05 102.108)
    (fp_text reference REF**131 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 143.51 102.108)
    (fp_text reference REF**121 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAB54)
    (at 146.6215 84.074 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C101 (at 0.8255 -1.016 180) (layer F.SilkS))
    (fp_text value 0.01uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAB59)
    (at 150.3045 84.074 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C102 (at 2.4765 -1.016 180) (layer F.SilkS))
    (fp_text value 330pf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 162.052 101.092 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAB36)
    (at 151.257 85.598)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at -3.429 2.032) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAC29)
    (at 150.114 90.6145)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at -3.048 0.5715) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAB3B)
    (at 151.257 87.122)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C106 (at -3.429 1.27) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C106-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAC3B)
    (at 150.114 98.552)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C107 (at -2.794 0.762) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAB41)
    (at 151.257 88.646)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C108 (at -3.429 0.508) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C108-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA1A2)
    (at 155.321 81.407 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C109 (at -1.905 -1.651 360) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C109-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAC66)
    (at 154.6225 91.567 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C110 (at -0.127 -1.9685 90) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C110-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAC69)
    (at 156.21 91.567 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C111 (at -0.127 -2.794 90) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C111-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 587EA949)
    (at 169.164 101.854 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C112 (at 3.302 -0.762 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAC53)
    (at 157.988 91.567 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C113 (at 0.889 1.016 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA190)
    (at 161.4805 84.2645 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C114 (at 0.1905 1.2065 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 587EA950)
    (at 169.164 99.568 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C115 (at 3.302 -0.762 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA1B8)
    (at 167.386 89.027 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C116 (at 0 1.143 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C116-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C116-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA1BC)
    (at 167.3225 91.2495 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C117 (at -0.0635 -1.2065 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C117-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA186)
    (at 161.4805 85.7885 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C118 (at -0.0635 -1.0795 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C118-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA932)
    (at 164.084 85.6615 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C119 (at -4.6355 0.762 270) (layer F.SilkS))
    (fp_text value 330pf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C119-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587FA93A)
    (at 164.9095 82.7405)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C120 (at -0.0635 -1.2065) (layer F.SilkS))
    (fp_text value 6800pf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C120-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587EAA26)
    (at 167.259 85.6615 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C121 (at -3.6195 -0.127 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C121-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 587EA985)
    (at 148.463 81.534 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D101 (at 0 2.159 270) (layer F.SilkS))
    (fp_text value BAV99 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAAF6)
    (at 152.4635 82.4865)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L101 (at -1.3335 -0.9525) (layer F.SilkS))
    (fp_text value 8.2nH (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(L101-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAA66)
    (at 158.115 80.772 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L102 (at -2.921 0.254 180) (layer F.SilkS))
    (fp_text value 150nh (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(L102-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(L102-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587FA195)
    (at 158.115 82.423 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L103 (at -2.921 0.381 180) (layer F.SilkS))
    (fp_text value 150nh (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(L103-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(L103-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 587EA96C)
    (at 140.97 91.7575)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P101 (at 2.286 -1.3335) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SCL))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SDA))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 587EAB50)
    (at 147.32 86.36)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P102 (at -1.524 0.254 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 30 "Net-(P102-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 587EAA88)
    (at 159.893 93.091)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P103 (at 1.905 0.889) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 31 "Net-(P103-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 58613369)
    (at 170.942 86.868)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P104 (at 0 -1.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 14 "Net-(C116-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 587EAA05)
    (at 170.942 93.218)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P105 (at 0 1.524) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 16 "Net-(C117-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 58613369)
    (at 173.482 86.868)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P106 (at 0 -1.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 32 "Net-(P106-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 587EAA09)
    (at 173.482 93.218)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P107 (at 0 1.524) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:PINTST (layer F.Cu) (tedit 58613369)
    (at 168.8465 82.3595)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P108 (at 0 -1.6) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 1.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.143 1.143) (drill 0.635) (layers *.Cu *.Mask)
      (net 33 "Net-(P108-Pad1)"))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAC2E)
    (at 149.987 92.202 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 2.921 -0.762 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /SCL))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EABA5)
    (at 149.987 97.028 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 2.921 -0.762 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAC33)
    (at 149.987 93.853)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at -2.921 0.635) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAB8E)
    (at 149.987 95.4405)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at -2.921 0.8255) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EA907)
    (at 154.432 101.346 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at -0.254 1.27 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C110-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R105-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAAEB)
    (at 152.4635 80.3275)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 0.4445 -1.3335) (layer F.SilkS))
    (fp_text value 10 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C109-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587FA17E)
    (at 161.6075 89.154 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R107 (at 0.0635 1.27 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C116-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R107-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587FA18A)
    (at 161.544 91.059 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R108 (at -0.508 -1.143 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C117-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R108-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EA9EE)
    (at 164.592 90.1065 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R109 (at 2.8575 0 270) (layer F.SilkS))
    (fp_text value DNI (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C116-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C117-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587FA937)
    (at 165.6715 85.5345 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R110 (at -4.5085 -0.9525 270) (layer F.SilkS))
    (fp_text value 1k8 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C120-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C119-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EA9D4)
    (at 175.7045 87.4395 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R111 (at 2.9845 0.4445 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J102-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P106-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587EAA1F)
    (at 168.8465 85.5345 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R112 (at -1.7145 -1.3335 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P108-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C121-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pulse_SMD_Balun (layer F.Cu) (tedit 587EAA13)
    (at 172.0215 90.1065 270)
    (fp_text reference T101 (at 2.8575 2.6035 270) (layer F.SilkS))
    (fp_text value TRANSFO4 (at 0 -0.5 270) (layer F.Fab))
    (pad 5 smd rect (at -1.27 -1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P106-Pad1)"))
    (pad 4 smd rect (at 1.27 -1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.27 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C116-Pad1)"))
    (pad 3 smd rect (at 1.27 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C117-Pad1)"))
    (pad 2 smd rect (at 0 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(T101-Pad2)"))
  )
  (module Crystals:Crystal_SMD_Abracon_ABM3C-4pin_5.0x3.2mm (layer F.Cu) (tedit 587EA91D)
    (at 158.242 101.346 180)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3C http://www.abracon.com/Resonators/abm3c.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference U101 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value TCXO (at 0 2.8 180) (layer F.Fab))
    (pad 1 smd rect (at -1.9 1.15 180) (size 1.6 1.3) (layers F.Cu F.Mask)
      (net 38 "Net-(U101-Pad1)"))
    (pad 2 smd rect (at 1.9 1.15 180) (size 1.6 1.3) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 1.9 -1.15 180) (size 1.6 1.3) (layers F.Cu F.Mask)
      (net 34 "Net-(R105-Pad2)"))
    (pad 4 smd rect (at -1.9 -1.15 180) (size 1.6 1.3) (layers F.Cu F.Mask)
      (net 5 +3V3))
    (model Crystals.3dshapes/Crystal_SMD_Abracon_ABM3C-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-223 (layer F.Cu) (tedit 587FAAAC)
    (at 176.8475 99.5045)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U103 (at 3.2385 -2.9845) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 4.5) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (zone_connect 2))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 587EA8FC)
    (at 159.004 96.774)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y101 (at 6.858 -1.778) (layer F.SilkS))
    (fp_text value 28.8MHz (at 0 3.55) (layer F.Fab))
    (pad 1 smd rect (at -4.25 0) (size 4.5 2) (layers F.Cu F.Mask)
      (net 11 "Net-(C110-Pad2)"))
    (pad 2 smd rect (at 4.25 0) (size 4.5 2) (layers F.Cu F.Mask)
      (net 12 "Net-(C111-Pad2)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA58B)
    (at 140.462 102.108)
    (fp_text reference REF** (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 587FA5EA)
    (at 140.97 102.108)
    (fp_text reference REF**111 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 4 GND) (zone_connect 2))
  )
  (module footprints:SMA_END (layer F.Cu) (tedit 58894D7D)
    (at 179.324 86.36)
    (fp_text reference J102 (at -3.81 -4.826) (layer F.SilkS))
    (fp_text value SMA (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 0 0) (size 5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J102-Pad1)"))
  )
  (module footprints:SMA_END (layer F.Cu) (tedit 58894D7D)
    (at 141.986 84.1375)
    (fp_text reference J101 (at -3.81 -4.826) (layer F.SilkS))
    (fp_text value SMA (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 0 0) (size 5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad2)"))
  )
  (module footprints:QFN-24-1EP_4x4mm_Pitch0.5mm_extended_pad (layer F.Cu) (tedit 5889512A)
    (at 156.310214 86.542)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U102 (at -2.894214 -2.722) (layer F.SilkS))
    (fp_text value R820T2 (at 0 3.375) (layer F.Fab))
    (pad 1 smd rect (at -2.05 -1.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U102-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -2.05 -0.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P102-Pad1)"))
    (pad 4 smd rect (at -2.05 0.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C106-Pad2)"))
    (pad 5 smd rect (at -2.05 0.75) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C108-Pad2)"))
    (pad 6 smd rect (at -2.05 1.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (pad 7 smd rect (at -1.25 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (pad 8 smd rect (at -0.75 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C110-Pad2)"))
    (pad 9 smd rect (at -0.25 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C111-Pad2)"))
    (pad 10 smd rect (at 0.25 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P103-Pad1)"))
    (pad 11 smd rect (at 0.75 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 12 smd rect (at 1.25 2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R108-Pad2)"))
    (pad 13 smd rect (at 2.05 1.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R107-Pad2)"))
    (pad 14 smd rect (at 2.05 0.75) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C121-Pad2)"))
    (pad 15 smd rect (at 2.05 0.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C119-Pad2)"))
    (pad 16 smd rect (at 2.05 -0.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 17 smd rect (at 2.05 -0.75) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C118-Pad2)"))
    (pad 18 smd rect (at 2.05 -1.25) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 19 smd rect (at 1.25 -2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(L103-Pad1)"))
    (pad 20 smd rect (at 0.75 -2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(L102-Pad1)"))
    (pad 21 smd rect (at 0.25 -2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(L103-Pad2)"))
    (pad 22 smd rect (at -0.25 -2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(L102-Pad2)"))
    (pad 23 smd rect (at -0.75 -2.05 90) (size 1 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C109-Pad2)"))
    (pad 24 smd rect (at -1.25 -2.05 90) (size 1.05 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(L101-Pad2)"))
    (pad 25 smd rect (at 0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "R820T2 Breakout v0.1\n(c) 2017 E. Brombaugh" (at 161.798 96.774) (layer B.SilkS))
  (gr_text IF (at 174.244 83.058) (layer F.SilkS))
  (gr_text RF (at 145.796 89.154) (layer F.SilkS))
  (gr_text GND (at 144.018 99.314) (layer F.SilkS))
  (gr_text SDA (at 144.018 96.774) (layer F.SilkS))
  (gr_text SCL (at 144.018 94.234) (layer F.SilkS))
  (gr_text +5V (at 144.018 91.694) (layer F.SilkS))
  (dimension 43.434 (width 0.3) (layer Dwgs.User)
    (gr_text "1.7100 in" (at 160.655 69.77) (layer Dwgs.User))
    (feature1 (pts (xy 182.372 78.232) (xy 182.372 68.42)))
    (feature2 (pts (xy 138.938 78.232) (xy 138.938 68.42)))
    (crossbar (pts (xy 138.938 71.12) (xy 182.372 71.12)))
    (arrow1a (pts (xy 182.372 71.12) (xy 181.245496 71.706421)))
    (arrow1b (pts (xy 182.372 71.12) (xy 181.245496 70.533579)))
    (arrow2a (pts (xy 138.938 71.12) (xy 140.064504 71.706421)))
    (arrow2b (pts (xy 138.938 71.12) (xy 140.064504 70.533579)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 188.04 90.932 270) (layer Dwgs.User))
    (feature1 (pts (xy 182.372 103.632) (xy 189.39 103.632)))
    (feature2 (pts (xy 182.372 78.232) (xy 189.39 78.232)))
    (crossbar (pts (xy 186.69 78.232) (xy 186.69 103.632)))
    (arrow1a (pts (xy 186.69 103.632) (xy 186.103579 102.505496)))
    (arrow1b (pts (xy 186.69 103.632) (xy 187.276421 102.505496)))
    (arrow2a (pts (xy 186.69 78.232) (xy 186.103579 79.358504)))
    (arrow2b (pts (xy 186.69 78.232) (xy 187.276421 79.358504)))
  )
  (gr_line (start 138.938 103.632) (end 138.938 78.232) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 103.632) (end 138.938 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 78.232) (end 182.372 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.938 78.232) (end 182.372 78.232) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 181.864 103.124) (xy 139.446 103.124) (xy 139.446 78.74) (xy 181.864 78.74) (xy 181.864 103.124)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 181.864 103.124) (xy 139.446 103.124) (xy 139.446 78.74) (xy 181.864 78.74) (xy 181.864 103.124)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 181.864 103.124) (xy 139.446 103.124) (xy 139.446 78.74) (xy 181.864 78.74) (xy 181.864 103.124)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 181.864 103.124) (xy 172.72 103.124) (xy 172.72 96.012) (xy 181.864 96.012) (xy 181.864 103.124)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 181.864 95.504) (xy 172.212 95.504) (xy 172.212 103.124) (xy 139.446 103.124) (xy 139.446 78.74)
        (xy 181.864 78.74) (xy 181.864 95.504)
      )
    )
  )
)
