(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 83)
    (tracks 32)
    (zones 0)
    (modules 8)
    (nets 6)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.12)
    (pad_size 1 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 126.72865 115.8751)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /G)
  (net 3 /GND)
  (net 4 "Net-(J4-Pad1)")
  (net 5 "Net-(J3-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /G)
    (add_net /GND)
    (add_net /VCC)
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
  )
  (module symbol:center-pos (layer Top) (tedit 0)
    (at 137.77865 104.5751 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Jumpers:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm (layer Top) (tedit 5FC2EE33)
    (at 139.0969 116.1002 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value JUMPER-SMT_3_NO_NO-SILK (at 0 2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 90) (size 1 1.5) (layers Top F.Mask)
      (net 4 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 1 1.5) (layers Top F.Mask)
      (net 1 /VCC))
    (pad 3 smd rect (at 1.3 0 90) (size 1 1.5) (layers Top F.Mask)
      (net 1 /VCC))
  )
  (module phils-connectors:T35-2 (layer Top) (tedit 5FC2CE77)
    (at 173.9969 105.1502 90)
    (fp_text reference J5 (at -3.5 -3.5 90) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x02 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at -1.75 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /GND) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at 1.75 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /VCC) (solder_mask_margin 0.0635))
  )
  (module phils-connectors:T35-2 (layer Top) (tedit 5FC2CE77)
    (at 142.31615 95.7776 180)
    (fp_text reference J1 (at -3.5 -3.5) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x02 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at -1.75 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /G) (solder_mask_margin 0.0635))
    (pad 1 thru_hole rect (at 1.75 0 180) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /VCC) (solder_mask_margin 0.0635))
  )
  (module phils-connectors:LG-2-PIN (layer Top) (tedit 5FC2CE0C)
    (at 146.5469 104.1502 180)
    (fp_text reference J6 (at -2.54 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 3.81 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /G) (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 /GND) (solder_mask_margin 0.1016))
  )
  (module phils-connectors:1X03 (layer Top) (tedit 5FC2CB40)
    (at 146.4469 110.2002 180)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference J3 (at -3.8862 -1.8288) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at -3.81 3.175) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad3)") (solder_mask_margin 0.0635))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /VCC) (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /VCC) (solder_mask_margin 0.0635))
  )
  (module phils-connectors:1X02 (layer Top) (tedit 5FC2CAF4)
    (at 133.5969 114.8502)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference J4 (at -2.6162 -1.8288) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at -2.54 3.175 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad3)") (solder_mask_margin 0.0635))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-Pad1)") (solder_mask_margin 0.0635))
  )
  (module phils-connectors:DC_Conn_PJ-002A (layer Top) (tedit 5FC1C8AC)
    (at 121.5969 105.4502)
    (fp_text reference J2 (at 5 5.5) (layer F.SilkS) hide)
    (fp_text value Barrel_Jack (at 7 -3) (layer F.Fab))
    (pad 3 thru_hole oval (at 10.7 4.7) (size 3.8 1.8) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 2 /G))
    (pad 2 thru_hole oval (at 7.7 0) (size 1.8 3.8) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 2 /G))
    (pad 1 thru_hole oval (at 13.7 0) (size 1.8 4.4) (drill oval 1 3.5) (layers *.Cu *.Mask)
      (net 1 /VCC))
  )
  (gr_text "Copyright © 2020 PL Barrett" (at 164.8469 117.5002) (layer F.SilkS))
  (gr_text dflt (at 150.0969 117.5002) (layer F.SilkS))
  (gr_text pwr (at 150.0969 116.0002) (layer F.SilkS))
  (gr_text self (at 150.0969 114.8502) (layer F.SilkS))
  (gr_text cut (at 137.1469 114.6002 90) (layer F.SilkS))
  (gr_text - (at 134.8969 112.7002) (layer F.SilkS))
  (gr_text + (at 132.3469 112.7002) (layer F.SilkS))
  (gr_text "Ext Pwr" (at 133.5469 117.2502) (layer F.SilkS))
  (gr_text "Ext Pwr" (at 144.7969 116.9502) (layer F.SilkS))
  (gr_text "Self Pwr" (at 145.0969 115.4502) (layer F.SilkS))
  (gr_text BK (at 143.9469 112.2002) (layer F.SilkS))
  (gr_circle (center 138.7469 110.2002) (end 140.769275 110.2002) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152.8969 102.4502) (end 153.1969 102.4502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.4969 101.8502) (end 149.1969 101.8502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.8969 102.1502) (end 149.4969 102.1502) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.1969 95.5502) (end 149.1969 101.8502) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 149.4969 95.5502) (end 149.4969 95.2502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 153.4969 115.8502) (end 153.1969 115.8502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.1969 115.8502) (end 172.1969 116.1502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.4969 110.7502) (end 172.4969 115.8502) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.1969 95.5502) (end 172.4969 95.5502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.4969 99.5502) (end 172.4969 95.5502) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.1969 99.5502) (end 172.1969 99.8502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.2469 99.8502) (end 172.1969 99.8502) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 170.2469 100.1502) (end 170.2469 99.8502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 170.2469 110.1502) (end 169.9469 110.1502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.1969 110.7502) (end 172.4969 110.7502) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.2469 110.4502) (end 172.1969 110.4502) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.9469 100.1502) (end 169.9469 110.1502) (layer Edge.Cuts) (width 0.05))
  (gr_text Input (at 132.6469 99.6502) (layer F.SilkS))
  (gr_text RD (at 150.74 106.3182) (layer F.SilkS))
  (gr_text BK (at 142.9803 106.3563) (layer F.SilkS))
  (gr_text "Thick\nWire" (at 144.42865 105.9751) (layer F.SilkS))
  (gr_text YL (at 149.0469 112.23) (layer F.SilkS))
  (gr_text RD (at 146.4469 112.2002) (layer F.SilkS))
  (gr_text "Thin Wire" (at 146.0969 113.4502) (layer F.SilkS))
  (gr_text V+ (at 173.5397 100.1718 270) (layer F.SilkS))
  (gr_text Gnd (at 173.5397 110.1794 270) (layer F.SilkS))
  (gr_text Gnd (at 144.21615 100.03) (layer F.SilkS))
  (gr_text V+ (at 140.11615 100.03) (layer F.SilkS))
  (gr_text Output (at 176.1559 97.708 270) (layer F.SilkS))
  (gr_text Input (at 137.7511 96.6412 270) (layer F.SilkS))
  (gr_line (start 127.04615 116.0926) (end 129.45915 116.0926) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.04615 95.5866) (end 127.04615 95.2691) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.45915 95.5866) (end 129.77665 95.5866) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.6323 118.79) (end 177.51615 118.79) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.51615 118.79) (end 177.51615 92.13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.51615 92.13) (end 124.6323 92.13) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.6323 92.13) (end 124.6323 118.79) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.45915 95.2691) (end 127.04615 95.2691) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.72865 95.5866) (end 126.72865 99.5375) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.72865 111.9313) (end 126.72865 115.7751) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.45915 99.8561) (end 127.04615 99.855) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.04615 111.6138) (end 129.45915 111.6149) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.04615 99.5375) (end 126.72865 99.5375) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.04615 115.7751) (end 126.72865 115.7751) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.04615 111.9313) (end 127.04615 111.6138) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.45915 115.7751) (end 129.77665 115.7751) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.77665 95.5866) (end 129.77665 99.5386) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.45915 99.5386) (end 129.77665 99.5386) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.77665 115.7751) (end 129.77665 111.9324) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 129.45915 111.9324) (end 129.77665 111.9324) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.1969 102.4502) (end 153.1969 115.8502) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.1969 95.2502) (end 149.4969 95.2502) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.1969 116.1502) (end 153.4969 116.1502) (layer Edge.Cuts) (width 0.05))
  (gr_text "Volt/Ammeter 2.51" (at 163.51615 94.43) (layer F.SilkS))
  (zone (net 3) (net_name /GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 179.01615 119.03) (xy 148.0469 119.2502) (xy 148.0469 105.6002) (xy 146.8969 105.6002) (xy 146.881525 102.7502)
        (xy 148.109841 102.750201) (xy 148.08396 90.900198) (xy 179.01615 90.83)
      )
    )
  )
  (zone (net 3) (net_name /GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 179.00185 118.9932) (xy 148.0469 119.2002) (xy 148.0469 105.6002) (xy 146.8969 105.6002) (xy 146.881525 102.7502)
        (xy 148.079588 102.785225) (xy 148.0969 90.9002) (xy 179.00185 90.9643)
      )
    )
  )
  (zone (net 2) (net_name /G) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 146.9969 101.88087) (xy 145.71615 101.88087) (xy 145.706525 106.4502) (xy 146.987275 106.4502) (xy 146.9469 119.23087)
        (xy 121.53435 118.97387) (xy 121.53435 89.99247) (xy 146.9969 90.23087)
      )
    )
  )
  (zone (net 2) (net_name /G) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 146.996902 101.9002) (xy 145.689177 101.9002) (xy 145.6969 106.4502) (xy 146.9969 106.4502) (xy 146.9469 119.0002)
        (xy 121.45815 118.9562) (xy 121.45815 90.6098) (xy 147.060388 90.5586)
      )
    )
  )
)
