(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 168)
    (zones 0)
    (modules 28)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 209.9 95.25)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "outputs/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /CO_11)
  (net 3 /CI_11)
  (net 4 /CO_10)
  (net 5 /CI_10)
  (net 6 /CO_9)
  (net 7 /CI_9)
  (net 8 /CO_8)
  (net 9 /CI_8)
  (net 10 /CO_7)
  (net 11 /CI_7)
  (net 12 /CO_6)
  (net 13 /CI_6)
  (net 14 /CO_5)
  (net 15 /CI_5)
  (net 16 /CO_4)
  (net 17 /CI_4)
  (net 18 /CO_3)
  (net 19 /CI_3)
  (net 20 /CO_2)
  (net 21 /CI_2)
  (net 22 /CO_1)
  (net 23 /CI_1)
  (net 24 /CO_0)
  (net 25 /CI_0)
  (net 26 "Net-(SW1-Pad3)")
  (net 27 "Net-(SW2-Pad3)")
  (net 28 "Net-(SW3-Pad3)")
  (net 29 "Net-(SW4-Pad3)")
  (net 30 "Net-(SW5-Pad3)")
  (net 31 "Net-(SW6-Pad3)")
  (net 32 "Net-(SW7-Pad3)")
  (net 33 "Net-(SW8-Pad3)")
  (net 34 "Net-(SW9-Pad3)")
  (net 35 "Net-(SW10-Pad3)")
  (net 36 "Net-(SW11-Pad3)")
  (net 37 "Net-(SW12-Pad3)")
  (net 38 /CLK_50)
  (net 39 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CI_0)
    (add_net /CI_1)
    (add_net /CI_10)
    (add_net /CI_11)
    (add_net /CI_2)
    (add_net /CI_3)
    (add_net /CI_4)
    (add_net /CI_5)
    (add_net /CI_6)
    (add_net /CI_7)
    (add_net /CI_8)
    (add_net /CI_9)
    (add_net /CLK_50)
    (add_net /CO_0)
    (add_net /CO_1)
    (add_net /CO_10)
    (add_net /CO_11)
    (add_net /CO_2)
    (add_net /CO_3)
    (add_net /CO_4)
    (add_net /CO_5)
    (add_net /CO_6)
    (add_net /CO_7)
    (add_net /CO_8)
    (add_net /CO_9)
    (add_net GND)
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(SW10-Pad3)")
    (add_net "Net-(SW11-Pad3)")
    (add_net "Net-(SW12-Pad3)")
    (add_net "Net-(SW2-Pad3)")
    (add_net "Net-(SW3-Pad3)")
    (add_net "Net-(SW4-Pad3)")
    (add_net "Net-(SW5-Pad3)")
    (add_net "Net-(SW6-Pad3)")
    (add_net "Net-(SW7-Pad3)")
    (add_net "Net-(SW8-Pad3)")
    (add_net "Net-(SW9-Pad3)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 184.9 83.25 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 165.9 83.25 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 179.9 95.25)
    (fp_text reference SW8 (at 0.14 12.33) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(SW8-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 /CO_7))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 /CI_7))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 172.4 95.25)
    (fp_text reference SW7 (at -0.295 12.33) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(SW7-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 /CO_6))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 /CI_6))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 134.9 95.25)
    (fp_text reference SW2 (at 0.34 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(SW2-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 /CO_1))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 23 /CI_1))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 127.4 95.25)
    (fp_text reference SW1 (at -0.095 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(SW1-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 24 /CO_0))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 /CI_0))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 209.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 /CI_11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 202.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 /CI_10))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 194.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /CI_9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 187.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 /CI_8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 179.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 /CI_7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 172.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 /CI_6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 164.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 /CI_5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 157.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 /CI_4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 /CI_3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 /CI_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 134.9 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 /CI_1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127.4 110.25 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 4.6K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 /CI_0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x14_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.4 85.25 90)
    (descr "Through hole straight pin header, 2x14, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x14 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x14_Odd_Even (at 1.27 35.35 90) (layer F.Fab))
    (fp_text user %R (at 1.27 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 +3V3))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /CLK_50))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /CO_11))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /CI_11))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /CO_10))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /CI_10))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CO_9))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CI_9))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /CO_8))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /CI_8))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /CO_7))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /CI_7))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CO_6))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /CI_6))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /CO_5))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CI_5))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /CO_4))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CI_4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CO_3))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /CI_3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /CO_2))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CI_2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /CO_1))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /CI_1))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /CO_0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /CI_0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:4-SMD (layer F.Cu) (tedit 5E4476EF)
    (at 179.15 84.75 270)
    (fp_text reference U1 (at 0 4.4 90) (layer F.SilkS))
    (fp_text value FN5000145 (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 2.54 2.2) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 38 /CLK_50))
    (pad 4 smd rect (at -2.54 2.2) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (pad 2 smd rect (at 2.54 -2.2) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.54 -2.2) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 209.9 95.25)
    (fp_text reference SW12 (at 0.105 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(SW12-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 /CO_11))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 /CI_11))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 202.4 95.25)
    (fp_text reference SW11 (at 0.175 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(SW11-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 /CO_10))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 /CI_10))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 194.9 95.25)
    (fp_text reference SW10 (at -0.26 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(SW10-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 /CO_9))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 /CI_9))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 187.4 95.25)
    (fp_text reference SW9 (at -0.06 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(SW9-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 /CO_8))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 /CI_8))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 164.9 95.25)
    (fp_text reference SW6 (at -0.06 12.33) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(SW6-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 14 /CO_5))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 15 /CI_5))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 157.4 95.25)
    (fp_text reference SW5 (at -0.095 12.33) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(SW5-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 16 /CO_4))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 17 /CI_4))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 149.9 95.25)
    (fp_text reference SW4 (at 0.105 12.33) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(SW4-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 /CO_3))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 19 /CI_3))
  )
  (module custom:CYLEWET_SPDT (layer F.Cu) (tedit 5E3EF204)
    (at 142.4 95.25)
    (fp_text reference SW3 (at 0.14 12.18) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -2.5) (layer F.Fab))
    (pad 3 thru_hole roundrect (at 0 9.4) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(SW3-Pad3)"))
    (pad 2 thru_hole roundrect (at 0 4.7) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 /CO_2))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.75 2.25) (drill oval 1.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 /CI_2))
  )
  (gr_line (start 122.9 80.25) (end 122.9 114.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.9 114.25) (end 122.9 114.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.9 80.25) (end 214.9 114.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 122.9 80.25) (end 214.9 80.25) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.9 80.25) (xy 122.9 114.25) (xy 214.9 114.25) (xy 214.9 80.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.9 80.25) (xy 122.9 114.25) (xy 214.9 114.25) (xy 214.9 80.25)
      )
    )
  )
)
