(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 171)
    (zones 0)
    (modules 12)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.000686)
    (uvia_drill 0.00033)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDREF)
  (net 2 "Net-(D1-Pad2)")
  (net 3 +5V)
  (net 4 +9V)
  (net 5 "Net-(RN1-Pad9)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(SW2-Pad5)")
  (net 10 "Net-(SW2-Pad6)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad6)")
  (net 13 "Net-(J1-Pad10)")
  (net 14 "Net-(J1-Pad12)")
  (net 15 "Net-(J1-Pad14)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(SW3-Pad2)")
  (net 18 "Net-(CON1-Pad3)")
  (net 19 "Net-(CON1-Pad2)")
  (net 20 "Net-(RN1-Pad10)")
  (net 21 "Net-(RN1-Pad11)")
  (net 22 "Net-(RN1-Pad12)")
  (net 23 "Net-(RN1-Pad13)")
  (net 24 "Net-(RN1-Pad14)")
  (net 25 "Net-(RN1-Pad15)")
  (net 26 "Net-(RN1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.000686)
    (uvia_drill 0.00033)
    (add_net +5V)
    (add_net +9V)
    (add_net GNDREF)
    (add_net "Net-(CON1-Pad2)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(RN1-Pad10)")
    (add_net "Net-(RN1-Pad11)")
    (add_net "Net-(RN1-Pad12)")
    (add_net "Net-(RN1-Pad13)")
    (add_net "Net-(RN1-Pad14)")
    (add_net "Net-(RN1-Pad15)")
    (add_net "Net-(RN1-Pad16)")
    (add_net "Net-(RN1-Pad9)")
    (add_net "Net-(SW2-Pad5)")
    (add_net "Net-(SW2-Pad6)")
    (add_net "Net-(SW3-Pad2)")
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 77 68.2 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.92) (layer F.SilkS))
    (fp_text value 110 (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.68 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 112.7 71.7 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U3 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value LM1084-5.0 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +9V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_THT_DPDT_Straight (layer F.Cu) (tedit 611ED4F0)
    (at 113.2 79.1 270)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (fp_text reference SW2 (at 2.3 6.8 90) (layer F.SilkS))
    (fp_text value SW_Push_DPDT (at 5.1 7.2 90) (layer F.Fab))
    (fp_text user %R (at 2.9 2.4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.7 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole circle (at 9.4 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 4 thru_hole circle (at 0 4.83 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 4.7 4.83 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(SW2-Pad5)"))
    (pad 6 thru_hole circle (at 9.4 4.83 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(SW2-Pad6)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_CuK_JS202011CQN_DPDT_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sensor_Audio:DIP-16_692_ELL (layer F.Cu) (tedit 0)
    (at 65.1 84.6 180)
    (fp_text reference U2 (at -11.14 0 90) (layer F.SilkS))
    (fp_text value DFPlayer (at 0.7 0.7) (layer F.Fab))
    (pad 16 thru_hole oval (at -8.89 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -8.89 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 15 thru_hole oval (at -6.35 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -6.35 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -3.81 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -3.81 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at -1.27 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -1.27 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 1.27 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 1.27 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 3.81 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(SW3-Pad2)"))
    (pad 6 thru_hole oval (at 3.81 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(CON1-Pad2)"))
    (pad 10 thru_hole oval (at 6.35 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 7 thru_hole oval (at 6.35 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 9 thru_hole oval (at 8.89 -8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 8.89 8.8 180) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(CON1-Pad3)"))
  )
  (module LED_THT:LED_D3.0mm_Clear (layer F.Cu) (tedit 5A6C9BC0)
    (at 73.2 60.4)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (fp_text reference D1 (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (fp_text user %R (at 1.47 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 102.6 84.9 270)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value 74LS688 (at 3.81 25.19 90) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 11 thru_hole oval (at 7.62 22.86 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(RN1-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(RN1-Pad16)"))
    (pad 12 thru_hole oval (at 7.62 20.32 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(RN1-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(RN1-Pad15)"))
    (pad 14 thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 15 thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(RN1-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RN1-Pad14)"))
    (pad 16 thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad6)"))
    (pad 17 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RN1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(RN1-Pad13)"))
    (pad 18 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 19 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(SW2-Pad5)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 20 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1405)
    (at 82.4 60.4)
    (descr "8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference SW1 (at 3.81 -3.42) (layer F.SilkS))
    (fp_text value SW_DIP_x08 (at 3.81 21.2) (layer F.Fab))
    (fp_text user %R (at 7.27 8.89 90) (layer F.Fab))
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RN1-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(RN1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(RN1-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(RN1-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(RN1-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RN1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(RN1-Pad15)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(RN1-Pad16)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TerminalBlock_Altech:Altech_AK300_1x16_P5.00mm_45-Degree (layer F.Cu) (tedit 5C27907F)
    (at 57.5 102.5)
    (descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
    (tags "Altech AK300 serie connector")
    (fp_text reference J1 (at 0 -7.2) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x16 (at 37.5 7.5) (layer F.Fab))
    (fp_text user %R (at 37.5 0.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 2 thru_hole circle (at 5 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 10 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 4 thru_hole circle (at 15 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 20 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 6 thru_hole circle (at 25 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 30 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 8 thru_hole circle (at 35 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 40 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 10 thru_hole circle (at 45 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 50 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 12 thru_hole circle (at 55 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at 60 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 14 thru_hole circle (at 65 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 70 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 16 thru_hole circle (at 75 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x16_P5.00mm_45-Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWire-0.75sqmm_1x02_P7mm_D1.25mm_OD3.5mm_Relief (layer F.Cu) (tedit 5EB70B44)
    (at 132.6 79.3 180)
    (descr "Soldered wire connection with feed through strain relief, for 2 times 0.75 mm² wires, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm strain-relief")
    (attr virtual)
    (fp_text reference J4 (at 3.5 -2.95 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 3.5 24.2 180) (layer F.Fab))
    (fp_text user %R (at 3.5 10.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142900000000001)
      (net 4 +9V))
    (pad 2 thru_hole circle (at 7 0 180) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad "" np_thru_hole circle (at 0 21 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7 21 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x02_P7mm_D1.25mm_OD3.5mm_Relief.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Term_Block_1x2_P5mm (layer F.Cu) (tedit 5D4199AF)
    (at 131.1 92 90)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx0162.pdf)
    (fp_text reference SW3 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value SW_Push (at 2.05 5.05 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(SW2-Pad6)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(SW3-Pad2)"))
  )
  (module digikey-footprints:Headphone_Jack_3.5mm_SJ1-3523N (layer F.Cu) (tedit 5C87D9A9)
    (at 67.2 64.4)
    (descr http://www.cui.com/product/resource/sj1-352xn-series.pdf)
    (fp_text reference CON1 (at -4.5 -7) (layer F.SilkS))
    (fp_text value SJ1-3523N (at -4.25 7.5) (layer F.Fab))
    (fp_text user %R (at -8.25 0) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 -5) (size 2.5 1.8) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(CON1-Pad3)"))
    (pad 2 thru_hole rect (at 0 5) (size 2.5 1.8) (drill oval 1.5 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(CON1-Pad2)"))
    (pad 1 thru_hole rect (at -5 0) (size 1.8 2.5) (drill oval 0.8 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5 -5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.5 -5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5 5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.5 5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-16_W7.62mm_LongPads (layer B.Cu) (tedit 5A02E8C5)
    (at 102.4 60.4 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference RN1 (at 3.81 2.33) (layer B.SilkS))
    (fp_text value R_Pack08 (at 3.81 -20.11) (layer B.Fab))
    (fp_text user %R (at 3.81 -8.89) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 9 thru_hole oval (at 7.62 -17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RN1-Pad9)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 10 thru_hole oval (at 7.62 -15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(RN1-Pad10)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 11 thru_hole oval (at 7.62 -12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(RN1-Pad11)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 12 thru_hole oval (at 7.62 -10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(RN1-Pad12)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 13 thru_hole oval (at 7.62 -7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(RN1-Pad13)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 14 thru_hole oval (at 7.62 -5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(RN1-Pad14)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 15 thru_hole oval (at 7.62 -2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(RN1-Pad15)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(RN1-Pad16)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "PUSH SWITCH" (at 124.9 89.5 90) (layer F.SilkS))
  (gr_text 8 (at 130.2 110.6) (layer F.SilkS))
  (gr_text 7 (at 120.1 110.6) (layer F.SilkS))
  (gr_text 6 (at 109.8 110.6) (layer F.SilkS))
  (gr_text 5 (at 100.1 110.6) (layer F.SilkS))
  (gr_text 4 (at 89.9 110.6) (layer F.SilkS))
  (gr_text 3 (at 80.2 110.6) (layer F.SilkS))
  (gr_text 2 (at 70.4 110.6) (layer F.SilkS))
  (gr_text 1 (at 60.6 110.6) (layer F.SilkS))
  (gr_text DISARM (at 118.8 79.1) (layer F.SilkS))
  (gr_text ARM (at 118.3 88.5) (layer F.SilkS))
  (gr_text ARMED (at 74.4 55.4) (layer F.SilkS))
  (gr_line (start 51.3 53.7) (end 51.3 54.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.3 53.7) (end 51.3 53.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.3 112.1) (end 137.3 53.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 51.3 112.1) (end 137.3 112.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 51.3 54.3) (end 51.3 112.1) (layer Edge.Cuts) (width 0.05))
)
