(kicad_pcb (version 4) (host pcbnew 4.0.2-2.fc24-product)
  (general
    (links 54)
    (no_connects 26)
    (area 124.409999 74.244999 170.230001 121.335001)
    (thickness 1.6)
    (drawings 38)
    (tracks 159)
    (zones 0)
    (modules 7)
    (nets 48)
  )
  (page A4)
  (title_block
    (title "Tektronix 155-0236-00 (U400) breakout module")
    (date 2016-08-09)
    (rev A)
    (company "(2016) Designed by Alexandru Gagniuc")
    (comment 1 "Bottom board: Breakout signals from ribbon cable")
    (comment 2 "Top board: Breakout Tek hybrid to ribbon cable")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad13)")
  (net 2 "Net-(P1-Pad12)")
  (net 3 "Net-(P1-Pad11)")
  (net 4 "Net-(P1-Pad10)")
  (net 5 "Net-(P1-Pad9)")
  (net 6 "Net-(P1-Pad8)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 "Net-(P1-Pad6)")
  (net 9 "Net-(P1-Pad5)")
  (net 10 "Net-(P1-Pad4)")
  (net 11 "Net-(P1-Pad3)")
  (net 12 "Net-(P1-Pad2)")
  (net 13 "Net-(P1-Pad1)")
  (net 14 "Net-(P1-Pad26)")
  (net 15 "Net-(P1-Pad25)")
  (net 16 "Net-(P1-Pad24)")
  (net 17 "Net-(P1-Pad23)")
  (net 18 "Net-(P1-Pad22)")
  (net 19 "Net-(P1-Pad21)")
  (net 20 "Net-(P1-Pad20)")
  (net 21 "Net-(P1-Pad19)")
  (net 22 "Net-(P1-Pad18)")
  (net 23 "Net-(P1-Pad17)")
  (net 24 "Net-(P1-Pad16)")
  (net 25 "Net-(P1-Pad15)")
  (net 26 "Net-(P1-Pad14)")
  (net 27 /I_BIAS)
  (net 28 VEE)
  (net 29 /CH_5-)
  (net 30 /~VS2)
  (net 31 /OUT-)
  (net 32 /~VS1)
  (net 33 GND)
  (net 34 /CH_1+)
  (net 35 /CH_4-)
  (net 36 /CH_4+)
  (net 37 /CH_1-)
  (net 38 /CH_3-)
  (net 39 /CH_2+)
  (net 40 /CH_3+)
  (net 41 /CH_2-)
  (net 42 /OUT+)
  (net 43 /HF_ADJ)
  (net 44 /CH_5+)
  (net 45 VCC)
  (net 46 /~VS3)
  (net 47 /~VS4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CH_1+)
    (add_net /CH_1-)
    (add_net /CH_2+)
    (add_net /CH_2-)
    (add_net /CH_3+)
    (add_net /CH_3-)
    (add_net /CH_4+)
    (add_net /CH_4-)
    (add_net /CH_5+)
    (add_net /CH_5-)
    (add_net /HF_ADJ)
    (add_net /I_BIAS)
    (add_net /OUT+)
    (add_net /OUT-)
    (add_net /~VS1)
    (add_net /~VS2)
    (add_net /~VS3)
    (add_net /~VS4)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
    (add_net VEE)
  )
  (module Connect:IDC_Header_Straight_26pins (layer F.Cu) (tedit 0)
    (at 162.56 82.55 180)
    (descr "26 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P2 (at 15.24 -7.62 180) (layer F.SilkS))
    (fp_text value CONN_02X13 (at 15.24 5.223 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad26)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad2)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P1-Pad25)"))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad3)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P1-Pad24)"))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P1-Pad23)"))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad5)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P1-Pad22)"))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad6)"))
    (pad 12 thru_hole oval (at 12.7 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad21)"))
    (pad 13 thru_hole oval (at 15.24 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad7)"))
    (pad 14 thru_hole oval (at 15.24 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P1-Pad20)"))
    (pad 15 thru_hole oval (at 17.78 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad8)"))
    (pad 16 thru_hole oval (at 17.78 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P1-Pad19)"))
    (pad 17 thru_hole oval (at 20.32 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad9)"))
    (pad 18 thru_hole oval (at 20.32 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 22.86 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad10)"))
    (pad 20 thru_hole oval (at 22.86 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P1-Pad17)"))
    (pad 21 thru_hole oval (at 25.4 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad11)"))
    (pad 22 thru_hole oval (at 25.4 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P1-Pad16)"))
    (pad 23 thru_hole oval (at 27.94 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad12)"))
    (pad 24 thru_hole oval (at 27.94 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P1-Pad15)"))
    (pad 25 thru_hole oval (at 30.48 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad13)"))
    (pad 26 thru_hole oval (at 30.48 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P1-Pad14)"))
  )
  (module Connect:IDC_Header_Straight_26pins (layer F.Cu) (tedit 57A944AD)
    (at 162.56 100.965 180)
    (descr "26 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P3 (at -6.35 0 180) (layer F.SilkS))
    (fp_text value DIL_26_PINS (at 15.24 5.223 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /I_BIAS))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 VEE))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /CH_5-))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~VS2))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /OUT-))
    (pad 6 thru_hole oval (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~VS1))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 8 thru_hole oval (at 7.62 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /CH_1+))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CH_4-))
    (pad 10 thru_hole oval (at 10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 11 thru_hole oval (at 12.7 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /CH_4+))
    (pad 12 thru_hole oval (at 12.7 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /CH_1-))
    (pad 13 thru_hole oval (at 15.24 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 14 thru_hole oval (at 15.24 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 15 thru_hole oval (at 17.78 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /CH_3-))
    (pad 16 thru_hole oval (at 17.78 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /CH_2+))
    (pad 17 thru_hole oval (at 20.32 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /CH_3+))
    (pad 18 thru_hole oval (at 20.32 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 19 thru_hole oval (at 22.86 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 20 thru_hole oval (at 22.86 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /CH_2-))
    (pad 21 thru_hole oval (at 25.4 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /OUT+))
    (pad 22 thru_hole oval (at 25.4 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HF_ADJ))
    (pad 23 thru_hole oval (at 27.94 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CH_5+))
    (pad 24 thru_hole oval (at 27.94 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 VCC))
    (pad 25 thru_hole oval (at 30.48 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~VS3))
    (pad 26 thru_hole oval (at 30.48 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~VS4))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57A944A6)
    (at 132.08 118.745 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 10.16 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~VS1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~VS2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~VS3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~VS4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57A944AB)
    (at 153.67 118.745 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -1.905 1.27 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /OUT+))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /OUT-))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /I_BIAS))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HF_ADJ))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A944A8)
    (at 162.56 111.125)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 VEE))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 57A944A3)
    (at 139.7 118.745 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 5.08 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /CH_1+))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /CH_1-))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /CH_2+))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /CH_2-))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /CH_3+))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /CH_3-))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /CH_4+))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CH_4-))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /CH_5+))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /CH_5-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Tek hybrids:Tek-DIL-26" (layer F.Cu) (tedit 576EB536)
    (at 128.27 74.295)
    (fp_text reference P1 (at 36.83 3.81) (layer B.SilkS))
    (fp_text value DIL_26_PINS (at 5.08 5.08) (layer F.Fab))
    (pad 13 connect rect (at 3.81 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 1 "Net-(P1-Pad13)"))
    (pad 12 connect rect (at 6.35 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 2 "Net-(P1-Pad12)"))
    (pad 11 connect rect (at 8.89 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 3 "Net-(P1-Pad11)"))
    (pad 10 connect rect (at 11.43 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 4 "Net-(P1-Pad10)"))
    (pad 9 connect rect (at 13.97 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 5 "Net-(P1-Pad9)"))
    (pad 8 connect rect (at 16.51 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 6 "Net-(P1-Pad8)"))
    (pad 7 connect rect (at 19.05 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 6 connect rect (at 21.59 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 8 "Net-(P1-Pad6)"))
    (pad 5 connect rect (at 24.13 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 9 "Net-(P1-Pad5)"))
    (pad 4 connect rect (at 26.67 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 10 "Net-(P1-Pad4)"))
    (pad 3 connect rect (at 29.21 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 11 "Net-(P1-Pad3)"))
    (pad 2 connect rect (at 31.75 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (pad 1 connect rect (at 34.29 1.27) (size 1.27 2) (layers B.Cu B.Mask)
      (net 13 "Net-(P1-Pad1)"))
    (pad 26 connect rect (at 34.29 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 14 "Net-(P1-Pad26)"))
    (pad 25 connect rect (at 31.75 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 15 "Net-(P1-Pad25)"))
    (pad 24 connect rect (at 29.21 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 16 "Net-(P1-Pad24)"))
    (pad 23 connect rect (at 26.67 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 17 "Net-(P1-Pad23)"))
    (pad 22 connect rect (at 24.13 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 18 "Net-(P1-Pad22)"))
    (pad 21 connect rect (at 21.59 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 19 "Net-(P1-Pad21)"))
    (pad 20 connect rect (at 19.05 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 20 "Net-(P1-Pad20)"))
    (pad 19 connect rect (at 16.51 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 21 "Net-(P1-Pad19)"))
    (pad 18 connect rect (at 13.97 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 22 "Net-(P1-Pad18)"))
    (pad 17 connect rect (at 11.43 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 23 "Net-(P1-Pad17)"))
    (pad 16 connect rect (at 8.89 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 24 "Net-(P1-Pad16)"))
    (pad 15 connect rect (at 6.35 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 25 "Net-(P1-Pad15)"))
    (pad 14 connect rect (at 3.81 17.78) (size 1.27 2) (layers B.Cu B.Mask)
      (net 26 "Net-(P1-Pad14)"))
  )
  (gr_text GND (at 156.21 112.395 90) (layer F.SilkS))
  (gr_text OUT (at 153.67 112.395 90) (layer F.SilkS))
  (gr_text I_BIAS (at 163.83 118.745) (layer F.SilkS))
  (gr_text HF_ADJ (at 158.75 111.125 90) (layer F.SilkS))
  (gr_text -5V (at 166.37 116.205) (layer F.SilkS))
  (gr_text GND (at 166.37 113.665) (layer F.SilkS))
  (gr_text +5V (at 166.37 111.125) (layer F.SilkS))
  (gr_text - (at 137.16 118.745) (layer F.SilkS))
  (gr_text + (at 137.16 116.205) (layer F.SilkS))
  (gr_text CH5 (at 149.86 112.395 90) (layer F.SilkS))
  (gr_text CH4 (at 147.32 112.395 90) (layer F.SilkS))
  (gr_text CH3 (at 144.78 112.395 90) (layer F.SilkS))
  (gr_text CH2 (at 142.24 112.395 90) (layer F.SilkS))
  (gr_text CH1 (at 139.7 112.395 90) (layer F.SilkS))
  (gr_line (start 146.05 93.345) (end 128.27 93.345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.05 95.885) (end 146.05 93.345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 95.885) (end 146.05 95.885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.59 95.885) (end 170.18 95.885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.59 93.345) (end 148.59 95.885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.37 93.345) (end 148.59 93.345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 121.285) (end 124.46 95.885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.18 121.285) (end 124.46 121.285) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.18 95.885) (end 170.18 121.285) (layer Edge.Cuts) (width 0.1))
  (gr_text ~VS4 (at 128.27 111.125) (layer F.SilkS))
  (gr_text ~VS3 (at 128.27 113.665) (layer F.SilkS))
  (gr_text ~VS2 (at 128.27 116.205) (layer F.SilkS))
  (gr_text ~VS1 (at 128.27 118.745) (layer F.SilkS))
  (gr_line (start 128.27 74.295) (end 128.27 93.345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.37 74.295) (end 128.27 74.295) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.37 93.345) (end 166.37 74.295) (layer Edge.Cuts) (width 0.1))
)
