(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 87)
    (no_connects 4)
    (area 118.712267 71.3886 146.463734 115.629591)
    (thickness 1.6)
    (drawings 41)
    (tracks 323)
    (zones 0)
    (modules 27)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF5F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C101-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C102-Pad1)")
  (net 4 /NRST)
  (net 5 +3.3VA)
  (net 6 +3V3)
  (net 7 +5V)
  (net 8 /PA15)
  (net 9 /PB3)
  (net 10 /PB4)
  (net 11 /PB5)
  (net 12 /PB6)
  (net 13 /PB7)
  (net 14 /PH3)
  (net 15 /PA0)
  (net 16 /PA1)
  (net 17 /PA12)
  (net 18 /PA11)
  (net 19 /PA10)
  (net 20 /PA9)
  (net 21 /PA8)
  (net 22 /PB1)
  (net 23 /PB0)
  (net 24 /PA7)
  (net 25 /PA6)
  (net 26 /PA5)
  (net 27 /PA4)
  (net 28 /PA3)
  (net 29 /PA2)
  (net 30 /SWCLK)
  (net 31 /SWDIO)
  (net 32 "Net-(J104-Pad2)")
  (net 33 "Net-(J104-Pad3)")
  (net 34 "Net-(J104-Pad4)")
  (net 35 "Net-(U102-Pad4)")
  (net 36 "Net-(R101-Pad1)")
  (net 37 "Net-(D101-Pad2)")
  (net 38 "Net-(D102-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /NRST)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA10)
    (add_net /PA11)
    (add_net /PA12)
    (add_net /PA15)
    (add_net /PA2)
    (add_net /PA3)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PA8)
    (add_net /PA9)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /PH3)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(D101-Pad2)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(J104-Pad2)")
    (add_net "Net-(J104-Pad3)")
    (add_net "Net-(J104-Pad4)")
    (add_net "Net-(R101-Pad1)")
    (add_net "Net-(U102-Pad4)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EB54)
    (at 128.27 104.902 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C101 (at 0.127 1.143 270) (layer F.SilkS))
    (fp_text value 4pf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EBBE)
    (at 130.81 104.902 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C102 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 4pf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EBC7)
    (at 132.334 102.362 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at -2.413 1.016 360) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /NRST))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EBD0)
    (at 134.366 102.362 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3VA))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 127.762 98.806 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EBF8)
    (at 136.779 91.821)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C106 (at 1.016 1.27) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59E3EC30)
    (at 138.176 80.518 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C107 (at -1.016 1.397 90) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59E3EC11)
    (at 135.255 88.646 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C108 (at 0.381 -1.524 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59E3EBD7)
    (at 135.636 102.362 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C109 (at -2.413 -1.905 360) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 1.016 -10.668 360) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3VA))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59E3F0BF)
    (at 123.698 76.7715 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J101 (at -1.905 -17.8435 450) (layer B.SilkS))
    (fp_text value CONN_01X14 (at 0 -35.35 180) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /PA15))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /PB3))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /PB4))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /PB5))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /PB6))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /PB7))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /PH3))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /NRST))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3.3VA))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /PA0))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /PA1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59E3F0B2)
    (at 141.478 76.708 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J102 (at 2.032 -17.907 450) (layer B.SilkS))
    (fp_text value CONN_01X14 (at 0 -35.35 180) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /PA12))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PA11))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /PA10))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PA9))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PA8))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PB1))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /PB0))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /PA7))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /PA6))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PA5))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PA4))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PA3))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PA2))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59E3ECEB)
    (at 127.127 76.7715)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J103 (at 0 12.0015 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /SWCLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SWDIO))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /NRST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 136.906 102.616 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L101 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3VA))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:JUMPER-SOLDER-SMD (layer B.Cu) (tedit 59E3EF96)
    (at 138.684 79.248 90)
    (fp_text reference SB101 (at 0.508 -2.667 180) (layer B.SilkS))
    (fp_text value NO (at 0 1.9304 90) (layer B.Fab))
    (pad 2 smd trapezoid (at 0 0.5) (size 0.6 1) (rect_delta 0.1 0 ) (layers B.Cu B.Mask)
      (net 18 /PA11) (solder_mask_margin 0.1))
    (pad 1 smd trapezoid (at 0 -0.5 180) (size 0.6 1) (rect_delta 0.1 0 ) (layers B.Cu B.Mask)
      (net 32 "Net-(J104-Pad2)") (solder_mask_margin 0.1))
  )
  (module footprints:JUMPER-SOLDER-SMD (layer B.Cu) (tedit 59E3EF8C)
    (at 138.684 76.708 90)
    (fp_text reference SB102 (at 1.016 -2.54 180) (layer B.SilkS))
    (fp_text value NO (at 0 1.9304 90) (layer B.Fab))
    (pad 2 smd trapezoid (at 0 0.5) (size 0.6 1) (rect_delta 0.1 0 ) (layers B.Cu B.Mask)
      (net 17 /PA12) (solder_mask_margin 0.1))
    (pad 1 smd trapezoid (at 0 -0.5 180) (size 0.6 1) (rect_delta 0.1 0 ) (layers B.Cu B.Mask)
      (net 33 "Net-(J104-Pad3)") (solder_mask_margin 0.1))
  )
  (module footprints:QFN-32-1EP_5x5mm_Pitch0.5mm_extended_pad (layer F.Cu) (tedit 59E3EB70)
    (at 132.842 95.758 90)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U101 (at -0.127 3.937 90) (layer F.SilkS))
    (fp_text value STM32L432KC (at 0 3.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.55 -1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -2.55 -1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
    (pad 3 smd rect (at -2.55 -0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 4 smd rect (at -2.55 -0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /NRST))
    (pad 5 smd rect (at -2.55 0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3.3VA))
    (pad 6 smd rect (at -2.55 0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /PA0))
    (pad 7 smd rect (at -2.55 1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /PA1))
    (pad 8 smd rect (at -2.55 1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /PA2))
    (pad 9 smd rect (at -1.75 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /PA3))
    (pad 10 smd rect (at -1.25 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /PA4))
    (pad 11 smd rect (at -0.75 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /PA5))
    (pad 12 smd rect (at -0.25 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /PA6))
    (pad 13 smd rect (at 0.25 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /PA7))
    (pad 14 smd rect (at 0.75 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /PB0))
    (pad 15 smd rect (at 1.25 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /PB1))
    (pad 16 smd rect (at 1.75 2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.55 1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 18 smd rect (at 2.55 1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /PA8))
    (pad 19 smd rect (at 2.55 0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /PA9))
    (pad 20 smd rect (at 2.55 0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /PA10))
    (pad 21 smd rect (at 2.55 -0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J104-Pad2)"))
    (pad 22 smd rect (at 2.55 -0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J104-Pad3)"))
    (pad 23 smd rect (at 2.55 -1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /SWDIO))
    (pad 24 smd rect (at 2.55 -1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /SWCLK))
    (pad 25 smd rect (at 1.75 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /PA15))
    (pad 26 smd rect (at 1.25 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /PB3))
    (pad 27 smd rect (at 0.75 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /PB4))
    (pad 28 smd rect (at 0.25 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /PB5))
    (pad 29 smd rect (at -0.25 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /PB6))
    (pad 30 smd rect (at -0.75 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /PB7))
    (pad 31 smd rect (at -1.25 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /PH3))
    (pad 32 smd rect (at -1.75 -2.55 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 33 smd rect (at 0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 90) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 59E3EC15)
    (at 136.652 85.344 270)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U102 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value MCP1802 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -1.35 0 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 4 smd rect (at 1.35 0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U102-Pad4)"))
    (pad 5 smd rect (at 1.35 -0.95 270) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:NX3215SA_XTAL (layer F.Cu) (tedit 59E3EB61)
    (at 129.54 101.854)
    (fp_text reference Y101 (at -2.794 0.254 90) (layer F.SilkS))
    (fp_text value 32768kHz (at 0.0635 -2.0955) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 1 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C101-Pad1)"))
  )
  (module footprints:JUMPER-SOLDER-SMD (layer F.Cu) (tedit 59E3EB3C)
    (at 138.557 106.68 90)
    (fp_text reference SB103 (at 0.889 -2.667 180) (layer F.SilkS))
    (fp_text value NO (at 0 -1.9304 90) (layer F.Fab))
    (pad 2 smd trapezoid (at 0 -0.5 180) (size 0.6 1) (rect_delta 0.1 0 ) (layers F.Cu F.Mask)
      (net 36 "Net-(R101-Pad1)") (solder_mask_margin 0.1))
    (pad 1 smd trapezoid (at 0 0.5) (size 0.6 1) (rect_delta 0.1 0 ) (layers F.Cu F.Mask)
      (net 29 /PA2) (solder_mask_margin 0.1))
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 59E3EBE6)
    (at 136.906 110.236 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D101 (at -2.54 0.635 270) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D101-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59E3EB45)
    (at 136.906 108.585 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0.762 1.27 180) (layer F.SilkS))
    (fp_text value R (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R101-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D101-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PUSHBUTTON_SMD_KMR2 (layer F.Cu) (tedit 59E3EB4E)
    (at 129.286 108.331 180)
    (fp_text reference SW101 (at -3.175 -0.254 450) (layer F.SilkS))
    (fp_text value switch_no (at 0 -0.5 180) (layer F.Fab))
    (pad 4 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /NRST))
    (pad 3 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /NRST))
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 59E3EC24)
    (at 131.318 84.201 270)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D102 (at -0.508 -1.27 270) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D102-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59E3EC1F)
    (at 129.794 84.201 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 3.429 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D102-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.969 88.392 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.715 103.251 270)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (module footprints:USB_Micro-B_10103594-0001LF_NoSlot (layer F.Cu) (tedit 59E40103)
    (at 133.096 78.486 180)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J104 (at -1.778 -3.81 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 6.17 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J104-Pad2)"))
    (pad 3 smd rect (at 0 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J104-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J104-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.42 -1.62 270) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.42 -1.62 270) (size 1.1 1.1) (drill oval 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.73 1.43 270) (size 1.7 1.7) (drill oval 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.73 1.43 270) (size 1.7 1.7) (drill oval 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.96 1.62 270) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.96 1.62 270) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text NRST (at 125.222 86.995 270) (layer F.SilkS))
  (gr_text SWDIO (at 125.222 84.455 270) (layer F.SilkS))
  (gr_text GND (at 125.222 81.915 270) (layer F.SilkS))
  (gr_text SWCLK (at 125.222 79.248 270) (layer F.SilkS))
  (gr_text +3.3V (at 125.222 76.581 270) (layer F.SilkS))
  (gr_text +5V (at 122.301 76.835 270) (layer F.SilkS))
  (gr_text +3.3V (at 122.301 79.375 270) (layer F.SilkS))
  (gr_text GND (at 122.301 81.915 270) (layer F.SilkS))
  (gr_text PA15 (at 122.301 84.455 270) (layer F.SilkS))
  (gr_text PB3 (at 122.301 86.995 270) (layer F.SilkS))
  (gr_text PB4 (at 122.301 89.535 270) (layer F.SilkS))
  (gr_text PB5 (at 122.301 91.948 270) (layer F.SilkS))
  (gr_text PB6 (at 122.301 94.615 270) (layer F.SilkS))
  (gr_text PB7 (at 122.301 97.155 270) (layer F.SilkS))
  (gr_text PH3 (at 122.301 99.568 270) (layer F.SilkS))
  (gr_text NRST (at 122.301 102.108 270) (layer F.SilkS))
  (gr_text +3.3A (at 122.301 104.775 270) (layer F.SilkS))
  (gr_text PA0 (at 122.301 107.315 270) (layer F.SilkS))
  (gr_text PA1 (at 122.301 109.855 270) (layer F.SilkS))
  (gr_text GND (at 142.748 109.728 270) (layer F.SilkS))
  (gr_text PA2 (at 142.748 107.188 270) (layer F.SilkS))
  (gr_text PA3 (at 142.748 104.648 270) (layer F.SilkS))
  (gr_text PA4 (at 142.748 102.108 270) (layer F.SilkS))
  (gr_text PA5 (at 142.748 99.568 270) (layer F.SilkS))
  (gr_text PA6 (at 142.748 97.028 270) (layer F.SilkS))
  (gr_text PA7 (at 142.748 94.488 270) (layer F.SilkS))
  (gr_text PB0 (at 142.748 91.948 270) (layer F.SilkS))
  (gr_text PB1 (at 142.748 89.408 270) (layer F.SilkS))
  (gr_text PA8 (at 142.748 86.868 270) (layer F.SilkS))
  (gr_text PA9 (at 142.748 84.328 270) (layer F.SilkS))
  (gr_text PA10 (at 142.748 81.788 270) (layer F.SilkS))
  (gr_text PA11 (at 142.748 79.248 270) (layer F.SilkS))
  (gr_text PA12 (at 142.748 76.708 270) (layer F.SilkS))
  (gr_text "L432 BOB V0.1\n(c)2017\nE. Brombaugh" (at 127.508 93.472 270) (layer F.SilkS))
  (gr_text USR (at 133.858 109.474 270) (layer F.SilkS))
  (gr_text RST (at 129.159 110.617) (layer F.SilkS))
  (gr_text PWR (at 131.318 87.757 270) (layer F.SilkS))
  (gr_line (start 121.92 111.76) (end 121.92 74.93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 111.76) (end 121.92 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.256 74.93) (end 143.256 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 74.93) (end 143.256 74.93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.875 111.379) (xy 122.301 111.379) (xy 122.301 75.311) (xy 142.875 75.311)
      )
    )
  )
)
