(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3V3")
  (net 3 "INA1")
  (net 4 "INB1")
  (net 5 "MA-")
  (net 6 "MB-")
  (net 7 "unconnected-(U1-Pad8)")
  (net 8 "INA2")
  (net 9 "INB2")
  (net 10 "MA+")
  (net 11 "MB+")
  (net 12 "/V+")
  (net 13 "+BATT")
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 143.5608 94.3864 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:SOIC-14_1mm" (layer "F.Cu")
    (tedit 6372F498)
    (at 148.4376 91.44 90)
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 -4.6 90) (layer "F.Fab"))
    (fp_text value "LB1836M" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.07 -3 90) (size 1.14 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -3.1 -2 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "INA1") (pinfunction "IN1") (pintype "input"))
    (pad "3" smd roundrect (at -3.1 -1 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "MA+") (pinfunction "OUT1") (pintype "output"))
    (pad "4" smd roundrect (at -3.1 0 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/V+") (pinfunction "VS1") (pintype "power_in"))
    (pad "5" smd roundrect (at -3.1 1 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "MA-") (pinfunction "OUT2") (pintype "output"))
    (pad "6" smd roundrect (at -3.1 2 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "INA2") (pinfunction "IN2") (pintype "input"))
    (pad "7" smd roundrect (at -3.1 3 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "8" smd roundrect (at 3.09 3 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(U1-Pad8)") (pinfunction "Vcont") (pintype "power_in+no_connect"))
    (pad "9" smd roundrect (at 3.09 2 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "INB2") (pinfunction "IN4") (pintype "input"))
    (pad "10" smd roundrect (at 3.1 1 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "MB-") (pinfunction "OUT4") (pintype "output"))
    (pad "11" smd roundrect (at 3.09 0 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/V+") (pinfunction "VS2") (pintype "power_in"))
    (pad "12" smd roundrect (at 3.1 -1 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "MB+") (pinfunction "OUT3") (pintype "output"))
    (pad "13" smd roundrect (at 3.1 -2 90) (size 1.2 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "INB1") (pinfunction "IN3") (pintype "input"))
    (pad "14" smd roundrect (at 3.07 -3 90) (size 1.14 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 6372E01B)
    (at 138.43 86.36 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "A2" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 135) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "INB1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "INB2") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "MB+") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "MB-") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x5.8" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 138.4808 91.44 -90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x5.8mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -4.35 90) (layer "F.Fab"))
    (fp_text value "220uF 10V" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.7 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 13 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 2.7 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 143.5608 88.4936)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/V+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 138.43 96.52 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "A1" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "INA1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "INA2") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "MA+") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "MA-") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 143.1544 91.44 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.82 90) (layer "F.Fab"))
    (fp_text value "350mA 16V" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 13 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 12 "/V+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 145.288 91.44 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.8 90) (layer "B.Fab"))
    (fp_text value "IN2" (at 0 -1.9 90) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 3 "INA1") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 4 "INB1") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 147.32 91.44 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 1.8 90) (layer "B.Fab"))
    (fp_text value "M+" (at 0 -1.9 90) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 10 "MA+") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 11 "MB+") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 149.352 91.44 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at 0 1.8 90) (layer "B.Fab"))
    (fp_text value "M-" (at 0 -1.9 90) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 5 "MA-") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 6 "MB-") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 151.384 91.44 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Tram_LB1836.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 1.8 90) (layer "B.Fab"))
    (fp_text value "IN1" (at 0 -1.9 90) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 8 "INA2") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 9 "INB2") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (gr_line (start 135.255 97.155) (end 135.255 85.725) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 152.527 97.155) (end 151.892 97.79) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 135.89 97.79) (end 135.255 97.155) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 152.527 85.725) (end 152.527 97.155) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 135.255 85.725) (end 135.89 85.09) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151.892 85.09) (end 152.527 85.725) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151.892 97.79) (end 135.89 97.79) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 135.89 85.09) (end 151.892 85.09) (layer "Edge.Cuts") (width 0.1))
  (gr_text "INA1" (at 143.51 94.996 180) (layer "B.SilkS"))
  (gr_text "Nov 2022" (at 140.208 91.44 90) (layer "B.SilkS"))
  (gr_text "GND" (at 140.97 87.884) (layer "B.SilkS"))
  (gr_text "INA2" (at 146.05 94.996 180) (layer "B.SilkS"))
  (gr_text "MA+" (at 148.59 94.996 180) (layer "B.SilkS"))
  (gr_text "MA-" (at 151.13 94.488 180) (layer "B.SilkS"))
  (gr_text "GND" (at 138.43 94.996 180) (layer "B.SilkS"))
  (gr_text "+3V3" (at 140.97 94.996 180) (layer "B.SilkS"))
  (gr_text "INB2" (at 146.05 87.884) (layer "B.SilkS"))
  (gr_text "BAT+" (at 138.43 87.884) (layer "B.SilkS"))
  (gr_text "LB1836 Motor Driver v1" (at 136.652 91.44 90) (layer "B.SilkS"))
  (gr_text "INB1" (at 143.51 87.884) (layer "B.SilkS"))
  (gr_text "MB-" (at 151.13 87.884) (layer "B.SilkS"))
  (gr_text "SHORT ALL FOR\nSINGLE MOTOR" (at 143.256 91.44 90) (layer "B.SilkS"))
  (gr_text "MB+" (at 148.59 87.884) (layer "B.SilkS"))
  (gr_text "+" (at 136.398 87.122 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 145.923 87.376)
        (xy 145.923 92.71)
        (xy 145.796 93.091)
        (xy 146.812 93.472)
        (xy 153.67 93.472)
        (xy 153.67 95.504)
        (xy 140.97 95.504)
        (xy 140.335 95.885)
        (xy 140.335 98.425)
        (xy 134.62 98.425)
        (xy 134.62 84.455)
        (xy 143.51 84.455)
        (xy 143.51 87.376)
      )
    )
  )
)
