(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 131)
    (tracks 546)
    (zones 0)
    (modules 32)
    (nets 75)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.8 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-PadA6)")
  (net 2 "Net-(U1-PadC4)")
  (net 3 "Net-(U1-PadD3)")
  (net 4 "Net-(U1-PadD4)")
  (net 5 "Net-(U1-PadE3)")
  (net 6 "Net-(U1-PadM2)")
  (net 7 "Net-(U1-PadE5)")
  (net 8 "Net-(U1-PadP5)")
  (net 9 "Net-(J4-Pad8)")
  (net 10 "Net-(J4-Pad7)")
  (net 11 "Net-(J4-Pad6)")
  (net 12 "Net-(J4-Pad5)")
  (net 13 "Net-(J5-Pad4)")
  (net 14 "Net-(J5-Pad3)")
  (net 15 "Net-(J5-Pad2)")
  (net 16 "Net-(J5-Pad1)")
  (net 17 "Net-(J2-Pad5)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad3)")
  (net 20 "Net-(J2-Pad2)")
  (net 21 "Net-(J2-Pad8)")
  (net 22 "Net-(J6-Pad3)")
  (net 23 "Net-(J6-Pad1)")
  (net 24 "Net-(J6-Pad2)")
  (net 25 "Net-(J3-Pad5)")
  (net 26 "Net-(J3-Pad3)")
  (net 27 "Net-(J3-Pad2)")
  (net 28 "Net-(J2-Pad7)")
  (net 29 "Net-(J2-Pad6)")
  (net 30 "Net-(J4-Pad3)")
  (net 31 "Net-(J4-Pad2)")
  (net 32 "Net-(J3-Pad8)")
  (net 33 "Net-(J3-Pad7)")
  (net 34 "Net-(J4-Pad1)")
  (net 35 "Net-(J4-Pad4)")
  (net 36 "Net-(J6-Pad8)")
  (net 37 "Net-(J5-Pad5)")
  (net 38 "Net-(J5-Pad6)")
  (net 39 "Net-(J5-Pad7)")
  (net 40 "Net-(J5-Pad8)")
  (net 41 "Net-(J6-Pad4)")
  (net 42 "Net-(J6-Pad5)")
  (net 43 "Net-(J6-Pad6)")
  (net 44 "Net-(J6-Pad7)")
  (net 45 "Net-(J3-Pad4)")
  (net 46 "Net-(J3-Pad6)")
  (net 47 "Net-(J2-Pad1)")
  (net 48 "Net-(J3-Pad1)")
  (net 49 "Net-(J7-Pad1)")
  (net 50 "Net-(J7-Pad2)")
  (net 51 "Net-(J7-Pad3)")
  (net 52 "Net-(J7-Pad4)")
  (net 53 "Net-(J7-Pad5)")
  (net 54 "Net-(J7-Pad6)")
  (net 55 "Net-(J7-Pad7)")
  (net 56 "Net-(J7-Pad8)")
  (net 57 "Net-(X1-Pad1)")
  (net 58 "Net-(R5-Pad2)")
  (net 59 "Net-(D4-Pad1)")
  (net 60 "Net-(R6-Pad2)")
  (net 61 "Net-(R7-Pad2)")
  (net 62 "Net-(J8-Pad1)")
  (net 63 "Net-(3OIKMG1-Pad6)")
  (net 64 "Net-(3OIKMG1-Pad1)")
  (net 65 "Net-(3OIKMG1-Pad5)")
  (net 66 "Net-(3OIKMG1-Pad4)")
  (net 67 "Net-(3OIKMG1-Pad2)")
  (net 68 "Net-(3OIKMG1-Pad3)")
  (net 69 "Net-(DA13-Pad2)")
  (net 70 "Net-(DA12-Pad2)")
  (net 71 "Net-(DA11-Pad2)")
  (net 72 "Net-(DA13-Pad1)")
  (net 73 "Net-(DA12-Pad1)")
  (net 74 "Net-(DA11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(3OIKMG1-Pad1)")
    (add_net "Net-(3OIKMG1-Pad2)")
    (add_net "Net-(3OIKMG1-Pad3)")
    (add_net "Net-(3OIKMG1-Pad4)")
    (add_net "Net-(3OIKMG1-Pad5)")
    (add_net "Net-(3OIKMG1-Pad6)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(DA11-Pad1)")
    (add_net "Net-(DA11-Pad2)")
    (add_net "Net-(DA12-Pad1)")
    (add_net "Net-(DA12-Pad2)")
    (add_net "Net-(DA13-Pad1)")
    (add_net "Net-(DA13-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(J6-Pad6)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J6-Pad8)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad8)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-PadA6)")
    (add_net "Net-(U1-PadC4)")
    (add_net "Net-(U1-PadD3)")
    (add_net "Net-(U1-PadD4)")
    (add_net "Net-(U1-PadE3)")
    (add_net "Net-(U1-PadE5)")
    (add_net "Net-(U1-PadM2)")
    (add_net "Net-(U1-PadP5)")
    (add_net "Net-(X1-Pad1)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Button_Switch_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 5A02FC95)
    (at 121.1506 87.63 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SWA9 (at -8.11 0.0762 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 5A02FC95)
    (at 121.1506 92.8624 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SWA8 (at -8.2624 -0.1524 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 180) (layer F.Fab))
    (pad 2 smd rect (at 4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd rect (at -4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 5A02FC95)
    (at 121.1506 97.79 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SWA7 (at -8.3005 -0.1143 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 180) (layer F.Fab))
    (pad 1 smd rect (at -4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 4.59 0 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 121.1416 78.6765)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference DA13 (at 4.0767 0.1651) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 72 "Net-(DA13-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 69 "Net-(DA13-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 121.1162 81.1784)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference DA12 (at 4.073 0.1016) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 70 "Net-(DA12-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 73 "Net-(DA12-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 121.158 83.5914)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference DA11 (at 4.1656 -0.0762) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 74 "Net-(DA11-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 71 "Net-(DA11-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 6118274C)
    (at 167.5638 83.0834)
    (descr "Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x03 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.77) (layer F.Fab))
    (fp_text value Conn_02x03_Odd_Even (at -1.27 7.85) (layer F.Fab))
    (fp_text user %R (at -1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 144.0688 91.9443 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -0.009 -1.9685 270) (layer B.SilkS))
    (fp_text value C (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 181.6608 95.377)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0.1651 -2.0955) (layer B.SilkS))
    (fp_text value C (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 152.0444 86.2113 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0.0164 -1.7145 90) (layer B.SilkS))
    (fp_text value C (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 144.0688 86.1859 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value C (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 152.0698 91.9062 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0.0291 1.7399 270) (layer B.SilkS))
    (fp_text value C (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 61182D2D)
    (at 175.2727 82.5627)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference 3OIKMG1 (at -2.587001 6.556999 90) (layer F.Fab))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(3OIKMG1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(3OIKMG1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(3OIKMG1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(3OIKMG1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SC-63 (layer B.Cu) (tedit 61182C3B)
    (at 166.1795 95.6945 180)
    (fp_text reference U2 (at 0 1.75 180) (layer F.Fab))
    (fp_text value LM7805_TO220 (at 0 2.75 180) (layer B.Fab))
    (pad 2 smd rect (at 0.1 2.25 180) (size 5.1 5.1) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd rect (at -2.29 -4.05 180) (size 1.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(J8-Pad1)"))
    (pad 3 smd rect (at 2.29 -4.05 180) (size 1.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 136.1821 88.646 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 2.9845 -0.0762) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 61 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 184.3659 77.8002)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at 3.048 -0.0254) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 59 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 136.1821 92.2782 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 2.8702 -0.0508 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 60 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 182.3085 77.8002 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.9845 0.0635 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 59 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 136.144 90.4875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.93 0 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 58 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 6117EF1D)
    (at 190.5127 72.4027 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J9 (at 2.1336 8.2423) (layer F.Fab))
    (fp_text value Conn_01x06 (at -0.0127 8.9027) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 61182493)
    (at 190.5 107.95 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J8 (at -2.6162 7.3025) (layer F.Fab))
    (fp_text value Conn_01x06 (at 0 7.62) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 119.0916 78.6765 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.1623 -0.0254 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 72 "Net-(DA13-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 119.1133 83.5914 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -3.048 0 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 74 "Net-(DA11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 119.0662 81.1784 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -3.2131 -0.0254 180) (layer B.SilkS))
    (fp_text value R_Small_US (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 73 "Net-(DA12-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_DIP-14 (layer F.Cu) (tedit 58CD3344)
    (at 188.214 97.282 90)
    (descr "Oscillator, DIP14, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at 8.3058 -3.6703 180) (layer F.SilkS))
    (fp_text value GTXO-S14T (at 7.62 3.74 90) (layer F.Fab))
    (fp_text user %R (at 7.62 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(X1-Pad1)"))
    (pad 14 thru_hole circle (at 0 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad 8 thru_hole circle (at 15.24 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-PadM2)"))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_DIP-14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 61182525)
    (at 175.2727 72.4027 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J7 (at 2.7559 8.1153) (layer F.Fab))
    (fp_text value Conn_01x08 (at -0.0127 8.9027) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J7-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J7-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J7-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J7-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J7-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J7-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 61182533)
    (at 116.8527 72.4027 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J6 (at -2.5908 9.398 180) (layer F.Fab))
    (fp_text value Conn_01x08 (at 0.0127 7.6073 180) (layer F.Fab))
    (fp_text user %R (at 0.7874 9.3726 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J6-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J6-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J6-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 61182545)
    (at 134.62 107.95 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J5 (at -2.413 8.8519) (layer F.Fab))
    (fp_text value Conn_01x08 (at 0 10.16) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 6118252D)
    (at 154.9527 72.4027 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 2.4384 9.2837) (layer F.Fab))
    (fp_text value Conn_01x08 (at -0.0127 7.6327) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 6118253A)
    (at 175.26 107.95 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at -2.3114 8.8646) (layer F.Fab))
    (fp_text value Conn_01x08 (at 0 10.16) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 6118253F)
    (at 154.94 107.95 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at -2.5146 9.3345) (layer F.Fab))
    (fp_text value Conn_01x08 (at 0 10.16 180) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_BGA:BGA-256_16x16_17.0x17.0mm (layer F.Cu) (tedit 61182B6C)
    (at 148.0566 89.0778 90)
    (attr smd)
    (fp_text reference U1 (at 0 -9.5 90) (layer F.Fab))
    (fp_text value XC95288XL-FGG256 (at 0 9.5 90) (layer F.Fab))
    (pad A1 smd circle (at -7.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad B1 smd circle (at -7.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J5-Pad4)"))
    (pad C1 smd circle (at -7.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad D1 smd circle (at -7.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J5-Pad2)"))
    (pad E1 smd circle (at -7.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J5-Pad1)"))
    (pad F1 smd circle (at -7.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad G1 smd circle (at -7.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad7)"))
    (pad H1 smd circle (at -7.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad6)"))
    (pad J1 smd circle (at -7.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad5)"))
    (pad K1 smd circle (at -7.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad L1 smd circle (at -7.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad M1 smd circle (at -7.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad N1 smd circle (at -7.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad1)"))
    (pad P1 smd circle (at -7.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J3-Pad8)"))
    (pad R1 smd circle (at -7.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J3-Pad7)"))
    (pad T1 smd circle (at -7.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad A2 smd circle (at -6.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad5)"))
    (pad B2 smd circle (at -6.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad C2 smd circle (at -6.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D2 smd circle (at -6.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E2 smd circle (at -6.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F2 smd circle (at -6.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G2 smd circle (at -6.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H2 smd circle (at -6.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J2 smd circle (at -6.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K2 smd circle (at -6.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L2 smd circle (at -6.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M2 smd circle (at -6.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-PadM2)"))
    (pad N2 smd circle (at -6.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P2 smd circle (at -6.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R2 smd circle (at -6.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad T2 smd circle (at -6.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J3-Pad6)"))
    (pad A3 smd circle (at -5.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J5-Pad6)"))
    (pad B3 smd circle (at -5.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd circle (at -5.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad D3 smd circle (at -5.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-PadD3)"))
    (pad E3 smd circle (at -5.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-PadE3)"))
    (pad F3 smd circle (at -5.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G3 smd circle (at -5.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H3 smd circle (at -5.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J3 smd circle (at -5.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K3 smd circle (at -5.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L3 smd circle (at -5.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M3 smd circle (at -5.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-PadM2)"))
    (pad N3 smd circle (at -5.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P3 smd circle (at -5.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad R3 smd circle (at -5.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T3 smd circle (at -5.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad5)"))
    (pad A4 smd circle (at -4.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J5-Pad7)"))
    (pad B4 smd circle (at -4.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C4 smd circle (at -4.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-PadC4)"))
    (pad D4 smd circle (at -4.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-PadD4)"))
    (pad E4 smd circle (at -4.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F4 smd circle (at -4.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G4 smd circle (at -4.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H4 smd circle (at -4.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J4 smd circle (at -4.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K4 smd circle (at -4.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad L4 smd circle (at -4.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M4 smd circle (at -4.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N4 smd circle (at -4.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P4 smd circle (at -4.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R4 smd circle (at -4.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T4 smd circle (at -4.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J3-Pad4)"))
    (pad A5 smd circle (at -3.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J5-Pad8)"))
    (pad B5 smd circle (at -3.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C5 smd circle (at -3.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D5 smd circle (at -3.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad E5 smd circle (at -3.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-PadE5)"))
    (pad F5 smd circle (at -3.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G5 smd circle (at -3.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H5 smd circle (at -3.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J5 smd circle (at -3.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K5 smd circle (at -3.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L5 smd circle (at -3.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M5 smd circle (at -3.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N5 smd circle (at -3.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P5 smd circle (at -3.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-PadP5)"))
    (pad R5 smd circle (at -3.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-PadP5)"))
    (pad T5 smd circle (at -3.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (pad A6 smd circle (at -2.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-PadA6)"))
    (pad B6 smd circle (at -2.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C6 smd circle (at -2.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D6 smd circle (at -2.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E6 smd circle (at -2.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F6 smd circle (at -2.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G6 smd circle (at -2.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad H6 smd circle (at -2.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad J6 smd circle (at -2.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad K6 smd circle (at -2.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad L6 smd circle (at -2.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M6 smd circle (at -2.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N6 smd circle (at -2.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P6 smd circle (at -2.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad R6 smd circle (at -2.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T6 smd circle (at -2.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad2)"))
    (pad A7 smd circle (at -1.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R6-Pad2)"))
    (pad B7 smd circle (at -1.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C7 smd circle (at -1.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad D7 smd circle (at -1.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E7 smd circle (at -1.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F7 smd circle (at -1.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G7 smd circle (at -1.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad H7 smd circle (at -1.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad J7 smd circle (at -1.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad K7 smd circle (at -1.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad L7 smd circle (at -1.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M7 smd circle (at -1.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N7 smd circle (at -1.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P7 smd circle (at -1.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R7 smd circle (at -1.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T7 smd circle (at -1.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J3-Pad1)"))
    (pad A8 smd circle (at -0.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R5-Pad2)"))
    (pad B8 smd circle (at -0.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C8 smd circle (at -0.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D8 smd circle (at -0.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E8 smd circle (at -0.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F8 smd circle (at -0.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G8 smd circle (at -0.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad H8 smd circle (at -0.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad J8 smd circle (at -0.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad K8 smd circle (at -0.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad L8 smd circle (at -0.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M8 smd circle (at -0.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N8 smd circle (at -0.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P8 smd circle (at -0.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R8 smd circle (at -0.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T8 smd circle (at -0.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J7-Pad1)"))
    (pad A9 smd circle (at 0.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R7-Pad2)"))
    (pad B9 smd circle (at 0.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C9 smd circle (at 0.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D9 smd circle (at 0.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E9 smd circle (at 0.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F9 smd circle (at 0.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G9 smd circle (at 0.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad H9 smd circle (at 0.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad J9 smd circle (at 0.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad K9 smd circle (at 0.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad L9 smd circle (at 0.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M9 smd circle (at 0.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N9 smd circle (at 0.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad P9 smd circle (at 0.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R9 smd circle (at 0.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T9 smd circle (at 0.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J7-Pad2)"))
    (pad A10 smd circle (at 1.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(3OIKMG1-Pad5)"))
    (pad B10 smd circle (at 1.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C10 smd circle (at 1.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad D10 smd circle (at 1.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E10 smd circle (at 1.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F10 smd circle (at 1.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G10 smd circle (at 1.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad H10 smd circle (at 1.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad J10 smd circle (at 1.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad K10 smd circle (at 1.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad L10 smd circle (at 1.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M10 smd circle (at 1.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N10 smd circle (at 1.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P10 smd circle (at 1.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R10 smd circle (at 1.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T10 smd circle (at 1.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J7-Pad3)"))
    (pad A11 smd circle (at 2.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(DA11-Pad2)"))
    (pad B11 smd circle (at 2.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C11 smd circle (at 2.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D11 smd circle (at 2.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E11 smd circle (at 2.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F11 smd circle (at 2.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad G11 smd circle (at 2.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad H11 smd circle (at 2.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad J11 smd circle (at 2.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad K11 smd circle (at 2.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad L11 smd circle (at 2.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M11 smd circle (at 2.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N11 smd circle (at 2.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P11 smd circle (at 2.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad R11 smd circle (at 2.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(3OIKMG1-Pad4)"))
    (pad T11 smd circle (at 2.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J7-Pad4)"))
    (pad A12 smd circle (at 3.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(DA12-Pad2)"))
    (pad B12 smd circle (at 3.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd circle (at 3.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D12 smd circle (at 3.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad E12 smd circle (at 3.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F12 smd circle (at 3.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G12 smd circle (at 3.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H12 smd circle (at 3.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J12 smd circle (at 3.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K12 smd circle (at 3.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L12 smd circle (at 3.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M12 smd circle (at 3.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N12 smd circle (at 3.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(3OIKMG1-Pad2)"))
    (pad P12 smd circle (at 3.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(3OIKMG1-Pad3)"))
    (pad R12 smd circle (at 3.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T12 smd circle (at 3.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J7-Pad5)"))
    (pad A13 smd circle (at 4.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(DA13-Pad2)"))
    (pad B13 smd circle (at 4.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd circle (at 4.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D13 smd circle (at 4.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E13 smd circle (at 4.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F13 smd circle (at 4.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G13 smd circle (at 4.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad H13 smd circle (at 4.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J13 smd circle (at 4.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K13 smd circle (at 4.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L13 smd circle (at 4.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M13 smd circle (at 4.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N13 smd circle (at 4.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P13 smd circle (at 4.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R13 smd circle (at 4.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T13 smd circle (at 4.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J7-Pad6)"))
    (pad A14 smd circle (at 5.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J6-Pad1)"))
    (pad B14 smd circle (at 5.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd circle (at 5.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad D14 smd circle (at 5.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E14 smd circle (at 5.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F14 smd circle (at 5.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G14 smd circle (at 5.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H14 smd circle (at 5.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J14 smd circle (at 5.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K14 smd circle (at 5.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L14 smd circle (at 5.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(3OIKMG1-Pad6)"))
    (pad M14 smd circle (at 5.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N14 smd circle (at 5.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P14 smd circle (at 5.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad R14 smd circle (at 5.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad T14 smd circle (at 5.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J7-Pad7)"))
    (pad A15 smd circle (at 6.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J6-Pad2)"))
    (pad B15 smd circle (at 6.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad C15 smd circle (at 6.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad D15 smd circle (at 6.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad E15 smd circle (at 6.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad F15 smd circle (at 6.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad G15 smd circle (at 6.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad H15 smd circle (at 6.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad J15 smd circle (at 6.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad K15 smd circle (at 6.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad L15 smd circle (at 6.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad M15 smd circle (at 6.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad N15 smd circle (at 6.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad P15 smd circle (at 6.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad R15 smd circle (at 6.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad T15 smd circle (at 6.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J7-Pad8)"))
    (pad A16 smd circle (at 7.5 -7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
    (pad B16 smd circle (at 7.5 -6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (pad C16 smd circle (at 7.5 -5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J6-Pad4)"))
    (pad D16 smd circle (at 7.5 -4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J6-Pad5)"))
    (pad E16 smd circle (at 7.5 -3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J6-Pad6)"))
    (pad F16 smd circle (at 7.5 -2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J6-Pad7)"))
    (pad G16 smd circle (at 7.5 -1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J6-Pad8)"))
    (pad H16 smd circle (at 7.5 -0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J4-Pad8)"))
    (pad J16 smd circle (at 7.5 0.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J4-Pad7)"))
    (pad K16 smd circle (at 7.5 1.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad6)"))
    (pad L16 smd circle (at 7.5 2.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J4-Pad5)"))
    (pad M16 smd circle (at 7.5 3.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J4-Pad4)"))
    (pad N16 smd circle (at 7.5 4.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J4-Pad3)"))
    (pad P16 smd circle (at 7.5 5.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad2)"))
    (pad R16 smd circle (at 7.5 6.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J4-Pad1)"))
    (pad T16 smd circle (at 7.5 7.5 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(3OIKMG1-Pad1)"))
  )
  (gr_text "RUE MOHR 288 CPLD - 2021" (at 148.59 78.74) (layer F.SilkS))
  (gr_text L1 (at 150.0759 105.283 270) (layer B.SilkS))
  (gr_text G1 (at 139.9286 105.41 270) (layer B.SilkS))
  (gr_text T5 (at 170.3959 105.283 270) (layer B.SilkS))
  (gr_text E1 (at 134.8359 105.3465 270) (layer B.SilkS))
  (gr_text M1 (at 152.6032 105.4989 270) (layer B.SilkS))
  (gr_text 3 (at 188.1124 105.3592) (layer B.SilkS))
  (gr_text G (at 183.0197 105.3338) (layer B.SilkS))
  (gr_text T2 (at 162.6743 105.3211 270) (layer B.SilkS))
  (gr_text T4 (at 167.8559 105.3338 270) (layer B.SilkS))
  (gr_text A2 (at 124.6759 105.3592 270) (layer B.SilkS))
  (gr_text 5 (at 190.6651 105.3338) (layer B.SilkS))
  (gr_text A5 (at 117.0178 105.3719 270) (layer B.SilkS))
  (gr_text K1 (at 147.5105 105.4354 270) (layer B.SilkS))
  (gr_text R1 (at 160.2359 105.4227 270) (layer B.SilkS))
  (gr_text N1 (at 155.1559 105.4608 270) (layer B.SilkS))
  (gr_text H1 (at 142.4305 105.41 270) (layer B.SilkS))
  (gr_text G (at 180.5305 105.3084) (layer B.SilkS))
  (gr_text G (at 177.9524 105.3338) (layer B.SilkS))
  (gr_text T7 (at 175.4886 105.3592 270) (layer B.SilkS))
  (gr_text 3 (at 185.6994 105.3338) (layer B.SilkS))
  (gr_text T3 (at 165.3032 105.3338 270) (layer B.SilkS))
  (gr_text A4 (at 119.5959 105.3719 270) (layer B.SilkS))
  (gr_text D1 (at 132.2705 105.3719 270) (layer B.SilkS))
  (gr_text B1 (at 127.1905 105.4481 270) (layer B.SilkS))
  (gr_text P1 (at 157.6832 105.4608 270) (layer B.SilkS))
  (gr_text C1 (at 129.794 105.4735 270) (layer B.SilkS))
  (gr_text J1 (at 145.0594 105.2957 270) (layer B.SilkS))
  (gr_text A3 (at 122.1232 105.3592 270) (layer B.SilkS))
  (gr_text F1 (at 137.3505 105.3719 270) (layer B.SilkS))
  (gr_text T6 (at 172.8978 105.2957 270) (layer B.SilkS))
  (gr_text T13 (at 162.5473 76.0603 270) (layer B.SilkS))
  (gr_text T8 (at 175.26 76.5683 270) (layer B.SilkS))
  (gr_text T9 (at 172.6565 76.5429 270) (layer B.SilkS))
  (gr_text T11 (at 167.6527 76.0476 270) (layer B.SilkS))
  (gr_text G (at 177.9143 75.184) (layer B.SilkS))
  (gr_text M16 (at 147.3454 75.7174 270) (layer B.SilkS))
  (gr_text T12 (at 165.1254 76.0603 270) (layer B.SilkS))
  (gr_text 3 (at 185.5597 75.2348) (layer B.SilkS))
  (gr_text R16 (at 154.9781 75.8698 270) (layer B.SilkS))
  (gr_text P16 (at 152.3746 75.7809 270) (layer B.SilkS))
  (gr_text A14 (at 116.84 75.8571 270) (layer B.SilkS))
  (gr_text C16 (at 124.4854 75.8825 270) (layer B.SilkS))
  (gr_text T15 (at 157.4419 76.0603 270) (layer B.SilkS))
  (gr_text A15 (at 119.3927 75.8952 270) (layer B.SilkS))
  (gr_text G16 (at 134.6581 75.819 270) (layer B.SilkS))
  (gr_text K16 (at 142.2527 75.819 270) (layer B.SilkS))
  (gr_text H16 (at 137.1727 75.8571 270) (layer B.SilkS))
  (gr_text G (at 180.5432 75.2729) (layer B.SilkS))
  (gr_text L16 (at 144.78 75.8825 270) (layer B.SilkS))
  (gr_text 5 (at 190.4619 75.311) (layer B.SilkS))
  (gr_text E16 (at 129.5527 75.8825 270) (layer B.SilkS))
  (gr_text N16 (at 149.8473 75.6793 270) (layer B.SilkS))
  (gr_text D16 (at 127 75.8825 270) (layer B.SilkS))
  (gr_text T10 (at 170.0276 76.073 270) (layer B.SilkS))
  (gr_text J16 (at 139.7127 75.9333 270) (layer B.SilkS))
  (gr_text B16 (at 121.9454 75.9079 270) (layer B.SilkS))
  (gr_text F16 (at 132.1181 75.8444 270) (layer B.SilkS))
  (gr_text T14 (at 159.9565 75.7047 270) (layer B.SilkS))
  (gr_text G (at 182.9308 75.2348) (layer B.SilkS))
  (gr_text 3 (at 188.0743 75.2729) (layer B.SilkS))
  (gr_text "3 O I K M G" (at 172.7835 88.7476 90) (layer F.SilkS))
  (gr_text uPC29M33T (at 161.1884 95.9485 90) (layer B.SilkS))
  (gr_text "XL95288XL FG256" (at 146.8628 99.3013) (layer F.SilkS))
  (gr_text T7 (at 175.2854 105.283 270) (layer F.SilkS))
  (gr_text T6 (at 172.6946 105.3465 270) (layer F.SilkS))
  (gr_text T5 (at 170.1927 105.3592 270) (layer F.SilkS))
  (gr_text T4 (at 167.6527 105.3084 270) (layer F.SilkS))
  (gr_text T3 (at 165.1 105.3084 270) (layer F.SilkS))
  (gr_text T2 (at 162.4711 105.3211 270) (layer F.SilkS))
  (gr_text R1 (at 160.0327 105.2195 270) (layer F.SilkS))
  (gr_text P1 (at 157.48 105.1814 270) (layer F.SilkS))
  (gr_text N1 (at 154.9527 105.1814 270) (layer F.SilkS))
  (gr_text M1 (at 152.4 105.1433 270) (layer F.SilkS))
  (gr_text L1 (at 149.8727 105.3592 270) (layer F.SilkS))
  (gr_text K1 (at 147.3073 105.2068 270) (layer F.SilkS))
  (gr_text J1 (at 144.8562 105.3465 270) (layer F.SilkS))
  (gr_text H1 (at 142.2273 105.2322 270) (layer F.SilkS))
  (gr_text G1 (at 139.7254 105.2322 270) (layer F.SilkS))
  (gr_text F1 (at 137.1473 105.2703 270) (layer F.SilkS))
  (gr_text E1 (at 134.6327 105.2957 270) (layer F.SilkS))
  (gr_text D1 (at 132.0673 105.2703 270) (layer F.SilkS))
  (gr_text C1 (at 129.5908 105.1687 270) (layer F.SilkS))
  (gr_text B1 (at 126.9873 105.1941 270) (layer F.SilkS))
  (gr_text A2 (at 124.4727 105.283 270) (layer F.SilkS))
  (gr_text A3 (at 121.92 105.283 270) (layer F.SilkS))
  (gr_text A4 (at 119.3927 105.2703 270) (layer F.SilkS))
  (gr_text A5 (at 116.8146 105.2703 270) (layer F.SilkS))
  (gr_text A14 (at 116.84 75.819 270) (layer F.SilkS))
  (gr_text A15 (at 119.3927 75.7809 270) (layer F.SilkS))
  (gr_text E16 (at 129.5527 75.7936 270) (layer F.SilkS))
  (gr_text B16 (at 121.9454 75.7682 270) (layer F.SilkS))
  (gr_text C16 (at 124.4854 75.7936 270) (layer F.SilkS))
  (gr_text D16 (at 127 75.7936 270) (layer F.SilkS))
  (gr_text F16 (at 132.1181 75.8317 270) (layer F.SilkS))
  (gr_text G16 (at 134.6581 75.8571 270) (layer F.SilkS))
  (gr_text H16 (at 137.1727 75.819 270) (layer F.SilkS))
  (gr_text J16 (at 139.7127 75.7428 270) (layer F.SilkS))
  (gr_text K16 (at 142.2527 75.8571 270) (layer F.SilkS))
  (gr_text L16 (at 144.78 75.7936 270) (layer F.SilkS))
  (gr_text M16 (at 147.3454 75.9587 270) (layer F.SilkS))
  (gr_text N16 (at 149.8473 75.9968 270) (layer F.SilkS))
  (gr_text P16 (at 152.3746 75.8952 270) (layer F.SilkS))
  (gr_text R16 (at 154.9781 75.8063 270) (layer F.SilkS))
  (gr_text T15 (at 157.4419 75.6158 270) (layer F.SilkS))
  (gr_text T14 (at 159.9565 75.9714 270) (layer F.SilkS))
  (gr_text T13 (at 162.5473 75.6158 270) (layer F.SilkS))
  (gr_text T12 (at 165.1254 75.6158 270) (layer F.SilkS))
  (gr_text T11 (at 167.6527 75.6285 270) (layer F.SilkS))
  (gr_text T10 (at 170.0276 75.6031 270) (layer F.SilkS))
  (gr_text T9 (at 172.6565 75.1332 270) (layer F.SilkS))
  (gr_text T8 (at 175.26 75.1078 270) (layer F.SilkS))
  (gr_text G (at 177.7492 105.3084) (layer F.SilkS))
  (gr_text G (at 180.3273 105.3338) (layer F.SilkS))
  (gr_text G (at 182.8165 105.3084) (layer F.SilkS))
  (gr_text 3 (at 185.4962 105.3084) (layer F.SilkS))
  (gr_text 3 (at 187.9092 105.283) (layer F.SilkS))
  (gr_text 5 (at 190.4619 105.3084) (layer F.SilkS))
  (gr_text G (at 177.8381 75.184) (layer F.SilkS))
  (gr_text G (at 180.467 75.0951) (layer F.SilkS))
  (gr_text G (at 182.8546 75.1332) (layer F.SilkS))
  (gr_text 3 (at 185.4835 75.1332) (layer F.SilkS))
  (gr_text 3 (at 187.9981 75.0951) (layer F.SilkS))
  (gr_text 5 (at 190.3857 75.057) (layer F.SilkS))
  (gr_line (start 114.3 110.49) (end 114.3 69.85) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 110.49) (end 114.3 110.49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 69.85) (end 193.04 110.49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 69.85) (end 193.04 69.85) (layer Edge.Cuts) (width 0.15))
  (zone (net 64) (net_name "Net-(3OIKMG1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.4091 72.39) (xy 184.0103 72.4027) (xy 184.0357 76.2635) (xy 181.8386 76.3143) (xy 181.8386 78.8797)
        (xy 178.5112 78.8797) (xy 177.8635 79.5147) (xy 177.8762 83.5533) (xy 173.355 83.5406) (xy 173.3423 97.4598)
        (xy 171.0817 99.6569) (xy 171.1071 103.7717) (xy 165.0238 98.0694) (xy 158.1785 91.3384) (xy 163.6268 85.8774)
        (xy 163.703 82.9437)
      )
    )
  )
  (zone (net 64) (net_name "Net-(3OIKMG1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.9604 72.4027) (xy 190.5 72.39) (xy 190.6143 107.9373) (xy 115.0493 107.9373)
      )
    )
  )
  (zone (net 64) (net_name "Net-(3OIKMG1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.1627 98.7171) (xy 184.1373 107.9881) (xy 176.784 107.9881) (xy 176.7332 98.7171)
      )
    )
  )
)
