<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<text>THIS PCB DESIGNED FOR:</text>
<text>Sarah Blog</text>
<circle x="124.659" y="90.4875" radius="2.2479" width="0.0254" layer="20"/>
<circle x="124.659" y="49.2125" radius="2.2479" width="0.0254" layer="20"/>
<circle x="31.75" y="120.142" radius="3.3782" width="0.0254" layer="20"/>
<circle x="31.75" y="19.558" radius="3.3782" width="0.0254" layer="20"/>
<circle x="9.525" y="130.175" radius="2.2479" width="0.0254" layer="20"/>
<circle x="9.525" y="9.525" radius="2.2479" width="0.0254" layer="20"/>
<circle x="155.575" y="130.175" radius="2.2479" width="0.0254" layer="20"/>
<circle x="155.575" y="9.525" radius="2.2479" width="0.0254" layer="20"/>
<wire x1="0" y1="81.28" x2="0" y2="139.7" width="0" layer="20"/>
<wire x1="0" y1="81.28" x2="19.05" y2="81.28" width="0" layer="20"/>
<wire x1="19.05" y1="58.42" x2="0" y2="58.42" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="58.42" width="0" layer="20"/>
<wire x1="0" y1="139.7" x2="165.1" y2="139.7" width="0" layer="20"/>
<wire x1="165.1" y1="139.7" x2="165.1" y2="82.55" width="0" layer="20"/>
<wire x1="165.1" y1="82.55" x2="228.6" y2="82.55" width="0" layer="20"/>
<wire x1="228.6" y1="82.55" x2="228.6" y2="57.15" width="0" layer="20"/>
<wire x1="228.6" y1="57.15" x2="165.1" y2="57.15" width="0" layer="20"/>
<wire x1="165.1" y1="57.15" x2="165.1" y2="0" width="0" layer="20"/>
<wire x1="165.1" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="58.42" x2="19.05" y2="81.28" width="0" layer="20"/>
<hole x="31.776846875" y="120.15581875" drill="6.7564"/>
<hole x="31.776846875" y="19.525309375" drill="6.7564"/>
<hole x="9.546690625" y="9.55784375" drill="4.4958"/>
<hole x="155.61106875" y="9.55784375" drill="4.4958"/>
<hole x="124.65250625" y="90.5264875" drill="4.4958"/>
<hole x="124.65250625" y="49.1546375" drill="4.4958"/>
<hole x="155.61106875" y="130.123284375" drill="4.4958"/>
<hole x="9.546690625" y="130.123284375" drill="4.4958"/>
<hole x="7.874" y="86.995" drill="5.1054"/>
<hole x="7.874" y="52.705" drill="5.1054"/>
</plain>
<libraries>
<library name="CONRADS">
<packages>
<package name="CONRADSNEW_V1G">
</package>
<package name="SLIMMOX102">
</package>
<package name="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES">
</package>
<package name="CONN5_1814832-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="CONRADS" package="CONRADSNEW_V1G" value="V1G"/>
<element name="R1" library="CONRADS" package="SLIMMOX102" value="OHMITE_SLIMMOX102"/>
<element name="R2" library="CONRADS" package="SLIMMOX102" value="OHMITE_SLIMMOX102"/>
<element name="R3" library="CONRADS" package="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES" value="TFSF_FLAT_RESISTOR"/>
<element name="R4" library="CONRADS" package="CONRADSNEW_OHMITE-TFSF(FLAT)-SERIES" value="TFSF_FLAT_RESISTOR"/>
<element name="U1" library="CONRADS" package="CONN5_1814832-1" value="5-1814832-1">
<attribute name="MANUFACTURER_PART_NUMBER" value="518148321"/>
<attribute name="VENDOR" value="TE Connectivity"/>
</element>
</elements>
<signals>
<signal name="HOT">
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="SWITCH_HOT">
<contactref element="R3" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="LV"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="CVR_GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
