<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="92.71" y1="33.655" x2="0" y2="33.655" width="0" layer="20"/>
<wire x1="0" y1="33.655" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="92.71" y2="0.01" width="0" layer="20"/>
<wire x1="92.71" y1="0.01" x2="92.71" y2="33.655" width="0" layer="20"/>
<text>ControllerPro v0.6</text>
<text>By Joel Bradshaw</text>
<text>2015-09-09</text>
<text>1</text>
<text>2</text>
<text>4</text>
<text>3</text>
<text>BlueSMiRF</text>
<text>4</text>
</plain>
<libraries>
<library name="custom">
<packages>
<package name="NINTENDO-MULTI">
</package>
<package name="TEENSY_MC_BT_PINS">
</package>
<package name="RN42">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PORT3" library="custom" package="NINTENDO-MULTI" value="NINTENDO-MULTI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORT4" library="custom" package="NINTENDO-MULTI" value="NINTENDO-MULTI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORT1" library="custom" package="NINTENDO-MULTI" value="NINTENDO-MULTI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORT2" library="custom" package="NINTENDO-MULTI" value="NINTENDO-MULTI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY2.0" library="custom" package="TEENSY_MC_BT_PINS" value="TEENSY_MC_BT_PINS">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$1" library="custom" package="RN42" value="RN42"/>
</elements>
<signals>
<signal name="CLOCK">
<contactref element="PORT3" pad="2"/>
<contactref element="PORT4" pad="2"/>
<contactref element="PORT2" pad="2"/>
<contactref element="PORT1" pad="2"/>
<contactref element="TEENSY2.0" pad="D7"/>
</signal>
<signal name="LATCH">
<contactref element="PORT3" pad="3"/>
<contactref element="PORT4" pad="3"/>
<contactref element="PORT2" pad="3"/>
<contactref element="PORT1" pad="3"/>
<contactref element="TEENSY2.0" pad="D6"/>
</signal>
<signal name="VCC">
<contactref element="PORT3" pad="10"/>
<contactref element="PORT2" pad="10"/>
<contactref element="PORT1" pad="10"/>
<contactref element="PORT4" pad="10"/>
<contactref element="TEENSY2.0" pad="+5V"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="PORT3" pad="5"/>
<contactref element="PORT4" pad="5"/>
<contactref element="PORT2" pad="5"/>
<contactref element="PORT1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="PORT4" pad="7"/>
<contactref element="PORT2" pad="7"/>
<contactref element="PORT3" pad="7"/>
<contactref element="PORT1" pad="7"/>
<contactref element="TEENSY2.0" pad="GND"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="5VDATA0">
<contactref element="TEENSY2.0" pad="B2"/>
<contactref element="PORT3" pad="4"/>
</signal>
<signal name="5VDATA1">
<contactref element="TEENSY2.0" pad="B3"/>
<contactref element="PORT4" pad="4"/>
</signal>
<signal name="5VDATA2">
<contactref element="TEENSY2.0" pad="B0"/>
<contactref element="PORT1" pad="4"/>
</signal>
<signal name="5VDATA3">
<contactref element="TEENSY2.0" pad="B1"/>
<contactref element="PORT2" pad="4"/>
</signal>
<signal name="S_OR_NES0">
<contactref element="PORT3" pad="1"/>
<contactref element="TEENSY2.0" pad="F6"/>
</signal>
<signal name="S_OR_NES1">
<contactref element="PORT4" pad="1"/>
<contactref element="TEENSY2.0" pad="F7"/>
</signal>
<signal name="S_OR_NES2">
<contactref element="PORT1" pad="1"/>
<contactref element="TEENSY2.0" pad="F4"/>
</signal>
<signal name="S_OR_NES3">
<contactref element="PORT2" pad="1"/>
<contactref element="TEENSY2.0" pad="F5"/>
</signal>
<signal name="3VDATA0">
<contactref element="TEENSY2.0" pad="B6"/>
<contactref element="PORT3" pad="6"/>
</signal>
<signal name="3VDATA1">
<contactref element="TEENSY2.0" pad="B7"/>
<contactref element="PORT4" pad="6"/>
</signal>
<signal name="3VDATA2">
<contactref element="TEENSY2.0" pad="B4"/>
<contactref element="PORT1" pad="6"/>
</signal>
<signal name="3VDATA3">
<contactref element="TEENSY2.0" pad="B5"/>
<contactref element="PORT2" pad="6"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$13">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="TEENSY2.0" pad="D2"/>
<contactref element="U$1" pad="TX-0"/>
</signal>
<signal name="N$5">
<contactref element="TEENSY2.0" pad="D3"/>
<contactref element="U$1" pad="RX-I"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="CTS-I"/>
<contactref element="U$1" pad="RTS-0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
