(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/VD4")
  (net 2 "/VD3")
  (net 3 "/VD2")
  (net 4 "/VD1")
  (net 5 "/VD0")
  (net 6 "VCC")
  (net 7 "GND")
  (net 8 "unconnected-(U1-VMA-Pad19)")
  (net 9 "unconnected-(U1-E-Pad20)")
  (net 10 "unconnected-(U1-FC2-Pad26)")
  (net 11 "/VA1")
  (net 12 "/VA2")
  (net 13 "/VA3")
  (net 14 "/VA4")
  (net 15 "/VA5")
  (net 16 "/VA6")
  (net 17 "/VA7")
  (net 18 "/VA8")
  (net 19 "/VA9")
  (net 20 "/VA10")
  (net 21 "/VA11")
  (net 22 "/VA12")
  (net 23 "/VA13")
  (net 24 "/VA14")
  (net 25 "/VA15")
  (net 26 "/VA16")
  (net 27 "/VA17")
  (net 28 "/VA18")
  (net 29 "/VA19")
  (net 30 "/VA20")
  (net 31 "/VA21")
  (net 32 "/VA22")
  (net 33 "/VA23")
  (net 34 "/VD15")
  (net 35 "/VD14")
  (net 36 "/VD13")
  (net 37 "/VD12")
  (net 38 "/VD11")
  (net 39 "/VD10")
  (net 40 "/VD9")
  (net 41 "/VD8")
  (net 42 "/VD7")
  (net 43 "/VD6")
  (net 44 "/VD5")
  (net 45 "/~{ZRES}")
  (net 46 "Net-(U4-~{ZBR})")
  (net 47 "unconnected-(U6-~{HALT}-Pad18)")
  (net 48 "/ZCLK")
  (net 49 "unconnected-(U6-~{RFSH}-Pad28)")
  (net 50 "unconnected-(U8-~{SE1}-Pad9)")
  (net 51 "unconnected-(U8-~{WE1}-Pad14)")
  (net 52 "unconnected-(U8-RD0-Pad18)")
  (net 53 "unconnected-(U8-RD1-Pad19)")
  (net 54 "unconnected-(U8-RD2-Pad20)")
  (net 55 "unconnected-(U8-RD3-Pad21)")
  (net 56 "unconnected-(U8-RD4-Pad22)")
  (net 57 "unconnected-(U8-RD5-Pad23)")
  (net 58 "unconnected-(U8-RD6-Pad24)")
  (net 59 "unconnected-(U8-RD7-Pad25)")
  (net 60 "/~{DTAK}")
  (net 61 "/~{HL}")
  (net 62 "/~{CE0}")
  (net 63 "/~{M3}")
  (net 64 "/EDCK")
  (net 65 "unconnected-(U8-RA0-Pad120)")
  (net 66 "unconnected-(U8-RA1-Pad121)")
  (net 67 "unconnected-(U8-RA2-Pad122)")
  (net 68 "unconnected-(U8-RA3-Pad123)")
  (net 69 "unconnected-(U8-RA4-Pad124)")
  (net 70 "unconnected-(U8-RA5-Pad125)")
  (net 71 "unconnected-(U8-RA6-Pad126)")
  (net 72 "unconnected-(U8-RA7-Pad127)")
  (net 73 "Net-(U4-~{WAIT})")
  (net 74 "/~{HSYNC}")
  (net 75 "/~{INTAK}")
  (net 76 "/~{VSYNC}")
  (net 77 "/~{MREQ}")
  (net 78 "Net-(J11-Pin_1)")
  (net 79 "Net-(J11-Pin_2)")
  (net 80 "Net-(EM4-Pad3)")
  (net 81 "Net-(EM5-Pad3)")
  (net 82 "Net-(EM11-Pad3)")
  (net 83 "Net-(EM12-Pad3)")
  (net 84 "Net-(EM13-Pad3)")
  (net 85 "Net-(EM16-Pad3)")
  (net 86 "Net-(EM21-Pad3)")
  (net 87 "Net-(EM22-Pad3)")
  (net 88 "Net-(EM23-Pad3)")
  (net 89 "Net-(EM24-Pad3)")
  (net 90 "PA6")
  (net 91 "/ZD1")
  (net 92 "/ZD0")
  (net 93 "/ZD2")
  (net 94 "/ZD6")
  (net 95 "/ZD5")
  (net 96 "/ZD3")
  (net 97 "/ZD4")
  (net 98 "/ZA15")
  (net 99 "/ZA14")
  (net 100 "/ZA13")
  (net 101 "/ZA12")
  (net 102 "/ZA11")
  (net 103 "/ZA10")
  (net 104 "/ZA9")
  (net 105 "/ZA8")
  (net 106 "/ZA7")
  (net 107 "/ZA6")
  (net 108 "/ZA5")
  (net 109 "/ZA4")
  (net 110 "/ZA3")
  (net 111 "/ZD7")
  (net 112 "/ZA0")
  (net 113 "/ZA1")
  (net 114 "/ZA2")
  (net 115 "PA3")
  (net 116 "PA0")
  (net 117 "PA1")
  (net 118 "PA2")
  (net 119 "PA4")
  (net 120 "PA5")
  (net 121 "/SD0")
  (net 122 "/SD1")
  (net 123 "/SD2")
  (net 124 "/SD3")
  (net 125 "/SD4")
  (net 126 "/SD5")
  (net 127 "/SD6")
  (net 128 "/SD7")
  (net 129 "/A0")
  (net 130 "/A1")
  (net 131 "/A2")
  (net 132 "/A3")
  (net 133 "/A4")
  (net 134 "/A7")
  (net 135 "Net-(EM8-Pad3)")
  (net 136 "Net-(U13-R_IN)")
  (net 137 "Net-(U13-G_IN)")
  (net 138 "Net-(J5-Pad7)")
  (net 139 "PB4")
  (net 140 "PB6")
  (net 141 "PB0")
  (net 142 "PB1")
  (net 143 "PB2")
  (net 144 "PB3")
  (net 145 "PB5")
  (net 146 "Net-(EM7-Pad3)")
  (net 147 "Net-(J5-Pad9)")
  (net 148 "/A5")
  (net 149 "/A6")
  (net 150 "Net-(EM25-Pad3)")
  (net 151 "Net-(EM26-Pad3)")
  (net 152 "Net-(EM27-Pad3)")
  (net 153 "Net-(EM28-Pad3)")
  (net 154 "Net-(J6-Pad7)")
  (net 155 "Net-(J6-Pad9)")
  (net 156 "Net-(FB3-Pad1)")
  (net 157 "Net-(FB4-Pad1)")
  (net 158 "/~{ROM}")
  (net 159 "/~{OE0}")
  (net 160 "/~{FDC}")
  (net 161 "Net-(U4-EDCK)")
  (net 162 "/~{IREQ}")
  (net 163 "/~{YS}")
  (net 164 "Net-(C25-Pad1)")
  (net 165 "/~{VDPM}")
  (net 166 "Net-(U13-B_IN)")
  (net 167 "Net-(C26-Pad1)")
  (net 168 "Net-(U1-HALT)")
  (net 169 "Net-(U1-VPA)")
  (net 170 "Net-(FB5-Pad1)")
  (net 171 "Net-(EM31-Pad3)")
  (net 172 "Net-(EM32-Pad3)")
  (net 173 "Net-(EM33-Pad3)")
  (net 174 "Net-(EM34-Pad3)")
  (net 175 "Net-(EM35-Pad3)")
  (net 176 "Net-(EM36-Pad3)")
  (net 177 "PC0")
  (net 178 "PC1")
  (net 179 "PC2")
  (net 180 "PC3")
  (net 181 "PC4")
  (net 182 "PC6")
  (net 183 "Net-(EM37-Pad3)")
  (net 184 "PC5")
  (net 185 "Net-(EM38-Pad3)")
  (net 186 "unconnected-(J2-Pin_a2-Pada2)")
  (net 187 "/~{FDHR}")
  (net 188 "/~{CAS2}")
  (net 189 "/~{RAS2}")
  (net 190 "unconnected-(J2-Pin_a27-Pada27)")
  (net 191 "Net-(U13-XO_IN)")
  (net 192 "Net-(C27-Pad1)")
  (net 193 "Net-(U13-AUDIO_OUT)")
  (net 194 "VDDA")
  (net 195 "/FRES")
  (net 196 "/~{ZRD}")
  (net 197 "unconnected-(J2-Pin_b25-Padb25)")
  (net 198 "unconnected-(J2-Pin_b27-Padb27)")
  (net 199 "Net-(SW1-B)")
  (net 200 "unconnected-(SW1-C-Pad3)")
  (net 201 "unconnected-(U11-IRQ-Pad13)")
  (net 202 "/~{SOUND}")
  (net 203 "/VCLK")
  (net 204 "/~{ZWR}")
  (net 205 "MCLK")
  (net 206 "Net-(OSC1-Vcontrol)")
  (net 207 "Net-(OSC1-OUT)")
  (net 208 "Net-(C92-Pad2)")
  (net 209 "Net-(FB8-Pad1)")
  (net 210 "Net-(FB10-Pad1)")
  (net 211 "VCCQ")
  (net 212 "Net-(C32-Pad2)")
  (net 213 "Net-(U13-G_OUT)")
  (net 214 "Net-(U13-R_OUT)")
  (net 215 "unconnected-(U11-NC-Pad10)")
  (net 216 "+9V")
  (net 217 "Net-(U13-B_OUT)")
  (net 218 "/~{AS}")
  (net 219 "/~{UDS}")
  (net 220 "/~{LDS}")
  (net 221 "/~{R{slash}W}")
  (net 222 "/FC1")
  (net 223 "/FC0")
  (net 224 "/BG")
  (net 225 "/BGACK")
  (net 226 "/BR")
  (net 227 "/IPL2")
  (net 228 "/IPL1")
  (net 229 "/~{RAS0}")
  (net 230 "/~{LWR}")
  (net 231 "/~{UWR}")
  (net 232 "+9VA")
  (net 233 "/~{JAP}")
  (net 234 "Net-(C31-Pad1)")
  (net 235 "Net-(U13-C_VIDEO_OUT)")
  (net 236 "Net-(C32-Pad1)")
  (net 237 "Net-(U10-~{RAS})")
  (net 238 "Net-(U10-~{CAS})")
  (net 239 "Net-(U10-~{WB}{slash}~{WE})")
  (net 240 "Net-(U10-~{SE})")
  (net 241 "Net-(U10-SC)")
  (net 242 "Net-(U10-~{DT}{slash}~{OE})")
  (net 243 "Net-(RF1-VIDEO)")
  (net 244 "Net-(RF1-+B)")
  (net 245 "Net-(RF1-AUDIO)")
  (net 246 "Net-(J10-Pin_2)")
  (net 247 "Net-(J10-Pin_1)")
  (net 248 "Net-(J110-Pin_2)")
  (net 249 "/AudioShield")
  (net 250 "Net-(J10-Pin_4)")
  (net 251 "Net-(J110-Pin_4)")
  (net 252 "unconnected-(J10-Pin_3-Pad3)")
  (net 253 "unconnected-(J110-Pin_3-Pad3)")
  (net 254 "Net-(U4-~{WRES})")
  (net 255 "/SL1")
  (net 256 "unconnected-(U13-XO_OUT-Pad5)")
  (net 257 "/iA14")
  (net 258 "Net-(U8-R)")
  (net 259 "Net-(U8-G)")
  (net 260 "Net-(U8-B)")
  (net 261 "Net-(U8-SBCR)")
  (net 262 "Net-(C28-Pad2)")
  (net 263 "Net-(J9-Pin_1)")
  (net 264 "/~{ASEL}")
  (net 265 "/~{VRES}")
  (net 266 "/~{TIME}")
  (net 267 "/~{CART}")
  (net 268 "/~{DISK}")
  (net 269 "Net-(U13-AUDIO_IN)")
  (net 270 "unconnected-(U13-C_SYNC_OUT-Pad11)")
  (net 271 "Net-(C30-Pad2)")
  (net 272 "Net-(U12-EQ_OUT_(A))")
  (net 273 "/~{SRES}")
  (net 274 "/NTSC")
  (net 275 "/~{CAS0}")
  (net 276 "Net-(U12-EQ_OUT_(B))")
  (net 277 "Net-(U11-MOL)")
  (net 278 "Net-(U11-MOR)")
  (net 279 "Net-(C43-Pad2)")
  (net 280 "Net-(C41-Pad2)")
  (net 281 "Net-(U12-IN_(A))")
  (net 282 "Net-(U14A--)")
  (net 283 "Net-(U12-VOL_IN)")
  (net 284 "Net-(R58-Pad1)")
  (net 285 "Net-(U12-NF_(A))")
  (net 286 "Net-(U12-NF_(B))")
  (net 287 "Net-(U12-Vreg)")
  (net 288 "Net-(U12-OUT_(A))")
  (net 289 "Net-(C50-Pad2)")
  (net 290 "Net-(U12-OUT_(B))")
  (net 291 "Net-(C51-Pad2)")
  (net 292 "Net-(U8-SOUND)")
  (net 293 "Net-(C40-Pad1)")
  (net 294 "Net-(U12-EQ_IN_(B))")
  (net 295 "/~{MRES}")
  (net 296 "/~{INT}")
  (net 297 "/~{EOE}")
  (net 298 "/~{NOE}")
  (net 299 "Net-(U12-EQ_IN_(A))")
  (net 300 "Net-(C61-Pad1)")
  (net 301 "Net-(C42-Pad1)")
  (net 302 "Net-(C44-Pad1)")
  (net 303 "/SL2")
  (net 304 "/SR2")
  (net 305 "/SR1")
  (net 306 "Net-(C62-Pad1)")
  (net 307 "Net-(U8-CLK0)")
  (net 308 "/~{M1}")
  (net 309 "/VREF")
  (net 310 "Net-(U14B-+)")
  (net 311 "Net-(U13-I_REF)")
  (net 312 "Net-(U13-C_SYNC_IN)")
  (net 313 "Net-(U13-Y_OUT)")
  (net 314 "Net-(U13-Y_IN)")
  (net 315 "Net-(C86-Pad1)")
  (net 316 "Net-(C86-Pad2)")
  (net 317 "Net-(C87-Pad1)")
  (net 318 "/~{ZRAM}")
  (net 319 "/~{REF}")
  (net 320 "/~{ZBAK}")
  (net 321 "/~{NMI}")
  (net 322 "Net-(C35-Pad2)")
  (net 323 "Net-(U13-CHROMA_IN)")
  (net 324 "Net-(C33-Pad2)")
  (net 325 "Net-(C37-Pad1)")
  (net 326 "Net-(C96-Pad1)")
  (net 327 "Net-(U13-CHROMA_OUT)")
  (net 328 "Net-(FB9-Pad1)")
  (net 329 "Net-(U8-SPA{slash}B)")
  (net 330 "Net-(U8-CLK1)")
  (net 331 "/DCin1")
  (net 332 "/DCin2")
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 84.408 171.577)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C40" (at 7.413 2.921) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 293 "Net-(C40-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 292 "Net-(U8-SOUND)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 63.373 64.469 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C63" (at 2.5 -3.5 -90) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 58.881 92.837)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C74" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 170.815 182.601 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 263 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 60.706 44.069 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB13" (at -3.937 0.508 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 243 "Net-(RF1-VIDEO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 316 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (at 222.4028 203.6596)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "9-pin male plug pin D-SUB connector")
    (property "ki_keywords" "connector male plug D-SUB DB9")
    (attr through_hole)
    (fp_text reference "J6" (at 5.54 -2.8) (layer "F.SilkS"))
    (fp_text value "Player2" (at 5.54 18.44) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.54 13.94) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -6.96 1.42) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "0" thru_hole circle (at 18.04 1.42) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(EM21-Pad3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.77 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(EM22-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.54 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(EM23-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 8.31 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(EM24-Pad3)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 11.08 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(EM25-Pad3)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 1.385 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 151 "Net-(EM26-Pad3)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 4.155 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 154 "Net-(J6-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 6.925 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 157 "Net-(FB4-Pad1)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 9.695 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 155 "Net-(J6-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 246.507 152.039)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, open")
    (property "ki_keywords" "Jumper SPST")
    (attr through_hole)
    (fp_text reference "JP1" (at 8.636 -0.02) (layer "F.SilkS"))
    (fp_text value "JAP" (at 11.557 -0.02) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 233 "/~{JAP}") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 51.054 128.223 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C79" (at 2.5 -3.5 -90) (layer "F.SilkS"))
    (fp_text value "100uF 16V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 42.291 163.449)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 3.937 1.524 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(J11-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(J11-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 239.141 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM28" (at -4.953 -0.254 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 145 "PB5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 153 "Net-(EM28-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite_THT:LairdTech_28C0236-0JW-10" (layer "F.Cu")
    (at 139.446 146.558 180)
    (descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
    (tags "Ferrite vertical LairdTech 28C0236-0JW-10")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB6" (at 2.54 -4.064) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 4.953) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 207 "Net-(OSC1-OUT)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 180) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 205 "MCLK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (at 263.779 45.212 180)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J110" (at 0 9.906 270) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 8.06 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 249 "/AudioShield") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 248 "Net-(J110-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 253 "unconnected-(J110-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 251 "Net-(J110-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite_THT:LairdTech_28C0236-0JW-10" (layer "F.Cu")
    (at 61.976 198.628 90)
    (descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
    (tags "Ferrite vertical LairdTech 28C0236-0JW-10")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB12" (at 8.509 -1.397 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 4.953 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 246 "Net-(J10-Pin_2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 291 "Net-(C51-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 68.072 92.837 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L3" (at 2.54 -1.92 90) (layer "F.SilkS"))
    (fp_text value "100uH" (at 2.54 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 322 "Net-(C35-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 314 "Net-(U13-Y_IN)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4mm" (layer "F.Cu")
    (at 42.037 209.423)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 5.969 -2.032) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 63.754 103.077 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C30" (at 6.016 -3.302 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.016 -3.048 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 269 "Net-(U13-AUDIO_IN)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 271 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:PQFP-160_28x28mm_P0.65mm" (layer "F.Cu")
    (at 202.173 117.239)
    (descr "PQFP, 160 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "PQFP QFP")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at -1.1574 -18.7886) (layer "F.SilkS"))
    (fp_text value "315-5402" (at 3.44 -0.272 270 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -15.125 -12.675) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "2" smd roundrect (at -15.125 -12.025) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "MCLK") (pinfunction "MCLK") (pintype "unspecified"))
    (pad "3" smd roundrect (at -15.125 -11.375) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 267 "/~{CART}") (pinfunction "~{CART}") (pintype "unspecified"))
    (pad "4" smd roundrect (at -15.125 -10.725) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 318 "/~{ZRAM}") (pinfunction "~{ZRAM}") (pintype "unspecified"))
    (pad "5" smd roundrect (at -15.125 -10.075) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 319 "/~{REF}") (pinfunction "~{RAF}") (pintype "unspecified"))
    (pad "6" smd roundrect (at -15.125 -9.425) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 308 "/~{M1}") (pinfunction "~{MI}") (pintype "unspecified"))
    (pad "7" smd roundrect (at -15.125 -8.775) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/~{ZRES}") (pinfunction "~{ZRES}") (pintype "unspecified"))
    (pad "8" smd roundrect (at -15.125 -8.125) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(U4-~{ZBR})") (pinfunction "~{ZBR}") (pintype "unspecified"))
    (pad "9" smd roundrect (at -15.125 -7.475) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(U4-~{WAIT})") (pinfunction "~{WAIT}") (pintype "unspecified"))
    (pad "10" smd roundrect (at -15.125 -6.825) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 320 "/~{ZBAK}") (pinfunction "~{ZBAR}") (pintype "unspecified"))
    (pad "11" smd roundrect (at -15.125 -6.175) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 204 "/~{ZWR}") (pinfunction "~{EWR}") (pintype "unspecified"))
    (pad "12" smd roundrect (at -15.125 -5.525) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 196 "/~{ZRD}") (pinfunction "~{ERD}") (pintype "unspecified"))
    (pad "13" smd roundrect (at -15.125 -4.875) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "/~{IREQ}") (pinfunction "~{TREQ}") (pintype "unspecified"))
    (pad "14" smd roundrect (at -15.125 -4.225) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/~{MREQ}") (pinfunction "~{MREQ}") (pintype "unspecified"))
    (pad "15" smd roundrect (at -15.125 -3.575) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 321 "/~{NMI}") (pinfunction "~{NMI}") (pintype "unspecified"))
    (pad "16" smd roundrect (at -15.125 -2.925) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/ZD1") (pinfunction "ZD1") (pintype "unspecified"))
    (pad "17" smd roundrect (at -15.125 -2.275) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/ZD0") (pinfunction "ZD0") (pintype "unspecified"))
    (pad "18" smd roundrect (at -15.125 -1.625) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/ZD7") (pinfunction "ZD7") (pintype "unspecified"))
    (pad "19" smd roundrect (at -15.125 -0.975) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "20" smd roundrect (at -15.125 -0.325) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "21" smd roundrect (at -15.125 0.325) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "22" smd roundrect (at -15.125 0.975) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/ZCLK") (pinfunction "ZCLK") (pintype "unspecified"))
    (pad "23" smd roundrect (at -15.125 1.625) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 254 "Net-(U4-~{WRES})") (pinfunction "~{WRES}") (pintype "unspecified"))
    (pad "24" smd roundrect (at -15.125 2.275) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "/ZD2") (pinfunction "ZD2") (pintype "unspecified"))
    (pad "25" smd roundrect (at -15.125 2.925) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/ZD6") (pinfunction "ZD6") (pintype "unspecified"))
    (pad "26" smd roundrect (at -15.125 3.575) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "/ZD5") (pinfunction "ZD5") (pintype "unspecified"))
    (pad "27" smd roundrect (at -15.125 4.225) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "/ZD3") (pinfunction "ZD3") (pintype "unspecified"))
    (pad "28" smd roundrect (at -15.125 4.875) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "/ZD4") (pinfunction "ZD4") (pintype "unspecified"))
    (pad "29" smd roundrect (at -15.125 5.525) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/ZA15") (pinfunction "ZA15") (pintype "unspecified"))
    (pad "30" smd roundrect (at -15.125 6.175) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/ZA14") (pinfunction "ZA14") (pintype "unspecified"))
    (pad "31" smd roundrect (at -15.125 6.825) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/ZA13") (pinfunction "ZA13") (pintype "unspecified"))
    (pad "32" smd roundrect (at -15.125 7.475) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "/ZA12") (pinfunction "ZA12") (pintype "unspecified"))
    (pad "33" smd roundrect (at -15.125 8.125) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "/ZA11") (pinfunction "ZA11") (pintype "unspecified"))
    (pad "34" smd roundrect (at -15.125 8.775) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/ZA10") (pinfunction "ZA10") (pintype "unspecified"))
    (pad "35" smd roundrect (at -15.125 9.425) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "/ZA9") (pinfunction "ZA9") (pintype "unspecified"))
    (pad "36" smd roundrect (at -15.125 10.075) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "/ZA8") (pinfunction "ZA8") (pintype "unspecified"))
    (pad "37" smd roundrect (at -15.125 10.725) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/ZA7") (pinfunction "ZA7") (pintype "unspecified"))
    (pad "38" smd roundrect (at -15.125 11.375) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "/ZA6") (pinfunction "ZA6") (pintype "unspecified"))
    (pad "39" smd roundrect (at -15.125 12.025) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/ZA5") (pinfunction "ZA5") (pintype "unspecified"))
    (pad "40" smd roundrect (at -15.125 12.675) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "41" smd roundrect (at -12.675 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "42" smd roundrect (at -12.025 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "43" smd roundrect (at -11.375 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/ZA4") (pinfunction "ZA4") (pintype "unspecified"))
    (pad "44" smd roundrect (at -10.725 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/ZA3") (pinfunction "ZA3") (pintype "unspecified"))
    (pad "45" smd roundrect (at -10.075 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "/ZA2") (pinfunction "ZA2") (pintype "unspecified"))
    (pad "46" smd roundrect (at -9.425 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/ZA1") (pinfunction "ZA1") (pintype "unspecified"))
    (pad "47" smd roundrect (at -8.775 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/ZA0") (pinfunction "ZA0") (pintype "unspecified"))
    (pad "48" smd roundrect (at -8.125 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "PA4") (pinfunction "PA4") (pintype "unspecified"))
    (pad "49" smd roundrect (at -7.475 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "PA6") (pinfunction "PA6") (pintype "unspecified"))
    (pad "50" smd roundrect (at -6.825 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "PA0") (pinfunction "PA0") (pintype "unspecified"))
    (pad "51" smd roundrect (at -6.175 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "PA1") (pinfunction "PA1") (pintype "unspecified"))
    (pad "52" smd roundrect (at -5.525 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "PA2") (pinfunction "PA2") (pintype "unspecified"))
    (pad "53" smd roundrect (at -4.875 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "PA3") (pinfunction "PA3") (pintype "unspecified"))
    (pad "54" smd roundrect (at -4.225 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "PA5") (pinfunction "PA5") (pintype "unspecified"))
    (pad "55" smd roundrect (at -3.575 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "PB4") (pinfunction "PB4") (pintype "unspecified"))
    (pad "56" smd roundrect (at -2.925 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "PB6") (pinfunction "PB6") (pintype "unspecified"))
    (pad "57" smd roundrect (at -2.275 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "PB0") (pinfunction "PB0") (pintype "unspecified"))
    (pad "58" smd roundrect (at -1.625 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "PB1") (pinfunction "PB1") (pintype "unspecified"))
    (pad "59" smd roundrect (at -0.975 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "PB2") (pinfunction "PB2") (pintype "unspecified"))
    (pad "60" smd roundrect (at -0.325 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "PB3") (pinfunction "PB3") (pintype "unspecified"))
    (pad "61" smd roundrect (at 0.325 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "PB5") (pinfunction "PB5") (pintype "unspecified"))
    (pad "62" smd roundrect (at 0.975 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 177 "PC0") (pinfunction "PC0") (pintype "unspecified"))
    (pad "63" smd roundrect (at 1.625 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "PC1") (pinfunction "PC1") (pintype "unspecified"))
    (pad "64" smd roundrect (at 2.275 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "PC2") (pinfunction "PC2") (pintype "unspecified"))
    (pad "65" smd roundrect (at 2.925 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "PC3") (pinfunction "PC3") (pintype "unspecified"))
    (pad "66" smd roundrect (at 3.575 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "PC4") (pinfunction "PC4") (pintype "unspecified"))
    (pad "67" smd roundrect (at 4.225 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "PC5") (pinfunction "PC5") (pintype "unspecified"))
    (pad "68" smd roundrect (at 4.875 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "PC6") (pinfunction "PC6") (pintype "unspecified"))
    (pad "69" smd roundrect (at 5.525 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "~{TEST0}") (pintype "unspecified"))
    (pad "70" smd roundrect (at 6.175 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "~{TEST1}") (pintype "unspecified"))
    (pad "71" smd roundrect (at 6.825 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "~{TEST2}") (pintype "unspecified"))
    (pad "72" smd roundrect (at 7.475 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 233 "/~{JAP}") (pinfunction "~{JAP}") (pintype "unspecified"))
    (pad "73" smd roundrect (at 8.125 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/VA1") (pinfunction "VA1") (pintype "unspecified"))
    (pad "74" smd roundrect (at 8.775 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/VA2") (pinfunction "VA2") (pintype "unspecified"))
    (pad "75" smd roundrect (at 9.425 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/VA3") (pinfunction "VA3") (pintype "unspecified"))
    (pad "76" smd roundrect (at 10.075 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/VA4") (pinfunction "VA4") (pintype "unspecified"))
    (pad "77" smd roundrect (at 10.725 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/VA5") (pinfunction "VA5") (pintype "unspecified"))
    (pad "78" smd roundrect (at 11.375 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/VA6") (pinfunction "VA6") (pintype "unspecified"))
    (pad "79" smd roundrect (at 12.025 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "80" smd roundrect (at 12.675 15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "81" smd roundrect (at 15.125 12.675) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "82" smd roundrect (at 15.125 12.025) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/VA7") (pinfunction "VA7") (pintype "unspecified"))
    (pad "83" smd roundrect (at 15.125 11.375) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/VA8") (pinfunction "VA8") (pintype "unspecified"))
    (pad "84" smd roundrect (at 15.125 10.725) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/VA9") (pinfunction "VA9") (pintype "unspecified"))
    (pad "85" smd roundrect (at 15.125 10.075) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/VA10") (pinfunction "VA10") (pintype "unspecified"))
    (pad "86" smd roundrect (at 15.125 9.425) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/VA11") (pinfunction "VA11") (pintype "unspecified"))
    (pad "87" smd roundrect (at 15.125 8.775) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/VA12") (pinfunction "VA12") (pintype "unspecified"))
    (pad "88" smd roundrect (at 15.125 8.125) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/VA13") (pinfunction "VA13") (pintype "unspecified"))
    (pad "89" smd roundrect (at 15.125 7.475) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/VA14") (pinfunction "VA14") (pintype "unspecified"))
    (pad "90" smd roundrect (at 15.125 6.825) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/VA15") (pinfunction "VA15") (pintype "unspecified"))
    (pad "91" smd roundrect (at 15.125 6.175) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/VA16") (pinfunction "VA16") (pintype "unspecified"))
    (pad "92" smd roundrect (at 15.125 5.525) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/VA17") (pinfunction "VA17") (pintype "unspecified"))
    (pad "93" smd roundrect (at 15.125 4.875) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/VA18") (pinfunction "VA18") (pintype "unspecified"))
    (pad "94" smd roundrect (at 15.125 4.225) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/VA19") (pinfunction "VA19") (pintype "unspecified"))
    (pad "95" smd roundrect (at 15.125 3.575) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/VA20") (pinfunction "VA20") (pintype "unspecified"))
    (pad "96" smd roundrect (at 15.125 2.925) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/VA21") (pinfunction "VA21") (pintype "unspecified"))
    (pad "97" smd roundrect (at 15.125 2.275) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/VA22") (pinfunction "VA22") (pintype "unspecified"))
    (pad "98" smd roundrect (at 15.125 1.625) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/VA23") (pinfunction "VA23") (pintype "unspecified"))
    (pad "99" smd roundrect (at 15.125 0.975) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "100" smd roundrect (at 15.125 0.325) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "101" smd roundrect (at 15.125 -0.325) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/~{HL}") (pintype "unspecified"))
    (pad "102" smd roundrect (at 15.125 -0.975) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "/~{FDHR}") (pintype "unspecified"))
    (pad "103" smd roundrect (at 15.125 -1.625) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "/~{FDC}") (pintype "unspecified"))
    (pad "104" smd roundrect (at 15.125 -2.275) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 268 "/~{DISK}") (pinfunction "~{DISK}") (pintype "unspecified"))
    (pad "105" smd roundrect (at 15.125 -2.925) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 195 "/FRES") (pinfunction "FRES") (pintype "unspecified"))
    (pad "106" smd roundrect (at 15.125 -3.575) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "/~{VDPM}") (pinfunction "~{VDPM}") (pintype "unspecified"))
    (pad "107" smd roundrect (at 15.125 -4.225) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "/~{ROM}") (pinfunction "~{ROM}") (pintype "unspecified"))
    (pad "108" smd roundrect (at 15.125 -4.875) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 264 "/~{ASEL}") (pintype "unspecified"))
    (pad "109" smd roundrect (at 15.125 -5.525) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 266 "/~{TIME}") (pinfunction "~{TIME}") (pintype "unspecified"))
    (pad "110" smd roundrect (at 15.125 -6.175) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "/~{RAS2}") (pinfunction "~{RAS2}") (pintype "unspecified"))
    (pad "111" smd roundrect (at 15.125 -6.825) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "/~{CAS2}") (pinfunction "~{CAS2}") (pintype "unspecified"))
    (pad "112" smd roundrect (at 15.125 -7.475) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "/~{OE0}") (pinfunction "~{OE0}") (pintype "unspecified"))
    (pad "113" smd roundrect (at 15.125 -8.125) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 275 "/~{CAS0}") (pintype "unspecified"))
    (pad "114" smd roundrect (at 15.125 -8.775) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 273 "/~{SRES}") (pinfunction "~{SRES}") (pintype "unspecified"))
    (pad "115" smd roundrect (at 15.125 -9.425) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/~{CE0}") (pinfunction "~{CE0}") (pintype "unspecified"))
    (pad "116" smd roundrect (at 15.125 -10.075) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 230 "/~{LWR}") (pinfunction "~{LWR}") (pintype "unspecified"))
    (pad "117" smd roundrect (at 15.125 -10.725) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 257 "/iA14") (pinfunction "iA14") (pintype "unspecified"))
    (pad "118" smd roundrect (at 15.125 -11.375) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 298 "/~{NOE}") (pinfunction "~{NOE}") (pintype "unspecified"))
    (pad "119" smd roundrect (at 15.125 -12.025) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 297 "/~{EOE}") (pinfunction "~{EOE}") (pintype "unspecified"))
    (pad "120" smd roundrect (at 15.125 -12.675) (size 1.75 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "unspecified"))
    (pad "121" smd roundrect (at 12.675 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "122" smd roundrect (at 12.025 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "123" smd roundrect (at 11.375 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 203 "/VCLK") (pinfunction "VCLK") (pintype "unspecified"))
    (pad "124" smd roundrect (at 10.725 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/~{M3}") (pinfunction "~{M3}") (pintype "unspecified"))
    (pad "125" smd roundrect (at 10.075 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 218 "/~{AS}") (pinfunction "~{AS}") (pintype "unspecified"))
    (pad "126" smd roundrect (at 9.425 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 220 "/~{LDS}") (pinfunction "~{LDS}") (pintype "unspecified"))
    (pad "127" smd roundrect (at 8.775 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 219 "/~{UDS}") (pinfunction "~{UDS}") (pintype "unspecified"))
    (pad "128" smd roundrect (at 8.125 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 221 "/~{R{slash}W}") (pinfunction "R/W") (pintype "unspecified"))
    (pad "129" smd roundrect (at 7.475 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/~{DTAK}") (pinfunction "~{DTAK}") (pintype "unspecified"))
    (pad "130" smd roundrect (at 6.825 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 224 "/BG") (pinfunction "~{BG}") (pintype "unspecified"))
    (pad "131" smd roundrect (at 6.175 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 225 "/BGACK") (pinfunction "~{BGAK}") (pintype "unspecified"))
    (pad "132" smd roundrect (at 5.525 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 226 "/BR") (pinfunction "~{BR}") (pintype "unspecified"))
    (pad "133" smd roundrect (at 4.875 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 168 "Net-(U1-HALT)") (pinfunction "~{HALT}") (pintype "unspecified"))
    (pad "134" smd roundrect (at 4.225 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 265 "/~{VRES}") (pinfunction "~{VRES}") (pintype "unspecified"))
    (pad "135" smd roundrect (at 3.575 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 169 "Net-(U1-VPA)") (pinfunction "~{VPA}") (pintype "unspecified"))
    (pad "136" smd roundrect (at 2.925 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 223 "/FC0") (pinfunction "FC0") (pintype "unspecified"))
    (pad "137" smd roundrect (at 2.275 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 222 "/FC1") (pinfunction "FC1") (pintype "unspecified"))
    (pad "138" smd roundrect (at 1.625 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/VD0") (pinfunction "VD0") (pintype "unspecified"))
    (pad "139" smd roundrect (at 0.975 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/VD1") (pinfunction "VD1") (pintype "unspecified"))
    (pad "140" smd roundrect (at 0.325 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/VD2") (pinfunction "VD2") (pintype "unspecified"))
    (pad "141" smd roundrect (at -0.325 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/VD3") (pinfunction "VD3") (pintype "unspecified"))
    (pad "142" smd roundrect (at -0.975 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/VD4") (pinfunction "VD4") (pintype "unspecified"))
    (pad "143" smd roundrect (at -1.625 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/VD5") (pinfunction "VD5") (pintype "unspecified"))
    (pad "144" smd roundrect (at -2.275 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/VD6") (pinfunction "VD6") (pintype "unspecified"))
    (pad "145" smd roundrect (at -2.925 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/VD7") (pinfunction "VD7") (pintype "unspecified"))
    (pad "146" smd roundrect (at -3.575 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/VD8") (pinfunction "VD8") (pintype "unspecified"))
    (pad "147" smd roundrect (at -4.225 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/VD9") (pinfunction "VD9") (pintype "unspecified"))
    (pad "148" smd roundrect (at -4.875 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/VD10") (pinfunction "VD10") (pintype "unspecified"))
    (pad "149" smd roundrect (at -5.525 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VD11") (pinfunction "VD11") (pintype "unspecified"))
    (pad "150" smd roundrect (at -6.175 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/VD12") (pinfunction "VD12") (pintype "unspecified"))
    (pad "151" smd roundrect (at -6.825 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/VD13") (pinfunction "VD13") (pintype "unspecified"))
    (pad "152" smd roundrect (at -7.475 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/VD14") (pinfunction "VD14") (pintype "unspecified"))
    (pad "153" smd roundrect (at -8.125 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/VD15") (pinfunction "VD15") (pintype "unspecified"))
    (pad "154" smd roundrect (at -8.775 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 274 "/NTSC") (pinfunction "NTSC") (pintype "unspecified"))
    (pad "155" smd roundrect (at -9.425 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/~{HSYNC}") (pinfunction "~{HSYNC}") (pintype "unspecified"))
    (pad "156" smd roundrect (at -10.075 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 202 "/~{SOUND}") (pinfunction "~{SOUND}") (pintype "unspecified"))
    (pad "157" smd roundrect (at -10.725 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/~{INTAK}") (pinfunction "~{INTAR}") (pintype "unspecified"))
    (pad "158" smd roundrect (at -11.375 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "Net-(U4-EDCK)") (pinfunction "EDCK") (pintype "unspecified"))
    (pad "159" smd roundrect (at -12.025 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "160" smd roundrect (at -12.675 -15.125) (size 0.4 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-160_28x28mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (at 79.883 178.562 -90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U12" (at -2.032 8.255 -180) (layer "F.SilkS"))
    (fp_text value "CXA1034P" (at 3.81 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 272 "Net-(U12-EQ_OUT_(A))") (pinfunction "EQ_OUT_(A)") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 299 "Net-(U12-EQ_IN_(A))") (pinfunction "EQ_IN_(A)") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(U12-IN_(A))") (pinfunction "IN_(A)") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND_(2)") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(U12-IN_(A))") (pinfunction "Vref") (pintype "power_in"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(U12-IN_(A))") (pinfunction "IN_(B)") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 294 "Net-(U12-EQ_IN_(B))") (pinfunction "EQ_IN_(B)") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 276 "Net-(U12-EQ_OUT_(B))") (pinfunction "EQ_OUT_(B)") (pintype "output"))
    (pad "9" thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 283 "Net-(U12-VOL_IN)") (pinfunction "VOL_IN") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 286 "Net-(U12-NF_(B))") (pinfunction "NF_(B)") (pintype "unspecified"))
    (pad "11" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 290 "Net-(U12-OUT_(B))") (pinfunction "OUT_(B)") (pintype "output"))
    (pad "12" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "power_in"))
    (pad "13" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND_(1)") (pintype "power_in"))
    (pad "14" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 288 "Net-(U12-OUT_(A))") (pinfunction "OUT_(A)") (pintype "output"))
    (pad "15" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 285 "Net-(U12-NF_(A))") (pinfunction "NF_(A)") (pintype "unspecified"))
    (pad "16" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 287 "Net-(U12-Vreg)") (pinfunction "Vreg") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 86.36 176.991 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C62" (at 3.095 -4.445 90) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 306 "Net-(C62-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 304 "/SR2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 229.87 130.556)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "CP112" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 89.836 147.701 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C41" (at -3.001 -2.032) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 277 "Net-(U11-MOL)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 280 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 123.825 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM33" (at -5.715 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 179 "PC2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 173 "Net-(EM33-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 78.74 190.072 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C53" (at -0.969 -2.667 -90) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 287 "Net-(U12-Vreg)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 75.819 74.676)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C24" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "10uF 10V Tantalum" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.556 0.889) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (at 106.9788 36.2688 180)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "9-pin female receptacle socket D-SUB connector")
    (property "ki_keywords" "connector receptacle female D-SUB DB9")
    (attr through_hole)
    (fp_text reference "J4" (at -5.54 -2.8 180) (layer "F.SilkS"))
    (fp_text value "EXT" (at -5.54 18.61 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.54 14.025 180) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -18.04 1.42 180) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "0" thru_hole circle (at 6.96 1.42 180) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 175 "Net-(EM35-Pad3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 174 "Net-(EM34-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 173 "Net-(EM33-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 172 "Net-(EM32-Pad3)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 171 "Net-(EM31-Pad3)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.385 2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 185 "Net-(EM38-Pad3)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -4.155 2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 170 "Net-(FB5-Pad1)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -6.925 2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 183 "Net-(EM37-Pad3)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -9.695 2.84 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 176 "Net-(EM36-Pad3)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 70.612 69.723 90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C86" (at -4.191 2.921 90) (layer "F.SilkS"))
    (fp_text value "220uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 315 "Net-(C86-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 316 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 56.642 43.942 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB9" (at 2.54 -4.064 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 328 "Net-(FB9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 236 "Net-(C32-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 66.548 101.346 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L7" (at 2.54 -1.92 90) (layer "F.SilkS"))
    (fp_text value "100uH" (at 2.54 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 326 "Net-(C96-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 324 "Net-(C33-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 52.15 158.496)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "220uF 16V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_Tactile_Straight_KSA0Axx1LFTR" (layer "F.Cu")
    (at 69.596 200.533)
    (descr "SW PUSH SMALL http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SW PUSH SMALL Tactile C&K")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW2" (at 2.286 9.652) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.81 7.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 254 "Net-(U4-~{WRES})") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.62 5.08) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask")
      (net 254 "Net-(U4-~{WRES})") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Tactile_Straight_KSA0Axx1LFTR.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite_THT:LairdTech_28C0236-0JW-10" (layer "F.Cu")
    (at 173.609 102.235)
    (descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
    (tags "Ferrite vertical LairdTech 28C0236-0JW-10")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB7" (at 2.54 -4.064) (layer "F.SilkS"))
    (fp_text value "4T Radial" (at 2.54 4.953) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "/EDCK") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 208 "Net-(C92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:HeadphoneVolumeSlider" (layer "F.Cu")
    (at 45.593 165.227)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -5.8674 19.939 90 unlocked) (layer "F.SilkS"))
    (fp_text value "50K" (at 0 -1.5 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.54 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at -2.54 35.56) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 5.08) (size 2.5 2.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 38.1) (size 2.5 2.5) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 283 "Net-(U12-VOL_IN)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 38.1) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 283 "Net-(U12-VOL_IN)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 284 "Net-(R58-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 33.02) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 284 "Net-(R58-Pad1)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 68.119 74.295 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C32" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "220uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.128 -2.032) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 236 "Net-(C32-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 212 "Net-(C32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 231.14 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM24" (at -3.429 0.889 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 144 "PB3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(EM24-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 194.056 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM13" (at -3.683 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 118 "PA2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(EM13-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 111.633 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM38" (at -5.842 -1.143 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 184 "PC5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 185 "Net-(EM38-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 58.293 117.348 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C23" (at 2.54 4.445 -90) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 194 "VDDA") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 184.658 134.874)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID2" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 45.974 43.942)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID6" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 182.118 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM16" (at 1.778 3.683 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 119 "PA4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(EM16-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 235.077 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM25" (at -4.318 2.794 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 150 "Net-(EM25-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:ZIP-24" (layer "F.Cu")
    (at 109.982 62.23)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "65536 Word x 4bit Dynamic RAM")
    (property "ki_keywords" "RAM MEMORY")
    (attr through_hole)
    (fp_text reference "U9" (at -6.35 25.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "M5M4C264L" (at -4.675 25.4 90 unlocked) (layer "F.Fab"))
    (fp_text user "2" (at 1.905 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "24" (at 1.905 38.1 90 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -1.27 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "23" (at -1.27 38.1 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -3.175 25.4 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -1.27 5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 131 "/A2") (pinfunction "W2/IO2") (pintype "tri_state"))
    (pad "2" thru_hole circle (at 1.27 6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 132 "/A3") (pinfunction "W3/IO3") (pintype "tri_state"))
    (pad "3" thru_hole circle (at -1.27 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 240 "Net-(U10-~{SE})") (pinfunction "~{SE}") (pintype "input"))
    (pad "4" thru_hole circle (at 1.27 8.89) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 123 "/SD2") (pinfunction "SIO2") (pintype "tri_state"))
    (pad "5" thru_hole circle (at -1.27 10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 124 "/SD3") (pinfunction "SIO3") (pintype "tri_state"))
    (pad "6" thru_hole circle (at 1.27 11.43) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole circle (at -1.27 12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 241 "Net-(U10-SC)") (pinfunction "SC") (pintype "input"))
    (pad "8" thru_hole circle (at 1.27 13.97) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 121 "/SD0") (pinfunction "SIO0") (pintype "tri_state"))
    (pad "9" thru_hole circle (at -1.27 15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 122 "/SD1") (pinfunction "SIO1") (pintype "tri_state"))
    (pad "10" thru_hole circle (at 1.27 16.51) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 242 "Net-(U10-~{DT}{slash}~{OE})") (pinfunction "~{DT}/~{OE}") (pintype "input"))
    (pad "11" thru_hole circle (at -1.27 17.78) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 129 "/A0") (pinfunction "W0/IO0") (pintype "tri_state"))
    (pad "12" thru_hole circle (at 1.27 19.05) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 130 "/A1") (pinfunction "W1/IO1") (pintype "tri_state"))
    (pad "13" thru_hole circle (at -1.27 20.32) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 239 "Net-(U10-~{WB}{slash}~{WE})") (pinfunction "~{WB}/~{WE}") (pintype "input"))
    (pad "14" thru_hole circle (at 1.27 21.59) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 237 "Net-(U10-~{RAS})") (pinfunction "~{RAS}") (pintype "input"))
    (pad "15" thru_hole circle (at -1.27 22.86) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 149 "/A6") (pinfunction "A5") (pintype "input"))
    (pad "16" thru_hole circle (at 1.27 24.13) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 148 "/A5") (pinfunction "A6") (pintype "input"))
    (pad "17" thru_hole circle (at -1.27 25.4) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 133 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "18" thru_hole circle (at 1.27 26.67) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "19" thru_hole circle (at -1.27 27.94) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 134 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "20" thru_hole circle (at 1.27 29.21) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 132 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "21" thru_hole circle (at -1.27 30.48) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 131 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "22" thru_hole circle (at 1.27 31.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 130 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "23" thru_hole circle (at -1.27 33.02) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 129 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "24" thru_hole circle (at 1.27 34.29) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 238 "Net-(U10-~{CAS})") (pinfunction "~{CAS}") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SIP.3dshapes/SIP-9_21.54x3mm_P2.54mm.wrl"
      (offset (xyz 0 -9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 92.075 138.256 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C43" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.206 -4.191 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 278 "Net-(U11-MOR)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 279 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-24_W15.24mm" (layer "F.Cu")
    (at 57.531 140.97 90)
    (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U11" (at 18.669 21.082 180) (layer "F.SilkS"))
    (fp_text value "YM2612" (at 9.017 9.144 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 13.97 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "/ZD0") (pinfunction "D0") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/ZD1") (pinfunction "D1") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/ZD2") (pinfunction "D2") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "/ZD3") (pinfunction "D3") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 97 "/ZD4") (pinfunction "D4") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "/ZD5") (pinfunction "D5") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "/ZD6") (pinfunction "D6") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 111 "/ZD7") (pinfunction "D7") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 215 "unconnected-(U11-NC-Pad10)") (pinfunction "NC") (pintype "input+no_connect"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "/~{ZRES}") (pinfunction "IC") (pintype "input"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "input"))
    (pad "13" thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 201 "unconnected-(U11-IRQ-Pad13)") (pinfunction "IRQ") (pintype "input+no_connect"))
    (pad "14" thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 202 "/~{SOUND}") (pinfunction "CS") (pintype "input"))
    (pad "15" thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 204 "/~{ZWR}") (pinfunction "WR") (pintype "input"))
    (pad "16" thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 196 "/~{ZRD}") (pinfunction "RD") (pintype "input"))
    (pad "17" thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "/ZA0") (pinfunction "A0") (pintype "input"))
    (pad "18" thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/ZA1") (pinfunction "A1") (pintype "input"))
    (pad "19" thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "AGND") (pintype "input"))
    (pad "20" thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 278 "Net-(U11-MOR)") (pinfunction "MOR") (pintype "input"))
    (pad "21" thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 277 "Net-(U11-MOL)") (pinfunction "MOL") (pintype "input"))
    (pad "22" thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 194 "VDDA") (pinfunction "AVcc") (pintype "input"))
    (pad "23" thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "Vcc") (pintype "input"))
    (pad "24" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 203 "/VCLK") (pinfunction "CLOCK_IN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 252.349 69.676 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C68" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 84.455 69.088)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole exclude_from_bom)
    (fp_text reference "L6" (at 2.54 -2.77) (layer "F.SilkS"))
    (fp_text value "0" (at 2.54 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 244 "Net-(RF1-+B)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 142.16 67.31 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C65" (at 2.5 4.064) (layer "F.SilkS"))
    (fp_text value "47uF 16V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 102.87 49.911 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM37" (at -5.334 0 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 182 "PC6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 183 "Net-(EM37-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:DIP-28_DoubleLast" (layer "F.Cu")
    (at 196.596 182.372 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "256K (32K x 8) Static RAM, 70ns, DIP-28")
    (property "ki_keywords" "RAM SRAM CMOS MEMORY")
    (attr through_hole)
    (fp_text reference "U3" (at 18.415 16.51 180) (layer "F.SilkS"))
    (fp_text value "uPD42832C-15" (at 2.921 17.145 unlocked) (layer "F.SilkS"))
    (fp_text user "15" (at 16.5 33.9 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -0.8 -3.2 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 16.51 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/VA15") (pinfunction "A14") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/VA13") (pinfunction "A12") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/VA8") (pinfunction "A7") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/VA7") (pinfunction "A6") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/VA6") (pinfunction "A5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/VA5") (pinfunction "A4") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/VA4") (pinfunction "A3") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/VA3") (pinfunction "A2") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/VA2") (pinfunction "A1") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/VA1") (pinfunction "A0") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "/VD8") (pinfunction "Q0") (pintype "tri_state"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "/VD9") (pinfunction "Q1") (pintype "tri_state"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "/VD10") (pinfunction "Q2") (pintype "tri_state"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/VD11") (pinfunction "Q3") (pintype "tri_state"))
    (pad "15" thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/VD11") (pinfunction "Q3") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/VD12") (pinfunction "Q4") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/VD12") (pinfunction "Q4") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/VD13") (pinfunction "Q5") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/VD13") (pinfunction "Q5") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/VD14") (pinfunction "Q6") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/VD14") (pinfunction "Q6") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/VD15") (pinfunction "Q7") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/VD15") (pinfunction "Q7") (pintype "tri_state"))
    (pad "20" thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 229 "/~{RAS0}") (pinfunction "~{CS}") (pintype "input"))
    (pad "20" thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 229 "/~{RAS0}") (pinfunction "~{CS}") (pintype "input"))
    (pad "21" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "A10") (pintype "input"))
    (pad "21" thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "A10") (pintype "input"))
    (pad "22" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 297 "/~{EOE}") (pinfunction "~{OE}") (pintype "input"))
    (pad "22" thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 297 "/~{EOE}") (pinfunction "~{OE}") (pintype "input"))
    (pad "23" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "A11") (pintype "input"))
    (pad "23" thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "A11") (pintype "input"))
    (pad "24" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "A9") (pintype "input"))
    (pad "24" thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "A9") (pintype "input"))
    (pad "25" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "A8") (pintype "input"))
    (pad "25" thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "A8") (pintype "input"))
    (pad "26" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/VA14") (pinfunction "A13") (pintype "input"))
    (pad "26" thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/VA14") (pinfunction "A13") (pintype "input"))
    (pad "27" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 231 "/~{UWR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "27" thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 231 "/~{UWR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "28" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (pad "28" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 57.531 62.992 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB10" (at 2.54 -2.77 -90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 210 "Net-(FB10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 58.674 54.229 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB8" (at 1.778 3.556 -90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 209 "Net-(FB8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 234 "Net-(C31-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 84.408 165.354)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C44" (at 7.54 2.54) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 302 "Net-(C44-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 305 "/SR1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:BarrelJack_CUI_PJ-002A_Horizontal" (layer "F.Cu")
    (at 268.5596 149.3004)
    (descr "https://www.mouser.de/datasheet/2/670/pj_002a-1778764.pdf")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "DC Barrel Jack")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "Jack-DC" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 5.1 6.3 90) (size 6 2.54) (drill oval 3.5 1) (layers "*.Cu" "*.Mask")
      (net 331 "/DCin1") (pintype "passive"))
    (pad "2" thru_hole oval (at -0.9 6.3 270) (size 4.8 2.54) (drill oval 3 1) (layers "*.Cu" "*.Mask")
      (net 332 "/DCin2") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.1 11 180) (size 4.8 2.54) (drill oval 3 1) (layers "*.Cu" "*.Mask")
      (net 332 "/DCin2") (pintype "passive"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 116.713 55.198 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C71" (at 7.54 -3.302 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_5mm" (layer "F.Cu")
    (at 272.4404 28.6004)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H13" (at 0 -6) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "SEGA:QFP128" (layer "F.Cu")
    (at 132.125 116.518 -90)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at -20.4552 -0.6662 unlocked) (layer "F.SilkS"))
    (fp_text value "312-5313A" (at -1.202 -2.241 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -17.2 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -12.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/SD0") (pinfunction "SD0") (pintype "unspecified"))
    (pad "2" smd rect (at -11.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "/SD1") (pinfunction "SD1") (pintype "unspecified"))
    (pad "3" smd rect (at -10.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "/SD2") (pinfunction "SD2") (pintype "unspecified"))
    (pad "4" smd rect (at -10 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "/SD3") (pinfunction "SD3") (pintype "unspecified"))
    (pad "5" smd rect (at -9.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "/SD4") (pinfunction "SD4") (pintype "unspecified"))
    (pad "6" smd rect (at -8.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "/SD5") (pinfunction "SD5") (pintype "unspecified"))
    (pad "7" smd rect (at -7.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "/SD6") (pinfunction "SD6") (pintype "unspecified"))
    (pad "8" smd rect (at -6.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "/SD7") (pinfunction "SD7") (pintype "unspecified"))
    (pad "9" smd rect (at -6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "unconnected-(U8-~{SE1}-Pad9)") (pinfunction "~{SE1}") (pintype "unspecified+no_connect"))
    (pad "10" smd rect (at -5.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "Net-(U10-~{SE})") (pinfunction "~{SE0}") (pintype "unspecified"))
    (pad "11" smd rect (at -4.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "Net-(U10-SC)") (pinfunction "SC") (pintype "unspecified"))
    (pad "12" smd rect (at -3.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "Net-(U10-~{RAS})") (pinfunction "~{RAS1}") (pintype "unspecified"))
    (pad "13" smd rect (at -2.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "Net-(U10-~{CAS})") (pinfunction "~{CAS1}") (pintype "unspecified"))
    (pad "14" smd rect (at -2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "unconnected-(U8-~{WE1}-Pad14)") (pinfunction "~{WE1}") (pintype "unspecified+no_connect"))
    (pad "15" smd rect (at -1.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(U10-~{WB}{slash}~{WE})") (pinfunction "~{WE0}") (pintype "unspecified"))
    (pad "16" smd rect (at -0.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "Net-(U10-~{DT}{slash}~{OE})") (pinfunction "~{OE1}") (pintype "unspecified"))
    (pad "17" smd rect (at 0.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "18" smd rect (at 1.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(U8-RD0-Pad18)") (pinfunction "RD0") (pintype "unspecified+no_connect"))
    (pad "19" smd rect (at 2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "unconnected-(U8-RD1-Pad19)") (pinfunction "RD1") (pintype "unspecified+no_connect"))
    (pad "20" smd rect (at 2.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "unconnected-(U8-RD2-Pad20)") (pinfunction "RD2") (pintype "unspecified+no_connect"))
    (pad "21" smd rect (at 3.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "unconnected-(U8-RD3-Pad21)") (pinfunction "RD3") (pintype "unspecified+no_connect"))
    (pad "22" smd rect (at 4.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "unconnected-(U8-RD4-Pad22)") (pinfunction "RD4") (pintype "unspecified+no_connect"))
    (pad "23" smd rect (at 5.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "unconnected-(U8-RD5-Pad23)") (pinfunction "RD5") (pintype "unspecified+no_connect"))
    (pad "24" smd rect (at 6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "unconnected-(U8-RD6-Pad24)") (pinfunction "RD6") (pintype "unspecified+no_connect"))
    (pad "25" smd rect (at 6.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "unconnected-(U8-RD7-Pad25)") (pinfunction "RD7") (pintype "unspecified+no_connect"))
    (pad "26" smd rect (at 7.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "AGC") (pintype "unspecified"))
    (pad "27" smd rect (at 8.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "Net-(U8-R)") (pinfunction "R") (pintype "unspecified"))
    (pad "28" smd rect (at 9.2 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "Net-(U8-G)") (pinfunction "G") (pintype "unspecified"))
    (pad "29" smd rect (at 10 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "Net-(U8-B)") (pinfunction "B") (pintype "unspecified"))
    (pad "30" smd rect (at 10.8 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "VCCQ") (pinfunction "AVC") (pintype "unspecified"))
    (pad "31" smd rect (at 11.6 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "/A0") (pinfunction "AD0") (pintype "unspecified"))
    (pad "32" smd rect (at 12.4 15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/A1") (pinfunction "AD1") (pintype "unspecified"))
    (pad "33" smd rect (at 15.2 12.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/A2") (pinfunction "AD2") (pintype "unspecified"))
    (pad "34" smd rect (at 15.2 11.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "/A3") (pinfunction "AD3") (pintype "unspecified"))
    (pad "35" smd rect (at 15.2 10.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "/A4") (pinfunction "AD4") (pintype "unspecified"))
    (pad "36" smd rect (at 15.2 10 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "/A5") (pinfunction "AD5") (pintype "unspecified"))
    (pad "37" smd rect (at 15.2 9.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "/A6") (pinfunction "AD6") (pintype "unspecified"))
    (pad "38" smd rect (at 15.2 8.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "/A7") (pinfunction "AD7") (pintype "unspecified"))
    (pad "39" smd rect (at 15.2 7.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "/~{YS}") (pinfunction "~{YS}") (pintype "unspecified"))
    (pad "40" smd rect (at 15.2 6.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "Net-(U8-SPA{slash}B)") (pinfunction "SPA/B") (pintype "unspecified"))
    (pad "41" smd rect (at 15.2 6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/~{VSYNC}") (pinfunction "~{VSYNC}") (pintype "unspecified"))
    (pad "42" smd rect (at 15.2 5.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "Net-(U13-C_SYNC_IN)") (pinfunction "~{CSYNC}") (pintype "unspecified"))
    (pad "43" smd rect (at 15.2 4.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/~{HSYNC}") (pinfunction "~{HSYNC}") (pintype "unspecified"))
    (pad "44" smd rect (at 15.2 3.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/~{HL}") (pinfunction "~{HL}") (pintype "unspecified"))
    (pad "45" smd rect (at 15.2 2.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/~{M3}") (pinfunction "SEL0") (pintype "unspecified"))
    (pad "46" smd rect (at 15.2 2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "/NTSC") (pinfunction "~{PAL}") (pintype "unspecified"))
    (pad "47" smd rect (at 15.2 1.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "/~{SRES}") (pinfunction "~{RESET}") (pintype "unspecified"))
    (pad "48" smd rect (at 15.2 0.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "SEL1") (pintype "unspecified"))
    (pad "49" smd rect (at 15.2 -0.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "Net-(U8-CLK1)") (pinfunction "CLK1") (pintype "unspecified"))
    (pad "50" smd rect (at 15.2 -1.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "Net-(U8-SBCR)") (pinfunction "SBCR") (pintype "unspecified"))
    (pad "51" smd rect (at 15.2 -2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "Net-(U8-CLK0)") (pinfunction "CLK0") (pintype "unspecified"))
    (pad "52" smd rect (at 15.2 -2.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "MCLK") (pinfunction "MCX") (pintype "unspecified"))
    (pad "53" smd rect (at 15.2 -3.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/EDCK") (pinfunction "EDCK") (pintype "unspecified"))
    (pad "54" smd rect (at 15.2 -4.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "VCC") (pinfunction "VDD") (pintype "unspecified"))
    (pad "55" smd rect (at 15.2 -5.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/VD0") (pinfunction "CD0") (pintype "unspecified"))
    (pad "56" smd rect (at 15.2 -6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/VD1") (pinfunction "CD1") (pintype "unspecified"))
    (pad "57" smd rect (at 15.2 -6.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VD2") (pinfunction "CD2") (pintype "unspecified"))
    (pad "58" smd rect (at 15.2 -7.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/VD3") (pinfunction "CD3") (pintype "unspecified"))
    (pad "59" smd rect (at 15.2 -8.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/VD4") (pinfunction "CD4") (pintype "unspecified"))
    (pad "60" smd rect (at 15.2 -9.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/VD5") (pinfunction "CD5") (pintype "unspecified"))
    (pad "61" smd rect (at 15.2 -10 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/VD6") (pinfunction "CD6") (pintype "unspecified"))
    (pad "62" smd rect (at 15.2 -10.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/VD7") (pinfunction "CD7") (pintype "unspecified"))
    (pad "63" smd rect (at 15.2 -11.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/VD8") (pinfunction "CD8") (pintype "unspecified"))
    (pad "64" smd rect (at 15.2 -12.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/VD9") (pinfunction "CD9") (pintype "unspecified"))
    (pad "65" smd rect (at 12.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/VD10") (pinfunction "CD10") (pintype "unspecified"))
    (pad "66" smd rect (at 11.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/VD11") (pinfunction "CD11") (pintype "unspecified"))
    (pad "67" smd rect (at 10.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/VD12") (pinfunction "CD12") (pintype "unspecified"))
    (pad "68" smd rect (at 10 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/VD13") (pinfunction "CD13") (pintype "unspecified"))
    (pad "69" smd rect (at 9.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/VD14") (pinfunction "CD14") (pintype "unspecified"))
    (pad "70" smd rect (at 8.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/VD15") (pinfunction "CD15") (pintype "unspecified"))
    (pad "71" smd rect (at 7.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/VA1") (pinfunction "CA0") (pintype "unspecified"))
    (pad "72" smd rect (at 6.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/VA2") (pinfunction "CA1") (pintype "unspecified"))
    (pad "73" smd rect (at 6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/VA3") (pinfunction "CA2") (pintype "unspecified"))
    (pad "74" smd rect (at 5.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/VA4") (pinfunction "CA3") (pintype "unspecified"))
    (pad "75" smd rect (at 4.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/VA5") (pinfunction "CA4") (pintype "unspecified"))
    (pad "76" smd rect (at 3.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VA6") (pinfunction "CA5") (pintype "unspecified"))
    (pad "77" smd rect (at 2.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/VA7") (pinfunction "CA6") (pintype "unspecified"))
    (pad "78" smd rect (at 2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/VA8") (pinfunction "CA7") (pintype "unspecified"))
    (pad "79" smd rect (at 1.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/VA9") (pinfunction "CA8") (pintype "unspecified"))
    (pad "80" smd rect (at 0.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/VA10") (pinfunction "CA9") (pintype "unspecified"))
    (pad "81" smd rect (at -0.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/VA11") (pinfunction "CA10") (pintype "unspecified"))
    (pad "82" smd rect (at -1.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/VA12") (pinfunction "CA11") (pintype "unspecified"))
    (pad "83" smd rect (at -2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/VA13") (pinfunction "CA12") (pintype "unspecified"))
    (pad "84" smd rect (at -2.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/VA14") (pinfunction "CA13") (pintype "unspecified"))
    (pad "85" smd rect (at -3.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/VA15") (pinfunction "CA14") (pintype "unspecified"))
    (pad "86" smd rect (at -4.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VA16") (pinfunction "CA15") (pintype "unspecified"))
    (pad "87" smd rect (at -5.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/VA17") (pinfunction "CA16") (pintype "unspecified"))
    (pad "88" smd rect (at -6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/VA18") (pinfunction "CA17") (pintype "unspecified"))
    (pad "89" smd rect (at -6.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/VA19") (pinfunction "CA18") (pintype "unspecified"))
    (pad "90" smd rect (at -7.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/VA20") (pinfunction "CA19") (pintype "unspecified"))
    (pad "91" smd rect (at -8.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/VA21") (pinfunction "CA20") (pintype "unspecified"))
    (pad "92" smd rect (at -9.2 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/VA22") (pinfunction "CA21") (pintype "unspecified"))
    (pad "93" smd rect (at -10 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/VA23") (pinfunction "CA22") (pintype "unspecified"))
    (pad "94" smd rect (at -10.8 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "VDDA") (pinfunction "AYS") (pintype "unspecified"))
    (pad "95" smd rect (at -11.6 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "Net-(U8-SOUND)") (pinfunction "SOUND") (pintype "unspecified"))
    (pad "96" smd rect (at -12.4 -15.2 270) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "AGS") (pintype "unspecified"))
    (pad "97" smd rect (at -15.2 -12.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "98" smd rect (at -15.2 -11.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "/~{INT}") (pinfunction "~{INT}") (pintype "unspecified"))
    (pad "99" smd rect (at -15.2 -10.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "/BR") (pinfunction "~{BR}") (pintype "unspecified"))
    (pad "100" smd rect (at -15.2 -10 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "/BGACK") (pinfunction "~{BGAK}") (pintype "unspecified"))
    (pad "101" smd rect (at -15.2 -9.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "/BG") (pinfunction "~{BG}") (pintype "unspecified"))
    (pad "102" smd rect (at -15.2 -8.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/~{VDPM}") (pinfunction "~{MREQ}") (pintype "unspecified"))
    (pad "103" smd rect (at -15.2 -7.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/~{INTAK}") (pinfunction "~{INTAK}") (pintype "unspecified"))
    (pad "104" smd rect (at -15.2 -6.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "/IPL1") (pinfunction "~{IPL1}") (pintype "unspecified"))
    (pad "105" smd rect (at -15.2 -6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "/IPL2") (pinfunction "~{IPL2}") (pintype "unspecified"))
    (pad "106" smd rect (at -15.2 -5.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "/~{IREQ}") (pinfunction "~{IORQ}") (pintype "unspecified"))
    (pad "107" smd rect (at -15.2 -4.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "/~{ZRD}") (pinfunction "~{RD}") (pintype "unspecified"))
    (pad "108" smd rect (at -15.2 -3.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "/~{ZWR}") (pinfunction "~{WR}") (pintype "unspecified"))
    (pad "109" smd rect (at -15.2 -2.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "/~{M1}") (pinfunction "~{M1}") (pintype "unspecified"))
    (pad "110" smd rect (at -15.2 -2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "/~{AS}") (pinfunction "~{AS}") (pintype "unspecified"))
    (pad "111" smd rect (at -15.2 -1.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "/~{UDS}") (pinfunction "~{UDS}") (pintype "unspecified"))
    (pad "112" smd rect (at -15.2 -0.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "/~{LDS}") (pinfunction "~{LDS}") (pintype "unspecified"))
    (pad "113" smd rect (at -15.2 0.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "/~{R{slash}W}") (pinfunction "R/W") (pintype "unspecified"))
    (pad "114" smd rect (at -15.2 1.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/~{DTAK}") (pinfunction "~{DTAK}") (pintype "unspecified"))
    (pad "115" smd rect (at -15.2 2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "/~{UWR}") (pinfunction "~{UWR}") (pintype "unspecified"))
    (pad "116" smd rect (at -15.2 2.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "/~{LWR}") (pinfunction "~{LWR}") (pintype "unspecified"))
    (pad "117" smd rect (at -15.2 3.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "/~{OE0}") (pinfunction "~{OE0}") (pintype "unspecified"))
    (pad "118" smd rect (at -15.2 4.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "/~{CAS0}") (pinfunction "~{CAS0}") (pintype "unspecified"))
    (pad "119" smd rect (at -15.2 5.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "/~{RAS0}") (pinfunction "~{RAS0}") (pintype "unspecified"))
    (pad "120" smd rect (at -15.2 6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "unconnected-(U8-RA0-Pad120)") (pinfunction "RA0") (pintype "unspecified+no_connect"))
    (pad "121" smd rect (at -15.2 6.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "unconnected-(U8-RA1-Pad121)") (pinfunction "RA1") (pintype "unspecified+no_connect"))
    (pad "122" smd rect (at -15.2 7.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "unconnected-(U8-RA2-Pad122)") (pinfunction "RA2") (pintype "unspecified+no_connect"))
    (pad "123" smd rect (at -15.2 8.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "unconnected-(U8-RA3-Pad123)") (pinfunction "RA3") (pintype "unspecified+no_connect"))
    (pad "124" smd rect (at -15.2 9.2 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "unconnected-(U8-RA4-Pad124)") (pinfunction "RA4") (pintype "unspecified+no_connect"))
    (pad "125" smd rect (at -15.2 10 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "unconnected-(U8-RA5-Pad125)") (pinfunction "RA5") (pintype "unspecified+no_connect"))
    (pad "126" smd rect (at -15.2 10.8 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "unconnected-(U8-RA6-Pad126)") (pinfunction "RA6") (pintype "unspecified+no_connect"))
    (pad "127" smd rect (at -15.2 11.6 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "unconnected-(U8-RA7-Pad127)") (pinfunction "RA7") (pintype "unspecified+no_connect"))
    (pad "128" smd rect (at -15.2 12.4 180) (size 0.4 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "VCC") (pinfunction "VDD") (pintype "unspecified"))
    (model "${KICAD7_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-144_28x28mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 210.566 195.326 90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB3" (at 8.763 0.127 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 156 "Net-(FB3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 55.753 179.404 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C58" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 283 "Net-(U12-VOL_IN)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:ZIP-24" (layer "F.Cu")
    (at 103.632 62.23)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "65536 Word x 4bit Dynamic RAM")
    (property "ki_keywords" "RAM MEMORY")
    (attr through_hole)
    (fp_text reference "U10" (at -6.35 25.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "M5M4C264L" (at -4.675 25.4 90 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at -1.27 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "23" (at -1.27 38.1 90 unlocked) (layer "F.SilkS"))
    (fp_text user "2" (at 1.905 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "24" (at 1.905 38.1 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -3.175 25.4 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -1.27 5.08) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 149 "/A6") (pinfunction "W2/IO2") (pintype "tri_state"))
    (pad "2" thru_hole circle (at 1.27 6.35) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 134 "/A7") (pinfunction "W3/IO3") (pintype "tri_state"))
    (pad "3" thru_hole circle (at -1.27 7.62) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 240 "Net-(U10-~{SE})") (pinfunction "~{SE}") (pintype "input"))
    (pad "4" thru_hole circle (at 1.27 8.89) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 127 "/SD6") (pinfunction "SIO2") (pintype "tri_state"))
    (pad "5" thru_hole circle (at -1.27 10.16) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 128 "/SD7") (pinfunction "SIO3") (pintype "tri_state"))
    (pad "6" thru_hole circle (at 1.27 11.43) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole circle (at -1.27 12.7) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 241 "Net-(U10-SC)") (pinfunction "SC") (pintype "input"))
    (pad "8" thru_hole circle (at 1.27 13.97) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 125 "/SD4") (pinfunction "SIO0") (pintype "tri_state"))
    (pad "9" thru_hole circle (at -1.27 15.24) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 126 "/SD5") (pinfunction "SIO1") (pintype "tri_state"))
    (pad "10" thru_hole circle (at 1.27 16.51) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 242 "Net-(U10-~{DT}{slash}~{OE})") (pinfunction "~{DT}/~{OE}") (pintype "input"))
    (pad "11" thru_hole circle (at -1.27 17.78) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 133 "/A4") (pinfunction "W0/IO0") (pintype "tri_state"))
    (pad "12" thru_hole circle (at 1.27 19.05) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 148 "/A5") (pinfunction "W1/IO1") (pintype "tri_state"))
    (pad "13" thru_hole circle (at -1.27 20.32) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 239 "Net-(U10-~{WB}{slash}~{WE})") (pinfunction "~{WB}/~{WE}") (pintype "input"))
    (pad "14" thru_hole circle (at 1.27 21.59) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 237 "Net-(U10-~{RAS})") (pinfunction "~{RAS}") (pintype "input"))
    (pad "15" thru_hole circle (at -1.27 22.86) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 149 "/A6") (pinfunction "A5") (pintype "input"))
    (pad "16" thru_hole circle (at 1.27 24.13) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 148 "/A5") (pinfunction "A6") (pintype "input"))
    (pad "17" thru_hole circle (at -1.27 25.4) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 133 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "18" thru_hole circle (at 1.27 26.67) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "19" thru_hole circle (at -1.27 27.94) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 134 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "20" thru_hole circle (at 1.27 29.21) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 132 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "21" thru_hole circle (at -1.27 30.48) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 131 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "22" thru_hole circle (at 1.27 31.75) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 130 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "23" thru_hole circle (at -1.27 33.02) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 129 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "24" thru_hole circle (at 1.27 34.29) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 238 "Net-(U10-~{CAS})") (pinfunction "~{CAS}") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SIP.3dshapes/SIP-9_21.54x3mm_P2.54mm.wrl"
      (offset (xyz 0 -9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 246.507 159.893)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, open")
    (property "ki_keywords" "Jumper SPST")
    (attr through_hole)
    (fp_text reference "JP4" (at 8.509 0) (layer "F.SilkS"))
    (fp_text value "NTSC" (at 11.938 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 274 "/NTSC") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P5.08mm_Vertical_AnodeUp" (layer "F.Cu")
    (at 86.995 190.246 -90)
    (descr "Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D3" (at 8.255 0.127 90) (layer "F.SilkS"))
    (fp_text value "ISR35-100A" (at 2.54 2.47 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.47 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 232 "+9VA") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P5.08mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 116.078 132.588)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID4" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 107.442 44.831 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB5" (at 10.795 -0.254 -90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 170 "Net-(FB5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite_THT:LairdTech_28C0236-0JW-10" (layer "F.Cu")
    (at 66.421 195.199 90)
    (descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
    (tags "Ferrite vertical LairdTech 28C0236-0JW-10")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB11" (at 4.699 -2.54 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 4.953 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 250 "Net-(J10-Pin_4)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 289 "Net-(C50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:DIP-28_DoubleFirst" (layer "F.Cu")
    (at 129.54 183.642 -90)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at -3.175 25.781) (layer "F.SilkS"))
    (fp_text value "uPD4364" (at 11.303 16.129 -180 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -0.16 -2.52 unlocked) (layer "F.SilkS"))
    (fp_text user "15" (at 16.55 36.96 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 16.51 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 319 "/~{REF}") (pinfunction "~{RFSH}") (pintype "input"))
    (pad "1" thru_hole rect (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 319 "/~{REF}") (pinfunction "~{RFSH}") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 101 "/ZA12") (pinfunction "A12") (pintype "input"))
    (pad "2" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 101 "/ZA12") (pinfunction "A12") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "/ZA7") (pinfunction "A7") (pintype "input"))
    (pad "3" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "/ZA7") (pinfunction "A7") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 107 "/ZA6") (pinfunction "A6") (pintype "input"))
    (pad "4" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 107 "/ZA6") (pinfunction "A6") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "/ZA5") (pinfunction "A5") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "/ZA5") (pinfunction "A5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 109 "/ZA4") (pinfunction "A4") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 109 "/ZA4") (pinfunction "A4") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 110 "/ZA3") (pinfunction "A3") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 110 "/ZA3") (pinfunction "A3") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "/ZA2") (pinfunction "A2") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "/ZA2") (pinfunction "A2") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/ZA1") (pinfunction "A1") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/ZA1") (pinfunction "A1") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "/ZA0") (pinfunction "A0") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "/ZA0") (pinfunction "A0") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "/ZD0") (pinfunction "D0") (pintype "tri_state"))
    (pad "11" thru_hole oval (at 7.62 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "/ZD0") (pinfunction "D0") (pintype "tri_state"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/ZD1") (pinfunction "D1") (pintype "tri_state"))
    (pad "12" thru_hole oval (at 7.62 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/ZD1") (pinfunction "D1") (pintype "tri_state"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/ZD2") (pinfunction "D2") (pintype "tri_state"))
    (pad "13" thru_hole oval (at 7.62 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/ZD2") (pinfunction "D2") (pintype "tri_state"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" thru_hole oval (at 7.62 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "/ZD3") (pinfunction "D3") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 97 "/ZD4") (pinfunction "D4") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "/ZD5") (pinfunction "D5") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "/ZD6") (pinfunction "D6") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 111 "/ZD7") (pinfunction "D7") (pintype "tri_state"))
    (pad "20" thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 318 "/~{ZRAM}") (pinfunction "~{CE1}") (pintype "input"))
    (pad "21" thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 103 "/ZA10") (pinfunction "A10") (pintype "input"))
    (pad "22" thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 196 "/~{ZRD}") (pinfunction "~{OE}") (pintype "input"))
    (pad "23" thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 102 "/ZA11") (pinfunction "A11") (pintype "input"))
    (pad "24" thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 104 "/ZA9") (pinfunction "A9") (pintype "input"))
    (pad "25" thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 105 "/ZA8") (pinfunction "A8") (pintype "input"))
    (pad "26" thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "CE2") (pintype "input"))
    (pad "27" thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 204 "/~{ZWR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "28" thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 7.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x04_P2.00mm_Vertical" (layer "F.Cu")
    (at 53.213 203.327 90)
    (descr "Through hole straight pin header, 1x04, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.00mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 2.794 1.778 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 8.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(J10-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 246 "Net-(J10-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 252 "unconnected-(J10-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 250 "Net-(J10-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 189.484 167.72 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C111" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 147.193 59.516 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 119.761 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM34" (at 2.5 -2.7 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 180 "PC3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 174 "Net-(EM34-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:DIP-28_DoubleLast" (layer "F.Cu")
    (at 201.676 161.036 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "256K (32K x 8) Static RAM, 70ns, DIP-28")
    (property "ki_keywords" "RAM SRAM CMOS MEMORY")
    (attr through_hole)
    (fp_text reference "U2" (at 18.669 16.51 180) (layer "F.SilkS"))
    (fp_text value "uPD42832C-15" (at 3.556 16.002 unlocked) (layer "F.SilkS"))
    (fp_text user "15" (at 16.5 33.9 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -0.8 -3.2 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 16.51 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/VA15") (pinfunction "A14") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/VA13") (pinfunction "A12") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/VA8") (pinfunction "A7") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/VA7") (pinfunction "A6") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/VA6") (pinfunction "A5") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/VA5") (pinfunction "A4") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/VA4") (pinfunction "A3") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/VA3") (pinfunction "A2") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/VA2") (pinfunction "A1") (pintype "input"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/VA1") (pinfunction "A0") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/VD0") (pinfunction "Q0") (pintype "tri_state"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/VD1") (pinfunction "Q1") (pintype "tri_state"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/VD2") (pinfunction "Q2") (pintype "tri_state"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "/VD3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "15" thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "/VD3") (pinfunction "Q3") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "/VD4") (pinfunction "Q4") (pintype "tri_state"))
    (pad "16" thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "/VD4") (pinfunction "Q4") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/VD5") (pinfunction "Q5") (pintype "tri_state"))
    (pad "17" thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/VD5") (pinfunction "Q5") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/VD6") (pinfunction "Q6") (pintype "tri_state"))
    (pad "18" thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/VD6") (pinfunction "Q6") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "/VD7") (pinfunction "Q7") (pintype "tri_state"))
    (pad "19" thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "/VD7") (pinfunction "Q7") (pintype "tri_state"))
    (pad "20" thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 229 "/~{RAS0}") (pinfunction "~{CS}") (pintype "input"))
    (pad "20" thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 229 "/~{RAS0}") (pinfunction "~{CS}") (pintype "input"))
    (pad "21" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "A10") (pintype "input"))
    (pad "21" thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "A10") (pintype "input"))
    (pad "22" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 298 "/~{NOE}") (pinfunction "~{OE}") (pintype "input"))
    (pad "22" thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 298 "/~{NOE}") (pinfunction "~{OE}") (pintype "input"))
    (pad "23" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "A11") (pintype "input"))
    (pad "23" thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "A11") (pintype "input"))
    (pad "24" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "A9") (pintype "input"))
    (pad "24" thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "A9") (pintype "input"))
    (pad "25" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "A8") (pintype "input"))
    (pad "25" thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "A8") (pintype "input"))
    (pad "26" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 257 "/iA14") (pinfunction "A13") (pintype "input"))
    (pad "26" thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 257 "/iA14") (pinfunction "A13") (pintype "input"))
    (pad "27" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 230 "/~{LWR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "27" thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 230 "/~{LWR}") (pinfunction "~{WE}") (pintype "input"))
    (pad "28" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (pad "28" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 152.146 32.004)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 4.826) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 52.07 145.796 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB2" (at 2.54 -2.77 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(J11-Pin_2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 48.968 94.294 -90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")
    (property "ki_keywords" "Voltage Regulator 1.5A Positive")
    (attr through_hole)
    (fp_text reference "U17" (at 1.464 6.677 90) (layer "F.SilkS"))
    (fp_text value "L7805" (at 2.54 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -1.88 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 49.911 175.387 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C57" (at -3.683 1.143 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 286 "Net-(U12-NF_(B))") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 219.202 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM21" (at -3.429 -0.762 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 141 "PB0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 86 "Net-(EM21-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 95.377 209.423)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H12" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 206.121 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM8" (at -4.064 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 120 "PA5") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 135 "Net-(EM8-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 98.806 49.911 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM36" (at -5.334 -0.381 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 181 "PC4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 176 "Net-(EM36-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 223.139 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM22" (at -3.175 -1.016 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 142 "PB1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(EM22-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 69.596 101.346 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L5" (at 2.54 -1.92 90) (layer "F.SilkS"))
    (fp_text value "12uH" (at 2.54 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 325 "Net-(C37-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 68.453 79.629 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C38" (at 5.635 3.302 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 309 "/VREF") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 109.474 168.402 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at 1.905 5.207 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 59.055 88.265)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L2" (at 2.54 -1.92) (layer "F.SilkS"))
    (fp_text value "100uH" (at 2.54 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 194 "VDDA") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Oscillator:Oscillator_DIP-14" (layer "F.Cu")
    (at 146.05 151.638)
    (descr "Oscillator, DIP14, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags "oscillator")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Voltage-Controlled Crystal Clock Oscillator, DIP14-style metal package")
    (property "ki_keywords" "Crystal Clock Oscillator")
    (attr through_hole)
    (fp_text reference "OSC1" (at 7.62 -11.26) (layer "F.SilkS"))
    (fp_text value "CK5545AC" (at 7.62 3.74) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 -3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 206 "Net-(OSC1-Vcontrol)") (pinfunction "Vcontrol") (pintype "input"))
    (pad "7" thru_hole circle (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle (at 15.24 -7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 207 "Net-(OSC1-OUT)") (pinfunction "OUT") (pintype "output"))
    (pad "14" thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "Vcc") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_DIP-14.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 51.816 193.628 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C51" (at 6.905 2.54 90) (layer "F.SilkS"))
    (fp_text value "220uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 290 "Net-(U12-OUT_(B))") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 291 "Net-(C51-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 246.507 154.813)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr through_hole)
    (fp_text reference "JP2" (at 8.636 0.127) (layer "F.SilkS"))
    (fp_text value "ENG" (at 11.557 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 233 "/~{JAP}") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-64_W22.86mm" (layer "F.Cu")
    (at 233.934 42.926 -90)
    (descr "64-lead though-hole mounted DIP package, row spacing 22.86 mm (900 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 22.86mm 900mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "16/32-bit Microprocessor")
    (property "ki_keywords" "68000 Microprocessor CPU")
    (attr through_hole)
    (fp_text reference "U1" (at -5.207 43.434) (layer "F.SilkS"))
    (fp_text value "68000D" (at 11.811 42.164 -180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 11.43 39.37 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "/VD4") (pinfunction "D4") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "/VD3") (pinfunction "D3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/VD2") (pinfunction "D2") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/VD1") (pinfunction "D1") (pintype "bidirectional"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/VD0") (pinfunction "D0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 218 "/~{AS}") (pinfunction "AS") (pintype "output"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 219 "/~{UDS}") (pinfunction "UDS") (pintype "output"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 220 "/~{LDS}") (pinfunction "LDS") (pintype "output"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 221 "/~{R{slash}W}") (pinfunction "R/W") (pintype "output"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "/~{DTAK}") (pinfunction "DTACK") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 224 "/BG") (pinfunction "BG") (pintype "output"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 225 "/BGACK") (pinfunction "BGACK") (pintype "input"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 226 "/BR") (pinfunction "BR") (pintype "input"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 203 "/VCLK") (pinfunction "CLK") (pintype "input"))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 168 "Net-(U1-HALT)") (pinfunction "HALT") (pintype "bidirectional"))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 265 "/~{VRES}") (pinfunction "RESET") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(U1-VMA-Pad19)") (pinfunction "VMA") (pintype "output+no_connect"))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(U1-E-Pad20)") (pinfunction "E") (pintype "output+no_connect"))
    (pad "21" thru_hole oval (at 0 50.8 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 169 "Net-(U1-VPA)") (pinfunction "VPA") (pintype "input"))
    (pad "22" thru_hole oval (at 0 53.34 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "BERR") (pintype "input"))
    (pad "23" thru_hole oval (at 0 55.88 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 227 "/IPL2") (pinfunction "IPL2") (pintype "input"))
    (pad "24" thru_hole oval (at 0 58.42 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 228 "/IPL1") (pinfunction "IPL1") (pintype "input"))
    (pad "25" thru_hole oval (at 0 60.96 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "IPL0") (pintype "input"))
    (pad "26" thru_hole oval (at 0 63.5 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(U1-FC2-Pad26)") (pinfunction "FC2") (pintype "output+no_connect"))
    (pad "27" thru_hole oval (at 0 66.04 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 222 "/FC1") (pinfunction "FC1") (pintype "output"))
    (pad "28" thru_hole oval (at 0 68.58 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 223 "/FC0") (pinfunction "FC0") (pintype "output"))
    (pad "29" thru_hole oval (at 0 71.12 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "/VA1") (pinfunction "A1") (pintype "output"))
    (pad "30" thru_hole oval (at 0 73.66 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "/VA2") (pinfunction "A2") (pintype "output"))
    (pad "31" thru_hole oval (at 0 76.2 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/VA3") (pinfunction "A3") (pintype "output"))
    (pad "32" thru_hole oval (at 0 78.74 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/VA4") (pinfunction "A4") (pintype "output"))
    (pad "33" thru_hole oval (at 22.86 78.74 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/VA5") (pinfunction "A5") (pintype "output"))
    (pad "34" thru_hole oval (at 22.86 76.2 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/VA6") (pinfunction "A6") (pintype "output"))
    (pad "35" thru_hole oval (at 22.86 73.66 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/VA7") (pinfunction "A7") (pintype "output"))
    (pad "36" thru_hole oval (at 22.86 71.12 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/VA8") (pinfunction "A8") (pintype "output"))
    (pad "37" thru_hole oval (at 22.86 68.58 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "A9") (pintype "output"))
    (pad "38" thru_hole oval (at 22.86 66.04 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "A10") (pintype "output"))
    (pad "39" thru_hole oval (at 22.86 63.5 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "A11") (pintype "output"))
    (pad "40" thru_hole oval (at 22.86 60.96 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "A12") (pintype "output"))
    (pad "41" thru_hole oval (at 22.86 58.42 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/VA13") (pinfunction "A13") (pintype "output"))
    (pad "42" thru_hole oval (at 22.86 55.88 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/VA14") (pinfunction "A14") (pintype "output"))
    (pad "43" thru_hole oval (at 22.86 53.34 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/VA15") (pinfunction "A15") (pintype "output"))
    (pad "44" thru_hole oval (at 22.86 50.8 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/VA16") (pinfunction "A16") (pintype "output"))
    (pad "45" thru_hole oval (at 22.86 48.26 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/VA17") (pinfunction "A17") (pintype "output"))
    (pad "46" thru_hole oval (at 22.86 45.72 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/VA18") (pinfunction "A18") (pintype "output"))
    (pad "47" thru_hole oval (at 22.86 43.18 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "/VA19") (pinfunction "A19") (pintype "output"))
    (pad "48" thru_hole oval (at 22.86 40.64 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/VA20") (pinfunction "A20") (pintype "output"))
    (pad "49" thru_hole oval (at 22.86 38.1 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "50" thru_hole oval (at 22.86 35.56 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "/VA21") (pinfunction "A21") (pintype "output"))
    (pad "51" thru_hole oval (at 22.86 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/VA22") (pinfunction "A22") (pintype "output"))
    (pad "52" thru_hole oval (at 22.86 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "/VA23") (pinfunction "A23") (pintype "output"))
    (pad "53" thru_hole oval (at 22.86 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "54" thru_hole oval (at 22.86 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/VD15") (pinfunction "D15") (pintype "bidirectional"))
    (pad "55" thru_hole oval (at 22.86 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "/VD14") (pinfunction "D14") (pintype "bidirectional"))
    (pad "56" thru_hole oval (at 22.86 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/VD13") (pinfunction "D13") (pintype "bidirectional"))
    (pad "57" thru_hole oval (at 22.86 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "/VD12") (pinfunction "D12") (pintype "bidirectional"))
    (pad "58" thru_hole oval (at 22.86 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/VD11") (pinfunction "D11") (pintype "bidirectional"))
    (pad "59" thru_hole oval (at 22.86 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "/VD10") (pinfunction "D10") (pintype "bidirectional"))
    (pad "60" thru_hole oval (at 22.86 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "/VD9") (pinfunction "D9") (pintype "bidirectional"))
    (pad "61" thru_hole oval (at 22.86 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "/VD8") (pinfunction "D8") (pintype "bidirectional"))
    (pad "62" thru_hole oval (at 22.86 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "/VD7") (pinfunction "D7") (pintype "bidirectional"))
    (pad "63" thru_hole oval (at 22.86 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/VD6") (pinfunction "D6") (pintype "bidirectional"))
    (pad "64" thru_hole oval (at 22.86 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "/VD5") (pinfunction "D5") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-64_W22.86mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-40_W15.24mm" (layer "F.Cu")
    (at 164.338 163.068 -90)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-bit General Purpose Microprocessor, DIP-40")
    (property "ki_keywords" "Z80 CPU uP")
    (attr through_hole)
    (fp_text reference "U6" (at -3.048 17.526) (layer "F.SilkS"))
    (fp_text value "Z80CPU" (at 8.636 24.003 -180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.62 24.13 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 102 "/ZA11") (pinfunction "A11") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 101 "/ZA12") (pinfunction "A12") (pintype "output"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 100 "/ZA13") (pinfunction "A13") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 99 "/ZA14") (pinfunction "A14") (pintype "output"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 98 "/ZA15") (pinfunction "A15") (pintype "output"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/ZCLK") (pinfunction "~{CLK}") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 97 "/ZD4") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "/ZD3") (pinfunction "D3") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "/ZD5") (pinfunction "D5") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "/ZD6") (pinfunction "D6") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "VCC") (pintype "power_in"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/ZD2") (pinfunction "D2") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 111 "/ZD7") (pinfunction "D7") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "/ZD0") (pinfunction "D0") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/ZD1") (pinfunction "D1") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 296 "/~{INT}") (pinfunction "~{INT}") (pintype "input"))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 321 "/~{NMI}") (pinfunction "~{NMI}") (pintype "input"))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U6-~{HALT}-Pad18)") (pinfunction "~{HALT}") (pintype "output+no_connect"))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "/~{MREQ}") (pinfunction "~{MREQ}") (pintype "output"))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 162 "/~{IREQ}") (pinfunction "~{IORQ}") (pintype "output"))
    (pad "21" thru_hole oval (at 15.24 48.26 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 196 "/~{ZRD}") (pinfunction "~{RD}") (pintype "output"))
    (pad "22" thru_hole oval (at 15.24 45.72 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 204 "/~{ZWR}") (pinfunction "~{WR}") (pintype "output"))
    (pad "23" thru_hole oval (at 15.24 43.18 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 320 "/~{ZBAK}") (pinfunction "~{BUSACK}") (pintype "output"))
    (pad "24" thru_hole oval (at 15.24 40.64 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(U4-~{WAIT})") (pinfunction "~{WAIT}") (pintype "input"))
    (pad "25" thru_hole oval (at 15.24 38.1 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(U4-~{ZBR})") (pinfunction "~{BUSRQ}") (pintype "input"))
    (pad "26" thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "/~{ZRES}") (pinfunction "~{RESET}") (pintype "input"))
    (pad "27" thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 308 "/~{M1}") (pinfunction "~{M1}") (pintype "output"))
    (pad "28" thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U6-~{RFSH}-Pad28)") (pinfunction "~{RFSH}") (pintype "output+no_connect"))
    (pad "29" thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "/ZA0") (pinfunction "A0") (pintype "output"))
    (pad "31" thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/ZA1") (pinfunction "A1") (pintype "output"))
    (pad "32" thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "/ZA2") (pinfunction "A2") (pintype "output"))
    (pad "33" thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 110 "/ZA3") (pinfunction "A3") (pintype "output"))
    (pad "34" thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 109 "/ZA4") (pinfunction "A4") (pintype "output"))
    (pad "35" thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "/ZA5") (pinfunction "A5") (pintype "output"))
    (pad "36" thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 107 "/ZA6") (pinfunction "A6") (pintype "output"))
    (pad "37" thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "/ZA7") (pinfunction "A7") (pintype "output"))
    (pad "38" thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 105 "/ZA8") (pinfunction "A8") (pintype "output"))
    (pad "39" thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 104 "/ZA9") (pinfunction "A9") (pintype "output"))
    (pad "40" thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 103 "/ZA10") (pinfunction "A10") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 59.944 145.669 -90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB1" (at 2.54 -2.77 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "Net-(J11-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 199 "Net-(SW1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 72.39 190.072 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C50" (at -0.715 3.429 -90) (layer "F.SilkS"))
    (fp_text value "220uF 10V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 288 "Net-(U12-OUT_(A))") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 289 "Net-(C50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 243.586 195.453 90)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB4" (at 9.271 0.127 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 157 "Net-(FB4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (at 246.507 157.353)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr through_hole)
    (fp_text reference "JP3" (at 8.636 0) (layer "F.SilkS"))
    (fp_text value "PAL" (at 11.557 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 274 "/NTSC") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P5.08mm_Vertical_AnodeUp" (layer "F.Cu")
    (at 119.507 151.892 180)
    (descr "Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 2.54 -2.47) (layer "F.SilkS"))
    (fp_text value "1S2475" (at 2.54 2.47) (layer "F.Fab"))
    (fp_text user "A" (at 3.48 0.9) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.47) (layer "F.Fab"))
    (fp_text user "A" (at 3.48 0.9) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 295 "/~{MRES}") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P5.08mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 102.87 209.423)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H11" (at 1.143 -5.334) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 269.494 196.596)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID5" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 219.71 99.568)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID1" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 215.138 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM7" (at -3.683 -0.635 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 90 "PA6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 146 "Net-(EM7-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 127.889 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM32" (at -5.715 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 178 "PC1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 172 "Net-(EM32-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 266.065 185.801)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H9" (at -0.889 -5.461) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 49.022 64.135 -90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")
    (property "ki_keywords" "Voltage Regulator 1.5A Positive")
    (attr through_hole)
    (fp_text reference "U15" (at 2.159 6.731 90) (layer "F.SilkS"))
    (fp_text value "L7805" (at 2.54 2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-24_W10.16mm" (layer "F.Cu")
    (at 83.185 107.188 180)
    (descr "24-lead though-hole mounted DIP package, row spacing 10.16 mm (400 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 10.16mm 400mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U13" (at -3.175 16.002 270) (layer "F.SilkS"))
    (fp_text value "~" (at 5.08 30.27 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.953 14.732 270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 136 "Net-(U13-R_IN)") (pinfunction "R_IN") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 137 "Net-(U13-G_IN)") (pinfunction "G_IN") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 166 "Net-(U13-B_IN)") (pinfunction "B_IN") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 256 "unconnected-(U13-XO_OUT-Pad5)") (pinfunction "XO_OUT") (pintype "output+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 191 "Net-(U13-XO_IN)") (pinfunction "XO_IN") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 274 "/NTSC") (pinfunction "NTSC/PAL") (pintype "input"))
    (pad "8" thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 269 "Net-(U13-AUDIO_IN)") (pinfunction "AUDIO_IN") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 193 "Net-(U13-AUDIO_OUT)") (pinfunction "AUDIO_OUT") (pintype "output"))
    (pad "10" thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 312 "Net-(U13-C_SYNC_IN)") (pinfunction "C_SYNC_IN") (pintype "input"))
    (pad "11" thru_hole oval (at 0 25.4 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 270 "unconnected-(U13-C_SYNC_OUT-Pad11)") (pinfunction "C_SYNC_OUT") (pintype "output+no_connect"))
    (pad "12" thru_hole oval (at 0 27.94 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "Vcc1") (pintype "power_in"))
    (pad "13" thru_hole oval (at 10.16 27.94 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 311 "Net-(U13-I_REF)") (pinfunction "I_REF") (pintype "unspecified"))
    (pad "14" thru_hole oval (at 10.16 25.4 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 309 "/VREF") (pinfunction "V_REF") (pintype "unspecified"))
    (pad "15" thru_hole oval (at 10.16 22.86 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 327 "Net-(U13-CHROMA_OUT)") (pinfunction "CHROMA_OUT") (pintype "output"))
    (pad "16" thru_hole oval (at 10.16 20.32 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 313 "Net-(U13-Y_OUT)") (pinfunction "Y_OUT") (pintype "output"))
    (pad "17" thru_hole oval (at 10.16 17.78 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 323 "Net-(U13-CHROMA_IN)") (pinfunction "CHROMA_IN") (pintype "input"))
    (pad "18" thru_hole oval (at 10.16 15.24 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 314 "Net-(U13-Y_IN)") (pinfunction "Y_IN") (pintype "input"))
    (pad "19" thru_hole oval (at 10.16 12.7 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "Vcc2") (pintype "power_in"))
    (pad "20" thru_hole oval (at 10.16 10.16 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 235 "Net-(U13-C_VIDEO_OUT)") (pinfunction "C_VIDEO_OUT") (pintype "output"))
    (pad "21" thru_hole oval (at 10.16 7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 217 "Net-(U13-B_OUT)") (pinfunction "B_OUT") (pintype "output"))
    (pad "22" thru_hole oval (at 10.16 5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 213 "Net-(U13-G_OUT)") (pinfunction "G_OUT") (pintype "output"))
    (pad "23" thru_hole oval (at 10.16 2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 214 "Net-(U13-R_OUT)") (pinfunction "R_OUT") (pintype "output"))
    (pad "24" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND_2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W10.16mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 127.381 142.494 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C72" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 59.563 107.395 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C60" (at 3.73 4.064 90) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 194 "VDDA") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 274.828 146.431 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J111" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 332 "/DCin2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 331 "/DCin1") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 202.057 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM5" (at -3.81 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(EM5-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 248.92 200.533)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H10" (at 1.016 4.826) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 57.992 98.806)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 -3.5) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 42.164 49.53)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 6.223 0.381) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "SEGA:Jack_3.5mm" (layer "F.Cu")
    (at 273.75 41.529 90)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
    (tags "TRS audio jack stereo horizontal")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS)")
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J8" (at 7.366 -7.812 90) (layer "F.SilkS"))
    (fp_text value "AudioJack3" (at 0 -10 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -5 0 90) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 -5 90) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 1.2) (layers "F&B.Cu" "*.Mask"))
    (pad "R" thru_hole oval (at -5 -5 90) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 248 "Net-(J110-Pin_2)") (pintype "passive"))
    (pad "S" thru_hole oval (at 0 0 90) (size 2.2 1.2) (drill oval 1.4 0.4) (layers "*.Cu" "*.Mask")
      (net 249 "/AudioShield") (pintype "passive"))
    (pad "T" thru_hole oval (at 5 -5 270) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 251 "Net-(J110-Pin_4)") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 84.408 153.289)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C42" (at 8.302 2.413) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 301 "Net-(C42-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 255 "/SL1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_5mm" (layer "F.Cu")
    (at 267.4112 146.1008)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H15" (at 0 -6) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 189.992 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM12" (at -3.81 0 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 117 "PA1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(EM12-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 54.366349 173.863)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C52" (at 4.434651 -3.683) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 229.87 106.426 180)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "JP6" (at -3.556 -0.127) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 298 "/~{NOE}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 50.673 184.484 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C55" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 285 "Net-(U12-NF_(A))") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 42.164 114.046)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 241.173 76.153 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C66" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 156.21 209.804 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J99" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 263 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 186.055 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM11" (at -8.763 1.905 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "PA0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(EM11-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 51.816 164.799 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C49" (at 2.5 -3.5 -90) (layer "F.SilkS"))
    (fp_text value "100uF 10V" (at 2.5 3.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(U12-IN_(A))") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 73.533 112.014 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low-Power, Dual Operational Amplifiers, DIP-8/SOIC-8/TO-99-8")
    (property "ki_keywords" "dual opamp")
    (attr through_hole)
    (fp_text reference "U14" (at -2.667 2.667 -180) (layer "F.SilkS"))
    (fp_text value "LM358" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.413 2.54 -180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 271 "Net-(C30-Pad2)") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 282 "Net-(U14A--)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 281 "Net-(U12-IN_(A))") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 310 "Net-(U14B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 309 "/VREF") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 273 "/~{SRES}") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 194 "VDDA") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 173.863 209.677)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 1.905 -3.683) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 197.993 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM4" (at -3.683 0.127 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "PA3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(EM4-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 131.953 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM31" (at -5.715 -0.508 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 177 "PC0") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 171 "Net-(EM31-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 59.135 81.788)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C59" (at -3.763 0.381) (layer "F.SilkS"))
    (fp_text value "47uF 10V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 42.164 56.642)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 6.223 0.127) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "SEGA:SEGA_2x32_Female_Vertical_THT" (layer "F.Cu")
    (at 172.212 83.566)
    (descr "DIN41612 connector, type B, Vertical, 2 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
    (tags "DIN 41612 IEC 60603 B")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x32, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -8.89 180) (layer "F.SilkS"))
    (fp_text value "Cartridge" (at 0 -6.35 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -47.244 0 90) (size 4 4) (drill 4) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 47.244 0 90) (size 4 4) (drill 4) (layers "F&B.Cu" "*.Mask"))
    (pad "a1" thru_hole roundrect (at -39.37 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1612896774)
      (net 7 "GND") (pinfunction "Pin_a1") (pintype "passive"))
    (pad "a2" thru_hole circle (at -36.83 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "Pin_a2") (pintype "passive"))
    (pad "a3" thru_hole circle (at -34.29 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/VA8") (pinfunction "Pin_a3") (pintype "passive"))
    (pad "a4" thru_hole circle (at -31.75 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/VA11") (pinfunction "Pin_a4") (pintype "passive"))
    (pad "a5" thru_hole circle (at -29.21 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/VA7") (pinfunction "Pin_a5") (pintype "passive"))
    (pad "a6" thru_hole circle (at -26.67 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/VA12") (pinfunction "Pin_a6") (pintype "passive"))
    (pad "a7" thru_hole circle (at -24.13 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/VA6") (pinfunction "Pin_a7") (pintype "passive"))
    (pad "a8" thru_hole circle (at -21.59 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/VA13") (pinfunction "Pin_a8") (pintype "passive"))
    (pad "a9" thru_hole circle (at -19.05 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/VA5") (pinfunction "Pin_a9") (pintype "passive"))
    (pad "a10" thru_hole circle (at -16.51 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/VA14") (pinfunction "Pin_a10") (pintype "passive"))
    (pad "a11" thru_hole circle (at -13.97 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/VA4") (pinfunction "Pin_a11") (pintype "passive"))
    (pad "a12" thru_hole circle (at -11.43 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/VA15") (pinfunction "Pin_a12") (pintype "passive"))
    (pad "a13" thru_hole circle (at -8.89 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/VA3") (pinfunction "Pin_a13") (pintype "passive"))
    (pad "a14" thru_hole circle (at -6.35 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "/VA16") (pinfunction "Pin_a14") (pintype "passive"))
    (pad "a15" thru_hole circle (at -3.81 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/VA2") (pinfunction "Pin_a15") (pintype "passive"))
    (pad "a16" thru_hole circle (at -1.27 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "/VA17") (pinfunction "Pin_a16") (pintype "passive"))
    (pad "a17" thru_hole circle (at 1.27 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/VA1") (pinfunction "Pin_a17") (pintype "passive"))
    (pad "a18" thru_hole circle (at 3.81 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_a18") (pintype "passive"))
    (pad "a19" thru_hole circle (at 6.35 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "/VD7") (pinfunction "Pin_a19") (pintype "passive"))
    (pad "a20" thru_hole circle (at 8.89 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/VD0") (pinfunction "Pin_a20") (pintype "passive"))
    (pad "a21" thru_hole circle (at 11.43 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/VD8") (pinfunction "Pin_a21") (pintype "passive"))
    (pad "a22" thru_hole circle (at 13.97 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/VD6") (pinfunction "Pin_a22") (pintype "passive"))
    (pad "a23" thru_hole circle (at 16.51 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/VD1") (pinfunction "Pin_a23") (pintype "passive"))
    (pad "a24" thru_hole circle (at 19.05 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "/VD9") (pinfunction "Pin_a24") (pintype "passive"))
    (pad "a25" thru_hole circle (at 21.59 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/VD5") (pinfunction "Pin_a25") (pintype "passive"))
    (pad "a26" thru_hole circle (at 24.13 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/VD2") (pinfunction "Pin_a26") (pintype "passive"))
    (pad "a27" thru_hole circle (at 26.67 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "/VD10") (pinfunction "Pin_a27") (pintype "passive"))
    (pad "a28" thru_hole circle (at 29.21 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/VD4") (pinfunction "Pin_a28") (pintype "passive"))
    (pad "a29" thru_hole circle (at 31.75 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/VD3") (pinfunction "Pin_a29") (pintype "passive"))
    (pad "a30" thru_hole circle (at 34.29 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "/VD11") (pinfunction "Pin_a30") (pintype "passive"))
    (pad "a31" thru_hole circle (at 36.83 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "Pin_a31") (pintype "passive"))
    (pad "a32" thru_hole circle (at 39.37 -2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_a32") (pintype "passive"))
    (pad "b1" thru_hole circle (at -39.37 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 255 "/SL1") (pinfunction "Pin_b1") (pintype "passive"))
    (pad "b2" thru_hole circle (at -36.83 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 295 "/~{MRES}") (pinfunction "Pin_b2") (pintype "passive"))
    (pad "b3" thru_hole circle (at -34.29 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 305 "/SR1") (pinfunction "Pin_b3") (pintype "passive"))
    (pad "b4" thru_hole circle (at -31.75 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/VA9") (pinfunction "Pin_b4") (pintype "passive"))
    (pad "b5" thru_hole circle (at -29.21 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/VA10") (pinfunction "Pin_b5") (pintype "passive"))
    (pad "b6" thru_hole circle (at -26.67 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "/VA18") (pinfunction "Pin_b6") (pintype "passive"))
    (pad "b7" thru_hole circle (at -24.13 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "/VA19") (pinfunction "Pin_b7") (pintype "passive"))
    (pad "b8" thru_hole circle (at -21.59 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/VA20") (pinfunction "Pin_b8") (pintype "passive"))
    (pad "b9" thru_hole circle (at -19.05 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/VA21") (pinfunction "Pin_b9") (pintype "passive"))
    (pad "b10" thru_hole circle (at -16.51 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/VA22") (pinfunction "Pin_b10") (pintype "passive"))
    (pad "b11" thru_hole circle (at -13.97 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/VA23") (pinfunction "Pin_b11") (pintype "passive"))
    (pad "b12" thru_hole circle (at -11.43 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 163 "/~{YS}") (pinfunction "Pin_b12") (pintype "passive"))
    (pad "b13" thru_hole circle (at -8.89 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 76 "/~{VSYNC}") (pinfunction "Pin_b13") (pintype "passive"))
    (pad "b14" thru_hole circle (at -6.35 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 74 "/~{HSYNC}") (pinfunction "Pin_b14") (pintype "passive"))
    (pad "b15" thru_hole circle (at -3.81 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/EDCK") (pinfunction "Pin_b15") (pintype "passive"))
    (pad "b16" thru_hole circle (at -1.27 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 275 "/~{CAS0}") (pinfunction "Pin_b16") (pintype "passive"))
    (pad "b17" thru_hole circle (at 1.27 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "/~{CE0}") (pinfunction "Pin_b17") (pintype "passive"))
    (pad "b18" thru_hole circle (at 3.81 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 218 "/~{AS}") (pinfunction "Pin_b18") (pintype "passive"))
    (pad "b19" thru_hole circle (at 6.35 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 203 "/VCLK") (pinfunction "Pin_b19") (pintype "passive"))
    (pad "b20" thru_hole circle (at 8.89 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/~{DTAK}") (pinfunction "Pin_b20") (pintype "passive"))
    (pad "b21" thru_hole circle (at 11.43 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 188 "/~{CAS2}") (pinfunction "Pin_b21") (pintype "passive"))
    (pad "b22" thru_hole circle (at 13.97 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "/VD15") (pinfunction "Pin_b22") (pintype "passive"))
    (pad "b23" thru_hole circle (at 16.51 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "/VD14") (pinfunction "Pin_b23") (pintype "passive"))
    (pad "b24" thru_hole circle (at 19.05 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 36 "/VD13") (pinfunction "Pin_b24") (pintype "passive"))
    (pad "b25" thru_hole circle (at 21.59 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "/VD12") (pinfunction "Pin_b25") (pintype "passive"))
    (pad "b26" thru_hole circle (at 24.13 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 264 "/~{ASEL}") (pinfunction "Pin_b26") (pintype "passive"))
    (pad "b27" thru_hole circle (at 26.67 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 265 "/~{VRES}") (pinfunction "Pin_b27") (pintype "passive"))
    (pad "b28" thru_hole circle (at 29.21 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 230 "/~{LWR}") (pinfunction "Pin_b28") (pintype "passive"))
    (pad "b29" thru_hole circle (at 31.75 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 231 "/~{UWR}") (pinfunction "Pin_b29") (pintype "passive"))
    (pad "b30" thru_hole circle (at 34.29 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/~{M3}") (pinfunction "Pin_b30") (pintype "passive"))
    (pad "b31" thru_hole circle (at 36.83 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 266 "/~{TIME}") (pinfunction "Pin_b31") (pintype "passive"))
    (pad "b32" thru_hole circle (at 39.37 2.54 90) (size 1.55 1.55) (drill 1) (layers "*.Cu" "*.Mask")
      (net 267 "/~{CART}") (pinfunction "Pin_b32") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x32_P2.54mm_Vertical.wrl"
      (offset (xyz 39.5 -1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Diode_THT:D_A-405_P5.08mm_Vertical_AnodeUp" (layer "F.Cu")
    (at 83.693 190.246 -90)
    (descr "Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 8.128 0 90) (layer "F.SilkS"))
    (fp_text value "ISR35-100A" (at 2.54 2.47 90) (layer "F.Fab"))
    (fp_text user "A" (at 3.48 0.9 90) (layer "F.SilkS"))
    (fp_text user "A" (at 3.48 0.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.128 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 216 "+9V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 232 "+9VA") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P5.08mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:DIN8Video" (layer "F.Cu")
    (at 51.181 27.973)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8-pin DIN connector")
    (property "ki_keywords" "circular DIN connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 13.5 unlocked) (layer "F.SilkS"))
    (fp_text value "Video" (at 0 -6.5 unlocked) (layer "F.Fab"))
    (fp_text user "1" (at -11.5 5.5 unlocked) (layer "F.SilkS"))
    (fp_text user "6" (at -11.5 11 unlocked) (layer "F.SilkS"))
    (fp_text user "3" (at 9 5 unlocked) (layer "F.SilkS"))
    (fp_text user "7" (at 9 11 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -7.5 5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 209 "Net-(FB8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at -9.5 -1.5) (size 3 5) (drill oval 1.25 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 -2.5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 -2.5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 9.5 -1.5) (size 3 5) (drill oval 1.25 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.5 5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 328 "Net-(FB9-Pad1)") (pintype "passive"))
    (pad "4" thru_hole circle (at -5 7.5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 210 "Net-(FB10-Pad1)") (pintype "passive"))
    (pad "5" thru_hole circle (at 5 7.5) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 213 "Net-(U13-G_OUT)") (pintype "passive"))
    (pad "6" thru_hole circle (at -7.5 10) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 214 "Net-(U13-R_OUT)") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.5 10) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 312 "Net-(U13-C_SYNC_IN)") (pintype "passive"))
    (pad "8" thru_hole circle (at 0 10) (size 3 3) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 217 "Net-(U13-B_OUT)") (pintype "passive"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 229.87 103.886 180)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "JP7" (at -3.937 0) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 297 "/~{EOE}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 115.697 49.657 90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM35" (at -5.842 -2.54 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 175 "Net-(EM35-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_5mm" (layer "F.Cu")
    (at 272.4912 53.848)
    (descr "Mounting Hole 5mm, no annular")
    (tags "mounting hole 5mm no annular")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H14" (at 0 -6) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Inductor_THT:L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC" (layer "F.Cu")
    (at 75.565 68.961)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=7*3.3mm^2, Fastron, MICC, http://www.fastrongroup.com/image-show/70/MICC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 7mm diameter 3.3mm Fastron MICC")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB14" (at 2.54 -2.77) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.77) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 317 "Net-(C87-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 245 "Net-(RF1-AUDIO)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L7.0mm_D3.3mm_P5.08mm_Vertical_Fastron_MICC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 217.297 32.004)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 4.699) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (at 190.3924 203.6596)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "9-pin male plug pin D-SUB connector")
    (property "ki_keywords" "connector male plug D-SUB DB9")
    (attr through_hole)
    (fp_text reference "J5" (at 5.54 -2.8) (layer "F.SilkS"))
    (fp_text value "Player1" (at 5.54 18.44) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.54 13.94) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -6.96 1.42) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "0" thru_hole circle (at 18.04 1.42) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 82 "Net-(EM11-Pad3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.77 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 83 "Net-(EM12-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.54 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 84 "Net-(EM13-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 8.31 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 80 "Net-(EM4-Pad3)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 11.08 0) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 81 "Net-(EM5-Pad3)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 1.385 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "Net-(EM16-Pad3)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 4.155 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 138 "Net-(J5-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 6.925 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 156 "Net-(FB3-Pad1)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 9.695 2.84) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 147 "Net-(J5-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Ferrite_THT:LairdTech_28C0236-0JW-10" (layer "F.Cu")
    (at 57.785 198.628 90)
    (descr "Ferrite, vertical, LairdTech 28C0236-0JW-10, https://assets.lairdtech.com/home/brandworld/files/28C0236-0JW-10.pdf, JW Miller core https://www.bourns.com/products/magnetic-products/j.w.-miller-through-hole-ferrite-beads-emi-filters")
    (tags "Ferrite vertical LairdTech 28C0236-0JW-10")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr through_hole)
    (fp_text reference "FB15" (at 8.382 -0.127 90) (layer "F.SilkS"))
    (fp_text value "FerriteBead" (at 2.54 4.953 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 247 "Net-(J10-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Ferrite_THT.3dshapes/LairdTech_28C0236-0JW-10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 84.408 159.385)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C61" (at 8.048 2.159) (layer "F.SilkS"))
    (fp_text value "1uF 50V" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 300 "Net-(C61-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 303 "/SL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_1.5mm_Mask4.5mm" (layer "F.Cu")
    (at 147.574 98.044)
    (descr "Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening")
    (tags "fiducial")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID3" (at 0 -3.175) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 3.175) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 1.5) (clearance 1.5))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 227.076 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM23" (at -3.302 -0.254 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 143 "PB2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(EM23-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:RFmod" (layer "F.Cu")
    (at 79.375 21.209)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RF1" (at 19.431 40.894 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -6.985 25.4) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 244 "Net-(RF1-+B)") (pinfunction "+B") (pintype "unspecified"))
    (pad "1" thru_hole circle (at 5.08 43.18) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 244 "Net-(RF1-+B)") (pinfunction "+B") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -9.525 25.4) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 243 "Net-(RF1-VIDEO)") (pinfunction "VIDEO") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 2.54 43.18) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 243 "Net-(RF1-VIDEO)") (pinfunction "VIDEO") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -12.065 25.4) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 245 "Net-(RF1-AUDIO)") (pinfunction "AUDIO") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 0 43.18) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 245 "Net-(RF1-AUDIO)") (pinfunction "AUDIO") (pintype "unspecified"))
    (pad "4" thru_hole oval (at -15.24 27.94 180) (size 2 4) (drill oval 1 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" thru_hole oval (at -13.97 17.78 180) (size 2 4) (drill oval 1 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" thru_hole oval (at -3.175 6.985 90) (size 2 4) (drill oval 1 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" thru_hole oval (at 13.97 17.78 180) (size 2 4) (drill oval 1 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
    (pad "4" thru_hole oval (at 15.24 27.94 180) (size 2 4) (drill oval 1 2) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "GND") (pintype "unspecified"))
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 109.982 146.765 -90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C64" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 295 "/~{MRES}") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 121.031 97.663)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "JP5" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 229 "/~{RAS0}") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 251.968 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM26" (at -4.953 -0.381 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 139 "PB4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 151 "Net-(EM26-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P5.00mm" (layer "F.Cu")
    (at 58.293 78.025 90)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C31" (at 2.5 -3.5 90) (layer "F.SilkS"))
    (fp_text value "10uF 16V" (at 2.5 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.587 -4.064 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 234 "Net-(C31-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 193 "Net-(U13-AUDIO_OUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (at 249.936 209.55)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at -4.191 3.81) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Crystal:Resonator-3Pin_W6.0mm_H3.0mm" (layer "F.Cu")
    (at 248.031 190.246 -90)
    (descr "Ceramic Resomator/Filter 6.0x3.0mm^2, length*width=6.0x3.0mm^2 package, package length=6.0mm, package width=3.0mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Feedthrough capacitor")
    (property "ki_keywords" "EMI filter feedthrough capacitor")
    (attr through_hole)
    (fp_text reference "EM27" (at -4.953 -0.381 90) (layer "F.SilkS"))
    (fp_text value "100pF 50v" (at 2.5 2.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 140 "PB6") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 152 "Net-(EM27-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Resonator-3Pin_W6.0mm_H3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_E-Switch_EG1224_SPDT_Angled" (layer "F.Cu")
    (at 68.994 169.74)
    (descr "E-Switch slide switch, EG series, SPDT, right angle, http://spec_sheets.e-switch.com/specs/P040042.pdf")
    (tags "switch SPDT")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at 4 -2.95) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at 4 14.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4 1.25) (layer "F.Fab"))
    (pad "" thru_hole circle (at -2 -1.75) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at -2 4.25) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 10 -1.75) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 10 4.25) (size 2 2) (drill 1.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 232 "+9VA") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 4 0) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 199 "Net-(SW1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 8 0) (size 1.7 1.7) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 200 "unconnected-(SW1-C-Pad3)") (pinfunction "C") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_E-Switch_EG1224_SPDT_Angled.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 62.3335 116.332 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R65" (at 4.6755 1.27) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 310 "Net-(U14B-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 273 "/~{SRES}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 74.6995 156.083)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R40" (at 5.6915 0) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 272 "Net-(U12-EQ_OUT_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 89.154 141.1205 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R54" (at -5.8655 -0.127 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 278 "Net-(U11-MOR)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 158.877 199.3665 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R77" (at -1.2465 2.286 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 92 "/ZD0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 172.974 55.6495 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -6.1195 0.127 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 228 "/IPL1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 63.373 112.334 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C118" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "C" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 273 "/~{SRES}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 64.2385 77.597)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at -4.9295 -2.159) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 212 "Net-(C32-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 235 "Net-(U13-C_VIDEO_OUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 175.133 194.0795 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.0235 2.286 90) (layer "B.SilkS"))
    (fp_text value "120" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 263 "Net-(J9-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 70.358 58.1425 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R70" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 315 "Net-(C86-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 235 "Net-(U13-C_VIDEO_OUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 221.488 118.679 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C85" (at 6.157 -0.381 90) (layer "B.SilkS"))
    (fp_text value "1000pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 273 "/~{SRES}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 94.7655 177.8 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R49" (at 0.1505 2.921) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 304 "/SR2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 67.9215 158.369 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R37" (at 1.3735 2.794) (layer "B.SilkS"))
    (fp_text value "51k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 293 "Net-(C40-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 70.739 86.807 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C34" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "180pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 314 "Net-(U13-Y_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 87.884 86.2565 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 312 "Net-(U13-C_SYNC_IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 62.23 84.4315 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at -0.4045 -2.413 90) (layer "B.SilkS"))
    (fp_text value "24k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 311 "Net-(U13-I_REF)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 69.281 108.077 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C37" (at -0.061 -2.159) (layer "B.SilkS"))
    (fp_text value "100pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 325 "Net-(C37-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 74.7795 147.193 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at -5.7385 0.127) (layer "B.SilkS"))
    (fp_text value "51k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 293 "Net-(C40-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 74.8265 153.162)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 5.4375 0) (layer "B.SilkS"))
    (fp_text value "47k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 301 "Net-(C42-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 199.1125 106.934)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R67" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 74 "/~{HSYNC}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 155.956 192.5085 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R79" (at 5.0565 0.127 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 93 "/ZD2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 93.98 59.5865 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 305 "/SR1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 88.8765 156.591)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 255 "/SL1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 67.3335 116.078 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R64" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 295 "/~{MRES}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 310 "Net-(U14B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 213.421 102.997 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C77" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "1000pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "/~{M3}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 87.823 98.298 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at -5.776 0.254) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 192 "Net-(C27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(U13-B_IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 46.863 182.6495 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R66" (at 1.2465 3.429 90) (layer "B.SilkS"))
    (fp_text value "30k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 284 "Net-(R58-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 80.7485 115.443 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at -0.0235 -2.54) (layer "B.SilkS"))
    (fp_text value "3.3k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 261 "Net-(U8-SBCR)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 262 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 115.0385 111.125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R56" (at -4.5955 0.127) (layer "B.SilkS"))
    (fp_text value "5.6k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 259 "Net-(U8-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 125.984 124.526 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C88" (at -5.146 0.127 90) (layer "B.SilkS"))
    (fp_text value "47pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 307 "Net-(U8-CLK0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 138.491 114.427 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 5.141 0.254) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 194 "VDDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 118.491 71.44 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C106" (at 6.157 -0.127 270 unlocked) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 241 "Net-(U10-SC)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 183.007 54.4595 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -5.8185 0.381 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 225 "/BGACK") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 133.8815 138.176)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 296 "/~{INT}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 194.498 58.039)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C81" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "220pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/VA21") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 117.033 104.394 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C116" (at 5.273 0.254) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "/~{HSYNC}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 123.063 100.965 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C110" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 163 "/~{YS}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEGA:Expansion" (layer "B.Cu")
    (at 275.209 101.6 90)
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x30, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at 0 -18.669 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "Floppy" (at 0 4.08 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.58 270 unlocked) (layer "B.Fab"))
    (pad "a1" smd rect (at -35.56 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "GND") (pinfunction "Pin_a1") (pintype "passive"))
    (pad "a2" smd rect (at -33.02 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 186 "unconnected-(J2-Pin_a2-Pada2)") (pinfunction "Pin_a2") (pintype "passive+no_connect"))
    (pad "a3" smd rect (at -30.48 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 275 "/~{CAS0}") (pinfunction "Pin_a3") (pintype "passive"))
    (pad "a4" smd rect (at -27.94 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/VD0") (pinfunction "Pin_a4") (pintype "passive"))
    (pad "a5" smd rect (at -25.4 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/VD1") (pinfunction "Pin_a5") (pintype "passive"))
    (pad "a6" smd rect (at -22.86 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/VD2") (pinfunction "Pin_a6") (pintype "passive"))
    (pad "a7" smd rect (at -20.32 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/VD3") (pinfunction "Pin_a7") (pintype "passive"))
    (pad "a8" smd rect (at -17.78 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/VD4") (pinfunction "Pin_a8") (pintype "passive"))
    (pad "a9" smd rect (at -15.24 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "/VD5") (pinfunction "Pin_a9") (pintype "passive"))
    (pad "a10" smd rect (at -12.7 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "/VD6") (pinfunction "Pin_a10") (pintype "passive"))
    (pad "a11" smd rect (at -10.16 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "/VD7") (pinfunction "Pin_a11") (pintype "passive"))
    (pad "a12" smd rect (at -7.62 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "GND") (pinfunction "Pin_a12") (pintype "passive"))
    (pad "a13" smd rect (at -5.08 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/VD8") (pinfunction "Pin_a13") (pintype "passive"))
    (pad "a14" smd rect (at -2.54 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/VD9") (pinfunction "Pin_a14") (pintype "passive"))
    (pad "a15" smd rect (at 0 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/VD10") (pinfunction "Pin_a15") (pintype "passive"))
    (pad "a16" smd rect (at 2.54 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/VD11") (pinfunction "Pin_a16") (pintype "passive"))
    (pad "a17" smd rect (at 5.08 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/VD12") (pinfunction "Pin_a17") (pintype "passive"))
    (pad "a18" smd rect (at 7.62 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/VD13") (pinfunction "Pin_a18") (pintype "passive"))
    (pad "a19" smd rect (at 10.16 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/VD14") (pinfunction "Pin_a19") (pintype "passive"))
    (pad "a20" smd rect (at 12.7 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/VD15") (pinfunction "Pin_a20") (pintype "passive"))
    (pad "a21" smd rect (at 15.24 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "/~{ROM}") (pinfunction "Pin_a21") (pintype "passive"))
    (pad "a22" smd rect (at 17.78 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 264 "/~{ASEL}") (pinfunction "Pin_a22") (pintype "passive"))
    (pad "a23" smd rect (at 20.32 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "/~{RAS2}") (pinfunction "Pin_a23") (pintype "passive"))
    (pad "a24" smd rect (at 22.86 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "/~{FDC}") (pinfunction "Pin_a24") (pintype "passive"))
    (pad "a25" smd rect (at 25.4 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "/FRES") (pinfunction "Pin_a25") (pintype "passive"))
    (pad "a26" smd rect (at 27.94 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "VCC") (pinfunction "Pin_a26") (pintype "passive"))
    (pad "a27" smd rect (at 30.48 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 190 "unconnected-(J2-Pin_a27-Pada27)") (pinfunction "Pin_a27") (pintype "passive+no_connect"))
    (pad "a28" smd rect (at 33.02 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 232 "+9VA") (pinfunction "Pin_a28") (pintype "passive"))
    (pad "a29" smd rect (at 35.56 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 304 "/SR2") (pinfunction "Pin_a29") (pintype "passive"))
    (pad "a30" smd rect (at 38.1 -2.54 90) (size 1.75 8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "GND") (pinfunction "Pin_a30") (pintype "passive"))
    (pad "b1" smd rect (at -35.56 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "Pin_b1") (pintype "passive"))
    (pad "b2" smd rect (at -33.02 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "/~{DISK}") (pinfunction "Pin_b2") (pintype "passive"))
    (pad "b3" smd rect (at -30.48 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/VA1") (pinfunction "Pin_b3") (pintype "passive"))
    (pad "b4" smd rect (at -27.94 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/VA2") (pinfunction "Pin_b4") (pintype "passive"))
    (pad "b5" smd rect (at -25.4 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/VA3") (pinfunction "Pin_b5") (pintype "passive"))
    (pad "b6" smd rect (at -22.86 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/VA4") (pinfunction "Pin_b6") (pintype "passive"))
    (pad "b7" smd rect (at -20.32 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/VA5") (pinfunction "Pin_b7") (pintype "passive"))
    (pad "b8" smd rect (at -17.78 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VA6") (pinfunction "Pin_b8") (pintype "passive"))
    (pad "b9" smd rect (at -15.24 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/VA7") (pinfunction "Pin_b9") (pintype "passive"))
    (pad "b10" smd rect (at -12.7 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/VA8") (pinfunction "Pin_b10") (pintype "passive"))
    (pad "b11" smd rect (at -10.16 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/VA9") (pinfunction "Pin_b11") (pintype "passive"))
    (pad "b12" smd rect (at -7.62 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "Pin_b12") (pintype "passive"))
    (pad "b13" smd rect (at -5.08 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/VA10") (pinfunction "Pin_b13") (pintype "passive"))
    (pad "b14" smd rect (at -2.54 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/VA11") (pinfunction "Pin_b14") (pintype "passive"))
    (pad "b15" smd rect (at 0 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/VA12") (pinfunction "Pin_b15") (pintype "passive"))
    (pad "b16" smd rect (at 2.54 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/VA13") (pinfunction "Pin_b16") (pintype "passive"))
    (pad "b17" smd rect (at 5.08 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/VA14") (pinfunction "Pin_b17") (pintype "passive"))
    (pad "b18" smd rect (at 7.62 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/VA15") (pinfunction "Pin_b18") (pintype "passive"))
    (pad "b19" smd rect (at 10.16 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VA16") (pinfunction "Pin_b19") (pintype "passive"))
    (pad "b20" smd rect (at 12.7 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/VA17") (pinfunction "Pin_b20") (pintype "passive"))
    (pad "b21" smd rect (at 15.24 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "/~{LWR}") (pinfunction "Pin_b21") (pintype "passive"))
    (pad "b22" smd rect (at 17.78 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "/~{UWR}") (pinfunction "Pin_b22") (pintype "passive"))
    (pad "b23" smd rect (at 20.32 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "/~{CAS2}") (pinfunction "Pin_b23") (pintype "passive"))
    (pad "b24" smd rect (at 22.86 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "/~{FDHR}") (pinfunction "Pin_b24") (pintype "passive"))
    (pad "b25" smd rect (at 25.4 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "unconnected-(J2-Pin_b25-Padb25)") (pinfunction "Pin_b25") (pintype "passive+no_connect"))
    (pad "b26" smd rect (at 27.94 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "VCC") (pinfunction "Pin_b26") (pintype "passive"))
    (pad "b27" smd rect (at 30.48 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "unconnected-(J2-Pin_b27-Padb27)") (pinfunction "Pin_b27") (pintype "passive+no_connect"))
    (pad "b28" smd rect (at 33.02 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "+9VA") (pinfunction "Pin_b28") (pintype "passive"))
    (pad "b29" smd rect (at 35.56 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "/SL2") (pinfunction "Pin_b29") (pintype "passive"))
    (pad "b30" smd rect (at 38.1 -2.54 90) (size 1.75 8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "GND") (pinfunction "Pin_b30") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 67.31 54.7605 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R73" (at 1.2465 2.667 90) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 317 "Net-(C87-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 115.0385 108.585 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R57" (at -4.5955 0.127) (layer "B.SilkS"))
    (fp_text value "5.6k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 258 "Net-(U8-R)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 256.54 134.559 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C90" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "/VA1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.7475 79.883)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0.3575 -2.667) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 309 "/VREF") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 314 "Net-(U13-Y_IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 198.882 152.974 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 177.673 165.669 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 150.495 145.1845 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R69" (at 5.3575 -0.254 90) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 207 "Net-(OSC1-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 70.739 81.849 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C95" (at -4.887 0.889 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 311 "Net-(U13-I_REF)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 256.987 109.855 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C120" (at 0 3.048) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/VA7") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 62.865 145.476 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C121" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "100nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 199 "Net-(SW1-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 55.8565 162.052)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R43" (at -5.4375 0) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 282 "Net-(U14A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 276 "Net-(U12-EQ_OUT_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 69.276 104.775)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C96" (at -4.887 0.762) (layer "B.SilkS"))
    (fp_text value "12pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 326 "Net-(C96-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 325 "Net-(C37-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 151.003 192.5085 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R84" (at 5.4375 0.127 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 111 "/ZD7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 46.736 176.6805 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R58" (at 5.3575 2.794 90) (layer "B.SilkS"))
    (fp_text value "36k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 284 "Net-(R58-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 281 "Net-(U12-IN_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 63.434 31.75)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C113" (at 4.511 0.127) (layer "B.SilkS"))
    (fp_text value "39pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 312 "Net-(U13-C_SYNC_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 159.004 193.5245 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R83" (at 5.3105 0.127 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 94 "/ZD6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 115.0385 114.427 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R55" (at -4.8495 0.127) (layer "B.SilkS"))
    (fp_text value "5.6k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 260 "Net-(U8-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 132.08 124.526 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C78" (at -5.273 0.127 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 330 "Net-(U8-CLK1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 110.871 125.664 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -2.794 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 165.415 102.87)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C112" (at 0.066 -2.921) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/EDCK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 77.79 104.013 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0.32 4.953) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 262 "Net-(C28-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 87.6535 107.95)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 5.4375 -2.794) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 164 "Net-(C25-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.8275 85.852)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 3.4525 0 90) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 313 "Net-(U13-Y_OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 322 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 58.42 135.448 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 0.569 3.048 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 61.783 167.386)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C47" (at 0 2.54) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 281 "Net-(U12-IN_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 90.297 186.756 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C89" (at 0 -3.556 90) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 232 "+9VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 74.483 182.499 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C46" (at 5.014 0.127) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 281 "Net-(U12-IN_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 62.738 120.97 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C69" (at -0.32 -2.159 90) (layer "B.SilkS"))
    (fp_text value "330pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 194 "VDDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 88.839 168.91 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C39" (at -4.633 1.651) (layer "B.SilkS"))
    (fp_text value "330pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 292 "Net-(U8-SOUND)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 184.531 105.852 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C92" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 208 "Net-(C92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 67.9215 161.163 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R39" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "47k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 302 "Net-(C44-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 87.696 104.521 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at -4.76 1.524) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(C25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(U13-R_IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 242.062 200.1755 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 154 "Net-(J6-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 152 "Net-(EM27-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 110.937 202.184)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C114" (at -5.273 0.127) (layer "B.SilkS"))
    (fp_text value "150pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 318 "/~{ZRAM}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 127.381 71.44 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C108" (at 0.315 3.683 270 unlocked) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 238 "Net-(U10-~{CAS})") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 163.957 193.5245 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R82" (at -5.6115 0.254 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 95 "/ZD5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 95.824 87.884 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 88.199 200.914 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C80" (at -0.066 -2.286) (layer "B.SilkS"))
    (fp_text value "C" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 254 "Net-(U4-~{WRES})") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 204.1144 200.3025 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 135 "Net-(EM8-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 147 "Net-(J5-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 76.835 58.1 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C87" (at -5.268 0 90) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 317 "Net-(C87-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(U13-AUDIO_OUT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 48.448 60.833 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 216 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 150.434 151.638)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C122" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "C" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 206 "Net-(OSC1-Vcontrol)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 55.753 168.4255 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R42" (at 5.8185 -1.778 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 282 "Net-(U14A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 272 "Net-(U12-EQ_OUT_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 124.333 71.435 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C107" (at 4.76 0 270 unlocked) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 237 "Net-(U10-~{RAS})") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 119.507 79.695 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at -4.633 -1.143 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 186.817 165.674 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 47.94 104.394 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C73" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 61.783 163.83 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C48" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 276 "Net-(U12-EQ_OUT_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 155.067 147.127 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C82" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "20pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 207 "Net-(OSC1-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 105.791 118.938 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C103" (at 0.066 -2.54 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 312 "Net-(U13-C_SYNC_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 231.201 171.704)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C117" (at 5.4 -0.127) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 297 "/~{EOE}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 216.8925 56.515 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0.1035 -2.667) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 60 "/~{DTAK}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 75.819 193.36 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C75" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 288 "Net-(U12-OUT_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 93.8295 113.919 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at -4.8495 0.254) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 260 "Net-(U8-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 192 "Net-(C27-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 93.8295 110.744 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -4.7225 0.254) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 259 "Net-(U8-G)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 167 "Net-(C26-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 253.746 64.577 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C91" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "330pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 232 "+9VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 61.8255 161.163 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R41" (at -0.5315 -10.541) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 276 "Net-(U12-EQ_OUT_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 79.8595 181.864)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R51" (at 4.4685 -2.286) (layer "B.SilkS"))
    (fp_text value "3.3k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 300 "Net-(C61-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 87.7335 113.919)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0.1505 4.826) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 192 "Net-(C27-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.8275 82.931)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 3.5795 -0.762 90) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 327 "Net-(U13-CHROMA_OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 325 "Net-(C37-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 74.676 159.004)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C45" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 272 "Net-(U12-EQ_OUT_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 87.7335 110.744)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0.1505 6.35) (layer "B.SilkS"))
    (fp_text value "1.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 167 "Net-(C26-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 116.3555 148.336 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "47k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 295 "/~{MRES}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 250.063 64.577 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C93" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "330pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 188 "/~{CAS2}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 121.539 71.44 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C109" (at 6.035 -0.381 270 unlocked) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 242 "Net-(U10-~{DT}{slash}~{OE})") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 61.8255 158.115 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R38" (at 5.1835 1.778) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 279 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 226.695 78.674 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C119" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 267 "/~{CART}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 218.059 118.679 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at -6.03 0.381 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.8745 94.107 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at -2.8975 -1.778) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 324 "Net-(C33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 216.8125 53.34 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd exclude_from_bom)
    (fp_text reference "R68" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "220" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 218 "/~{AS}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 156.022 142.494)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 96.2895 69.088)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R50" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "75" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 303 "/SL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 88.8765 150.495 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R53" (at -4.7225 0) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 277 "Net-(U11-MOL)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 70.739 91.247 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C35" (at -0.188 4.318 90) (layer "B.SilkS"))
    (fp_text value "12pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 314 "Net-(U13-Y_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 322 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 140.081 192.339 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 4.887 -0.127 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 88.6441 162.3568 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 292 "Net-(U8-SOUND)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 73.3025 115.951)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R74" (at 3.7865 1.016) (layer "B.SilkS"))
    (fp_text value "33k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 282 "Net-(U14A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 271 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 136.591 132.334)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at -3.368 0) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 47.371 196.408 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "10nF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 290 "Net-(U12-OUT_(B))") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 87.884 80.325 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C105" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 312 "Net-(U13-C_SYNC_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 210.886 56.515 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0.701 3.302) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 63.4765 34.798 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R71" (at -4.5955 -0.889) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 316 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 185.928 54.4595 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at -5.6915 0.127 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 226 "/BR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 80.711 112.395 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 2.921) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 191 "Net-(U13-XO_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 262 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 253.492 57.47 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "dnp" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd exclude_from_bom)
    (fp_text reference "C94" (at 0.193 3.175 90) (layer "B.SilkS"))
    (fp_text value "220p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 218 "/~{AS}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 77.912 89.408)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C33" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.01u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 323 "Net-(U13-CHROMA_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 324 "Net-(C33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 116.901 101.473 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C115" (at 0.061 3.048) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "/~{VSYNC}") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 128.778 124.521 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C102" (at -5.395 -0.127 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 261 "Net-(U8-SBCR)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 61.8255 155.321 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R52" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "47k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 306 "Net-(C62-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(U12-EQ_IN_(B))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 147.955 192.3015 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R59" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 112 "/ZA0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 187.325 105.0055 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R85" (at -0.9925 -3.048 90) (layer "B.SilkS"))
    (fp_text value "10" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 161 "Net-(U4-EDCK)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 208 "Net-(C92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 47.94 91.186 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C83" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 216 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.8745 106.553)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at -2.3095 2.794) (layer "B.SilkS"))
    (fp_text value "1k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 7 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 262 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 93.8295 107.95 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at -4.7225 0.254) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 258 "Net-(U8-R)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 164 "Net-(C25-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 198.501 116.774 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 4.638 0 90) (layer "B.SilkS"))
    (fp_text value "22pF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 133.8345 135.001)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at -3.2785 0.127) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 329 "Net-(U8-SPA{slash}B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 176.022 55.6495 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -5.7385 0.254 90) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 227 "/IPL2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 6 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 206.5528 200.3025 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 146 "Net-(EM7-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 138 "Net-(J5-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 87.696 101.473 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at -6.03 0.635) (layer "B.SilkS"))
    (fp_text value "22nF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(C26-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(U13-G_IN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 236.8804 200.1501 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 155 "Net-(J6-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 153 "Net-(EM28-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 48.194 74.168 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 143.002 192.5085 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R78" (at 5.1835 -0.127 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 91 "/ZD1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 74.7795 150.114 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at -5.8655 0) (layer "B.SilkS"))
    (fp_text value "2.2k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 280 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(U12-EQ_IN_(A))") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 73.533 58.1425 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R72" (at 5.3105 -0.127 90) (layer "B.SilkS"))
    (fp_text value "1.3k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 193 "Net-(U13-AUDIO_OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 317 "Net-(C87-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 172.085 193.5715 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R81" (at 5.3575 0.127 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 97 "/ZD4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 167.132 193.5245 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "MegaDrive.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R80" (at -5.6115 -0.254 90) (layer "B.SilkS"))
    (fp_text value "4.7k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 211 "VCCQ") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 96 "/ZD3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 251.206 40.386) (mid 245.23697 45.978139) (end 239.516481 40.132)
    (layer "Edge.Cuts"))
  (gr_arc (start 136.392481 37.338) (mid 142.361511 31.745861) (end 148.082 37.592)
    (layer "Edge.Cuts"))
  (gr_arc (start 59.309 208.407) (mid 60.96 210.058) (end 59.309 211.709)
    (layer "Edge.Cuts"))
  (gr_line (start 59.309 211.709) (end 52.324 211.709)
    (layer "Edge.Cuts"))
  (gr_circle (center 256.54 28.956) (end 256.54 27.178)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 253.486481 204.47) (mid 259.455511 198.877861) (end 265.176 204.724)
    (layer "Edge.Cuts"))
  (gr_circle (center 261.62 150.114) (end 261.62 149.606)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 253.486481 207.01) (end 253.486481 204.47)
    (layer "Edge.Cuts"))
  (gr_rect (start 261.112 152.019) (end 262.128 159.639)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 136.144 204.216) (mid 142.11303 198.623861) (end 147.833519 204.47)
    (layer "Edge.Cuts"))
  (gr_arc (start 239.516481 37.592) (mid 245.485511 31.999861) (end 251.206 37.846)
    (layer "Edge.Cuts"))
  (gr_line (start 59.309 208.407) (end 52.324 208.407)
    (layer "Edge.Cuts"))
  (gr_circle (center 256.54 36.576) (end 256.54 34.798)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 261.747 49.276) (end 261.747 48.768)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 261.747 31.75) (end 261.747 31.242)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 265.176 207.264) (mid 259.20697 212.856139) (end 253.486481 207.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 147.833519 207.01) (mid 141.864489 212.602139) (end 136.144 206.756)
    (layer "Edge.Cuts"))
  (gr_rect (start 261.366 34.163) (end 262.128 47.117)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 148.082 40.132) (end 148.082 37.592)
    (layer "Edge.Cuts"))
  (gr_line (start 136.144 206.756) (end 136.144 204.216)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.082 40.132) (mid 142.11297 45.724139) (end 136.392481 39.878)
    (layer "Edge.Cuts"))
  (gr_line (start 239.516481 40.132) (end 239.516481 37.592)
    (layer "Edge.Cuts"))
  (gr_line (start 265.176 207.264) (end 265.176 204.724)
    (layer "Edge.Cuts"))
  (gr_line (start 136.392481 39.878) (end 136.392481 37.338)
    (layer "Edge.Cuts"))
  (gr_arc (start 52.324 211.709) (mid 50.673 210.058) (end 52.324 208.407)
    (layer "Edge.Cuts"))
  (gr_poly
    (pts
      (xy 261.366 51.816)
      (xy 262.128 51.816)
      (xy 262.128 53.73)
      (xy 267.208 58.73)
      (xy 276.86 58.73)
      (xy 276.86 23.114)
      (xy 267.081 23.114)
      (xy 262.128 28.73)
      (xy 262.128 29.591)
      (xy 261.366 29.591)
      (xy 261.366 23.114)
      (xy 180.594 23.114)
      (xy 179.07 25.146)
      (xy 165.608 25.146)
      (xy 163.83 23.114)
      (xy 128.397 23.114)
      (xy 127.127 25.654)
      (xy 97.282 25.527)
      (xy 96.774 23.114)
      (xy 37.592 23.114)
      (xy 37.592 214.122)
      (xy 276.86 214.122)
      (xy 276.86 168.402)
      (xy 261.112 168.402)
      (xy 261.112 164.465)
      (xy 262.128 164.465)
      (xy 262.128 167.386)
      (xy 276.86 167.386)
      (xy 276.86 141.478)
      (xy 262.128 141.351)
      (xy 262.128 147.828)
      (xy 261.112 147.828)
      (xy 261.112 139.446)
      (xy 276.86 139.446)
      (xy 276.86 60.96)
      (xy 261.366 60.96)
    )
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 261.62 161.925) (end 261.62 161.417)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 147.833519 207.01) (end 147.833519 204.47)
    (layer "Edge.Cuts"))
  (gr_line (start 251.206 40.386) (end 251.206 37.846)
    (layer "Edge.Cuts"))
  (gr_text "171-5674" (at 264.287 29.21 90) (layer "B.Cu"))
  (gr_text "1991" (at 267.716 50.8 90) (layer "B.Cu"))
  (gr_text "SEGS" (at 128.016 204.5716) (layer "B.SilkS"))
  (gr_text "2413" (at 171.577 126.238) (layer "B.SilkS"))
  (gr_text "839-" (at 263.906 53.34 90) (layer "F.SilkS"))
  (gr_text "JP5" (at 226.314 141.351) (layer "F.SilkS"))
  (gr_text "SEGA" (at 137.033 111.506 270) (layer "F.SilkS"))
  (gr_text "IC BD M5 PAL" (at 134.366 197.104) (layer "F.SilkS"))
  (gr_text "0262" (at 272.542 166.878) (layer "F.SilkS"))
  (gr_text "YAMAHA" (at 63.373 130.175) (layer "F.SilkS"))
  (gr_text "SEGA" (at 207.645 116.713 270) (layer "F.SilkS"))
  (gr_text "JP7" (at 204.47 164.465) (layer "F.SilkS"))
  (gr_text "0199" (at 265.43 52.832 90) (layer "F.SilkS"))
  (gr_text "315-5402:VA5\n316-5433:VA6" (at 191.897 141.605) (layer "F.SilkS"))
  (gr_text "JP6" (at 208.534 141.478) (layer "F.SilkS"))
  (gr_text "839-" (at 272.288 165.354) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 37.592 23.114) (xy 276.86 23.114))
    (height -16.519666)
    (gr_text "239,2680 mm" (at 157.226 5.444334) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 276.86 214.122) (xy 276.86 23.749))
    (height 29.845)
    (gr_text "190,3730 mm" (at 305.555 118.9355 90) (layer "User.1"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.3")
    (pts (xy 272.4912 53.848) (xy 272.4404 28.6004))
    (height 7.1628)
    (gr_text "25,2477 mm" (at 280.778584 41.207474 -89.8847169) (layer "User.3"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 249) (net_name "/AudioShield") (layer "F.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 276.86 23.114)
        (xy 276.86 58.674)
        (xy 267.208 58.674)
        (xy 262.128 53.721)
        (xy 262.128 28.702)
        (xy 267.081 23.114)
      )
    )
  )
  (zone (net 331) (net_name "/DCin1") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 262.128 141.351)
        (xy 276.86 141.351)
        (xy 276.86 167.386)
        (xy 262.128 167.386)
      )
    )
  )
  (zone (net 7) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0.6))
    (min_thickness 0.4) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 38.2524 25.0952)
        (xy 39.2176 24.2824)
        (xy 94.641161 24.460201)
        (xy 95.784161 25.476201)
        (xy 95.784161 27.508201)
        (xy 128.804161 27.508201)
        (xy 128.804161 25.603201)
        (xy 129.185161 25.222201)
        (xy 162.460269 25.095201)
        (xy 164.364161 27.000201)
        (xy 180.11129 27.000201)
        (xy 182.271161 25.095201)
        (xy 258.979161 25.222201)
        (xy 259.614161 25.857201)
        (xy 259.614161 60.655201)
        (xy 261.579261 62.687305)
        (xy 261.392161 171.018201)
        (xy 275.870161 171.018201)
        (xy 275.819361 213.080601)
        (xy 275.184361 213.715601)
        (xy 149.276561 213.969601)
        (xy 148.768561 213.461601)
        (xy 148.870161 205.816201)
        (xy 147.346161 201.371201)
        (xy 141.758161 198.450201)
        (xy 135.916161 201.371201)
        (xy 134.646161 205.816201)
        (xy 134.646161 213.461601)
        (xy 134.138161 213.969601)
        (xy 64.161161 214.198201)
        (xy 62.637161 212.674201)
        (xy 62.637161 208.356201)
        (xy 61.875161 207.594201)
        (xy 46.508161 207.594201)
        (xy 44.8564 205.3844)
        (xy 41.326561 204.139801)
        (xy 40.2844 204.1652)
        (xy 38.354 205.5876)
      )
    )
  )
  (zone (net 6) (net_name "VCC") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 123.444 111.506)
        (xy 123.444 90.932)
        (xy 127 90.932)
        (xy 127 80.01)
        (xy 122.682 80.01)
        (xy 122.682 54.356)
        (xy 118.11 54.356)
        (xy 118.11 81.534)
        (xy 115.57 84.074)
        (xy 115.57 102.108)
        (xy 121.412 108.712)
        (xy 121.412 111.506)
      )
    )
  )
  (zone (net 7) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 38.227 25.146)
        (xy 38.354 205.613)
        (xy 40.259 204.47)
        (xy 44.958 204.47)
        (xy 47.498 207.264)
        (xy 62.484 207.264)
        (xy 63.5 208.153)
        (xy 63.5 213.106)
        (xy 64.135 213.614)
        (xy 244.856 213.487)
        (xy 252.603 205.613)
        (xy 259.715 197.612)
        (xy 259.715 213.487)
        (xy 276.098 213.487)
        (xy 276.86 212.725)
        (xy 276.86 170.053)
        (xy 276.352 169.672)
        (xy 261.747 169.672)
        (xy 259.715 167.64)
        (xy 259.715 140.97)
        (xy 259.969 24.892)
        (xy 259.207 24.003)
        (xy 181.864 24.13)
        (xy 180.086 25.908)
        (xy 164.719 25.908)
        (xy 163.068 24.13)
        (xy 129.794 24.13)
        (xy 128.778 24.892)
        (xy 128.778 26.67)
        (xy 96.012 26.67)
        (xy 96.012 24.765)
        (xy 95.25 24.13)
        (xy 39.243 24.257)
      )
    )
  )
  (zone (net 251) (net_name "Net-(J110-Pin_4)") (layer "B.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 263.779 39.878)
        (xy 270.51 39.878)
        (xy 270.51 35.052)
        (xy 265.684 35.052)
        (xy 265.684 38.608)
        (xy 263.779 38.608)
      )
    )
  )
  (zone (net 332) (net_name "/DCin2") (layer "B.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 262.128 141.351)
        (xy 276.86 141.351)
        (xy 276.86 167.386)
        (xy 262.128 167.386)
      )
    )
  )
  (zone (net 248) (net_name "Net-(J110-Pin_2)") (layer "B.Cu") (hatch edge 0.5)
    (priority 7)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 267.208 42.545)
        (xy 268.097 43.434)
        (xy 270.51 43.434)
        (xy 270.51 48.514)
        (xy 268.732 48.514)
        (xy 266.192 50.419)
        (xy 266.192 54.991)
        (xy 268.732 57.404)
        (xy 268.732 58.166)
        (xy 267.335 58.166)
        (xy 262.763 53.594)
        (xy 262.763 42.545)
      )
    )
  )
)
