<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="40.64" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="38.1" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="38.1" y1="2.54" x2="38.1" y2="40.64" width="0" layer="20"/>
<wire x1="38.1" y1="40.64" x2="35.56" y2="43.18" width="0" layer="20" curve="90"/>
<wire x1="35.56" y1="43.18" x2="24.384" y2="43.18" width="0" layer="20"/>
<wire x1="24.384" y1="43.18" x2="19.694421875" y2="40.005" width="0" layer="20" curve="-68.198591"/>
<wire x1="19.694421875" y1="40.005" x2="17.897578125" y2="40.005" width="0" layer="20"/>
<wire x1="17.897578125" y1="40.005" x2="13.208" y2="43.18" width="0" layer="20" curve="-68.198591"/>
<wire x1="13.208" y1="43.18" x2="2.54" y2="43.18" width="0" layer="20"/>
<wire x1="2.54" y1="43.18" x2="0" y2="40.64" width="0" layer="20" curve="90"/>
<text>Atmel SAM D09</text>
<text>RESET</text>
<text>PWR</text>
<text>PA25</text>
<text>VDD</text>
<text>PA05</text>
<text>PA14</text>
<text>PA15</text>
<text>PA28/!RST</text>
<text>PA30</text>
<text>GND</text>
<text>GND</text>
<text>PA31</text>
<text>PA24</text>
<text>PA25</text>
<text>PA02</text>
<text>PA04</text>
<text>VDD</text>
<text>C4</text>
<text>C5</text>
<text>C1</text>
<text>C3</text>
<text>R3</text>
<text>R4</text>
<text>R2</text>
<text>R1</text>
<text>C2</text>
<text>CORTEX DEBUG</text>
<text>D.W. 3/5/2016</text>
<text>CR2032</text>
<text>SAMD09C13A
XOSC 32.768kHz
VDD 2.4V-3.6V</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CR2032-SMD">
</package>
</packages>
</library>
<library name="SparkFun-ConnectorsNEW">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;For debuggers and/or programemrs that support the Cortex Debug Connector (10-pin) interface.&lt;/p&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.digikey.com/product-detail/en/20021111-00010T4LF/609-3712-ND/2209072"&gt;Example Digikey Part&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="_CustomParts">
<packages>
<package name="SO14">
</package>
<package name="C200C32768">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="adafruit" package="C0603" value="22p"/>
<element name="C5" library="adafruit" package="C0603" value="22p"/>
<element name="C3" library="adafruit" package="C0603" value="100n"/>
<element name="JP3" library="SparkFun-ConnectorsNEW" package="2X5-PTH-1.27MM" value="CORTEX_DEBUGPTH"/>
<element name="JP1" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="10k"/>
<element name="R2" library="adafruit" package="R0603" value="580"/>
<element name="U$1" library="_CustomParts" package="SO14" value="SAMD09_14SOIC"/>
<element name="U$2" library="_CustomParts" package="C200C32768" value="C200C32768"/>
<element name="H1" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H2" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H3" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H4" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="100n"/>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="580"/>
<element name="R4" library="adafruit" package="R0603" value="580"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-SMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="adafruit" package="CR2032-SMD" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="PA08">
<contactref element="U$2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="PA09">
<contactref element="U$2" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$1" pad="11"/>
<contactref element="C3" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP2" pad="7"/>
<contactref element="H1" pad="B3,3"/>
<contactref element="H2" pad="B3,3"/>
<contactref element="H3" pad="B3,3"/>
<contactref element="H4" pad="B3,3"/>
<contactref element="C1" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="U$3" pad="-"/>
</signal>
<signal name="PA05">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PA14">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PA15">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PA28">
<contactref element="U$1" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP3" pad="10"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="PA30">
<contactref element="U$1" pad="7"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="PA31">
<contactref element="U$1" pad="8"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="PA24">
<contactref element="U$1" pad="9"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="PA25">
<contactref element="U$1" pad="10"/>
<contactref element="JP2" pad="4"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="3V">
<contactref element="U$1" pad="12"/>
<contactref element="R1" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C1" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="U$3" pad="+$1"/>
<contactref element="U$3" pad="+$2"/>
</signal>
<signal name="PA02">
<contactref element="U$1" pad="13"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="PA04">
<contactref element="U$1" pad="14"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED2" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
