(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 19)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 154.6 135.8)
    (grid_origin 121.4 90.8)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
  )
  (module "BJW_Libraries:NKK G22 SPST Switch" (layer F.Cu) (tedit 5FF2082F)
    (at 162.1 124.5)
    (fp_text reference SW1 (at 0.635 2.54) (layer F.SilkS) hide)
    (fp_text value SW_DPDT (at 0 1) (layer F.Fab))
    (pad 6 thru_hole circle (at 2.54 1.23) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad1)"))
    (pad 5 thru_hole circle (at 0 1.23) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at -2.54 1.23) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 -1.31) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -1.31) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -1.31) (size 1.8 1.8) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad1)"))
    (model "${KIBJWLIB}/BJW-3dmodels/NKK G22AP.stp"
      (offset (xyz 0 0 5.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module BJW_Libraries:2_Pin_Header_.150 (layer F.Cu) (tedit 5FF2075F)
    (at 158.78 118.8 180)
    (fp_text reference J2 (at 0 2.6 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 -2.6 180) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 1.905 0 180) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at -1.905 0 180) (size 2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad1)"))
  )
  (module BJW_Libraries:ScrewTerminal_.150_x2 (layer F.Cu) (tedit 5FF0EA64)
    (at 158.78 131.9 180)
    (descr "<b>WR-TBL Serie 2433 - 3.81 mm Horizontal Entry Modular w. Rising Cage Clamp <br></b>Max Height =9.1mm , Pitch 3.81mm , 6 Pins")
    (fp_text reference J1 (at 0 -5.135) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 4.12 4.865) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.905 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -1.905 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
  )
  (gr_text "OP\n" (at 168.4 124.4) (layer F.SilkS))
  (gr_text LP (at 155.9 124.4) (layer F.SilkS))
  (gr_line (start 169.6 117.3) (end 169.6 135.8) (layer Edge.Cuts) (width 0.05))
  (gr_text Zmin (at 156.9 134.3) (layer B.SilkS))
  (gr_text Zmax (at 160.9 134.3) (layer B.SilkS))
  (gr_line (start 154.6 117.3) (end 169.6 117.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.6 135.8) (end 154.6 117.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.6 135.8) (end 154.6 135.8) (layer Edge.Cuts) (width 0.05))
)
