(kicad_pcb (version 20171130) (host pcbnew 5.1.6-1.fc32)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 515)
    (zones 0)
    (modules 84)
    (nets 24)
  )
  (page USLetter)
  (title_block
    (title "Multi Output Power Supply")
    (date 2020-09-20)
    (rev 2)
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.13)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (via_size 0.381)
    (via_drill 0.254)
    (via_min_size 0.02)
    (via_min_drill 0.01)
    (uvia_size 0.027)
    (uvia_drill 0.013)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(F1-Pad2)")
  (net 2 "Net-(F1-Pad1)")
  (net 3 "Net-(C11-Pad1)")
  (net 4 "Net-(C10-Pad2)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D9-Pad1)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(R2-Pad2)")
  (net 12 Earth)
  (net 13 "Net-(C9-Pad1)")
  (net 14 "Net-(C12-Pad2)")
  (net 15 "Net-(C21-Pad1)")
  (net 16 "Net-(C22-Pad2)")
  (net 17 "Net-(C23-Pad1)")
  (net 18 "Net-(C24-Pad2)")
  (net 19 "Net-(R6-Pad2)")
  (net 20 /REG1/V_POS)
  (net 21 /REG1/V_NEG)
  (net 22 /REG1/vb+)
  (net 23 /REG1/vb-)
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.2)
    (via_dia 0.381)
    (via_drill 0.254)
    (uvia_dia 0.027)
    (uvia_drill 0.013)
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R6-Pad2)")
  )
  (net_class AC ""
    (clearance 1.5)
    (trace_width 1.5)
    (via_dia 2)
    (via_drill 0.3)
    (uvia_dia 0.027)
    (uvia_drill 0.013)
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (net_class "DC Power" ""
    (clearance 0.13)
    (trace_width 0.4)
    (via_dia 0.4)
    (via_drill 0.254)
    (uvia_dia 0.027)
    (uvia_drill 0.013)
    (add_net /REG1/V_NEG)
    (add_net /REG1/V_POS)
    (add_net /REG1/vb+)
    (add_net /REG1/vb-)
    (add_net Earth)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D9-Pad1)")
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3269P_Horizontal (layer F.Cu) (tedit 5F6911FF)
    (at 133.9 62.4 180)
    (descr "Potentiometer, horizontal, Bourns 3269P, https://www.bourns.com/docs/Product-Datasheets/3269.pdf")
    (tags "Potentiometer horizontal Bourns 3269P")
    (attr smd)
    (fp_text reference RV1 (at 0 -4.425) (layer F.SilkS))
    (fp_text value 5K (at 0 4.425) (layer F.Fab))
    (fp_text user %R (at -0.05 0) (layer F.Fab))
    (pad 3 smd rect (at 3.2 2.54 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 12 Earth))
    (pad 2 smd rect (at -3.2 0 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 12 Earth))
    (pad 1 smd rect (at 3.2 -2.54 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3269P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F601311)
    (at 122.4 62.4 180)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J5 (at 5.75 -0.75) (layer F.SilkS))
    (fp_text value adj (at 6.25 1.75) (layer F.Fab))
    (fp_text user %R (at 1.27 2) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Earth))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTVN02A150.wrl"
      (offset (xyz -1.5 -3.5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 139.175 111.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 139.225 95.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.175 115.7026 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 110.1 90.3 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D17 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C24-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 126.6 88.475 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C21-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 125.475 95.125 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U5 (at 0 -6.65 90) (layer F.SilkS))
    (fp_text value LD1085 (at 0 6.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 /REG1/V_POS))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 114 95.1 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U6 (at 0 -6.65 90) (layer F.SilkS))
    (fp_text value LM337_TO263 (at 0 6.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C22-Pad2)"))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C24-Pad2)"))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 21 /REG1/V_NEG))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 121.6 107.5 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D10 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 2.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 20 /REG1/V_POS))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137.525 101.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C23-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137.425 105.225 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 104.745 99.375 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.8 (layer F.Cu) (tedit 5BCA39CF)
    (at 143.65 100.7 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C25 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 17 "Net-(C23-Pad1)"))
    (pad 2 smd roundrect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 104.745 94.975 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 117.875 107.475 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D13 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 143.675 111.675 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D14 (at 0 2.5 180) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.3 115.7 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /REG1/V_POS))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5F60134D)
    (at 151.4 100.6 90)
    (descr "Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J6 (at 2.54 -12.25 90) (layer F.SilkS))
    (fp_text value +/-out (at 2.54 -12 90) (layer F.Fab))
    (fp_text user %R (at 3.2 -13.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(C24-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Earth))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTVN03A150.wrl"
      (offset (xyz -1 -3.5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.675 105.45 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 115.125 88.4625 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.8 (layer F.Cu) (tedit 5BCA39CF)
    (at 143.65 95.775)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C26 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 12 Earth))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.95 99.475 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R6-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 124.125 88.3 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C23-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 86.3788 99.475 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 101.2398 97.175 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 3.4 270) (layer B.SilkS))
    (fp_text value TL071 (at 0 -3.4 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad2)"))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)"))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 129.35 107.475 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D12 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 2.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 143.725 95.175)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D21 (at 0 2.5) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 2.5) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformers:Hammond_229_series_low_profile_transformers (layer F.Cu) (tedit 5F601064)
    (at 100.9 113.9 90)
    (fp_text reference T1 (at 26.416 -33.528 90) (layer F.SilkS))
    (fp_text value Hammond_229B34 (at 25.4 -12.446 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -12.7 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 0 -38.1 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 4 thru_hole circle (at 0 -25.4 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 50.8 0 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 6 thru_hole circle (at 50.8 -12.7 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 7 thru_hole circle (at 50.8 -38.1 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 8 thru_hole circle (at 50.8 -25.4 90) (size 2.824 2.824) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model "${LOCAL_LIBS}/local/Transformers.pretty/Hammond 229/Hammond 229B34.wrl"
      (offset (xyz -7.5 -7 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 139.275 101.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 126.6 105.675 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.325 98.575 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /REG1/V_POS))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock-3_P5.08mm (layer F.Cu) (tedit 5F66FEEA)
    (at 52.1 98.6 270)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1 (at 5.05 4.7 90) (layer F.SilkS))
    (fp_text value "AC IN" (at 2.54 5.08 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 12 Earth))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTTA03416.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_18x22 (layer F.Cu) (tedit 5BCA39D1)
    (at 142.9 76.4 180)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1821, 18.0x22.0mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at 0 -10.55) (layer F.SilkS))
    (fp_text value 3000uF (at 0 10.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -6.75 0 180) (size 8.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.028409)
      (net 20 /REG1/V_POS))
    (pad 2 smd roundrect (at 6.75 0 180) (size 8.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.028409)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_18x22.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 65.396 71.1 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D1 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 3 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad "" smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 78 83.3 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D6 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 20 /REG1/V_POS))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Mounting_Hole_Plated_M2.5 (layer F.Cu) (tedit 5F5E4857)
    (at 51.66 116.02)
    (fp_text reference H4 (at 0.3556 1.7018) (layer F.SilkS) hide)
    (fp_text value hole (at 0.9906 -1.8796) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.75) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (module footprints:Mounting_Hole_Plated_M2.5 (layer F.Cu) (tedit 5F5E4857)
    (at 51.1 65.3)
    (fp_text reference H3 (at 0.3556 1.7018) (layer F.SilkS) hide)
    (fp_text value hole (at 0.9906 -1.8796) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.75) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 89.85 97.275 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0 3.4 90) (layer B.SilkS))
    (fp_text value TL071 (at 0 -3.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R6-Pad2)"))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C22-Pad2)"))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 117.85 90.275 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D19 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C22-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Mounting_Hole_Plated_M2.5 (layer F.Cu) (tedit 5F5E4857)
    (at 150.4 62.3)
    (fp_text reference H2 (at 0.3556 1.7018) (layer F.SilkS) hide)
    (fp_text value hole (at 0.9906 -1.8796) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.75) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (module footprints:Mounting_Hole_Plated_M2.5 (layer F.Cu) (tedit 5F5E4857)
    (at 150.9 116.8)
    (fp_text reference H1 (at 0.3556 1.7018) (layer F.SilkS) hide)
    (fp_text value hole (at 0.9906 -1.8796) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.7 4.7) (drill 2.75) (layers *.Cu *.Mask)
      (net 12 Earth))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 112.625 88.2625 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C22-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 76.3 92.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C53 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /REG1/V_POS))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.8 (layer F.Cu) (tedit 5BCA39CF)
    (at 143.625 105.725)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C14 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 12 Earth))
    (pad 2 smd roundrect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.8 (layer F.Cu) (tedit 5BCA39CF)
    (at 143.575 110.95 180)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C13 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 3 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 139.175 105.425 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F601311)
    (at 133.5 117.4)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at -0.1 -8.25) (layer F.SilkS))
    (fp_text value "power led" (at 1.65 -6.5) (layer F.Fab))
    (fp_text user %R (at -0.1 -8.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 /REG1/V_POS))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(D9-Pad1)"))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTVN02A150.wrl"
      (offset (xyz -1.5 -3.5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 90.7 83.3 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D7 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 12 Earth))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 83.2 104.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C58 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133 112.9 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value LED (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /REG1/V_POS))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 83.05 102.15)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C56 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 103.4 83.3 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D8 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 12 Earth))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 106.269 99.375 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(R2-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 124.125 105.475 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 240 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 103.4452 71.1 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D4 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (pad 3 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad "" smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Fuseholder5x20_horiz_open_lateral_Type-II (layer F.Cu) (tedit 5F5E911C)
    (at 54.7 75.1 270)
    (descr "Fuseholder, 5x20, open, horizontal, Type-II, lateral,")
    (tags "Fuseholder 5x20 open horizontal Type-II lateral Sicherungshalter offen ")
    (fp_text reference F1 (at 8.05 2.8 90) (layer F.SilkS))
    (fp_text value 120mA (at 7.8 0.8 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 5.08 270) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 15.32 5.08 270) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 15.32 0 270) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad2)"))
    (model "${LOCAL_LIBS}/local/3dmodels/LittleFuze/111 Series.wrl"
      (offset (xyz -2.5 -5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 76.2 104 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C57 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 78 71.1 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D2 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 3 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad "" smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 65.4 83.3 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D5 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 20 /REG1/V_POS))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 82.1 97.15 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U14 (at 0 3.4 90) (layer B.SilkS))
    (fp_text value L79L15_SO8 (at 0 -3.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 143.775 101.35 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D20 (at 0 2.5 180) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 143.7 105.5)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D15 (at 0 2.5 180) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 12 Earth))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 121.6 90.35 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D16 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 2.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 20 /REG1/V_POS))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5F60134D)
    (at 151.4 109.9 90)
    (descr "Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J4 (at 2.25 -12.75 90) (layer F.SilkS))
    (fp_text value +/-out (at 2 -12.25 90) (layer F.Fab))
    (fp_text user %R (at 2.75 -13.25 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(C12-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Earth))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad1)"))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTVN03A150.wrl"
      (offset (xyz -1 -3.5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Terminal_Block:TerminalBlock_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5F601311)
    (at 140.2 117.4)
    (descr "Terminal Block TE 282834-2, 2 pins, pitch 2.54mm, size 5.54x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-2 pitch 2.54mm size 5.54x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J3 (at -2.3 -7.75) (layer F.SilkS))
    (fp_text value adj (at -1.05 -5.75) (layer F.Fab))
    (fp_text user %R (at -2.3 -7.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Earth))
    (model "${LOCAL_LIBS}/local/Connector_Terminal_Block.pretty/On Shore Technology Inc/OSTVN02A150.wrl"
      (offset (xyz -1.5 -3.5 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 129.35 90.325 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D18 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 76.05 102.05 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C55 (at 0 1.65) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 75.1 97.1 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U13 (at 0 3.4 90) (layer B.SilkS))
    (fp_text value L78L15_SO8 (at 0 -3.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 /REG1/V_POS))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.15 98.575 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 80.85 92.35)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C54 (at 0 1.43) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137.5 94.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.3892 99.475 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C21-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer B.Cu) (tedit 5A70A390)
    (at 90.7 71.1 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference D3 (at 0 4.5 90) (layer B.SilkS))
    (fp_text value MBRD6100CTTR (at 0 -4.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (pad 3 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad "" smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers B.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 115.1 105.65 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_18x22 (layer F.Cu) (tedit 5BCA39D1)
    (at 119.6 76.5 180)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1821, 18.0x22.0mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -10.55) (layer F.SilkS))
    (fp_text value 3000uF (at 0 10.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -6.75 0 180) (size 8.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.028409)
      (net 12 Earth))
    (pad 2 smd roundrect (at 6.75 0 180) (size 8.8 9.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.028409)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_18x22.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 110.1 107.45 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D11 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value S1M-13-F (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 21 /REG1/V_NEG))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.6 112.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /REG1/V_NEG))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137.425 111.925 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.3892 95.075 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 1.43 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /REG1/vb+))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 125.475 112.275 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U2 (at 0 -6.65 90) (layer F.SilkS))
    (fp_text value LD1085 (at 0 6.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C9-Pad1)"))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 /REG1/V_POS))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 3 "Net-(C11-Pad1)"))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 114.0038 112.2526 270)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U3 (at 0 -6.65 90) (layer F.SilkS))
    (fp_text value LM337_TO263 (at 0 6.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C10-Pad2)"))
    (pad 3 smd rect (at -5.775 2.54 270) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at 3.375 0 270) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 21 /REG1/V_NEG))
    (pad "" smd rect (at 5.8 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 270) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775 270) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3269P_Horizontal (layer F.Cu) (tedit 5F6911FF)
    (at 149.4 89.6 180)
    (descr "Potentiometer, horizontal, Bourns 3269P, https://www.bourns.com/docs/Product-Datasheets/3269.pdf")
    (tags "Potentiometer horizontal Bourns 3269P")
    (attr smd)
    (fp_text reference RV2 (at 6.25 0.2 90) (layer F.SilkS))
    (fp_text value 5K (at 0 4.425) (layer F.Fab))
    (fp_text user %R (at -0.05 0) (layer F.Fab))
    (pad 1 smd rect (at 3.2 -2.54 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at -3.2 0 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 12 Earth))
    (pad 3 smd rect (at 3.2 2.54 180) (size 3.3 1.19) (layers F.Cu F.Paste F.Mask)
      (net 12 Earth))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3269P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 97.725 99.375 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 Earth))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /REG1/vb-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "PWR LED" (at 128.8 117.7 180) (layer B.SilkS))
  (gr_text " ~    ---     ~\nAC   GND  AC" (at 57.2 102.9 90) (layer B.SilkS))
  (gr_text "CH1 POT" (at 134 62.5 180) (layer B.SilkS))
  (gr_text "CH2 POT\n" (at 149.7 89.3 180) (layer B.SilkS))
  (gr_text CH2 (at 153.6 98.3 90) (layer B.SilkS))
  (gr_text CH1 (at 153.7 107.4 90) (layer B.SilkS))
  (gr_text "CH1\nADJ" (at 145.7 118 180) (layer B.SilkS))
  (gr_text "CH 2\nADJ" (at 116.2 62.2 180) (layer B.SilkS))
  (gr_text "Op Amp Power Supply V 2.0\nmarsairforce@gmail.com 2020-09-23\n" (at 131.8 68.9 180) (layer B.SilkS))
  (dimension 9.100824 (width 0.15) (layer Cmts.User)
    (gr_text "9.101 mm" (at 128.042322 315.04619 349.5543779) (layer Cmts.User))
    (feature1 (pts (xy 133.95 308.1) (xy 132.646696 315.169437)))
    (feature2 (pts (xy 125 306.45) (xy 123.696696 313.519437)))
    (crossbar (pts (xy 123.803015 312.942734) (xy 132.753015 314.592734)))
    (arrow1a (pts (xy 132.753015 314.592734) (xy 131.538861 314.965199)))
    (arrow1b (pts (xy 132.753015 314.592734) (xy 131.7515 313.811794)))
    (arrow2a (pts (xy 123.803015 312.942734) (xy 124.80453 313.723674)))
    (arrow2b (pts (xy 123.803015 312.942734) (xy 125.017169 312.570269)))
  )
  (gr_line (start 154.9 57.9) (end 154.9 121.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 46.834 121.1) (end 154.9 121.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 46.9 57.9) (end 154.9 57.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 46.9 57.9) (end 46.834 121.1) (layer Edge.Cuts) (width 0.05))
  (zone (net 12) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.916 121.1) (xy 46.834 121.1) (xy 46.802 57.9) (xy 154.884 57.9)
      )
    )
  )
  (zone (net 12) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.916 121.1) (xy 46.834 121.1) (xy 46.802 57.9) (xy 154.884 57.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.14 118.364) (xy 59.69 118.364) (xy 59.69 109.474) (xy 104.14 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.14 121.158) (xy 59.69 121.158) (xy 59.69 109.474) (xy 104.14 109.474)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.15 101.6) (xy 46.736 101.6) (xy 46.736 87.884) (xy 57.15 87.884)
      )
    )
  )
)
