(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 463)
    (no_connects 1)
    (area 67.999499 81.999499 140.000501 100.000501)
    (thickness 1.6)
    (drawings 222)
    (tracks 1841)
    (zones 0)
    (modules 141)
    (nets 107)
  )
  (page A4 portrait)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.19)
    (trace_clearance 0.127)
    (zone_clearance 0.128)
    (zone_45_only yes)
    (trace_min 0.126)
    (segment_width 0.1)
    (edge_width 0.02)
    (via_size 0.7)
    (via_drill 0.4)
    (via_min_size 0.1)
    (via_min_drill 0.1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.2 5.2)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCC609)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../../../Desktop/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(Q1-Pad1)")
  (net 3 "Net-(Q2-Pad1)")
  (net 4 VSS)
  (net 5 "Net-(Q3-Pad1)")
  (net 6 "Net-(Q5-Pad1)")
  (net 7 "Net-(Q6-Pad1)")
  (net 8 "Net-(C1-Pad1)")
  (net 9 "Net-(C2-Pad1)")
  (net 10 "Net-(C3-Pad1)")
  (net 11 "Net-(U4-Pad4)")
  (net 12 "Net-(U5-Pad4)")
  (net 13 "Net-(U6-Pad4)")
  (net 14 "Net-(U7-Pad4)")
  (net 15 "Net-(U7-Pad2)")
  (net 16 "Net-(U7-Pad3)")
  (net 17 "Net-(U7-Pad20)")
  (net 18 "Net-(U7-Pad21)")
  (net 19 "Net-(U7-Pad22)")
  (net 20 "Net-(U7-Pad23)")
  (net 21 "Net-(U7-Pad33)")
  (net 22 "Net-(U7-Pad40)")
  (net 23 "Net-(U7-Pad50)")
  (net 24 "Net-(U7-Pad51)")
  (net 25 "Net-(U7-Pad52)")
  (net 26 "Net-(U7-Pad53)")
  (net 27 "Net-(U7-Pad54)")
  (net 28 "Net-(U7-Pad55)")
  (net 29 "Net-(U7-Pad56)")
  (net 30 "Net-(U7-Pad25)")
  (net 31 "Net-(U7-Pad58)")
  (net 32 "Net-(U7-Pad59)")
  (net 33 "Net-(U7-Pad28)")
  (net 34 "Net-(U7-Pad29)")
  (net 35 "Net-(U7-Pad30)")
  (net 36 "Net-(P1-Pad1)")
  (net 37 "Net-(P2-Pad1)")
  (net 38 "Net-(P3-Pad1)")
  (net 39 SH1)
  (net 40 SH2)
  (net 41 SH3)
  (net 42 C1)
  (net 43 C2)
  (net 44 C3)
  (net 45 "Net-(C17-Pad2)")
  (net 46 "Net-(C18-Pad2)")
  (net 47 VCC)
  (net 48 SENS_SUPPLY)
  (net 49 "Net-(R6-Pad2)")
  (net 50 "Net-(R7-Pad2)")
  (net 51 "Net-(R8-Pad2)")
  (net 52 "Net-(R10-Pad2)")
  (net 53 "Net-(R11-Pad2)")
  (net 54 SENS_1)
  (net 55 SENS_2)
  (net 56 SENS_3)
  (net 57 I1)
  (net 58 I2)
  (net 59 I3)
  (net 60 LI1)
  (net 61 HI1)
  (net 62 LI2)
  (net 63 HI2)
  (net 64 LI3)
  (net 65 HI3)
  (net 66 "Net-(C23-Pad1)")
  (net 67 "Net-(C23-Pad2)")
  (net 68 "Net-(C22-Pad2)")
  (net 69 +9V)
  (net 70 "Net-(C26-Pad2)")
  (net 71 "Net-(C27-Pad1)")
  (net 72 "Net-(C27-Pad2)")
  (net 73 "Net-(P10-Pad2)")
  (net 74 USB-DM)
  (net 75 USB-DP)
  (net 76 "Net-(D3-Pad1)")
  (net 77 "Net-(D4-Pad1)")
  (net 78 LED_GREEN)
  (net 79 LED_RED)
  (net 80 HALL_1)
  (net 81 HALL_2)
  (net 82 HALL_3)
  (net 83 SWCLK)
  (net 84 SWDIO)
  (net 85 NRST)
  (net 86 "Net-(C30-Pad1)")
  (net 87 "Net-(C31-Pad1)")
  (net 88 SERVO)
  (net 89 "Net-(P10-Pad1)")
  (net 90 TEMP_MOTOR)
  (net 91 RX)
  (net 92 TX)
  (net 93 EN)
  (net 94 servoi)
  (net 95 "Net-(C77-Pad2)")
  (net 96 "Net-(R1-Pad3)")
  (net 97 "Net-(R1-Pad4)")
  (net 98 "Net-(R2-Pad3)")
  (net 99 "Net-(R2-Pad4)")
  (net 100 "Net-(R3-Pad3)")
  (net 101 "Net-(R3-Pad4)")
  (net 102 "Net-(Q4-Pad1)")
  (net 103 "Net-(R9-Pad2)")
  (net 104 "Net-(R4-Pad2)")
  (net 105 "Net-(R35-Pad1)")
  (net 106 "Net-(R35-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.19)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net C1)
    (add_net C2)
    (add_net C3)
    (add_net EN)
    (add_net HALL_1)
    (add_net HALL_2)
    (add_net HALL_3)
    (add_net HI1)
    (add_net HI2)
    (add_net HI3)
    (add_net I1)
    (add_net I2)
    (add_net I3)
    (add_net LED_GREEN)
    (add_net LED_RED)
    (add_net LI1)
    (add_net LI2)
    (add_net LI3)
    (add_net NRST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C27-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C77-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(R1-Pad3)")
    (add_net "Net-(R1-Pad4)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(R2-Pad4)")
    (add_net "Net-(R3-Pad3)")
    (add_net "Net-(R3-Pad4)")
    (add_net "Net-(R35-Pad1)")
    (add_net "Net-(R35-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad20)")
    (add_net "Net-(U7-Pad21)")
    (add_net "Net-(U7-Pad22)")
    (add_net "Net-(U7-Pad23)")
    (add_net "Net-(U7-Pad25)")
    (add_net "Net-(U7-Pad28)")
    (add_net "Net-(U7-Pad29)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad30)")
    (add_net "Net-(U7-Pad33)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad40)")
    (add_net "Net-(U7-Pad50)")
    (add_net "Net-(U7-Pad51)")
    (add_net "Net-(U7-Pad52)")
    (add_net "Net-(U7-Pad53)")
    (add_net "Net-(U7-Pad54)")
    (add_net "Net-(U7-Pad55)")
    (add_net "Net-(U7-Pad56)")
    (add_net "Net-(U7-Pad58)")
    (add_net "Net-(U7-Pad59)")
    (add_net RX)
    (add_net SENS_1)
    (add_net SENS_2)
    (add_net SENS_3)
    (add_net SENS_SUPPLY)
    (add_net SERVO)
    (add_net SH1)
    (add_net SH2)
    (add_net SH3)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TEMP_MOTOR)
    (add_net TX)
    (add_net USB-DM)
    (add_net USB-DP)
    (add_net VCC)
    (add_net VDD)
    (add_net VSS)
    (add_net servoi)
  )
  (net_class 05 ""
    (clearance 0.127)
    (trace_width 0.3)
    (via_dia 0.46)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class abc ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class vss ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5949890A)
    (at 78.1 97.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(R35-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.27mm (layer F.Cu) (tedit 58EFBF8F)
    (at 71 85)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch1.27mm (at 0 1.695) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.695) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.2 5.2) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.27mm (layer F.Cu) (tedit 58EFBF84)
    (at 71 97)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch1.27mm (at 0 1.695) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.695) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.2 5.2) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:2512R (layer B.Cu) (tedit 58EE59F1)
    (at 101 96.2)
    (fp_text reference R2 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 3 smd rect (at -2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R2-Pad3)"))
    (pad 4 smd rect (at 2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(R2-Pad4)"))
    (pad 1 smd rect (at -2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (pad 1 smd rect (at -2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer F.Cu) (tedit 58EE590B)
    (at 114.005 96.3 180)
    (fp_text reference Q4 (at -3.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 5.77 -0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (pad 3 smd rect (at 5.77 0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (pad 3 smd rect (at 5.77 1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (pad 1 smd rect (at 0 1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0 0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 3.555 0 180) (size 3.65 4.31) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (pad 3 smd rect (at 5.77 -1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer B.Cu) (tedit 58EE59FF)
    (at 108.445 91)
    (fp_text reference Q1 (at -1.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 3.5) (layer B.Fab))
    (pad 3 smd rect (at 5.77 0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at 0 -1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0 -0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (pad 2 smd rect (at 0 0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (pad 2 smd rect (at 0 1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (pad 3 smd rect (at 3.555 0) (size 3.65 4.31) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer F.Cu) (tedit 58EE58F8)
    (at 114 91 180)
    (fp_text reference Q2 (at -3.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 5.77 -0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (pad 3 smd rect (at 5.77 0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (pad 3 smd rect (at 5.77 1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (pad 1 smd rect (at 0 1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0 0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 3.555 0 180) (size 3.65 4.31) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (pad 3 smd rect (at 5.77 -1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer B.Cu) (tedit 58EE5A02)
    (at 108.445 96.3)
    (fp_text reference Q3 (at -1.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 3.5) (layer B.Fab))
    (pad 3 smd rect (at 5.77 0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at 0 -1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0 -0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (pad 2 smd rect (at 0 0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (pad 2 smd rect (at 0 1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (pad 3 smd rect (at 3.555 0) (size 3.65 4.31) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer B.Cu) (tedit 58EE59FD)
    (at 108.445 85.7)
    (fp_text reference Q5 (at -1.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 3.5) (layer B.Fab))
    (pad 3 smd rect (at 5.77 0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -0.635) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 -1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at 0 -1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 0 -0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (pad 2 smd rect (at 0 0.635) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (pad 2 smd rect (at 0 1.905) (size 1.25 0.5) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (pad 3 smd rect (at 3.555 0) (size 3.65 4.31) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 5.77 1.905) (size 0.79 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PQFN5x6B (layer F.Cu) (tedit 58EE58E8)
    (at 114.005 85.7 180)
    (fp_text reference Q6 (at -3.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at 2.75 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 5.77 -0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (pad 3 smd rect (at 5.77 0.635 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (pad 3 smd rect (at 5.77 1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (pad 1 smd rect (at 0 1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0 0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -0.635 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0 -1.905 180) (size 1.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 3.555 0 180) (size 3.65 4.31) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (pad 3 smd rect (at 5.77 -1.905 180) (size 0.79 0.5) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.01 0.098 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:2512R (layer B.Cu) (tedit 58EE5A7D)
    (at 101 91)
    (fp_text reference R1 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 3 smd rect (at -2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(R1-Pad3)"))
    (pad 4 smd rect (at 2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(R1-Pad4)"))
    (pad 1 smd rect (at -2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (pad 1 smd rect (at -2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:2512R (layer B.Cu) (tedit 58EE59EF)
    (at 101 85.8)
    (fp_text reference R3 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 3 smd rect (at -2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(R3-Pad3)"))
    (pad 4 smd rect (at 2.5 0) (size 3.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(R3-Pad4)"))
    (pad 1 smd rect (at -2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 2.5 1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (pad 1 smd rect (at -2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 2.5 -1.4) (size 3.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE5957)
    (at 100.9 91 180)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55 180) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1-Pad4)"))
    (pad 7 smd rect (at 2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 6 smd rect (at 2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 5 smd rect (at 2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 57 I1))
    (pad 4 smd rect (at -2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1-Pad3)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE595E)
    (at 101 96.25 180)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55 180) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(R2-Pad4)"))
    (pad 7 smd rect (at 2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 6 smd rect (at 2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 5 smd rect (at 2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 58 I2))
    (pad 4 smd rect (at -2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(R2-Pad3)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE594C)
    (at 101 85.75 180)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U6 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55 180) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(R3-Pad4)"))
    (pad 7 smd rect (at 2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 6 smd rect (at 2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 5 smd rect (at 2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 59 I3))
    (pad 4 smd rect (at -2.105 0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U6-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975 180) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(R3-Pad3)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A0C)
    (at 117.3 90.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A16)
    (at 117.3 94.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A06)
    (at 117.3 86.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module crf1:lqfp64_pad_mod (layer B.Cu) (tedit 58EE5A69)
    (at 84 91 90)
    (descr LQFP-64)
    (fp_text reference U7 (at 0 -1.143 90) (layer B.SilkS) hide)
    (fp_text value STM32F40X_LQFP64 (at 0 1.143 90) (layer B.SilkS) hide)
    (pad 4 smd rect (at -2.25044 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U7-Pad4)"))
    (pad 5 smd rect (at -1.75006 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(C30-Pad1)"))
    (pad 6 smd rect (at -1.24968 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(C31-Pad1)"))
    (pad 7 smd rect (at -0.7493 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 85 NRST))
    (pad 8 smd rect (at -0.24892 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 42 C1))
    (pad 1 smd rect (at -3.74904 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at -3.2512 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U7-Pad2)"))
    (pad 3 smd rect (at -2.75082 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U7-Pad3)"))
    (pad 17 smd rect (at 5.75056 -3.74904 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(C77-Pad2)"))
    (pad 18 smd rect (at 5.75056 -3.2512 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 19 smd rect (at 5.75056 -2.75082 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 20 smd rect (at 5.75056 -2.25044 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U7-Pad20)"))
    (pad 21 smd rect (at 5.75056 -1.75006 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U7-Pad21)"))
    (pad 22 smd rect (at 5.75056 -1.24968 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U7-Pad22)"))
    (pad 23 smd rect (at 5.75056 -0.7493 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U7-Pad23)"))
    (pad 24 smd rect (at 5.75056 -0.24892 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 90 TEMP_MOTOR))
    (pad 33 smd rect (at 3.74904 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U7-Pad33)"))
    (pad 34 smd rect (at 3.2512 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 60 LI1))
    (pad 35 smd rect (at 2.75082 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 62 LI2))
    (pad 36 smd rect (at 2.25044 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 64 LI3))
    (pad 37 smd rect (at 1.75006 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 80 HALL_1))
    (pad 38 smd rect (at 1.24968 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 81 HALL_2))
    (pad 39 smd rect (at 0.7493 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 82 HALL_3))
    (pad 40 smd rect (at 0.24892 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U7-Pad40)"))
    (pad 49 smd rect (at -5.75056 3.74904 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 83 SWCLK))
    (pad 50 smd rect (at -5.75056 3.2512 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U7-Pad50)"))
    (pad 51 smd rect (at -5.75056 2.75082 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U7-Pad51)"))
    (pad 52 smd rect (at -5.75056 2.25044 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U7-Pad52)"))
    (pad 53 smd rect (at -5.75056 1.75006 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U7-Pad53)"))
    (pad 54 smd rect (at -5.75056 1.24968 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U7-Pad54)"))
    (pad 55 smd rect (at -5.75056 0.7493 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U7-Pad55)"))
    (pad 56 smd rect (at -5.75056 0.24892 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U7-Pad56)"))
    (pad 9 smd rect (at 0.24892 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 43 C2))
    (pad 10 smd rect (at 0.7493 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 44 C3))
    (pad 11 smd rect (at 1.24968 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 48 SENS_SUPPLY))
    (pad 25 smd rect (at 5.75056 0.24892 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U7-Pad25)"))
    (pad 26 smd rect (at 5.75056 0.7493 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 78 LED_GREEN))
    (pad 27 smd rect (at 5.75056 1.24968 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 79 LED_RED))
    (pad 41 smd rect (at -0.24892 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 61 HI1))
    (pad 42 smd rect (at -0.7493 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 63 HI2))
    (pad 43 smd rect (at -1.24968 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 65 HI3))
    (pad 57 smd rect (at -5.75056 -0.24892 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 88 SERVO))
    (pad 58 smd rect (at -5.75056 -0.7493 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U7-Pad58)"))
    (pad 59 smd rect (at -5.75056 -1.24968 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U7-Pad59)"))
    (pad 12 smd rect (at 1.75006 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 13 smd rect (at 2.25044 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 14 smd rect (at 2.75082 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 54 SENS_1))
    (pad 15 smd rect (at 3.2512 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 55 SENS_2))
    (pad 16 smd rect (at 3.74904 -5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 56 SENS_3))
    (pad 28 smd rect (at 5.75056 1.75006 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U7-Pad28)"))
    (pad 29 smd rect (at 5.75056 2.25044 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U7-Pad29)"))
    (pad 30 smd rect (at 5.75056 2.75082 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U7-Pad30)"))
    (pad 31 smd rect (at 5.75056 3.2512 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(C17-Pad2)"))
    (pad 32 smd rect (at 5.75056 3.74904 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 44 smd rect (at -1.75006 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 74 USB-DM))
    (pad 45 smd rect (at -2.25044 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 75 USB-DP))
    (pad 46 smd rect (at -2.75082 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 84 SWDIO))
    (pad 47 smd rect (at -3.2512 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(C18-Pad2)"))
    (pad 48 smd rect (at -3.74904 5.75056 90) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 60 smd rect (at -5.75056 -1.75006 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 61 smd rect (at -5.75056 -2.25044 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 91 RX))
    (pad 62 smd rect (at -5.75056 -2.75082 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 92 TX))
    (pad 63 smd rect (at -5.75056 -3.2512 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 64 smd rect (at -5.75056 -3.74904 90) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/bldc-hardware-master/design/Libraries/3D/lqfp-64.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A24)
    (at 123.7 91 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A22)
    (at 123.7 95.25 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A29)
    (at 123.7 86.75 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE593A)
    (at 101.05 94 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE593D)
    (at 100.95 88.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE592F)
    (at 101 83.65 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:WSON (layer B.Cu) (tedit 58EE5A12)
    (at 120.5 91 90)
    (fp_text reference U1 (at 0 -5 90) (layer B.SilkS) hide)
    (fp_text value LM5107 (at 0 3.81 90) (layer B.Fab))
    (pad 7 smd rect (at 0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R6-Pad2)"))
    (pad 4 smd rect (at 0 0 90) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 39 SH1))
    (pad 5 smd rect (at -1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R7-Pad2)"))
    (pad 8 smd rect (at 1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 LI1))
    (pad 2 smd rect (at 0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 HI1))
    (pad 1 smd rect (at 1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 4 smd rect (at -1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz 0.08 0.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module kicad_subory:WSON (layer B.Cu) (tedit 58EE5A1C)
    (at 120.5 95.25 90)
    (fp_text reference U2 (at 0 -5 90) (layer B.SilkS) hide)
    (fp_text value LM5107 (at 0 3.81 90) (layer B.Fab))
    (pad 7 smd rect (at 0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R8-Pad2)"))
    (pad 4 smd rect (at 0 0 90) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 SH2))
    (pad 5 smd rect (at -1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(R9-Pad2)"))
    (pad 8 smd rect (at 1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 62 LI2))
    (pad 2 smd rect (at 0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 HI2))
    (pad 1 smd rect (at 1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 4 smd rect (at -1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz 0.08 0.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module kicad_subory:WSON (layer B.Cu) (tedit 58EE5A08)
    (at 120.5 86.75 90)
    (fp_text reference U3 (at 0 -5 90) (layer B.SilkS) hide)
    (fp_text value LM5107 (at 0 3.81 90) (layer B.Fab))
    (pad 7 smd rect (at 0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(R10-Pad2)"))
    (pad 4 smd rect (at 0 0 90) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -0.4 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 SH3))
    (pad 5 smd rect (at -1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R11-Pad2)"))
    (pad 8 smd rect (at 1.2 -1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 LI3))
    (pad 2 smd rect (at 0.4 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 HI3))
    (pad 1 smd rect (at 1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 69 +9V))
    (pad 4 smd rect (at -1.2 1.9 90) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz 0.08 0.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A70)
    (at 92 97.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 4n7 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 42 C1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A83)
    (at 92 92.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 4n7 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 43 C2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A76)
    (at 92 87 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 4n7 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 44 C3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A78)
    (at 90 84.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A6C)
    (at 90 97.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A7A)
    (at 78 84.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE59AC)
    (at 79.2 95.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 85 NRST))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A56)
    (at 78 97.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE597D)
    (at 85.3 95.65)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 SENS_SUPPLY))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE598C)
    (at 82.3 95.65)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 SENS_SUPPLY))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A26)
    (at 115.9 90.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A19)
    (at 116.65 92.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A73)
    (at 115.9 94.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A1F)
    (at 116.7 96.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A2B)
    (at 115.9 86.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A10)
    (at 116.7 88.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE594F)
    (at 104.5 89.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 SENS_1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 SH1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE594A)
    (at 104.5 92.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 SENS_1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5959)
    (at 104.5 95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 SENS_2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 SH2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE595C)
    (at 104.5 97.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 SENS_2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5941)
    (at 104.5 84.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 SENS_3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 SH3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5945)
    (at 104.5 87 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 SENS_3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE59F3)
    (at 92 95.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 100R (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 I1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 C1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE59F6)
    (at 92 89.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 100R (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 58 I2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 C2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE59FA)
    (at 92 84.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 100R (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 I3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 C3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A6)
    (at 81.7 88.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE59BA)
    (at 79 92.75 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C24 (at 0 -2.3 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5989)
    (at 84 92.75 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C25 (at 0 -2.3 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58EE5987)
    (at 81.5 92.75 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value D_Schottky (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/0sod-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PFD3215 (layer F.Cu) (tedit 58EE5995)
    (at 83.7 88.75 90)
    (fp_text reference L1 (at 0 5.3 90) (layer F.SilkS) hide)
    (fp_text value PFD3215 (at -0.1 -5.3 90) (layer F.Fab))
    (pad 4 smd rect (at -1.425 -0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 1 smd rect (at -1.425 0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 3 smd rect (at 1.425 -0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.425 0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C23-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.06 1.4 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A9)
    (at 79.2 86.35 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 510R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A1)
    (at 83.8 86.35 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 8k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58EE59A3)
    (at 79.5 88.7 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U8 (at 0 -2.9 270) (layer F.SilkS) hide)
    (fp_text value BD9G101G (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C23-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C22-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 93 EN))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C23-Pad1)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59BD)
    (at 81.5 86.35)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C22-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59C0)
    (at 88.9 86.35 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 220n (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE599B)
    (at 89.2 88.7 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C27-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5978)
    (at 91.5 92.75 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C29 (at 0 -2.3 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58EE5975)
    (at 89.2 92.8 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value D_Schottky (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/0sod-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:PFD3215 (layer F.Cu) (tedit 58EE5935)
    (at 91.2 88.7 90)
    (fp_text reference L2 (at 0 5.3 90) (layer F.SilkS) hide)
    (fp_text value PFD3215 (at -0.1 -5.3 90) (layer F.Fab))
    (pad 4 smd rect (at -1.425 -0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 1 smd rect (at -1.425 0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 3 smd rect (at 1.425 -0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C27-Pad1)"))
    (pad 2 smd rect (at 1.425 0.7365 90) (size 0.61 0.711) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C27-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.06 1.4 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5999)
    (at 86.5 86.35 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 750R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE598F)
    (at 91.3 85.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 2k55 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C26-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58EE5993)
    (at 86.8 88.75 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U9 (at 0 -2.9 270) (layer F.SilkS) hide)
    (fp_text value BD9G101G (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C27-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(C26-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C27-Pad1)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EFBE8E)
    (at 84.25 83.5)
    (fp_text reference P9 (at 0 9.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5) (layer F.Fab) hide)
    (pad 3 thru_hole rect (at 0.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 81 HALL_2))
    (pad 4 thru_hole rect (at -0.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 82 HALL_3))
    (pad 2 thru_hole rect (at 2.25 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 80 HALL_1))
    (pad 1 thru_hole rect (at 3.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 47 VCC))
    (pad 5 thru_hole rect (at -2.25 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 90 TEMP_MOTOR))
    (pad 6 thru_hole rect (at -3.75 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EE599E)
    (at 84.25 98.5 180)
    (fp_text reference P10 (at 0 9.5 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5 180) (layer F.Fab))
    (pad 3 thru_hole rect (at 0.75 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 SWDIO))
    (pad 4 thru_hole rect (at -0.75 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 83 SWCLK))
    (pad 2 thru_hole rect (at 2.25 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 73 "Net-(P10-Pad2)"))
    (pad 1 thru_hole rect (at 3.75 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 89 "Net-(P10-Pad1)"))
    (pad 5 thru_hole rect (at -2.25 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 85 NRST))
    (pad 6 thru_hole rect (at -3.75 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5973)
    (at 91.4 96)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 22R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(P10-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 USB-DM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE597B)
    (at 88.3 95.65)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 22R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(P10-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 USB-DP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE596F)
    (at 91.4 97.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 LED_GREEN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59C5)
    (at 91.3 84.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 LED_RED))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59C2)
    (at 91.3 83.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 220R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5965)
    (at 91.4 98.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 220R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A58)
    (at 74.5 89.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 18p (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A5B)
    (at 74.5 92.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 18p (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:5x3.2KRISTALL (layer B.Cu) (tedit 58EE5B34)
    (at 71.5 91 270)
    (fp_text reference X1 (at 0.25908 1.23952 270) (layer B.SilkS) hide)
    (fp_text value CRYSTAL_SMD (at 0.10922 -1.48082 270) (layer B.SilkS) hide)
    (pad 3 smd rect (at -1.99898 1.19888 270) (size 1.80086 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.99898 1.19888 270) (size 1.80086 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(C31-Pad1)"))
    (pad 1 smd rect (at -1.99898 -1.19888 270) (size 1.80086 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(C30-Pad1)"))
    (pad 3 smd rect (at 1.99898 -1.19888 270) (size 1.80086 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Crystals.3dshapes/Crystal_SMD_5032_4Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A46)
    (at 135.5 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A4B)
    (at 128.6 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A48)
    (at 133.2 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A41)
    (at 128.6 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C13 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A35)
    (at 128.6 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C33 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A3D)
    (at 128.6 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C34 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A31)
    (at 133.2 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C37 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A2F)
    (at 135.5 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C38 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE585F)
    (at 133.2 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C40 (at -0.85 -10.5 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE585B)
    (at 135.5 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C41 (at -0.85 -7.05 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58DD)
    (at 133.2 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C42 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58E1)
    (at 135.5 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C43 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5879)
    (at 124 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C44 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE588A)
    (at 124 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C45 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A5)
    (at 124 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C46 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58C7)
    (at 124 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C47 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5920)
    (at 120 82.45 180)
    (fp_text reference P7 (at 2 1 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.4 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 0.4 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 0.4 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5910)
    (at 120 97.35 180)
    (fp_text reference P8 (at 2 1 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.4 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 0.4 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 0.4 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.1 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 1.8 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 2.5 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.2 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -1.8 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -1.1 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 1 thru_hole rect (at 3.9 -0.4 180) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5873)
    (at 126.3 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C48 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5890)
    (at 126.3 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C49 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A9)
    (at 126.3 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C50 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58CA)
    (at 126.3 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C51 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE586D)
    (at 128.6 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C52 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5894)
    (at 128.6 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C53 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58AF)
    (at 128.6 93.05 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C54 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58CE)
    (at 128.6 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C55 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5869)
    (at 130.9 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C56 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5898)
    (at 130.9 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C57 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58BB)
    (at 130.9 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C58 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58D4)
    (at 130.9 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C59 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A4A)
    (at 130.9 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C64 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A3F)
    (at 130.9 89 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C65 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A3B)
    (at 130.9 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C66 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A33)
    (at 130.9 97 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C67 (at 0 1.85 90) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EE59B2)
    (at 76.5 91 270)
    (fp_text reference P11 (at 0 9.5 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5 270) (layer F.Fab))
    (pad 3 thru_hole rect (at 0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 91 RX))
    (pad 4 thru_hole rect (at -0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 92 TX))
    (pad 2 thru_hole rect (at 2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 94 servoi))
    (pad 1 thru_hole rect (at 3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 47 VCC))
    (pad 5 thru_hole rect (at -2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 93 EN))
    (pad 6 thru_hole rect (at -3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE587D)
    (at 121.5 85 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C68 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58F0)
    (at 121.5 89.05 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C69 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5914)
    (at 121.5 96.95 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C70 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A1)
    (at 121.5 93 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C71 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5886)
    (at 119 86.75 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C72 (at 0 -1.85 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58FC)
    (at 119 95.25 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C73 (at 0 -1.85 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE58F4)
    (at 115.8 91)
    (fp_text reference P12 (at 2 1) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4) (layer F.Fab))
    (pad 1 smd rect (at 0.4 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 0.4 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 0.4 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.1 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.1 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.1 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.8 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.8 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 1.8 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 2.5 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 2.5 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 2.5 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.2 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.2 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.2 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.9 -1.8) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.9 -1.1) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at 3.9 -0.4) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5937)
    (at 96.6 93.9 90)
    (fp_text reference P1 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5969)
    (at 94.4 94 270)
    (fp_text reference P2 (at 2 1 270) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 37 "Net-(P2-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5932)
    (at 96.55 87.85 90)
    (fp_text reference P3 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5928)
    (at 105.5 89.8 270)
    (fp_text reference P4 (at 2 1 270) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 1.1 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 1.1 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 1.8 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 1.8 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 1.8 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 2.5 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 2.5 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 3.2 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 3.2 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
    (pad 1 thru_hole rect (at 3.2 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 39 SH1))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE592B)
    (at 107.7 98.9 90)
    (fp_text reference P5 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 40 SH2))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5924)
    (at 107.7 88.7 90)
    (fp_text reference P6 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 41 SH3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59AE)
    (at 76.5 97.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59B7)
    (at 73.1 89.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C76 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 SERVO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59B5)
    (at 73.1 92.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 100R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 servoi))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 SERVO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.27mm (layer F.Cu) (tedit 58EFBF79)
    (at 137 91)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference REF** (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch1.27mm (at 0 1.695) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.695) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.2 5.2) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5941615C)
    (at 75.8 84.7 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C77 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(C77-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59406798)
    (at 75.1 84.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C77-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59406C29)
    (at 106.4 84)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 10kNTC (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(C77-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59416163)
    (at 75.9 97.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 93 EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594197D1)
    (at 76.5 84.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C78 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 90 TEMP_MOTOR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594197CB)
    (at 77.9 84.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 90 TEMP_MOTOR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59498658)
    (at 86.7 91.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R35-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(R35-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5949865D)
    (at 86.6 93.5)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U10 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value 2xfet (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R4-Pad2)"))
    (pad 5 smd rect (at 0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(R35-Pad2)"))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 +9V))
    (pad 4 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R35-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7 0.7 0.7))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text LM5107 (at 120.45 85.05) (layer B.SilkS))
  (gr_text LM5107 (at 120.5 89.3) (layer B.SilkS))
  (gr_text LM5107 (at 120.55 93.55) (layer B.SilkS))
  (gr_text "BENJAMIN VEDDER VESC CLONE" (at 84.25 94.8) (layer B.SilkS))
  (gr_text OpenScooter.com (at 83.9 90.05) (layer B.SilkS))
  (gr_text antonchromjak@gmail.com (at 84.05 87.35) (layer B.SilkS))
  (gr_text STM32F405RGT6V (at 83.95 92.75) (layer B.SilkS))
  (gr_text ABM3B8MHz (at 71.5 91.05 90) (layer B.SilkS))
  (gr_text 10p (at 74.55 92.65) (layer B.SilkS))
  (gr_text 10p (at 74.5 89.25) (layer B.SilkS))
  (gr_text DNP (at 75.95 97.35) (layer B.SilkS))
  (gr_text 2u2 (at 75.8 84.7) (layer B.SilkS))
  (gr_text 2u2 (at 78 84.7) (layer B.SilkS))
  (gr_text 2u2 (at 78 97.3) (layer B.SilkS))
  (gr_text 2u2 (at 90 97.2) (layer B.SilkS))
  (gr_text 2u2 (at 90 84.8) (layer B.SilkS))
  (gr_text 4n7 (at 92 87.05) (layer B.SilkS))
  (gr_text 4n7 (at 92 92.55) (layer B.SilkS))
  (gr_text 4n7 (at 92 98) (layer B.SilkS))
  (gr_text 100R (at 92 95.25) (layer B.SilkS))
  (gr_text 100R (at 92 89.75) (layer B.SilkS))
  (gr_text 100R (at 92 84.3) (layer B.SilkS))
  (gr_text IRFH7004 (at 109.65 85.6 90) (layer B.SilkS))
  (gr_text IRFH7004 (at 109.65 90.9 90) (layer B.SilkS))
  (gr_text IRFH7004 (at 109.7 96.2 90) (layer B.SilkS))
  (gr_text 7R5 (at 116.7 96.3) (layer B.SilkS))
  (gr_text 7R5 (at 115.9 94.25) (layer B.SilkS))
  (gr_text 7R5 (at 116.65 92.3) (layer B.SilkS))
  (gr_text 7R5 (at 115.9 90.25) (layer B.SilkS))
  (gr_text 7R5 (at 116.7 88.3) (layer B.SilkS))
  (gr_text 7R5 (at 115.9 86.25) (layer B.SilkS))
  (gr_text 220n (at 117.25 86.25) (layer B.SilkS))
  (gr_text 220n (at 117.3 90.25) (layer B.SilkS))
  (gr_text 220n (at 117.3 94.25) (layer B.SilkS))
  (gr_text 2u2 (at 123.7 95.25) (layer B.SilkS))
  (gr_text 2u2 (at 123.7 91) (layer B.SilkS))
  (gr_text 2u2 (at 123.7 86.75) (layer B.SilkS))
  (gr_text R001 (at 101.05 95.3) (layer B.SilkS))
  (gr_text R001 (at 101.05 90.05) (layer B.SilkS))
  (gr_text R001 (at 101.05 84.95) (layer B.SilkS))
  (gr_text 10uF (at 135.5 97) (layer B.SilkS))
  (gr_text 10uF (at 133.25 97) (layer B.SilkS))
  (gr_text 10uF (at 130.9 96.95) (layer B.SilkS))
  (gr_text 10uF (at 128.6 97) (layer B.SilkS))
  (gr_text 10uF (at 130.9 93) (layer B.SilkS))
  (gr_text 10uF (at 128.6 93.1) (layer B.SilkS))
  (gr_text 10uF (at 130.9 89.05) (layer B.SilkS))
  (gr_text 10uF (at 128.55 88.95) (layer B.SilkS))
  (gr_text 10uF (at 135.5 84.95) (layer B.SilkS))
  (gr_text 10uF (at 133.2 84.95) (layer B.SilkS))
  (gr_text 10uF (at 130.95 84.9) (layer B.SilkS))
  (gr_text 10uF (at 128.6 84.95) (layer B.SilkS))
  (gr_text BSS8402DW (at 86.7 93.5 90) (layer F.SilkS))
  (gr_text 2u2 (at 101.05 94) (layer F.SilkS))
  (gr_text 2u2 (at 100.95 88.7) (layer F.SilkS))
  (gr_text 2u2 (at 101 83.7) (layer F.SilkS))
  (gr_text 10kN (at 106.4 84) (layer F.SilkS))
  (gr_text 24k9 (at 104.5 95) (layer F.SilkS))
  (gr_text 2k2 (at 104.5 97.8) (layer F.SilkS))
  (gr_text 2k2 (at 104.5 87) (layer F.SilkS))
  (gr_text 24k9 (at 104.5 84.8) (layer F.SilkS))
  (gr_text 24k9 (at 104.5 89.8) (layer F.SilkS))
  (gr_text 2k2 (at 104.5 92.3) (layer F.SilkS))
  (gr_text AD8418 (at 101.1 95.6) (layer F.SilkS))
  (gr_text AD8418 (at 100.9 90.2) (layer F.SilkS))
  (gr_text AD8418 (at 101 85) (layer F.SilkS))
  (gr_text IRFH7004 (at 112.9 96.2 90) (layer F.SilkS))
  (gr_text IRFH7004 (at 112.9 90.9 90) (layer F.SilkS))
  (gr_text IRFH7004 (at 112.9 85.8 90) (layer F.SilkS))
  (gr_text 100R (at 73.1 92.3) (layer F.SilkS))
  (gr_text 100n (at 73.1 89.7) (layer F.SilkS))
  (gr_text RB060M (at 89.2 92) (layer F.SilkS))
  (gr_text RB060M (at 81.5 91.9) (layer F.SilkS))
  (gr_text BD9G101G (at 86.6 88.9) (layer F.SilkS))
  (gr_text BD9G101G (at 79.3 88.9) (layer F.SilkS))
  (gr_text 10uH (at 91.2 89.5) (layer F.SilkS))
  (gr_text 10uH (at 83.7 89.5) (layer F.SilkS))
  (gr_text 15nF (at 89.2 88.7) (layer F.SilkS))
  (gr_text 15nF (at 81.7 88.8) (layer F.SilkS))
  (gr_text 10k (at 77.9 84.5) (layer F.SilkS))
  (gr_text 2u2 (at 76.5 84.5) (layer F.SilkS))
  (gr_text 10k (at 75.1 84.5) (layer F.SilkS))
  (gr_text 10uF (at 135.6 97) (layer F.SilkS))
  (gr_text 10uF (at 133.3 97) (layer F.SilkS))
  (gr_text 10uF (at 131 97) (layer F.SilkS))
  (gr_text 10uF (at 128.7 97) (layer F.SilkS))
  (gr_text 10uF (at 126.3 97) (layer F.SilkS))
  (gr_text 10uF (at 124.1 97) (layer F.SilkS))
  (gr_text 10uF (at 121.6 97) (layer F.SilkS))
  (gr_text 10uF (at 119 95.1) (layer F.SilkS))
  (gr_text 10uF (at 124 93.1) (layer F.SilkS))
  (gr_text 10uF (at 126.3 93) (layer F.SilkS))
  (gr_text 10uF (at 128.6 93.2) (layer F.SilkS))
  (gr_text 10uF (at 131 93) (layer F.SilkS))
  (gr_text 10uF (at 130.9 89) (layer F.SilkS))
  (gr_text 10uF (at 128.6 88.9) (layer F.SilkS))
  (gr_text 10uF (at 126.3 88.9) (layer F.SilkS))
  (gr_text 10uF (at 124.1 89) (layer F.SilkS))
  (gr_text 10uF (at 121.6 89.1) (layer F.SilkS))
  (gr_text 10uF (at 119 86.8) (layer F.SilkS))
  (gr_text 10uF (at 135.5 84.9) (layer F.SilkS))
  (gr_text 10uF (at 133.2 84.9) (layer F.SilkS))
  (gr_text 10uF (at 130.9 84.9) (layer F.SilkS))
  (gr_text 10uF (at 128.6 84.9) (layer F.SilkS))
  (gr_text 10uF (at 126.4 84.9) (layer F.SilkS))
  (gr_text 10uF (at 124 84.9) (layer F.SilkS))
  (gr_text 10uF (at 121.6 84.9) (layer F.SilkS))
  (gr_text 10uF (at 84.1 92.8) (layer F.SilkS))
  (gr_text 10uF (at 91.6 92.7) (layer F.SilkS))
  (gr_text 10uF (at 79 92.9) (layer F.SilkS))
  (gr_text DNP (at 76.5 97.4) (layer F.SilkS))
  (gr_text 100k (at 78.1 97.4) (layer F.SilkS))
  (gr_text 100n (at 79.2 95.7) (layer F.SilkS))
  (gr_text 2k2 (at 82.3 95.7) (layer F.SilkS))
  (gr_text 24k9 (at 85.3 95.7) (layer F.SilkS))
  (gr_text 22R (at 88.3 95.7) (layer F.SilkS))
  (gr_text 22R (at 91.4 96) (layer F.SilkS))
  (gr_text 220R (at 91.4 97.3) (layer F.SilkS))
  (gr_text 220R (at 91.3 84.5) (layer F.SilkS))
  (gr_text 2k55 (at 91.3 85.8) (layer F.SilkS))
  (gr_text 220n (at 88.9 86.4) (layer F.SilkS))
  (gr_text 750R (at 86.5 86.4) (layer F.SilkS))
  (gr_text 8k (at 83.8 86.4) (layer F.SilkS))
  (gr_text 100n (at 81.5 86.4) (layer F.SilkS))
  (gr_text 510R (at 79.2 86.4) (layer F.SilkS))
  (gr_arc (start 137 85) (end 137 82) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_text L3 (at 93.95 85.65 90) (layer F.SilkS))
  (gr_text L2 (at 94 91.75 90) (layer F.SilkS))
  (gr_text L1 (at 94 96.1 90) (layer F.SilkS))
  (gr_text VDD (at 115.25 83.6 90) (layer F.SilkS))
  (gr_text VDD (at 115.2 98.2 90) (layer F.SilkS))
  (gr_text GND (at 115.3 89.85 90) (layer F.SilkS))
  (gr_text VCC (at 88 84.8 90) (layer F.SilkS))
  (gr_text HALL1 (at 86.55 84.8 90) (layer F.SilkS))
  (gr_text HALL2 (at 85.05 84.85 90) (layer F.SilkS))
  (gr_text HALL3 (at 83.5 84.85 90) (layer F.SilkS))
  (gr_text TEMP (at 82 84.85 90) (layer F.SilkS))
  (gr_text GND (at 80.5 84.8 90) (layer F.SilkS))
  (gr_text VCC (at 75.1 94.65 90) (layer F.SilkS))
  (gr_text SERVO (at 75.1 93.25 90) (layer F.SilkS))
  (gr_text RX (at 75.1 91.7 90) (layer F.SilkS))
  (gr_text TX (at 75.1 90.25 90) (layer F.SilkS))
  (gr_text EN (at 75.05 88.7 90) (layer F.SilkS))
  (gr_text GND (at 75.05 87.25 90) (layer F.SilkS))
  (gr_text USBP (at 82.1 97.2 90) (layer F.SilkS))
  (gr_text USBM (at 80.55 97.2 90) (layer F.SilkS))
  (gr_text GND (at 88.05 97.3 90) (layer F.SilkS))
  (gr_text NRST (at 86.55 97.2 90) (layer F.SilkS))
  (gr_text SWCLK (at 85.05 97.1 90) (layer F.SilkS))
  (gr_text SWDIO (at 83.55 97.1 90) (layer F.SilkS))
  (gr_arc (start 71 85) (end 68 85) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 71 97) (end 71 100) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 137 97) (end 140 97) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 68 85) (end 68 97) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 140 85) (end 140 97) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 71 100) (end 137 100) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 71 82) (end 137 82) (layer Edge.Cuts) (width 0.001))
  (dimension 72 (width 0.3) (layer Dwgs.User)
    (gr_text "72.000 mm" (at 103.970639 78.644215) (layer Dwgs.User))
    (feature1 (pts (xy 67.970639 81.994215) (xy 67.970639 77.294215)))
    (feature2 (pts (xy 139.970639 81.994215) (xy 139.970639 77.294215)))
    (crossbar (pts (xy 139.970639 79.994215) (xy 67.970639 79.994215)))
    (arrow1a (pts (xy 67.970639 79.994215) (xy 69.097143 79.407794)))
    (arrow1b (pts (xy 67.970639 79.994215) (xy 69.097143 80.580636)))
    (arrow2a (pts (xy 139.970639 79.994215) (xy 138.844135 79.407794)))
    (arrow2b (pts (xy 139.970639 79.994215) (xy 138.844135 80.580636)))
  )
  (dimension 18 (width 0.3) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 64.65 90.956115 90) (layer Dwgs.User))
    (feature1 (pts (xy 68 81.956115) (xy 63.3 81.956115)))
    (feature2 (pts (xy 68 99.956115) (xy 63.3 99.956115)))
    (crossbar (pts (xy 66 99.956115) (xy 66 81.956115)))
    (arrow1a (pts (xy 66 81.956115) (xy 66.586421 83.082619)))
    (arrow1b (pts (xy 66 81.956115) (xy 65.413579 83.082619)))
    (arrow2a (pts (xy 66 99.956115) (xy 66.586421 98.829611)))
    (arrow2b (pts (xy 66 99.956115) (xy 65.413579 98.829611)))
  )
  (zone (net 36) (net_name "Net-(P1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.4 89) (xy 94.4 89) (xy 94.4 93) (xy 97.4 93)
      )
    )
  )
  (zone (net 38) (net_name "Net-(P3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.8 83.8) (xy 97.6 83.8) (xy 97.6 87.8) (xy 94.8 87.8)
      )
    )
  )
  (zone (net 37) (net_name "Net-(P2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.4 94.2) (xy 97.4 94.2) (xy 97.4 98.2) (xy 94.4 98.2)
      )
    )
  )
  (zone (net 38) (net_name "Net-(P3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.6 88.2) (xy 96.6 82) (xy 94.3 82) (xy 94.3 88.2)
      )
    )
  )
  (zone (net 37) (net_name "Net-(P2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.6 93.8) (xy 94.3 93.8) (xy 94.3 100) (xy 96.6 100)
      )
    )
  )
  (zone (net 36) (net_name "Net-(P1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.6 88.5) (xy 94.3 88.5) (xy 94.3 93.5) (xy 96.6 93.5)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 21)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.5 82) (xy 140 82) (xy 140 100) (xy 112.5 100)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.5 82) (xy 109.5 100) (xy 140 100) (xy 140 82)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (priority 30)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 82) (xy 115.7 82) (xy 115.7 84.6) (xy 118.1 85.8) (xy 136.4 85.8)
        (xy 136.4 87.1) (xy 133.166025 88.080905) (xy 120.7 90) (xy 120.7 92) (xy 133.123484 93.912649)
        (xy 136.6 95) (xy 136.6 96.1) (xy 118.2 96.2) (xy 115.7 97.4) (xy 115.7 100)
        (xy 140 100)
      )
    )
  )
  (zone (net 39) (net_name SH1) (layer B.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.3 93.5) (xy 109.3 88.5) (xy 101.3 88.5) (xy 101.3 93.5)
      )
    )
  )
  (zone (net 41) (net_name SH3) (layer B.Cu) (hatch edge 0.508)
    (priority 19)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.3 88.2) (xy 109.3 82) (xy 101.3 82) (xy 101.3 88.2)
      )
    )
  )
  (zone (net 40) (net_name SH2) (layer B.Cu) (hatch edge 0.508)
    (priority 19)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.3 93.8) (xy 109.3 100) (xy 101.3 100) (xy 101.3 93.8)
      )
    )
  )
  (zone (net 36) (net_name "Net-(P1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 88.5) (xy 101 93.5) (xy 93.5 93.5) (xy 93.5 88.5)
      )
    )
  )
  (zone (net 38) (net_name "Net-(P3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 19)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.9 88.2) (xy 100.9 82) (xy 93.5 82) (xy 93.5 88.25)
      )
    )
  )
  (zone (net 37) (net_name "Net-(P2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 19)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 93.75) (xy 93.5 93.75) (xy 93.5 100) (xy 101 100)
      )
    )
  )
  (zone (net 39) (net_name SH1) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.25 88.5) (xy 105.25 88.5) (xy 105.25 93.5) (xy 112.25 93.5)
      )
    )
  )
  (zone (net 41) (net_name SH3) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.3 88.2) (xy 112.3 83.6) (xy 107 83.6) (xy 107 84.5) (xy 105.3 84.5)
        (xy 105.3 88.2)
      )
    )
  )
  (zone (net 40) (net_name SH2) (layer F.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.3 93.8) (xy 112.3 98.4) (xy 105.3 98.4) (xy 105.3 93.8)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 100) (xy 140 82) (xy 68 82) (xy 68 100)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In2.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 82) (xy 140 100) (xy 68 100) (xy 68 82)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.4 82) (xy 115.4 83.5) (xy 93 83.5) (xy 93 98.6) (xy 115.4 98.6)
        (xy 115.4 100) (xy 68 100) (xy 68 82)
      )
    )
  )
  (zone (net 66) (net_name "Net-(C23-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 22)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.3 89.2) (xy 83.3 89.9) (xy 83.4 90.5) (xy 83.4 91.9) (xy 80.9 91.9)
        (xy 80.1 91.9) (xy 80.1 89.2)
      )
    )
  )
  (zone (net 67) (net_name "Net-(C23-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 26)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 87) (xy 80 88.3) (xy 82.2 88.3) (xy 82.2 87)
      )
    )
  )
  (zone (net 71) (net_name "Net-(C27-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 23)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.1 91.9) (xy 87.6 91.9) (xy 87.6 89.2) (xy 88.7 89.2) (xy 88.7 87.1)
        (xy 92.2 87.1) (xy 92.2 89.7) (xy 89.8 89.7) (xy 89.8 91.9)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (priority 22)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.8 89.2) (xy 79.8 91.9) (xy 78.1 91.9) (xy 78.1 90.5) (xy 78.1 89.2)
        (xy 79.1 89.2)
      )
    )
  )
  (zone (net 69) (net_name +9V) (layer F.Cu) (hatch edge 0.508)
    (priority 23)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.4 88.3) (xy 87.1 88.3) (xy 87.1 91.9) (xy 82.5 91.8) (xy 82.5 89.5)
        (xy 84.3 89.5) (xy 84.3 87.4) (xy 82.5 87.4) (xy 82.5 85.9) (xy 85.4 85.9)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 23)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.2 85.2) (xy 123 85.2) (xy 124.1 86.3) (xy 124.1 95.7) (xy 123 96.8)
        (xy 119.2 96.8)
      )
    )
  )
  (zone (net 47) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (priority 22)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.5 93.6) (xy 92.5 98.1) (xy 93.9 98.1) (xy 93.85 83.3) (xy 90.3 83.3)
        (xy 90.3 86.1) (xy 88.2 86.077962) (xy 88.2 89.8) (xy 90 89.8) (xy 90 93.6)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 22)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.7 86) (xy 136.3 86) (xy 136.3 86.9) (xy 132.8 88) (xy 130.3 88)
        (xy 127.7 88)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 22)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.7 94) (xy 130.3 94) (xy 132.9 94) (xy 136.4 95.1) (xy 136.4 96)
        (xy 127.7 96)
      )
    )
  )
  (zone (net 41) (net_name SH3) (layer In2.Cu) (hatch edge 0.508)
    (priority 25)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.7 87.9) (xy 118.3 87.9) (xy 118.3 86.5) (xy 118.3 85.2) (xy 105.7 85.2)
      )
    )
  )
  (zone (net 39) (net_name SH1) (layer In2.Cu) (hatch edge 0.508)
    (priority 25)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.6 90.6) (xy 118.4 90.6) (xy 118.4 93.3) (xy 105.6 93.3)
      )
    )
  )
  (zone (net 40) (net_name SH2) (layer In2.Cu) (hatch edge 0.508)
    (priority 25)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.6 95.4) (xy 107.6 95.4) (xy 108.7 94.3) (xy 118.3 94.3) (xy 118.3 96.4)
        (xy 110.3 96.4) (xy 107.6 98.1) (xy 105.6 98.1)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 21)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.75 83.35) (xy 105 83.35) (xy 105 98.6) (xy 112.75 98.6) (xy 112.75 100)
        (xy 68 100) (xy 68 82) (xy 112.75 82)
      )
    )
    (polygon
      (pts        (xy 93 83.35) (xy 93 98.25) (xy 96.9 98.25) (xy 96.9 83.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.95 87.9) (xy 136.05 88.05) (xy 135.25 88.45) (xy 134.55 89.1) (xy 134.1 89.9)
        (xy 133.9 90.75) (xy 134 91.75) (xy 134.25 92.45) (xy 134.7 93.1) (xy 135.3 93.6)
        (xy 135.9 93.9) (xy 136.45 94.05) (xy 137.15 94.1) (xy 138 93.95) (xy 138.7 93.6)
        (xy 139.2 93.2) (xy 139.7 92.55) (xy 140 91.85) (xy 140.1 91.15) (xy 140.05 90.45)
        (xy 139.8 89.7) (xy 139.45 89.1) (xy 138.95 88.6) (xy 138.3 88.2) (xy 137.7 88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.95 81.85) (xy 70.05 82.05) (xy 69.25 82.45) (xy 68.55 83.1) (xy 68.1 83.9)
        (xy 67.9 84.75) (xy 68 85.75) (xy 68.25 86.45) (xy 68.7 87.1) (xy 69.3 87.6)
        (xy 69.9 87.9) (xy 70.45 88.05) (xy 71.15 88.1) (xy 72 87.95) (xy 72.7 87.6)
        (xy 73.3 87.15) (xy 73.7 86.55) (xy 74 85.9) (xy 74.15 85.15) (xy 74.1 84.45)
        (xy 73.85 83.7) (xy 73.5 83.1) (xy 73.05 82.6) (xy 72.35 82.15) (xy 71.75 81.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.923685 93.907895) (xy 70.023685 94.057895) (xy 69.223685 94.457895) (xy 68.523685 95.107895) (xy 68.073685 95.907895)
        (xy 67.873685 96.757895) (xy 67.973685 97.757895) (xy 68.223685 98.457895) (xy 68.673685 99.107895) (xy 69.273685 99.607895)
        (xy 69.873685 99.907895) (xy 70.423685 100.057895) (xy 71.123685 100.107895) (xy 71.973685 99.957895) (xy 72.673685 99.607895)
        (xy 73.173685 99.207895) (xy 73.673685 98.557895) (xy 73.973685 97.857895) (xy 74.073685 97.157895) (xy 74.023685 96.457895)
        (xy 73.773685 95.707895) (xy 73.423685 95.107895) (xy 72.923685 94.607895) (xy 72.273685 94.207895) (xy 71.673685 94.007895)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.95 81.85) (xy 70.05 82.05) (xy 69.25 82.45) (xy 68.55 83.1) (xy 68.1 83.9)
        (xy 67.9 84.75) (xy 68 85.75) (xy 68.25 86.45) (xy 68.7 87.1) (xy 69.3 87.6)
        (xy 69.9 87.9) (xy 70.45 88.05) (xy 71.15 88.1) (xy 72 87.95) (xy 72.7 87.6)
        (xy 73.3 87.15) (xy 73.7 86.55) (xy 74 85.9) (xy 74.15 85.15) (xy 74.1 84.45)
        (xy 73.85 83.7) (xy 73.5 83.1) (xy 73.05 82.6) (xy 72.35 82.15) (xy 71.75 81.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.923685 93.907895) (xy 70.023685 94.057895) (xy 69.223685 94.457895) (xy 68.523685 95.107895) (xy 68.073685 95.907895)
        (xy 67.873685 96.757895) (xy 67.973685 97.757895) (xy 68.223685 98.457895) (xy 68.673685 99.107895) (xy 69.273685 99.607895)
        (xy 69.873685 99.907895) (xy 70.423685 100.057895) (xy 71.123685 100.107895) (xy 71.973685 99.957895) (xy 72.673685 99.607895)
        (xy 73.173685 99.207895) (xy 73.673685 98.557895) (xy 73.973685 97.857895) (xy 74.073685 97.157895) (xy 74.023685 96.457895)
        (xy 73.773685 95.707895) (xy 73.423685 95.107895) (xy 72.923685 94.607895) (xy 72.273685 94.207895) (xy 71.673685 94.007895)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch none 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.95 87.9) (xy 136.05 88.05) (xy 135.25 88.45) (xy 134.55 89.1) (xy 134.1 89.9)
        (xy 133.9 90.75) (xy 134 91.75) (xy 134.25 92.45) (xy 134.7 93.1) (xy 135.3 93.6)
        (xy 135.9 93.9) (xy 136.45 94.05) (xy 137.15 94.1) (xy 138 93.95) (xy 138.7 93.6)
        (xy 139.2 93.2) (xy 139.7 92.55) (xy 140 91.85) (xy 140.1 91.15) (xy 140.05 90.45)
        (xy 139.8 89.7) (xy 139.45 89.1) (xy 138.95 88.6) (xy 138.3 88.2) (xy 137.7 88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.38 84.91) (xy 68.38 95.34) (xy 68.4 99.49) (xy 71.05 99.73) (xy 72.66 99.62)
        (xy 136.96 99.62) (xy 138 99.41) (xy 138.84 98.85) (xy 139.41 98) (xy 139.62 96.96)
        (xy 139.62 85.04) (xy 139.41 83.99) (xy 138.85 83.15) (xy 138 82.58) (xy 136.96 82.38)
        (xy 71 82.38) (xy 72.32 73.87) (xy 149.52 72.79) (xy 152.29 114.43) (xy 44.96 115.66)
        (xy 46.2 74.64)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.38 84.91) (xy 68.38 95.34) (xy 68.4 99.49) (xy 71.05 99.73) (xy 72.66 99.62)
        (xy 136.96 99.62) (xy 138 99.41) (xy 138.84 98.85) (xy 139.41 98) (xy 139.62 96.96)
        (xy 139.62 85.04) (xy 139.41 83.99) (xy 138.85 83.15) (xy 138 82.58) (xy 136.96 82.38)
        (xy 71 82.38) (xy 72.32 73.87) (xy 149.52 72.79) (xy 152.29 114.43) (xy 44.96 115.66)
        (xy 46.2 74.64)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.38 84.91) (xy 68.38 95.34) (xy 68.4 99.49) (xy 71.05 99.73) (xy 72.66 99.62)
        (xy 136.96 99.62) (xy 138 99.41) (xy 138.84 98.85) (xy 139.41 98) (xy 139.62 96.96)
        (xy 139.62 85.04) (xy 139.41 83.99) (xy 138.85 83.15) (xy 138 82.58) (xy 136.96 82.38)
        (xy 71 82.38) (xy 72.32 73.87) (xy 149.52 72.79) (xy 152.29 114.43) (xy 44.96 115.66)
        (xy 46.2 74.64)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.38 84.91) (xy 68.38 95.34) (xy 68.4 99.49) (xy 71.05 99.73) (xy 72.66 99.62)
        (xy 136.96 99.62) (xy 138 99.41) (xy 138.84 98.85) (xy 139.41 98) (xy 139.62 96.96)
        (xy 139.62 85.04) (xy 139.41 83.99) (xy 138.85 83.15) (xy 138 82.58) (xy 136.96 82.38)
        (xy 71 82.38) (xy 72.32 73.87) (xy 149.52 72.79) (xy 152.29 114.43) (xy 44.96 115.66)
        (xy 46.2 74.64)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.8 85.5) (xy 123.3 85.5) (xy 123.3 87.9) (xy 121.8 87.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.8 89.8) (xy 123.3 89.8) (xy 123.3 92.2) (xy 121.8 92.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.8 94) (xy 123.3 94) (xy 123.3 95.6) (xy 123.1 96.1) (xy 122.7 96.3)
        (xy 121.8 96.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 82.9) (xy 81 82.9) (xy 81 82.8) (xy 80 82.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 84.1) (xy 81 84.1) (xy 81 84.2) (xy 80 84.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.9 84) (xy 79.9 83) (xy 79.8 83) (xy 79.8 84)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76 86.6) (xy 77.1 86.6) (xy 77.1 86.5) (xy 76 86.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.9 87.8) (xy 75.8 87.8) (xy 75.8 86.7) (xy 75.9 86.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 99) (xy 88.6 98) (xy 88.7 98) (xy 88.7 99)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.1 82.9) (xy 79.9 82.9) (xy 79.9 82.8) (xy 81.1 82.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.1 84.1) (xy 81.1 84.2) (xy 79.9 84.2) (xy 79.9 84.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.9 83.1) (xy 79.9 83.9) (xy 79.8 83.9) (xy 79.8 83.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.2 86.7) (xy 77.2 86.5) (xy 76 86.5) (xy 76 86.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.9 87.8) (xy 75.9 86.8) (xy 75.8 86.8) (xy 75.8 87.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.4 99.1) (xy 88.6 99.1) (xy 88.6 99.2) (xy 87.4 99.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 98.9) (xy 88.6 98) (xy 88.7 98) (xy 88.7 98.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.4 99.1) (xy 88.6 99.1) (xy 88.6 99.2) (xy 87.4 99.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 99) (xy 88.6 98) (xy 88.7 98) (xy 88.7 99)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.4 99.1) (xy 87.4 99.1) (xy 87.4 99.2) (xy 88.4 99.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.9 82.9) (xy 79.9 83.95) (xy 79.75 83.95) (xy 79.75 82.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.05 82.9) (xy 81 82.9) (xy 81 82.75) (xy 80.05 82.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 86.65) (xy 77.1 86.65) (xy 77.1 86.5) (xy 76.2 86.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.9 87.85) (xy 75.7 87.85) (xy 75.7 86.95) (xy 75.9 86.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 86.65) (xy 77.1 86.65) (xy 77.1 86.5) (xy 76.2 86.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.9 86.95) (xy 75.9 87.8) (xy 75.75 87.8) (xy 75.75 86.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 98) (xy 88.75 98) (xy 88.75 98.9) (xy 88.6 98.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.4 99.1) (xy 88.45 99.1) (xy 88.45 99.25) (xy 87.4 99.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.05 82.9) (xy 81 82.9) (xy 81 82.75) (xy 80.05 82.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.9 83.1) (xy 79.9 83.95) (xy 79.75 83.95) (xy 79.75 83.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.05 84.1) (xy 80.05 84.25) (xy 81.05 84.25) (xy 81.05 84.1)
      )
    )
  )
)
