<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>CFRX</text>
<text>CFTX</text>
<text>CFRX</text>
<text>CFTX</text>
<text>GND</text>
<text>5V</text>
<text>D-</text>
<text>D+</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>Yellow</text>
<text>5V</text>
<text>D+</text>
<text>D-</text>
<text>VCOM</text>
<text>5V</text>
<text>CS</text>
<text>GND</text>
<text>VCOM</text>
<text>GND</text>
<text>CS</text>
<wire x1="-1.5" y1="34.3" x2="-1.5" y2="12.2" width="0.2032" layer="20"/>
<wire x1="7.5" y1="-0.8" x2="7.6" y2="-0.8" width="0.2032" layer="20"/>
<wire x1="7.6" y1="-0.8" x2="22.4" y2="-0.8" width="0.2032" layer="20"/>
<wire x1="31.1" y1="12.1" x2="31.1" y2="34.4" width="0.2032" layer="20"/>
<wire x1="-1.5" y1="12.1" x2="5.6" y2="12.1" width="0.1524" layer="20"/>
<wire x1="5.6" y1="12.1" x2="5.6" y2="-0.8" width="0.1524" layer="20"/>
<wire x1="5.6" y1="-0.8" x2="7.6" y2="-0.8" width="0.1524" layer="20"/>
<wire x1="31.1" y1="12" x2="24.7" y2="12" width="0.1524" layer="20"/>
<wire x1="24.7" y1="12" x2="24.7" y2="-0.8" width="0.1524" layer="20"/>
<wire x1="24.7" y1="-0.8" x2="22.4" y2="-0.8" width="0.1524" layer="20"/>
<wire x1="22.4" y1="-0.8" x2="22.4" y2="-0.7" width="0.1524" layer="20"/>
<wire x1="24.6" y1="34.4" x2="31.1" y2="34.4" width="0.1524" layer="20"/>
<wire x1="5.4" y1="48.4" x2="8.4" y2="51.9" width="0.254" layer="20"/>
<wire x1="8.4" y1="51.9" x2="22" y2="51.9" width="0.254" layer="20"/>
<wire x1="22" y1="51.9" x2="24.5" y2="48.5" width="0.254" layer="20"/>
<text>Green</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<wire x1="-1.5" y1="34.3" x2="5.3" y2="34.3" width="0.254" layer="20"/>
<wire x1="5.4" y1="48.3" x2="5.4" y2="34.3" width="0.254" layer="20"/>
<wire x1="24.5" y1="48.4" x2="24.5" y2="34.3" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="headers(2mm)">
<packages>
<package name="1X10">
</package>
<package name="1X4">
</package>
</packages>
</library>
<library name="TinyPICO_NANO_Eagle">
<packages>
<package name="TINYPICO-NANO-CONNECTOR">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CF_DECK_LEFT" library="headers(2mm)" package="1X10" value="1X10"/>
<element name="U$4" library="TinyPICO_NANO_Eagle" package="TINYPICO-NANO-CONNECTOR" value="TINYPICO-NANO-CONNECTOR"/>
<element name="NANO_FLASH" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="REG" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TEENSY_UL" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TEENSY_LL" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TEENSY_UR" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="TEENSY_LR" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="DVS" library="headers(2mm)" package="1X4" value="1X4"/>
<element name="PAD1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD9" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD10" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD11" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD12" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD13" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD14" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD15" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD16" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD17" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD18" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="headers(2mm)" package="1X10" value="1X10"/>
</elements>
<signals>
<signal name="3V3">
<contactref element="U$4" pad="3V3"/>
</signal>
<signal name="RX1">
<contactref element="TEENSY_LR" pad="2"/>
<contactref element="CF_DECK_LEFT" pad="3"/>
</signal>
<signal name="TX1">
<contactref element="TEENSY_LR" pad="3"/>
<contactref element="CF_DECK_LEFT" pad="2"/>
</signal>
<signal name="IO_4">
<contactref element="CF_DECK_LEFT" pad="9"/>
</signal>
<signal name="GND">
<contactref element="CF_DECK_LEFT" pad="10"/>
<contactref element="TEENSY_LR" pad="1"/>
<contactref element="DVS" pad="1"/>
<contactref element="U$4" pad="GND$3"/>
<contactref element="U$4" pad="GND$2"/>
<contactref element="U$4" pad="GND$1"/>
<contactref element="U$4" pad="GND$4"/>
<contactref element="NANO_FLASH" pad="1"/>
<contactref element="REG" pad="2"/>
</signal>
<signal name="5V">
<contactref element="TEENSY_LL" pad="1"/>
<contactref element="DVS" pad="4"/>
<contactref element="U$4" pad="5V"/>
<contactref element="NANO_FLASH" pad="2"/>
<contactref element="REG" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U$4" pad="VBAT"/>
</signal>
<signal name="SCK">
<contactref element="TEENSY_UL" pad="3"/>
<contactref element="U$4" pad="IO18"/>
</signal>
<signal name="MISO">
<contactref element="TEENSY_UR" pad="3"/>
<contactref element="U$4" pad="IO19"/>
</signal>
<signal name="MOSI">
<contactref element="TEENSY_UR" pad="2"/>
<contactref element="U$4" pad="IO23"/>
</signal>
<signal name="CS">
<contactref element="TEENSY_UR" pad="1"/>
<contactref element="U$4" pad="IO5"/>
</signal>
<signal name="MTX_SRX">
<contactref element="DVS" pad="2"/>
<contactref element="TEENSY_UL" pad="2"/>
</signal>
<signal name="MRX_STX">
<contactref element="DVS" pad="3"/>
<contactref element="TEENSY_UL" pad="1"/>
</signal>
<signal name="D-">
<contactref element="NANO_FLASH" pad="3"/>
<contactref element="U$4" pad="D-"/>
</signal>
<signal name="D+">
<contactref element="NANO_FLASH" pad="4"/>
<contactref element="U$4" pad="D+"/>
</signal>
<signal name="VCOM">
<contactref element="U$1" pad="9"/>
<contactref element="REG" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
