<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<text>VCC</text>
<wire x1="25.4" y1="2.54" x2="0" y2="2.54" width="0.01" layer="20"/>
<text>(-)</text>
<text>(-)</text>
<text>B-</text>
<text>VCC</text>
<hole x="17.526" y="17.526" drill="3.683"/>
<hole x="8.128" y="33.782" drill="3.683"/>
<text>OMSI Permafrost Exhibit</text>
<text>Starboard RGB LED</text>
<text>OMSI Permafrost Exhibit</text>
<text>VCC</text>
<text>KCITG 10/26/17</text>
<text>Starboard RGB LED</text>
<wire x1="25.4" y1="2.54" x2="25.4" y2="35.56" width="0" layer="20"/>
<wire x1="25.4" y1="35.56" x2="22.86" y2="38.1" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="38.1" x2="2.54" y2="38.1" width="0" layer="20"/>
<wire x1="2.54" y1="38.1" x2="0" y2="35.56" width="0" layer="20" curve="90"/>
<wire x1="0" y1="35.56" x2="0" y2="2.54" width="0" layer="20"/>
<text>G-</text>
<text>R-</text>
<text>R+</text>
<text>G+</text>
<text>B+</text>
<text>G-</text>
<text>R-</text>
<text>B-</text>
<text>B+</text>
<text>G+</text>
<text>R+</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS-KIT">
</package>
</packages>
</library>
<library name="th_libraries">
<packages>
<package name="SMD-PAD">
</package>
<package name="LARGE_PAD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="U$1" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
<element name="U$2" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
<element name="U$3" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
<element name="U$4" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
<element name="U$5" library="th_libraries" package="LARGE_PAD" value="STARBOARD_HEAT_SINK"/>
<element name="J5" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="J6" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="U$6" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
<element name="U$7" library="th_libraries" package="SMD-PAD" value="SMD_PAD.05X.15"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="1"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="J3" pad="1"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="J4" pad="1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="J5" pad="1"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="J6" pad="1"/>
<contactref element="U$7" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
